(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Eurorack Mixer")
    (date "2022-12-22")
    (rev "1.0.1")
    (company "Len Popp")
    (comment 1 "Copyright © 2022 Len Popp CC BY")
    (comment 2 "Board settings comply with requirements of OSH Park https://oshpark.com/")
    (comment 3 "Eurorack 3:1 mixer module - 4HP")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/gerbers/")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "-12V")
  (net 4 "GAIN")
  (net 5 "Net-(C9-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C8-Pad1)")
  (net 8 "Net-(C9-Pad2)")
  (net 9 "LED-RED")
  (net 10 "LED-GREEN")
  (net 11 "OUT")
  (net 12 "IN-ATTEN-1")
  (net 13 "IN-ATTEN-2")
  (net 14 "IN-ATTEN-3")
  (net 15 "GAIN-ATTEN")
  (net 16 "Net-(R13-Pad1)")
  (net 17 "Net-(R14-Pad1)")
  (net 18 "Net-(R15-Pad1)")
  (net 19 "unconnected-(U2-Pad1)")
  (net 20 "unconnected-(U2-Pad5)")
  (net 21 "unconnected-(U2-Pad8)")
  (net 22 "VREF-5")
  (net 23 "VREF-4")
  (net 24 "VREF-LO")
  (footprint "-lmp-misc:Logo_CC_BY" locked (layer "F.Cu")
    (tedit 0)
    (at 188.595 128.27)
    (attr through_hole)
    (fp_text reference "G1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_CC_BY" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "-lmp-misc:Logo_OSHW" locked (layer "F.Cu")
    (tedit 60F495A1)
    (at 180.848 128.016)
    (descr "Open Source Hardware logo")
    (tags "Open Source Hardware logo")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_OSHW" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 190.881 107.95 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-4K7?qs=oAGoVhmvjhwCB3QIStJPAg%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-4K7")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-4K7")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R15" (at 10.668 0) (layer "F.SilkS"))
    (fp_text value "4K7" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "LED-RED") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 190.881 75.037 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at -1.671 0 180) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 183.642 78.994)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R10" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "GAIN-ATTEN") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 201.676 113.919 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Distributor" "Digi-Key")
    (property "Distributor2" "Mouser")
    (property "DistributorPartLink" "https://www.digikey.ca/en/products/detail/texas-instruments/TL071BCP/1674458")
    (property "DistributorPartLink2" "https://www.mouser.ca/ProductDetail/Texas-Instruments/TL071IPE4?qs=odmYgEirbwzwe%252BIRDerVMA%3D%3D")
    (property "DistributorPartNum" "296-34258-5-ND")
    (property "DistributorPartNum2" "595-TL071IPE4")
    (property "Manufacturer" "Texas Instruments")
    (property "ManufacturerPartNum" "TL071BCP")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "TL071" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "unconnected-(U2-Pad1)") (pinfunction "NULL") (pintype "input+no_connect"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "VREF-4") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U2-Pad5)") (pinfunction "NULL") (pintype "input+no_connect"))
    (pad "6" thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R15-Pad1)") (pintype "output"))
    (pad "7" thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "unconnected-(U2-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 194.056 66.548)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=vxEfx8VrU7BHurOY5iQdiA%3D%3D")
    (property "DistributorPartNum" "595-TL074BCN")
    (property "Manufacturer" "Texas Instruments")
    (property "ManufacturerPartNum" "TL074BCN")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "TL074" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GAIN") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad2)") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R13-Pad1)") (pintype "output"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "VREF-5") (pinfunction "+") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "VREF-LO") (pinfunction "-") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R14-Pad1)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 180.213 72.39)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R6" (at -2.413 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "IN-ATTEN-2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 190.5 111.379 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 5.461 0.127) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 180.213 65.786)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R8" (at -2.413 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GAIN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 190.373 96.647 90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=0lQeLiL1qyZS6rosZp7Ehg%3D%3D")
    (property "DistributorPartNum" "512-1N4148T50R")
    (property "Manufacturer" "On Semi / Fairchild")
    (property "ManufacturerPartNum" "1N4148-T50R")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at -2.032 0 180) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.032 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 199.730004 128.016)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Distributor" "Mouser")
    (property "Distributor2" "Thonk")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/667-ECE-A1VKS100I")
    (property "DistributorPartLink2" "https://www.thonk.co.uk/shop/eurorack-diy-essentials/")
    (property "DistributorPartNum" "667-ECE-A1VKS100I")
    (property "DistributorPartNum2" "Group_Eurorack_DIY_Essential")
    (property "Manufacturer" "Panasonic")
    (property "ManufacturerPartNum" "ECE-A1VKS100I")
    (property "Note" "12 V decoupling")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at -1.991004 2.413) (layer "F.SilkS"))
    (fp_text value "10U" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 186.436 85.979)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R11" (at -2.921 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 190.881 69.088 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=qe%2F8UmbcoTBh6wC284cfAA%3D%3D")
    (property "DistributorPartNum" "80-C315C569D1G")
    (property "Manufacturer" "KEMET")
    (property "ManufacturerPartNum" "C315C569D1G5TA")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "C0G/NP0")
    (attr through_hole)
    (fp_text reference "C7" (at 4.953 0 180) (layer "F.SilkS"))
    (fp_text value "5P6" (at 1.25 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GAIN") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 204.47 66.548)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-10K?qs=oAGoVhmvjhzLlUYKKBtdYQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-10K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-10K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R14" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "10K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "LED-GREEN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 186.436 89.027 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=oAGoVhmvjhzVx2bdEH1TLQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-25FBF52-51R")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-25FBF52-51R")
    (property "Note" "Output limiting")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "5%, 1/4 W")
    (attr through_hole)
    (fp_text reference "R12" (at 12.446 0 180) (layer "F.SilkS"))
    (fp_text value "51R" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "OUT") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 180.213 69.088)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R5" (at -2.413 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "IN-ATTEN-1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 207.752 71.882 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at -2.814 -0.127) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 205.272 75.565)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at 5.294 0) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 199.476004 118.618 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Distributor" "Mouser")
    (property "Distributor2" "Thonk")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/667-ECE-A1VKS100I")
    (property "DistributorPartLink2" "https://www.thonk.co.uk/shop/eurorack-diy-essentials/")
    (property "DistributorPartNum" "667-ECE-A1VKS100I")
    (property "DistributorPartNum2" "Group_Eurorack_DIY_Essential")
    (property "Manufacturer" "Panasonic")
    (property "ManufacturerPartNum" "ECE-A1VKS100I")
    (property "Note" "12 V decoupling")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 3.937 3.261004 180) (layer "F.SilkS"))
    (fp_text value "10U" (at 1.25 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 180.213 75.692)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R7" (at -2.413 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "IN-ATTEN-3") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 212.09 79.248 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R9" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 205.105 101.219)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-11K?qs=oAGoVhmvjhx1sOCa0IR7aA%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-11K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-11K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R2" (at 7.747 -2.413) (layer "F.SilkS"))
    (fp_text value "11K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "VREF-5") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "VREF-4") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 198.247 93.472)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/603-MFR-12FTF52-200R")
    (property "DistributorPartNum" "603-MFR-12FTF52-200R")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-200R")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R4" (at 10.033 0) (layer "F.SilkS"))
    (fp_text value "200R" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "VREF-LO") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 207.752 106.299 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at 1.25 -2.5) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 194.056 101.219)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-75K?qs=oAGoVhmvjhxG7qVOuGlgew%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-75K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-75K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R1" (at -2.286 0) (layer "F.SilkS"))
    (fp_text value "75K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "VREF-5") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 205.867 97.282 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-36K?qs=oAGoVhmvjhyIq6EO5blb%252BQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-36K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-36K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R3" (at -2.413 -0.127) (layer "F.SilkS"))
    (fp_text value "36K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "VREF-4") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "VREF-LO") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 183.261 114.808)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=0lQeLiL1qyZS6rosZp7Ehg%3D%3D")
    (property "DistributorPartNum" "512-1N4148T50R")
    (property "Manufacturer" "On Semi / Fairchild")
    (property "ManufacturerPartNum" "1N4148-T50R")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "LED-RED") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-synth:IDC-Header-Eurorack-10-TH" (layer "F.Cu")
    (tedit 61A6FCF9)
    (at 210.947 128.778 180)
    (descr "Through-hole Eurorack 10-pin board power bus connector, shrouded")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row Eurorack")
    (property "Distributor" "Mouser")
    (property "Distributor2" "Thonk")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Wurth-Elektronik/61201021621?qs=%2Fha2pyFadugkhyfdWLPRIwz9kroMfF%252BXZWEETFcVSqiQRaqHzEC2RQ%3D%3D")
    (property "DistributorPartLink2" "https://www.thonk.co.uk/shop/eurorack-diy-essentials/")
    (property "DistributorPartNum" "710-61201021621")
    (property "DistributorPartNum2" "523-G821EU210AAL10Y")
    (property "Manufacturer" "Wurth Elektronik")
    (property "ManufacturerPartNum" "61201021621")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 1.27 16.51) (layer "F.SilkS"))
    (fp_text value "Conn_Eurorack_10" (at 1.27 14.986) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 "-12V") (pinfunction "-12V") (pintype "power_in"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "power_in"))
    (pad "3" thru_hole circle locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole circle locked (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle locked (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "power_in"))
    (pad "7" thru_hole circle locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "power_in"))
    (pad "9" thru_hole circle locked (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "+12V") (pintype "power_in"))
    (pad "10" thru_hole circle locked (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "power_in"))
    (model "${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 201.676 89.154 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-10K?qs=oAGoVhmvjhzLlUYKKBtdYQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-10K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-10K")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R13" (at -2.921 0.127) (layer "F.SilkS"))
    (fp_text value "10K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "LED-GREEN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 188.742 82.423)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=qe%2F8UmbcoTBh6wC284cfAA%3D%3D")
    (property "DistributorPartNum" "80-C315C569D1G")
    (property "Manufacturer" "KEMET")
    (property "ManufacturerPartNum" "C315C569D1G5TA")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "C0G/NP0")
    (attr through_hole)
    (fp_text reference "C9" (at -2.814 0) (layer "F.SilkS"))
    (fp_text value "5P6" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Horizontal" (layer "B.Cu")
    (tedit 59FED5CB)
    (at 177.8 81.28 180)
    (descr "Through hole angled pin header, 1x09, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x09 2.54mm single row")
    (property "Distributor" "Adafruit")
    (property "Distributor2" "Mouser")
    (property "DistributorPartLink" "https://www.adafruit.com/product/1540")
    (property "DistributorPartLink2" "https://www.mouser.ca/ProductDetail/Amphenol-FCI/10129379-936001BLF?qs=0lQeLiL1qyaSuTs3FuCL%2FQ%3D%3D")
    (property "DistributorPartNum" "1540")
    (property "DistributorPartNum2" "649-1012937993601BLF")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 0 2.27) (layer "B.SilkS"))
    (fp_text value "Conn_PCB_Back" (at 4.385 -22.59) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -10.16 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "IN-ATTEN-1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "IN-ATTEN-2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "IN-ATTEN-3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GAIN") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GAIN-ATTEN") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "LED-GREEN") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "LED-RED") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "OUT") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 176.53 134.112) (end 176.53 60.96) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 176.53 60.96) (end 214.503 60.96) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 214.503 134.112) (end 176.53 134.112) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 214.503 60.96) (end 214.503 134.112) (layer "Edge.Cuts") (width 0.1524))
  (gr_text "© 2022 Len Popp" (at 178.435 123.825) (layer "F.SilkS"))
  (gr_text "-12V" (at 201.295 132.842) (layer "F.SilkS"))
  (gr_text "1Mix" (at 178.181 119.253) (layer "F.SilkS"))
  (gr_text "https://len42.github.io/Synth/" (at 183.515 62.23) (layer "F.SilkS"))
  (gr_text "rev. ${REVISION}" (at 178.308 121.793) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.381) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 215.686996 135.001)
        (xy 175.554996 135.001)
        (xy 175.554996 60.071)
        (xy 215.686996 60.071)
      )
    )
  )
)
