(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin 100 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "LOGO" (layer "F.Cu")
    (tedit 0)
    (at 100 100)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 19.5 -6.3) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (gr_arc (start 113 91.2) (mid 113.707107 91.492893) (end 114 92.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 87 91.2) (end 113 91.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113 108.8) (end 87 108.8) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 114 107.8) (mid 113.707107 108.507107) (end 113 108.8) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 87 108.8) (mid 86.292893 108.507107) (end 86 107.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 86 107.8) (end 86 92.2) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 86 92.2) (mid 86.29289 91.492886) (end 87 91.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 114 107.8) (end 114 92.2) (layer "Edge.Cuts") (width 0.1))
)
