(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(U1-VCC)")
	(net 2 "GND")
	(net 3 "Net-(D1-K)")
	(net 4 "Net-(U2-VCC)")
	(net 5 "Net-(U1-BIAS)")
	(net 6 "Net-(D1-A)")
	(net 7 "Net-(D2-A)")
	(net 8 "Net-(U1-MODE)")
	(net 9 "Net-(U1-RT)")
	(net 10 "Net-(U1-COMP)")
	(net 11 "Net-(C2-Pad1)")
	(net 12 "Net-(U1-FB)")
	(net 13 "Net-(R6-Pad2)")
	(net 14 "Net-(U2-FB)")
	(net 15 "Net-(U2-COMP)")
	(net 16 "Net-(U2-RT)")
	(net 17 "Net-(U2-MODE)")
	(net 18 "+3.3V")
	(net 19 "unconnected-(U1-NC-Pad12)")
	(net 20 "unconnected-(U1-NC-Pad15)")
	(net 21 "Net-(U1-PGOOD)")
	(net 22 "Net-(U1-SS)")
	(net 23 "Net-(U2-SS)")
	(net 24 "unconnected-(U2-NC-Pad12)")
	(net 25 "Net-(C16-Pad1)")
	(net 26 "Net-(U2-PGOOD)")
	(net 27 "unconnected-(U2-NC-Pad15)")
	(net 28 "Net-(C17-Pad1)")
	(net 29 "Net-(R14-Pad2)")
	(net 30 "Net-(R12-Pad1)")
	(net 31 "Net-(R13-Pad2)")
	(net 32 "Net-(U1-EN_UVLO_SYNC)")
	(net 33 "Net-(U2-EN_UVLO_SYNC)")
	(net 34 "Net-(U3-Y)")
	(net 35 "Net-(U6-Y)")
	(net 36 "/Enable")
	(net 37 "/Sync_Clk")
	(net 38 "/Dual{slash}Single")
	(footprint "t_sot:sot-23-5"
		(layer "F.Cu")
		(at 106.21264 83.3755 -90)
		(descr "SOT-23")
		(property "Reference" "U6"
			(at -2.2225 1.94564 180)
			(layer "F.SilkS")
		)
		(property "Value" "7S08"
			(at 0 0.3302 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "/Enable")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/Dual{slash}Single")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(U6-Y)")
			(pinfunction "Y")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-5-2.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 124.333 96.52 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C7"
			(at -2.667 0.762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 131.572 97.131 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C17"
			(at 3.199 -0.254 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(C17-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 116.078 84.582)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R14"
			(at -1.863 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(R14-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 121.158 87.08 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R2"
			(at 0 -1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U1-RT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 131.318 93.218)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB2"
			(at 0.254 -1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(C17-Pad1)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 135.89 89.535)
		(property "Reference" "TP24"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(C17-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 96.52 104.14)
		(property "Reference" "TP22"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 124.333 89.723 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C13"
			(at 2.347 1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 96.52 73.66)
		(property "Reference" "TP20"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 97.155 97.155)
		(property "Reference" "TP6"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 122.682 91.44 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C4"
			(at 1.917 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VCC)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res2512W"
		(layer "F.Cu")
		(at 137.009 94.615 -90)
		(property "Reference" "R13"
			(at 4.699 -0.024 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 -0.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res2512W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(C17-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(R13-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/R2512W.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23-5"
		(layer "F.Cu")
		(at 101.727 87.884 -90)
		(descr "SOT-23")
		(property "Reference" "U4"
			(at -2.159 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "7S08"
			(at 0 0.3302 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U3-Y)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(U6-Y)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(U2-EN_UVLO_SYNC)")
			(pinfunction "Y")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-5-2.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 116.12 100.203 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R11"
			(at 1.82 -0.381 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U2-MODE)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 97.155 89.535)
		(property "Reference" "TP12"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 115.993 85.598 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R4"
			(at 1.82 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(R14-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 97.155 79.375)
		(property "Reference" "TP13"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3V"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 107.061 93.218)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB1"
			(at 0.127 -1.905 360)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 360)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(C16-Pad1)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 115.951 87.63)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R5"
			(at -1.693 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 97.155 94.615)
		(property "Reference" "TP3"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vin"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(R12-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 106.468 81.026)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C15"
			(at 0 -1.016 360)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 113.665 81.28)
		(property "Reference" "TP16"
			(at 0 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(R14-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 118.11 87.122 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C3"
			(at -2.667 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-COMP)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 141.605 94.615)
		(property "Reference" "TP4"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(R13-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 122.809 99.399 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R8"
			(at -2.074 -1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(U2-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 124.333 93.091 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C5"
			(at -3.683 -1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 120.65 81.28)
		(property "Reference" "TP14"
			(at 0.127 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(U1-COMP)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 139.7 73.66)
		(property "Reference" "TP21"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 118.66 85.598)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C2"
			(at 0 -2.413 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 121.158 85.09)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R9"
			(at 0 -0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(U2-COMP)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-COMP)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 121.793 104.394)
		(property "Reference" "TP2"
			(at 0 1.651 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(U2-PGOOD)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_qfn:RTE0016K-IPC_A"
		(layer "F.Cu")
		(at 119.749001 90.424 180)
		(tags "LM5158QRTERQ1 ")
		(property "Reference" "U1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LM5158QRTERQ1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:RTE0016K-IPC_A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5158-q1.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1731935599625&ref_url=https%253A%252F%252Fic-online.com%252F"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMPS Boost Regulator 60V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RTE0016K-IPC_A RTE0016K-IPC_B RTE0016K-IPC_C RTE0016K-MFG")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.504554 -0.749998 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.504554 -0.25 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VCC)")
			(pinfunction "VCC")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -1.504554 0.25 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pinfunction "BIAS")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.504554 0.750001 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U1-PGOOD)")
			(pinfunction "PGOOD")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at -0.749998 1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U1-RT)")
			(pinfunction "RT")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -0.25 1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(U1-EN_UVLO_SYNC)")
			(pinfunction "EN_UVLO_SYNC")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 0.25 1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 0.750001 1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-COMP)")
			(pinfunction "COMP")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 1.504554 0.750001 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at 1.504554 0.25 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(U1-SS)")
			(pinfunction "SS")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 1.504554 -0.25 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-MODE)")
			(pinfunction "MODE")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 1.504554 -0.749998 270)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "unconnected-(U1-NC-Pad12)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "13" smd rect
			(at 0.750001 -1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(D1-A)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at 0.25 -1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(D1-A)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at -0.25 -1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "unconnected-(U1-NC-Pad15)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "16" smd rect
			(at -0.749998 -1.504554 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 1.759999 1.759999)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_qfn/LM5158QRTERQ1.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 115.993 88.646)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C1"
			(at -1.693 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(U1-SS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 109.855 104.14)
		(property "Reference" "TP18"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 97.155 86.995)
		(property "Reference" "TP10"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Sync"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/Sync_Clk")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 107.95 97.155 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C16"
			(at 3.429 1.524 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(C16-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 111.252 85.09)
		(property "Reference" "TP5"
			(at -1.778 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(R6-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res2512W"
		(layer "F.Cu")
		(at 101.703 95.885 -90)
		(property "Reference" "R12"
			(at -4.572 -0.151 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 -0.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res2512W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(R12-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(C16-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/R2512W.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 123.317 86.487)
		(property "Reference" "TP1"
			(at 0.508 -1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(U1-PGOOD)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 100.33 101.092)
		(property "Reference" "TP26"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(R12-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 116.205 81.28)
		(property "Reference" "TP15"
			(at 0 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-K)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 101.685 81.026)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C14"
			(at 0 -1.016 360)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 139.7 104.14)
		(property "Reference" "TP23"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 118.303 104.394)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C18"
			(at -2.733 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOD-123"
		(layer "F.Cu")
		(at 120.262 95.885 180)
		(property "Reference" "D2"
			(at 0.217 0.0565 0)
			(layer "F.SilkS")
		)
		(property "Value" "SS36FA"
			(at 0.0635 1.8415 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:SOD-123"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.4445 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.025 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.025 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 111.252 87.63)
		(property "Reference" "TP8"
			(at -1.778 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 115.951 86.614)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R6"
			(at -1.735 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(R6-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 127 92.456 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C6"
			(at 3.048 1.143 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "F.Cu")
		(at 115.189 92.456)
		(property "Reference" "L1"
			(at -2.667 -2.921 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.2uH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(D1-A)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 141.605 97.155)
		(property "Reference" "TP7"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_sot:sot-23-5"
		(layer "F.Cu")
		(at 106.172 87.8205 -90)
		(descr "SOT-23")
		(property "Reference" "U5"
			(at -2.0955 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "7S08"
			(at 0 0.3302 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "/Enable")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/Sync_Clk")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(U1-EN_UVLO_SYNC)")
			(pinfunction "Y")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-5-2.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 97.155 84.455)
		(property "Reference" "TP11"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "D/~S"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/Dual{slash}Single")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 116.163 101.346)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C9"
			(at -1.863 0.508 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(U2-SS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 127 97.155 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C12"
			(at 3.175 -0.635 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 111.252 97.179 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C10"
			(at 3.532 1.397 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 124.333 104.394)
		(property "Reference" "TP19"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 97.155 81.915)
		(property "Reference" "TP9"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Enable"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/Enable")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 125.095 81.28)
		(property "Reference" "TP17"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 119.253 87.122 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R3"
			(at -2.667 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-COMP)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(C2-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 124.079 99.399 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R7"
			(at 1.566 -1.143 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U2-VCC)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(U2-FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 116.036 89.662)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R1"
			(at -1.609 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-MODE)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOD-123"
		(layer "F.Cu")
		(at 120.276 93.726 180)
		(property "Reference" "D1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SS36FA"
			(at 0.0635 1.8415 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:SOD-123"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.4445 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.025 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.025 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 111.252 92.456 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C11"
			(at 2.921 -1.524 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "F.Cu")
		(at 115.189 97.155)
		(property "Reference" "L2"
			(at -2.794 3.556 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.2uH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D2-A)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 102.87 101.092)
		(property "Reference" "TP27"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(C16-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_qfn:RTE0016K-IPC_A"
		(layer "F.Cu")
		(at 119.761 99.167554 90)
		(tags "LM5158QRTERQ1 ")
		(property "Reference" "U2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LM5158QRTERQ1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:RTE0016K-IPC_A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5158-q1.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1731935599625&ref_url=https%253A%252F%252Fic-online.com%252F"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMPS Boost Regulator 60V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RTE0016K-IPC_A RTE0016K-IPC_B RTE0016K-IPC_C RTE0016K-MFG")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.504554 -0.749998 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.504554 -0.25 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U2-VCC)")
			(pinfunction "VCC")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -1.504554 0.25 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BIAS)")
			(pinfunction "BIAS")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.504554 0.750001 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-PGOOD)")
			(pinfunction "PGOOD")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at -0.749998 1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(U2-RT)")
			(pinfunction "RT")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -0.25 1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(U2-EN_UVLO_SYNC)")
			(pinfunction "EN_UVLO_SYNC")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 0.25 1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 0.750001 1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(U2-COMP)")
			(pinfunction "COMP")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 1.504554 0.750001 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(U2-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at 1.504554 0.25 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(U2-SS)")
			(pinfunction "SS")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 1.504554 -0.25 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U2-MODE)")
			(pinfunction "MODE")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 1.504554 -0.749998 180)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "unconnected-(U2-NC-Pad12)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "13" smd rect
			(at 0.750001 -1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D2-A)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at 0.25 -1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D2-A)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at -0.25 -1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "unconnected-(U2-NC-Pad15)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "16" smd rect
			(at -0.749998 -1.504554 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 1.759999 1.759999)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_qfn/LM5158QRTERQ1.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23-5"
		(layer "F.Cu")
		(at 101.727 83.439 -90)
		(descr "SOT-23")
		(property "Reference" "U3"
			(at -2.159 2.159 180)
			(layer "F.SilkS")
		)
		(property "Value" "7SZ04"
			(at 0 0.3302 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd rect
			(at 0 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/Sync_Clk")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U3-Y)")
			(pinfunction "Y")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -0.9525 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-5-2.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 118.733 102.489)
		(descr "SMT resistor, 0603")
		(property "Reference" "C8"
			(at -2.02 0.127 360)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U2-VCC)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 123.317 101.219 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R10"
			(at -0.127 -1.016 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(U2-RT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 138.43 89.535)
		(property "Reference" "TP25"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PSBoostTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(R13-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(gr_rect
		(start 92.71 69.85)
		(end 143.51 107.95)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "GND\n"
		(at 93.218 90.297 0)
		(layer "F.SilkS")
	)
	(gr_text "GND\n"
		(at 140.081 99.822 0)
		(layer "F.SilkS")
	)
	(gr_text "Primary\nSide"
		(at 126.365 85.217 0)
		(layer "F.SilkS")
	)
	(gr_text "VOUT"
		(at 139.827 93.472 0)
		(layer "F.SilkS")
	)
	(gr_text "Secondary\nSide"
		(at 126.619 105.41 0)
		(layer "F.SilkS")
	)
	(gr_text "18 Nov 2024"
		(at 102.235 73.787 0)
		(layer "F.SilkS")
	)
	(gr_text "FB\nInjection"
		(at 112.014 78.867 0)
		(layer "F.SilkS")
	)
	(gr_text "Iout\nSense"
		(at 135.509 88.138 0)
		(layer "F.SilkS")
	)
	(gr_text "CLK\n"
		(at 93.218 87.757 0)
		(layer "F.SilkS")
	)
	(gr_text "Vadj"
		(at 109.347 83.693 0)
		(layer "F.SilkS")
	)
	(gr_text "VIN"
		(at 93.218 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "ENA"
		(at 93.091 82.677 0)
		(layer "F.SilkS")
	)
	(gr_text "Iin\nSense"
		(at 100.457 105.664 0)
		(layer "F.SilkS")
	)
	(gr_text "3.3V"
		(at 93.091 80.137 0)
		(layer "F.SilkS")
	)
	(gr_text "Dual LM5158 Test Board"
		(at 102.235 72.136 0)
		(layer "F.SilkS")
	)
	(gr_text "D/~{S}"
		(at 93.218 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "Sync Circuit"
		(at 99.568 79.121 0)
		(layer "F.SilkS")
	)
	(gr_text "DRM"
		(at 102.235 75.692 0)
		(layer "F.SilkS")
	)
	(gr_text "GND\n"
		(at 93.091 97.917 0)
		(layer "F.SilkS")
	)
	(gr_text "COMP"
		(at 119.253 78.867 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads thru_hole_only
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.808 90.678) (xy 115.443 90.678) (xy 115.443 98.933) (xy 114.935 98.933)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(D1-K)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.3048)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.666 96.647) (xy 123.317 96.647) (xy 123.698 96.266) (xy 129.286 96.266) (xy 129.794 95.758)
				(xy 129.794 94.488) (xy 130.048 94.234) (xy 130.048 91.948) (xy 129.794 91.694) (xy 128.905 91.694)
				(xy 128.651 91.948) (xy 128.651 92.837) (xy 128.397 93.091) (xy 121.666 93.091)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(C17-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.9149 92.3163) (xy 136.271 92.329) (xy 136.271 96.774) (xy 130.429 96.774) (xy 130.429 94.869)
				(xy 131.191 94.107) (xy 131.191 92.71) (xy 131.572 92.329)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D2-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.745 95.504) (xy 118.491 95.25) (xy 115.951 95.25) (xy 115.951 99.06) (xy 118.731001 99.037196)
				(xy 118.731001 98.297911) (xy 118.618 98.171) (xy 118.618 96.647) (xy 118.745 96.52)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(U1-BIAS)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.554 91.948) (xy 113.284 91.948) (xy 112.903 92.329) (xy 107.95 92.329) (xy 107.95 94.361)
				(xy 109.347 94.361) (xy 109.728 94.742) (xy 109.728 97.282) (xy 114.554 97.282)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(R12-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 95.885 93.853) (xy 95.885 95.377) (xy 96.393 95.885) (xy 98.298 95.885) (xy 99.314 96.901) (xy 100.965 96.901)
				(xy 101.003 92.385) (xy 99.403 92.385) (xy 98.298 93.345) (xy 96.393 93.345)
			)
		)
	)
	(zone
		(net 25)
		(net_name "Net-(C16-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 102.489 92.329) (xy 102.87 91.948) (xy 106.68 91.948) (xy 107.061 92.329) (xy 107.061 94.361)
				(xy 107.442 94.742) (xy 108.966 94.742) (xy 109.2 95.055) (xy 109.22 97.155) (xy 102.489 97.155)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(D1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.824 94.361) (xy 118.999 94.361) (xy 119.634 93.726) (xy 119.634 91.567) (xy 115.824 91.567)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(R13-Pad2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.875 93.853) (xy 142.875 95.504) (xy 142.367 95.885) (xy 137.922 95.885) (xy 137.922 93.345)
				(xy 142.367 93.345)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 93.345 70.485) (xy 142.875 70.485) (xy 142.875 107.315) (xy 93.345 107.315)
			)
		)
	)
)
