(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 404)
    (no_connects 0)
    (area 40.378572 40.1 143.471429 113.500001)
    (thickness 1.6)
    (drawings 30)
    (tracks 469)
    (zones 0)
    (modules 281)
    (nets 113)
  )
  (page A4)
  (title_block
    (title "IDT Clock Block")
    (date 2017-12-12)
    (rev V1.0)
    (company KD5SSJ)
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.01)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.508 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x000f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory meta/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 +3V3)
  (net 5 "Net-(C17-Pad2)")
  (net 6 "Net-(C17-Pad1)")
  (net 7 "Net-(C18-Pad2)")
  (net 8 "Net-(C18-Pad1)")
  (net 9 "Net-(C19-Pad2)")
  (net 10 "Net-(C19-Pad1)")
  (net 11 "Net-(C20-Pad2)")
  (net 12 "Net-(C20-Pad1)")
  (net 13 "Net-(C21-Pad2)")
  (net 14 "Net-(C21-Pad1)")
  (net 15 "Net-(C22-Pad2)")
  (net 16 "Net-(C22-Pad1)")
  (net 17 "Net-(C23-Pad2)")
  (net 18 "Net-(C23-Pad1)")
  (net 19 "Net-(C24-Pad2)")
  (net 20 "Net-(C24-Pad1)")
  (net 21 "Net-(C25-Pad2)")
  (net 22 "Net-(C25-Pad1)")
  (net 23 "Net-(C26-Pad2)")
  (net 24 "Net-(C26-Pad1)")
  (net 25 "Net-(C27-Pad2)")
  (net 26 "Net-(C27-Pad1)")
  (net 27 "Net-(C28-Pad2)")
  (net 28 "Net-(C28-Pad1)")
  (net 29 /Event)
  (net 30 /1PPS_Sync)
  (net 31 "Net-(J4-Pad2)")
  (net 32 "Net-(J5-Pad2)")
  (net 33 "Net-(J6-Pad2)")
  (net 34 "Net-(J7-Pad2)")
  (net 35 "Net-(J8-Pad2)")
  (net 36 "Net-(J9-Pad2)")
  (net 37 "Net-(J10-Pad2)")
  (net 38 "Net-(J11-Pad2)")
  (net 39 "Net-(J12-Pad2)")
  (net 40 "Net-(J13-Pad2)")
  (net 41 "Net-(J14-Pad1)")
  (net 42 "Net-(J15-Pad2)")
  (net 43 "Net-(J16-Pad2)")
  (net 44 "Net-(J17-Pad2)")
  (net 45 "Net-(J18-Pad2)")
  (net 46 "Net-(J19-Pad2)")
  (net 47 "Net-(J20-Pad2)")
  (net 48 "Net-(J21-Pad2)")
  (net 49 "Net-(J22-Pad2)")
  (net 50 "Net-(J23-Pad2)")
  (net 51 "Net-(J24-Pad1)")
  (net 52 "Net-(J24-Pad2)")
  (net 53 "Net-(J25-Pad2)")
  (net 54 /RPi_GPIO/PPS)
  (net 55 "Net-(J27-Pad2)")
  (net 56 "Net-(J28-Pad2)")
  (net 57 "Net-(J29-Pad2)")
  (net 58 "Net-(J30-Pad2)")
  (net 59 "Net-(J31-Pad2)")
  (net 60 "Net-(J31-Pad3)")
  (net 61 "Net-(J32-Pad2)")
  (net 62 "Net-(J45-Pad2)")
  (net 63 "Net-(J45-Pad3)")
  (net 64 "Net-(J45-Pad4)")
  (net 65 "Net-(J45-Pad5)")
  (net 66 "Net-(J45-Pad7)")
  (net 67 /RPi_GPIO/TxD)
  (net 68 /RPi_GPIO/RxD)
  (net 69 "Net-(J45-Pad11)")
  (net 70 "Net-(J45-Pad12)")
  (net 71 "Net-(J45-Pad13)")
  (net 72 /RPi_GPIO/Arm\)
  (net 73 /RPi_GPIO/Rise_Fall\)
  (net 74 "Net-(J45-Pad19)")
  (net 75 "Net-(J45-Pad21)")
  (net 76 /RPi_GPIO/TimestampRst\)
  (net 77 "Net-(J45-Pad23)")
  (net 78 "Net-(J45-Pad24)")
  (net 79 "Net-(J45-Pad26)")
  (net 80 "Net-(J45-Pad27)")
  (net 81 "Net-(J45-Pad28)")
  (net 82 "Net-(J45-Pad29)")
  (net 83 "Net-(J45-Pad31)")
  (net 84 "Net-(J45-Pad32)")
  (net 85 "Net-(J45-Pad33)")
  (net 86 "Net-(J45-Pad35)")
  (net 87 "Net-(J45-Pad36)")
  (net 88 "Net-(J45-Pad37)")
  (net 89 "Net-(J45-Pad38)")
  (net 90 "Net-(J45-Pad40)")
  (net 91 "Net-(R1-Pad1)")
  (net 92 "Net-(R3-Pad1)")
  (net 93 "Net-(R4-Pad2)")
  (net 94 "Net-(R5-Pad2)")
  (net 95 "Net-(R6-Pad2)")
  (net 96 "Net-(R7-Pad2)")
  (net 97 "Net-(R8-Pad2)")
  (net 98 "Net-(R9-Pad2)")
  (net 99 "Net-(R10-Pad2)")
  (net 100 "Net-(R11-Pad2)")
  (net 101 "Net-(R12-Pad2)")
  (net 102 "Net-(R13-Pad2)")
  (net 103 "Net-(R14-Pad2)")
  (net 104 "Net-(R15-Pad2)")
  (net 105 "Net-(R16-Pad2)")
  (net 106 "Net-(U2-Pad8)")
  (net 107 "Net-(U2-Pad21)")
  (net 108 "Net-(U4-Pad7)")
  (net 109 "Net-(U10-Pad1)")
  (net 110 "Net-(U10-Pad3)")
  (net 111 "Net-(U12-Pad1)")
  (net 112 "Net-(U12-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /1PPS_Sync)
    (add_net /Event)
    (add_net /RPi_GPIO/Arm\)
    (add_net /RPi_GPIO/PPS)
    (add_net /RPi_GPIO/Rise_Fall\)
    (add_net /RPi_GPIO/RxD)
    (add_net /RPi_GPIO/TimestampRst\)
    (add_net /RPi_GPIO/TxD)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C27-Pad2)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C28-Pad2)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad2)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J13-Pad2)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad2)")
    (add_net "Net-(J16-Pad2)")
    (add_net "Net-(J17-Pad2)")
    (add_net "Net-(J18-Pad2)")
    (add_net "Net-(J19-Pad2)")
    (add_net "Net-(J20-Pad2)")
    (add_net "Net-(J21-Pad2)")
    (add_net "Net-(J22-Pad2)")
    (add_net "Net-(J23-Pad2)")
    (add_net "Net-(J24-Pad1)")
    (add_net "Net-(J24-Pad2)")
    (add_net "Net-(J25-Pad2)")
    (add_net "Net-(J27-Pad2)")
    (add_net "Net-(J28-Pad2)")
    (add_net "Net-(J29-Pad2)")
    (add_net "Net-(J30-Pad2)")
    (add_net "Net-(J31-Pad2)")
    (add_net "Net-(J31-Pad3)")
    (add_net "Net-(J32-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J45-Pad11)")
    (add_net "Net-(J45-Pad12)")
    (add_net "Net-(J45-Pad13)")
    (add_net "Net-(J45-Pad19)")
    (add_net "Net-(J45-Pad2)")
    (add_net "Net-(J45-Pad21)")
    (add_net "Net-(J45-Pad23)")
    (add_net "Net-(J45-Pad24)")
    (add_net "Net-(J45-Pad26)")
    (add_net "Net-(J45-Pad27)")
    (add_net "Net-(J45-Pad28)")
    (add_net "Net-(J45-Pad29)")
    (add_net "Net-(J45-Pad3)")
    (add_net "Net-(J45-Pad31)")
    (add_net "Net-(J45-Pad32)")
    (add_net "Net-(J45-Pad33)")
    (add_net "Net-(J45-Pad35)")
    (add_net "Net-(J45-Pad36)")
    (add_net "Net-(J45-Pad37)")
    (add_net "Net-(J45-Pad38)")
    (add_net "Net-(J45-Pad4)")
    (add_net "Net-(J45-Pad40)")
    (add_net "Net-(J45-Pad5)")
    (add_net "Net-(J45-Pad7)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad3)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U12-Pad3)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U4-Pad7)")
  )
  (net_class Large ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 0.89916)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Small ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Typical ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 91.74734 76.8096)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 84.35848 73.63714)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 84.47024 77.0128)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 84.45246 78.92034)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 85.59546 80.68564)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 86.68512 84.36102)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 85.41258 88.0618)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 75.24496 88.06434)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 74.99604 81.05648)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 89.36228 79.56042)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 71.34098 81.05394)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 71.34098 77.978)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 79.248 63.36284)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 75.819 64.42202)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 53.85816 63.96482)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 62.34176 96.72066)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 52.05984 89.3953)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 56.88076 77.08138)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 62.25794 68.89496)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 56.88838 68.6689)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 60.30976 66.8909)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 64.643 89.408)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 94.107 89.916)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 95.33128 88.0745)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 96.901 87.122)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 98.806 85.217)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 100.203 79.883)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 102.489 79.375)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 83.566 68.707)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 84.582 69.723)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 92.329 69.723)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B09D2)
    (at 73.025 59.436)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B22A6)
    (at 51.689 58.928)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 81.534 68.707)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 78.74 69.85)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 89.789 69.723)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B09DC)
    (at 80.645 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B09AF)
    (at 57.785 59.436)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 82.55 66.04)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 84.455 63.5)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 87.122 69.723)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 94.869 69.723)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B09C5)
    (at 65.405 59.436)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 68.453 62.103)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 66.04 65.786)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 68.707 68.834)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 75.819 67.183)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2B08B8)
    (at 72.644 67.183)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 61.976 79.248)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 66.04 68.834)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 75.819 62.103)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 65.024 77.724)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 52.07 99.06)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 58.42 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 72.644 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 65.659 70.866)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 59.309 77.089)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 65.532 84.328)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 69.469 77.724)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 60.325 62.103)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 56.896 65.405)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 66.675 74.549)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 61.595 84.328)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 77.851 77.978)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 64.897 74.549)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 58.674 62.103)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 55.626 62.484)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 82.55)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 104.648 72.39)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 111.76 70.485)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 67.183 77.724)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 61.976 75.438)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 67.31 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 63.754 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 76.2 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 102.489 82.423)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 71.882 91.694)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 62.103 82.042)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 65.532 97.155)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 105.664 90.297)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 98.806 95.885)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 62.357 89.408)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 64.897 82.042)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 103.378 70.485)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 105.664 88.265)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 105.664 86.233)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 92.71 98.425)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 69.215 87.63)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 66.675 87.63)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 60.325 87.63)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 57.785 87.63)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 89.535 98.425)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 56.388 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 61.722 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 65.278 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 70.612 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 97.155 95.885)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 71.755 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 71.755 98.425)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 75.565 98.425)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 86.36 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 77.47 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 80.01 106.045)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 65.532 103.251)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 83.312 103.251)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 99.314 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 80.01 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 77.47 106.045)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 81.534 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 85.09 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 102.87 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 93.98 104.267)
    (fp_text reference "" (at 0.635 3.81) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 78.74 92.075)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 68.58 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 71.12 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 97.79 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 90.424 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 81.915 92.075)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 80.01 95.885)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 85.725 95.885)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 95.25 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 88.9 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 81.915 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 78.74 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 114.935 99.695)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 88.9 95.885)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 85.09 92.075)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 85.09 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 88.265 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 95.885 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 88.265 92.075)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 104.14 95.885)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 101.092 94.869)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 101.092 103.251)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 99.695 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 104.14 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 101.6)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 108.204 104.267)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 108.331 99.822)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 97.79)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 95.885 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 97.79 89.535)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 100.203 86.741)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 86.487)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 90.043)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 95.377)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 85.09)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 77.597)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 68.707)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 80.645)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 76.2)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 81.153)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 72.263)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 112.776 63.373)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 104.775 67.945)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 93.98)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 76.2)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 73.66)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 82.55)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 67.31)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 103.505 91.44)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 64.77)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 109.855 61.595)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 64.77)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 106.68 61.595)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 104.14 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 100.33 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 97.155 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 93.98 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 90.805 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS) hide)
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 59.055 91.44 180)
    (fp_text reference J44 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C28-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D5AE)
    (at 59.055 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at -0.889 -2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C28-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C28-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 67.945 91.44 180)
    (fp_text reference J43 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C27-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D5C8)
    (at 67.945 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at -0.127 2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C27-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C27-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D59C)
    (at 63.5 88.646 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at -0.127 2.159 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A28D628)
    (at 65.659 80.772 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J31 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J14-Pad1)"))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J31-Pad2)"))
    (pad 3 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J31-Pad3)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A28D61B)
    (at 61.214 80.772 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J32 (at 1.778 0 180) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J24-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J32-Pad2)"))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J31-Pad3)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28D5DB)
    (at 67.183 85.344 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C27-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A28D5EB)
    (at 63.5 84.328 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U14 (at -1.016 -3.302 360) (layer F.SilkS))
    (fp_text value 74LVC2G34 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J31-Pad2)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J32-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R16-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R15-Pad2)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 59.817 85.344)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C28-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_3.9x9.9mm_Pitch0.635mm (layer F.Cu) (tedit 5A28D870)
    (at 85.471 78.994)
    (descr "SSOP28: plastic shrink small outline package; 28 leads; body width 3.9 mm; lead pitch 0.635; (see http://cds.linear.com/docs/en/datasheet/38901fb.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U2 (at -4.445 -3.683) (layer F.SilkS))
    (fp_text value ICS525-02 (at -0.1 6.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.6 -4.1275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at -2.6 -3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J5-Pad2)"))
    (pad 3 smd rect (at -2.6 -2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J6-Pad2)"))
    (pad 4 smd rect (at -2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J7-Pad2)"))
    (pad 5 smd rect (at -2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J8-Pad2)"))
    (pad 6 smd rect (at -2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at -2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J14-Pad1)"))
    (pad 8 smd rect (at -2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 10 smd rect (at -2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J9-Pad2)"))
    (pad 11 smd rect (at -2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J10-Pad2)"))
    (pad 12 smd rect (at -2.6 2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J11-Pad2)"))
    (pad 13 smd rect (at -2.6 3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J12-Pad2)"))
    (pad 14 smd rect (at -2.6 4.1275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J13-Pad2)"))
    (pad 15 smd rect (at 2.6 4.1275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J23-Pad2)"))
    (pad 16 smd rect (at 2.6 3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J22-Pad2)"))
    (pad 17 smd rect (at 2.6 2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J21-Pad2)"))
    (pad 18 smd rect (at 2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J20-Pad2)"))
    (pad 19 smd rect (at 2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(R4-Pad2)"))
    (pad 20 smd rect (at 2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J31-Pad3)"))
    (pad 23 smd rect (at 2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 24 smd rect (at 2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J19-Pad2)"))
    (pad 25 smd rect (at 2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J18-Pad2)"))
    (pad 26 smd rect (at 2.6 -2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J17-Pad2)"))
    (pad 27 smd rect (at 2.6 -3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J16-Pad2)"))
    (pad 28 smd rect (at 2.6 -4.1275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J15-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-28_3.9x9.9mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:Pin_Header_Straight_2x20 locked (layer F.Cu) (tedit 5A28D74F)
    (at 83.3 54.8 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J45 (at -4.128 -24.118 180) (layer F.SilkS))
    (fp_text value RPi_GPIO (at -1.27 -27.23 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(J45-Pad2)"))
    (pad 3 thru_hole oval (at -1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(J45-Pad3)"))
    (pad 4 thru_hole oval (at 1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(J45-Pad4)"))
    (pad 5 thru_hole oval (at -1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(J45-Pad5)"))
    (pad 6 thru_hole oval (at 1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 7 thru_hole oval (at -1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J45-Pad7)"))
    (pad 8 thru_hole oval (at 1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /RPi_GPIO/TxD))
    (pad 9 thru_hole oval (at -1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 10 thru_hole oval (at 1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /RPi_GPIO/RxD))
    (pad 11 thru_hole oval (at -1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J45-Pad11)"))
    (pad 12 thru_hole oval (at 1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J45-Pad12)"))
    (pad 13 thru_hole oval (at -1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J45-Pad13)"))
    (pad 14 thru_hole oval (at 1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 15 thru_hole oval (at -1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 /RPi_GPIO/Arm\))
    (pad 16 thru_hole oval (at 1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 /RPi_GPIO/Rise_Fall\))
    (pad 17 thru_hole oval (at -1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 18 thru_hole oval (at 1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /RPi_GPIO/PPS))
    (pad 19 thru_hole oval (at -1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J45-Pad19)"))
    (pad 20 thru_hole oval (at 1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 21 thru_hole oval (at -1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J45-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 /RPi_GPIO/TimestampRst\))
    (pad 23 thru_hole oval (at -1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J45-Pad23)"))
    (pad 24 thru_hole oval (at 1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J45-Pad24)"))
    (pad 25 thru_hole oval (at -1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 26 thru_hole oval (at 1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(J45-Pad26)"))
    (pad 27 thru_hole oval (at -1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J45-Pad27)"))
    (pad 28 thru_hole oval (at 1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J45-Pad28)"))
    (pad 29 thru_hole oval (at -1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J45-Pad29)"))
    (pad 30 thru_hole oval (at 1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 31 thru_hole oval (at -1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J45-Pad31)"))
    (pad 32 thru_hole oval (at 1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J45-Pad32)"))
    (pad 33 thru_hole oval (at -1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J45-Pad33)"))
    (pad 34 thru_hole oval (at 1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 35 thru_hole oval (at -1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J45-Pad35)"))
    (pad 36 thru_hole oval (at 1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J45-Pad36)"))
    (pad 37 thru_hole oval (at -1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J45-Pad37)"))
    (pad 38 thru_hole oval (at 1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J45-Pad38)"))
    (pad 39 thru_hole oval (at -1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 40 thru_hole oval (at 1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(J45-Pad40)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 112.3 54.8)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 112.3 103.8)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CB9)
    (at 54.3 103.8)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 54.3 54.8)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 56.134 67.31 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 79.6925 78.0415 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D63B)
    (at 68.326 76.962 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.127 1.651 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A2A0403)
    (at 90.3605 78.8035 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.9685 -0.0635 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D6A3)
    (at 64.262 68.834 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.54 -0.127 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D767)
    (at 82.55 67.945 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DD82)
    (at 77.851 96.012)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 94.996 96.012)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D9E1)
    (at 104.648 80.899 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0.381 -1.651 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D99F)
    (at 104.648 74.041 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0.635 -2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DDD2)
    (at 65.532 101.473 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 2.159 -0.127 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DD36)
    (at 83.312 101.473 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 2.159 -0.127 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DB6A)
    (at 101.092 101.473 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 2.159 0 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DA37)
    (at 109.982 88.265)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 109.982 70.485)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DDA2)
    (at 69.977 100.457 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0 2.286 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C17-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C17-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DDEB)
    (at 61.087 100.457 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DD26)
    (at 87.757 100.457 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C19-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C19-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DD4B)
    (at 78.867 100.457 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at -0.127 -2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C20-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C20-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DC6F)
    (at 105.537 100.457 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C21-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C21-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28DB8B)
    (at 96.647 100.457 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C22-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C22-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 108.966 83.82 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C23-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C23-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 108.966 92.71 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C24-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C24-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A28D95A)
    (at 108.966 66.04 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at 0 1.397 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C25-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C25-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 108.966 74.93 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C26-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C26-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 5A28D719)
    (at 53.848 64.008 90)
    (fp_text reference J1 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 90) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 90) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 90) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 90) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 5A28D90A)
    (at 96.393 65.532 180)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference J2 (at -2.413 0 180) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 3.81 4.5 180) (layer F.Fab))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 /Event))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 /1PPS_Sync))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-04_04x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5A28D6F5)
    (at 53.594 67.31)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J3 (at 0 1.905) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D84F)
    (at 83.1215 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J4 (at 0.4445 -2.0955 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D815)
    (at 80.7085 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J5 (at -0.0635 2.2225 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J5-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D807)
    (at 78.1685 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at -0.0635 2.2225 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J6-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D7EB)
    (at 75.7555 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at -0.0635 2.3495 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J7-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D7D8)
    (at 73.3425 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J8 (at -0.0635 2.2225 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J8-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DB02)
    (at 75.2475 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J9 (at -0.0635 2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J9-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DAF8)
    (at 77.7875 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J10 (at -0.0635 -2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J10-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DAEC)
    (at 80.3275 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J11 (at 0.0635 2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J11-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DAD4)
    (at 82.8675 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J12 (at 0.0635 -2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J12-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DAC2)
    (at 85.4075 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J13 (at 0.0635 -2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J13-Pad2)"))
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5A28D6B6)
    (at 70.358 69.088)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J14 (at 2.413 0) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 41 "Net-(J14-Pad1)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D89A)
    (at 85.5345 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J15 (at 0.1905 -2.0955 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J15-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D8B4)
    (at 87.9475 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J16 (at 0.0635 -2.0955 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J16-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D8C5)
    (at 90.4875 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J17 (at 0.0635 2.2225 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J17-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D8E6)
    (at 92.9005 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J18 (at 0.0635 -2.0955 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J18-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D8F8)
    (at 95.3135 71.8185)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J19 (at 0.0635 2.2225 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J19-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DA89)
    (at 95.3135 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J20 (at 0.0635 -2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J20-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DA99)
    (at 92.9005 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J21 (at -0.0635 2.0955 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J21-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DAA2)
    (at 90.4875 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J22 (at 0.0635 -2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J22-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28DAB7)
    (at 87.9475 86.1695 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J23 (at 0.0635 -2.2225 360) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J23-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 58.674 70.739 90)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J24 (at 1.78 0 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J24-Pad1)"))
    (pad 2 smd rect (at 0 0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J24-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D67C)
    (at 58.674 73.152 90)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J25 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J24-Pad1)"))
    (pad 2 smd rect (at 0 0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J25-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A28D66E)
    (at 58.674 75.565 90)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J26 (at -3.429 0 180) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J24-Pad1)"))
    (pad 2 smd rect (at 0 0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 54 /RPi_GPIO/PPS))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A28DB0C)
    (at 74.422 91.694 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J27 (at -1.778 -0.127 360) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J27-Pad2)"))
    (pad 3 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A28DB14)
    (at 91.567 91.694 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J28 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J28-Pad2)"))
    (pad 3 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A2A043B)
    (at 100.203 84.328)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J29 (at -0.127 -2.794 180) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J29-Pad2)"))
    (pad 3 smd rect (at 0 1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A2A042A)
    (at 100.203 77.47)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J30 (at -0.127 -2.794 180) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J30-Pad2)"))
    (pad 3 smd rect (at 0 1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 69.977 104.267 180)
    (fp_text reference J33 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C17-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 61.087 104.267 180)
    (fp_text reference J34 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 87.757 104.267 180)
    (fp_text reference J35 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C19-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 78.867 104.267 180)
    (fp_text reference J36 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C20-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 105.537 104.267 180)
    (fp_text reference J37 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C21-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 597BEF84)
    (at 96.647 104.267 180)
    (fp_text reference J38 (at 0.025 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 180) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C22-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 5A28DA44)
    (at 112.776 83.82 270)
    (fp_text reference J39 (at -2.921 0 360) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 270) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 270) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C23-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 5A28DA51)
    (at 112.776 92.71 270)
    (fp_text reference J40 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 270) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 270) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C24-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 5A28D92A)
    (at 112.776 66.04 270)
    (fp_text reference J41 (at -2.921 -0.127 360) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 270) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 270) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C25-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:uFL_coax (layer F.Cu) (tedit 5A28D933)
    (at 112.776 74.93 270)
    (fp_text reference J42 (at -3.048 -0.127 360) (layer F.SilkS))
    (fp_text value CONN_COAXIAL_2EXT (at 0 2.75 270) (layer F.Fab))
    (pad 3 smd rect (at 1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.475 0 270) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 1.525 270) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C26-Pad1)"))
    (model "c:/Users/Cindy Sue/Documents/Kicad/conn_rf/coaxial_u.fl-r-smt-1.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DE27)
    (at 58.6105 66.6115 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.0635 -1.7145 360) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DE35)
    (at 58.6105 63.8175 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.8415 -0.1905 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DE32)
    (at 60.2615 63.8175 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.8415 0.3175 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A2A040E)
    (at 91.8845 78.8035 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.0635 -1.7145 360) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DDAE)
    (at 69.215 98.171 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C17-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DDE0)
    (at 61.849 98.171)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.286 0) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DD42)
    (at 79.629 98.298)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.286 0) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C20-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DC67)
    (at 104.775 98.298 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DD04)
    (at 97.409 98.298)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -2.794 0) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C22-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DA20)
    (at 106.68 84.582 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -2.032 -0.127 360) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C23-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DA66)
    (at 106.68 91.948 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C24-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28D965)
    (at 106.68 66.802 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 2.286 360) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C25-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28D986)
    (at 106.807 74.168 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0.889 2.159 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C26-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5A28D6C1)
    (at 65.2145 65.2145 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at -1.9685 5.0165 180) (layer F.SilkS))
    (fp_text value SN75176B (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(R1-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(R3-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J14-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5A28D692)
    (at 65.151 72.644 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at -2.032 5.08 180) (layer F.SilkS))
    (fp_text value pD11 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 54 /RPi_GPIO/PPS))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J25-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 30 /1PPS_Sync))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 72 /RPi_GPIO/Arm\))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J24-Pad2)"))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J14-Pad1)"))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5A28D77B)
    (at 77.47 65.278 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at -3.175 3.302 180) (layer F.SilkS))
    (fp_text value pP03 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U4-Pad7)"))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 68 /RPi_GPIO/RxD))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 29 /Event))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 76 /RPi_GPIO/TimestampRst\))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 73 /RPi_GPIO/Rise_Fall\))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J14-Pad1)"))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A28DD90)
    (at 74.422 94.996 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at -1.524 -2.794 360) (layer F.SilkS))
    (fp_text value LVC1G86 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad21)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J27-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U10-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A28DB29)
    (at 91.567 94.996 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U6 (at -1.651 -2.794 360) (layer F.SilkS))
    (fp_text value LVC1G86 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad21)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J28-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U10-Pad3)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A28D9D5)
    (at 103.505 84.328)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U7 (at -1.143 -2.413) (layer F.SilkS))
    (fp_text value LVC1G86 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad21)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J29-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U12-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A28D9A7)
    (at 103.505 77.47)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U8 (at -1.27 -2.413) (layer F.SilkS))
    (fp_text value LVC1G86 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad21)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J30-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U12-Pad3)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A28DDC5)
    (at 65.532 97.155 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U9 (at -1.016 -2.794 360) (layer F.SilkS))
    (fp_text value 74LVC2G34 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U10-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U10-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R6-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A28DD17)
    (at 83.312 97.155 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U10 (at -1.016 -3.302 360) (layer F.SilkS))
    (fp_text value 74LVC2G34 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U10-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U10-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R8-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R7-Pad2)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A28DB43)
    (at 101.092 97.155 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U11 (at -1.016 -3.302 360) (layer F.SilkS))
    (fp_text value 74LVC2G34 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U10-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U10-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(R10-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(R9-Pad2)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A28DA73)
    (at 105.664 88.265)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U12 (at -3.429 -0.762) (layer F.SilkS))
    (fp_text value 74LVC2G34 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U12-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U12-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(R12-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(R11-Pad2)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A28D944)
    (at 105.664 70.485)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U13 (at -3.429 -0.889) (layer F.SilkS))
    (fp_text value 74LVC2G34 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U12-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U12-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(R14-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(R13-Pad2)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A28DD2E)
    (at 86.995 98.298 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C19-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF:via_0_6mm (layer F.Cu) (tedit 5A2A1597)
    (at 87.63 60.325)
    (fp_text reference "" (at -0.025 3.1) (layer F.SilkS))
    (fp_text value via_03 (at -0.05 1.875) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module w_logo:Logo_silk_OSHW_12x13mm (layer B.Cu) (tedit 0)
    (at 105.32618 78.40218 180)
    (descr "Open Hardware Logo, 12x13mm")
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 -0.9 180) (layer B.SilkS) hide)
  )
  (gr_text V1.0 (at 64.01054 102.59822) (layer B.SilkS))
  (gr_text "IDT Clock Block" (at 89.40038 102.69474) (layer B.SilkS))
  (gr_text $ (at 85.57006 79.36738) (layer F.SilkS))
  (gr_text KD5SSJ (at 73.98004 79.58582) (layer B.SilkS))
  (dimension 56 (width 0.15) (layer Dwgs.User)
    (gr_text "56 mm (Thru-hole socket J2)" (at 126.15 79.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 116.8 107.3) (xy 127.5 107.3)))
    (feature2 (pts (xy 116.8 51.3) (xy 127.5 51.3)))
    (crossbar (pts (xy 124.8 51.3) (xy 124.8 107.3)))
    (arrow1a (pts (xy 124.8 107.3) (xy 124.213579 106.173496)))
    (arrow1b (pts (xy 124.8 107.3) (xy 125.386421 106.173496)))
    (arrow2a (pts (xy 124.8 51.3) (xy 124.213579 52.426504)))
    (arrow2b (pts (xy 124.8 51.3) (xy 125.386421 52.426504)))
  )
  (gr_arc (start 112.8 54.3) (end 112.8 51.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.8 51.3) (end 112.8 51.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 53.8 54.3) (end 50.8 54.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 59.3 110.8) (layer Dwgs.User))
    (feature1 (pts (xy 54.3 108.3) (xy 54.3 113.5)))
    (feature2 (pts (xy 50.8 108.3) (xy 50.8 113.5)))
    (crossbar (pts (xy 50.8 110.8) (xy 54.3 110.8)))
    (arrow1a (pts (xy 54.3 110.8) (xy 53.173496 111.386421)))
    (arrow1b (pts (xy 54.3 110.8) (xy 53.173496 110.213579)))
    (arrow2a (pts (xy 50.8 110.8) (xy 51.926504 111.386421)))
    (arrow2b (pts (xy 50.8 110.8) (xy 51.926504 110.213579)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 61.05 99.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 57.8 107.3) (xy 63.5 107.3)))
    (feature2 (pts (xy 57.8 103.8) (xy 63.5 103.8)))
    (crossbar (pts (xy 60.8 103.8) (xy 60.8 107.3)))
    (arrow1a (pts (xy 60.8 107.3) (xy 60.213579 106.173496)))
    (arrow1b (pts (xy 60.8 107.3) (xy 61.386421 106.173496)))
    (arrow2a (pts (xy 60.8 103.8) (xy 60.213579 104.926504)))
    (arrow2b (pts (xy 60.8 103.8) (xy 61.386421 104.926504)))
  )
  (dimension 49 (width 0.15) (layer Dwgs.User)
    (gr_text "49 mm" (at 121.149999 79.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 116.8 103.8) (xy 122.499999 103.8)))
    (feature2 (pts (xy 116.8 54.8) (xy 122.499999 54.8)))
    (crossbar (pts (xy 119.799999 54.8) (xy 119.799999 103.8)))
    (arrow1a (pts (xy 119.799999 103.8) (xy 119.213578 102.673496)))
    (arrow1b (pts (xy 119.799999 103.8) (xy 120.38642 102.673496)))
    (arrow2a (pts (xy 119.799999 54.8) (xy 119.213578 55.926504)))
    (arrow2b (pts (xy 119.799999 54.8) (xy 120.38642 55.926504)))
  )
  (dimension 19.5 (width 0.15) (layer Dwgs.User)
    (gr_text "19.5 mm" (at 45.45 97.55 270) (layer Dwgs.User))
    (feature1 (pts (xy 49.8 107.3) (xy 44.1 107.3)))
    (feature2 (pts (xy 49.8 87.8) (xy 44.1 87.8)))
    (crossbar (pts (xy 46.8 87.8) (xy 46.8 107.3)))
    (arrow1a (pts (xy 46.8 107.3) (xy 46.213579 106.173496)))
    (arrow1b (pts (xy 46.8 107.3) (xy 47.386421 106.173496)))
    (arrow2a (pts (xy 46.8 87.8) (xy 46.213579 88.926504)))
    (arrow2b (pts (xy 46.8 87.8) (xy 47.386421 88.926504)))
  )
  (dimension 17 (width 0.15) (layer Dwgs.User)
    (gr_text "17 mm" (at 60.15 79.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 56.8 87.8) (xy 61.5 87.8)))
    (feature2 (pts (xy 56.8 70.8) (xy 61.5 70.8)))
    (crossbar (pts (xy 58.8 70.8) (xy 58.8 87.8)))
    (arrow1a (pts (xy 58.8 87.8) (xy 58.213579 86.673496)))
    (arrow1b (pts (xy 58.8 87.8) (xy 59.386421 86.673496)))
    (arrow2a (pts (xy 58.8 70.8) (xy 58.213579 71.926504)))
    (arrow2b (pts (xy 58.8 70.8) (xy 59.386421 71.926504)))
  )
  (dimension 5 (width 0.15) (layer Dwgs.User)
    (gr_text "5 mm" (at 59.55 68.8) (layer Dwgs.User))
    (feature1 (pts (xy 55.8 70.8) (xy 55.8 66.1)))
    (feature2 (pts (xy 50.8 70.8) (xy 50.8 66.1)))
    (crossbar (pts (xy 50.8 68.8) (xy 55.8 68.8)))
    (arrow1a (pts (xy 55.8 68.8) (xy 54.673496 69.386421)))
    (arrow1b (pts (xy 55.8 68.8) (xy 54.673496 68.213579)))
    (arrow2a (pts (xy 50.8 68.8) (xy 51.926504 69.386421)))
    (arrow2b (pts (xy 50.8 68.8) (xy 51.926504 68.213579)))
  )
  (dimension 29 (width 0.15) (layer Dwgs.User)
    (gr_text "29 mm" (at 68.8 62.649999) (layer Dwgs.User))
    (feature1 (pts (xy 83.3 58.8) (xy 83.3 63.999999)))
    (feature2 (pts (xy 54.3 58.8) (xy 54.3 63.999999)))
    (crossbar (pts (xy 54.3 61.299999) (xy 83.3 61.299999)))
    (arrow1a (pts (xy 83.3 61.299999) (xy 82.173496 61.88642)))
    (arrow1b (pts (xy 83.3 61.299999) (xy 82.173496 60.713578)))
    (arrow2a (pts (xy 54.3 61.299999) (xy 55.426504 61.88642)))
    (arrow2b (pts (xy 54.3 61.299999) (xy 55.426504 60.713578)))
  )
  (dimension 58 (width 0.15) (layer Dwgs.User)
    (gr_text "58 mm" (at 83.3 45.95) (layer Dwgs.User))
    (feature1 (pts (xy 112.3 49.8) (xy 112.3 44.6)))
    (feature2 (pts (xy 54.3 49.8) (xy 54.3 44.6)))
    (crossbar (pts (xy 54.3 47.3) (xy 112.3 47.3)))
    (arrow1a (pts (xy 112.3 47.3) (xy 111.173496 47.886421)))
    (arrow1b (pts (xy 112.3 47.3) (xy 111.173496 46.713579)))
    (arrow2a (pts (xy 54.3 47.3) (xy 55.426504 47.886421)))
    (arrow2b (pts (xy 54.3 47.3) (xy 55.426504 46.713579)))
  )
  (dimension 65 (width 0.15) (layer Dwgs.User)
    (gr_text "65 mm" (at 83.3 41.45) (layer Dwgs.User))
    (feature1 (pts (xy 115.8 49.8) (xy 115.8 40.1)))
    (feature2 (pts (xy 50.8 49.8) (xy 50.8 40.1)))
    (crossbar (pts (xy 50.8 42.8) (xy 115.8 42.8)))
    (arrow1a (pts (xy 115.8 42.8) (xy 114.673496 43.386421)))
    (arrow1b (pts (xy 115.8 42.8) (xy 114.673496 42.213579)))
    (arrow2a (pts (xy 50.8 42.8) (xy 51.926504 43.386421)))
    (arrow2b (pts (xy 50.8 42.8) (xy 51.926504 42.213579)))
  )
  (gr_arc (start 51.8 88.8) (end 50.8 88.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 54.8 86.8) (end 55.8 86.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 54.8 71.8) (end 54.8 70.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 51.8 69.8) (end 51.8 70.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 112.8 104.3) (end 115.8 104.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 53.8 104.3) (end 53.8 107.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8 88.8) (end 50.8 104.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8 54.3) (end 50.8 69.80174) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8 87.8) (end 54.8 87.8) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8 70.8) (end 54.8 70.8) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.8 71.8) (end 55.8 86.8) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.8 107.3) (end 112.8 107.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.79606 54.30012) (end 115.8 104.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 108.966 58.166) (xy 115.57 58.166) (xy 115.57 100.457) (xy 108.966 100.457) (xy 108.966 107.061)
        (xy 57.658 107.061) (xy 57.658 100.457) (xy 51.054 100.457) (xy 51.054 88.9) (xy 51.816 88.138)
        (xy 55.118 88.138) (xy 56.134 87.122) (xy 56.134 71.374) (xy 55.372 70.612) (xy 52.07 70.612)
        (xy 51.054 69.596) (xy 51.054 58.166) (xy 57.658 58.166) (xy 57.658 51.562) (xy 108.966 51.562)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 108.966 58.166) (xy 115.57 58.166) (xy 115.57 100.457) (xy 108.966 100.457) (xy 108.966 107.061)
        (xy 57.658 107.061) (xy 57.658 100.457) (xy 51.054 100.457) (xy 51.054 88.9) (xy 51.816 88.138)
        (xy 55.118 88.138) (xy 56.134 87.122) (xy 56.134 71.374) (xy 55.372 70.612) (xy 52.07 70.612)
        (xy 51.054 69.596) (xy 51.054 58.166) (xy 57.658 58.166) (xy 57.658 51.562) (xy 108.966 51.562)
      )
    )
  )
)
