(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.62448)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01524)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.524)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01524)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010f0_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference no)
			(plotvalue no)
			(plotfptext no)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "./ref80-single-test")
		)
	)
	(net 0 "")
	(net 1 "GNDPWR")
	(net 2 "VDC")
	(net 3 "unconnected-(U1-NC-Pad11)")
	(net 4 "unconnected-(U1-NC-Pad6)")
	(net 5 "GND")
	(net 6 "unconnected-(U1-NC-Pad7)")
	(net 7 "VDD")
	(net 8 "VREF")
	(net 9 "GNDREF")
	(net 10 "unconnected-(U1-NC-Pad12)")
	(net 11 "OP_STBL")
	(net 12 "unconnected-(U1-NC-Pad2)")
	(net 13 "unconnected-(U1-NC-Pad8)")
	(net 14 "unconnected-(U1-NC-Pad9)")
	(net 15 "Net-(U1-REFZ_S)")
	(net 16 "unconnected-(U1-NC-Pad10)")
	(net 17 "/T_SET")
	(net 18 "unconnected-(U1-NC-Pad1)")
	(net 19 "unconnected-(J1-Pin_5-Pad5)")
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 10.3 11.1 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -0.1 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_2220_5750Metric"
		(layer "F.Cu")
		(at 5.8 21.6)
		(descr "Capacitor SMD 2220 (5750 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -4.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 3.65 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_2220_5750Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.55 0)
			(size 1.8 5.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 8 "VREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 2.55 0)
			(size 1.8 5.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.138889)
			(net 9 "GNDREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 10.3 5.2 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0.1 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "800k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDPWR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/T_SET")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 10.3 7.3 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VDC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDPWR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 8.4 15.7 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.47u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 8 "VREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 9 "GNDREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 14 23)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 2.325 8.6)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "J1"
			(at 1.27 -2.33 360)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x04_Odd_Even"
			(at 1.27 9.95 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDPWR")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VDC")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "VDD")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J1-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "OP_STBL")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "VREF")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "GNDREF")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 35 2)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 14 2)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "NetTie:NetTie-2_SMD_Pad0.5mm"
		(layer "F.Cu")
		(at 10 13.7 90)
		(descr "Net tie, 2 pin, 0.5mm square SMD pads")
		(tags "net tie")
		(property "Reference" "NT2"
			(at 0 -1.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NetTie_2"
			(at 0 1.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "NetTie:NetTie-2_SMD_Pad0.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Net tie, 2 pins"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Net*Tie*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd circle
			(at -0.5 0 90)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 8 "VREF")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd circle
			(at 0.5 0 90)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 15 "Net-(U1-REFZ_S)")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 35 23)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "NetTie:NetTie-2_SMD_Pad0.5mm"
		(layer "F.Cu")
		(at 29.85 14.4 -90)
		(descr "Net tie, 2 pin, 0.5mm square SMD pads")
		(tags "net tie")
		(property "Reference" "NT1"
			(at 0 -1.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NetTie_2"
			(at 0 1.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "NetTie:NetTie-2_SMD_Pad0.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Net tie, 2 pins"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Net*Tie*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd circle
			(at -0.5 0 270)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 5 "GND")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd circle
			(at 0.5 0 270)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 9 "GNDREF")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 7.3 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.6 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4u7"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VDC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDPWR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 8.4 11.1 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "4u7"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "my-ic:LCCC-20-NAJ"
		(layer "F.Cu")
		(at 24.5 12.5)
		(descr "TI NAJ LCCC 20 Pin")
		(tags "NAJ LCC LCCC 20")
		(property "Reference" "U1"
			(at -5.9 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "REF80"
			(at 0 6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "my-ic:LCCC-20-NAJ"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref80.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.5V 0.05% 4mA Extremely Low Noise High Precision Voltage Reference, VSSOP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*NAJ* *LCCC*20*")
		(sheetname "Root")
		(sheetfile "ref80-single.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at 0 -3.61)
			(size 0.61 2.78)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "unconnected-(U1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.27 -4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "unconnected-(U1-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.54 -4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/T_SET")
			(pinfunction "T_SET")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -4.055 -2.54)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "VREF")
			(pinfunction "REFZ_F")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -4.055 -1.27)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U1-REFZ_S)")
			(pinfunction "REFZ_S")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -4.055 0)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "unconnected-(U1-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -4.055 1.27)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "unconnected-(U1-NC-Pad7)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -4.055 2.54)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "unconnected-(U1-NC-Pad8)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -2.54 4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "unconnected-(U1-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -1.27 4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "unconnected-(U1-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 0 4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "unconnected-(U1-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 1.27 4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "unconnected-(U1-NC-Pad12)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.54 4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 4.055 2.54)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "GNDREF")
			(pinfunction "REF_GND_S")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 4.055 1.27)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "REF_GND_F")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 4.055 0)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDPWR")
			(pinfunction "HEATM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 4.055 -1.27)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDPWR")
			(pinfunction "HEATM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 4.055 -2.54)
			(size 1.89 0.61)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VDC")
			(pinfunction "HEATP")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 2.54 -4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 1.27 -4.055)
			(size 0.61 1.89)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "OP_STBL")
			(pinfunction "OP_STBL")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD_3RD_PARTY}/3d/NAJ0020A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(gr_line
		(start 29.7 8.2)
		(end 30.5 9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 18.5 9)
		(end 19.3 8.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.25 22.5)
		(end 29.75 22.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28.5 5.5)
		(end 29.55 6.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 34.5 7.25)
		(end 29.75 2.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 14.5 17.75)
		(end 19.25 22.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28.8 17.7)
		(end 28 18.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.5 12)
		(end 34.5 12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 30.45 7.45)
		(end 31.5 8.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 34.5 13)
		(end 34.5 17.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.3 8.2)
		(end 18.55 7.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.75 22.5)
		(end 34.5 17.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.3 16.8)
		(end 18.55 17.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 14.5 9.5)
		(end 15.5 9.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.7 16.8)
		(end 30.45 17.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.55 18.45)
		(end 28.5 19.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 15.5 9.5)
		(end 15.5 7.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.25 21.5)
		(end 19.75 21.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 14.5 7.25)
		(end 14.5 9.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.75 21.5)
		(end 15.5 17.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 15.5 17.25)
		(end 15.5 15.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.2 17.7)
		(end 19.45 18.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.5 5.5)
		(end 28.5 5.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.3 16.8)
		(end 18.5 16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.5 17.25)
		(end 29.25 21.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 17.5 8.5)
		(end 17.5 16.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 18.55 17.55)
		(end 17.5 16.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 30.5 9)
		(end 30.5 16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 37 2)
		(end 37 23)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 14.5 13.8)
		(end 15.5 13.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28.8 17.7)
		(end 29.55 18.45)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 37 23)
		(mid 36.414214 24.414214)
		(end 35 25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.2 7.3)
		(end 21 6.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 34.5 7.25)
		(end 34.5 12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 2 0)
		(end 35 0)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.75 3.5)
		(end 29.25 3.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21 6.5)
		(end 28 6.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 15.5 7.75)
		(end 19.75 3.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.5 7.75)
		(end 33.5 12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35 25)
		(end 2 25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 2 25)
		(mid 0.585786 24.414214)
		(end 0 23)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 18.5 16)
		(end 18.5 9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.7 8.2)
		(end 30.45 7.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 15.5 13.8)
		(end 15.5 11.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.25 2.5)
		(end 14.5 7.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 30.5 16)
		(end 29.7 16.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21 18.5)
		(end 20.2 17.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.25 3.5)
		(end 33.5 7.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 14.5 15.5)
		(end 14.5 17.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 31.5 16.5)
		(end 31.5 8.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 15.5 11.2)
		(end 14.5 11.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 15.5 15.5)
		(end 14.5 15.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.5 19.5)
		(end 28.5 19.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 14.5 11.2)
		(end 14.5 13.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.5 13)
		(end 34.5 13)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 0 2)
		(mid 0.585786 0.585786)
		(end 2 0)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 31.5 16.5)
		(end 30.45 17.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28 6.5)
		(end 28.8 7.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 19.45 6.55)
		(end 20.5 5.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28 18.5)
		(end 21 18.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.75 2.5)
		(end 19.25 2.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28.8 7.3)
		(end 29.55 6.55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 35 0)
		(mid 36.414214 0.585786)
		(end 37 2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.5 19.5)
		(end 19.45 18.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.2 7.3)
		(end 19.45 6.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 23)
		(end 0 2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.5 17.25)
		(end 33.5 13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 17.5 8.5)
		(end 18.55 7.45)
		(layer "Edge.Cuts")
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.444454 11.714125) (xy 9.349697 11.714835) (xy 9.25494 11.700681) (xy 9.160184 11.671662) (xy 9.065427 11.627778)
				(xy 8.970671 11.56903) (xy 8.399293 12.050707) (xy 9.105447 12.396453) (xy 9.201532 12.244864) (xy 9.297618 12.114979)
				(xy 9.393703 12.006797) (xy 9.489789 11.920319) (xy 9.585875 11.855546)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VDC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.625 8.05) (xy 9.494134 8.029805) (xy 9.363268 7.991611) (xy 9.232402 7.935418) (xy 9.101536 7.861224)
				(xy 8.970671 7.76903) (xy 8.399 8.25) (xy 8.970671 8.73097) (xy 9.101536 8.638775) (xy 9.232402 8.564581)
				(xy 9.363268 8.508388) (xy 9.494134 8.470194) (xy 9.625 8.45)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.175 12.15) (xy 7.305865 12.180764) (xy 7.436731 12.234244) (xy 7.567597 12.310438) (xy 7.698463 12.409346)
				(xy 7.829329 12.53097) (xy 8.401 12.05) (xy 7.829329 11.56903) (xy 7.698463 11.690653) (xy 7.567597 11.789561)
				(xy 7.436731 11.865755) (xy 7.305865 11.919235) (xy 7.175 11.95)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.89 11.48) (xy 10.816715 11.467731) (xy 10.74343 11.444662) (xy 10.670145 11.410794) (xy 10.59686 11.366125)
				(xy 10.523576 11.310657) (xy 10.299 11.58) (xy 10.523576 11.849343) (xy 10.59686 11.793874) (xy 10.670145 11.749205)
				(xy 10.74343 11.715337) (xy 10.816715 11.692268) (xy 10.89 11.68)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 5.080667 17.727115) (xy 4.937693 17.484267) (xy 5.008499 17.285268) (xy 5.207755 17.089508)
				(xy 5.450131 16.856382) (xy 5.650298 16.545281) (xy 4.864293 16.219293) (xy 4.079702 16.545281)
				(xy 4.212908 16.943981) (xy 4.275658 17.248591) (xy 4.336546 17.50739) (xy 4.464167 17.768656) (xy 4.727115 18.080667)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VDC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.175 8.45) (xy 7.305865 8.470194) (xy 7.436731 8.508388) (xy 7.567597 8.564581) (xy 7.698463 8.638775)
				(xy 7.829329 8.73097) (xy 8.401 8.25) (xy 7.829329 7.76903) (xy 7.698463 7.861224) (xy 7.567597 7.935418)
				(xy 7.436731 7.991611) (xy 7.305865 8.029805) (xy 7.175 8.05)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.175 6.55) (xy 7.305865 6.570194) (xy 7.436731 6.608388) (xy 7.567597 6.664581) (xy 7.698463 6.738775)
				(xy 7.829329 6.83097) (xy 8.401 6.35) (xy 7.829329 5.86903) (xy 7.698463 5.961224) (xy 7.567597 6.035418)
				(xy 7.436731 6.091611) (xy 7.305865 6.129805) (xy 7.175 6.15)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.391968 13.92) (xy 29.491564 13.934238) (xy 29.554304 13.971155) (xy 29.603482 14.022049)
				(xy 29.662392 14.07822) (xy 29.754329 14.13097) (xy 29.851 13.9) (xy 29.85 13.65) (xy 29.736266 13.64688)
				(xy 29.655723 13.63944) (xy 29.586243 13.63056) (xy 29.5057 13.62312) (xy 29.391968 13.62)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.45 6.25) (xy 10.474 6.175089) (xy 10.498 6.107378) (xy 10.522 6.046868) (xy 10.546 5.993557)
				(xy 10.57 5.947447) (xy 10.3 5.709) (xy 10.03 5.947447) (xy 10.054 5.993557) (xy 10.078 6.046868)
				(xy 10.102 6.107378) (xy 10.126 6.175089) (xy 10.15 6.25)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 2.784017 18.296571) (xy 2.701019 18.499959) (xy 2.618022 18.677429) (xy 2.535024 18.82898) (xy 2.452027 18.954614)
				(xy 2.36903 19.054329) (xy 3.250707 21.600707) (xy 3.929377 18.905843) (xy 3.771015 18.788072) (xy 3.612654 18.632905)
				(xy 3.454293 18.440339) (xy 3.295932 18.210377) (xy 3.137571 17.943017)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 3.456371 9.867208) (xy 3.164455 10.098234) (xy 2.913374 10.188769) (xy 2.662586 10.21254) (xy 2.371549 10.243275)
				(xy 1.999719 10.354702) (xy 2.324293 11.140707) (xy 3.110298 11.465281) (xy 3.221723 11.09345) (xy 3.252458 10.802412)
				(xy 3.27623 10.551624) (xy 3.366765 10.300544) (xy 3.597792 10.008629)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.700797 10.542219) (xy 9.762983 10.578205) (xy 9.82517 10.624991) (xy 9.887357 10.682577) (xy 9.949544 10.750963)
				(xy 10.011731 10.83015) (xy 10.300707 10.620707) (xy 10.076424 10.350657) (xy 10.029583 10.375055)
				(xy 9.982742 10.392269) (xy 9.9359 10.402297) (xy 9.889059 10.405139) (xy 9.842219 10.400797)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(U1-REFZ_S)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.524592 13.216829) (xy 10.434699 13.132905) (xy 10.363854 13.081242) (xy 10.295064 13.046762)
				(xy 10.211334 13.014384) (xy 10.095671 12.96903) (xy 9.999293 13.199293) (xy 10.095671 13.43097)
				(xy 10.1776 13.383565) (xy 10.241783 13.33111) (xy 10.297117 13.29172) (xy 10.352499 13.283508)
				(xy 10.416829 13.324592)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VDC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.4788 9.35) (xy 28.433039 9.433876) (xy 28.387279 9.506315) (xy 28.34152 9.567315) (xy 28.29576 9.616876)
				(xy 28.25 9.655) (xy 28.555 9.961) (xy 28.86 9.655) (xy 28.814239 9.616876) (xy 28.768479 9.567315)
				(xy 28.72272 9.506315) (xy 28.67696 9.433876) (xy 28.6312 9.35)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VDC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 6.404541 8.412617) (xy 6.154524 8.55905) (xy 5.950462 8.483461) (xy 5.749982 8.274862) (xy 5.510713 8.022271)
				(xy 5.190281 7.814702) (xy 4.864293 8.600707) (xy 5.190281 9.385298) (xy 5.58243 9.248386) (xy 5.878365 9.174063)
				(xy 6.127935 9.099211) (xy 6.380991 8.960715) (xy 6.687383 8.695459)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.88617 13.724039) (xy 29.799663 13.699538) (xy 29.713157 13.665737) (xy 29.626652 13.622636)
				(xy 29.540146 13.570235) (xy 29.45364 13.508534) (xy 28.554293 13.769293) (xy 29.405859 14.063392)
				(xy 29.459494 14.020138) (xy 29.51313 13.985789) (xy 29.566767 13.960344) (xy 29.620403 13.943804)
				(xy 29.674039 13.93617)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.67111 14.866759) (xy 29.618059 14.8602) (xy 29.565009 14.844905) (xy 29.511959 14.820875)
				(xy 29.458909 14.788109) (xy 29.405859 14.746608) (xy 28.554293 15.040707) (xy 29.45823 15.295998)
				(xy 29.543232 15.233976) (xy 29.628234 15.181254) (xy 29.713236 15.137833) (xy 29.798238 15.103711)
				(xy 29.883241 15.07889)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 6.490088 21.494642) (xy 6.68207 21.590492) (xy 6.874052 21.725155) (xy 7.066035 21.898631) (xy 7.258017 22.110918)
				(xy 7.45 22.362019) (xy 8.350707 21.600707) (xy 7.45 20.536802) (xy 7.328728 20.709022) (xy 7.207456 20.85556)
				(xy 7.086185 20.976417) (xy 6.964913 21.071593) (xy 6.843642 21.141088)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.760764 13.468526) (xy 29.802202 13.536769) (xy 29.786628 13.593907) (xy 29.736161 13.650502)
				(xy 29.672921 13.717121) (xy 29.61903 13.804329) (xy 29.850707 13.900707) (xy 30.08097 13.804329)
				(xy 30.039432 13.687649) (xy 30.015614 13.600126) (xy 29.991321 13.526585) (xy 29.948356 13.451855)
				(xy 29.868526 13.360764)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.644454 10.203033) (xy 9.525918 10.152823) (xy 9.407383 10.079737) (xy 9.288847 9.983776) (xy 9.170312 9.864937)
				(xy 9.051777 9.723223) (xy 8.399293 10.149293) (xy 8.970671 10.63097) (xy 9.077143 10.537393) (xy 9.183615 10.461953)
				(xy 9.290088 10.404649) (xy 9.39656 10.365483) (xy 9.503033 10.344454)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/T_SET")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.45 4.508) (xy 10.4511 4.403346) (xy 10.456688 4.328602) (xy 10.470192 4.265105) (xy 10.495041 4.194192)
				(xy 10.534665 4.097202) (xy 10.3 3.999) (xy 10.065335 4.097202) (xy 10.104957 4.194192) (xy 10.129806 4.265105)
				(xy 10.143311 4.328602) (xy 10.148899 4.403346) (xy 10.15 4.508)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.39865 15.19) (xy 29.510839 15.18584) (xy 29.590149 15.17592) (xy 29.6585 15.16408) (xy 29.73781 15.15416)
				(xy 29.85 15.15) (xy 29.851 14.9) (xy 29.754329 14.66903) (xy 29.66316 14.722776) (xy 29.605865 14.781423)
				(xy 29.558587 14.835293) (xy 29.497467 14.87471) (xy 29.39865 14.89)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.669974 9.028553) (xy 29.603456 8.943433) (xy 29.57873 8.869887) (xy 29.573732 8.796325) (xy 29.566398 8.711158)
				(xy 29.534665 8.602798) (xy 29.299293 8.699293) (xy 29.120395 8.879605) (xy 29.213846 8.960806)
				(xy 29.289567 9.007316) (xy 29.359378 9.042261) (xy 29.4351 9.088771) (xy 29.528553 9.169974)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 2.378033 6.839125) (xy 2.21655 7.094332) (xy 2.055068 7.313023) (xy 1.893587 7.495198) (xy 1.732105 7.640857)
				(xy 1.570623 7.75) (xy 2.324293 8.600707) (xy 3.175 7.75) (xy 3.072175 7.673091) (xy 2.96935 7.571833)
				(xy 2.866525 7.446227) (xy 2.7637 7.296271) (xy 2.660875 7.121967)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 6.188066 11.95) (xy 5.914021 11.887638) (xy 5.796655 11.717505) (xy 5.762535 11.465024) (xy 5.738227 11.15562)
				(xy 5.650298 10.814719) (xy 4.864 11.14) (xy 4.865 11.99) (xy 5.194508 12.00664) (xy 5.426673 12.04632)
				(xy 5.626391 12.09368) (xy 5.858557 12.13336) (xy 6.188066 12.15)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.89 6.62) (xy 10.806 6.613599) (xy 10.722 6.602399) (xy 10.638 6.5864) (xy 10.554 6.5656)
				(xy 10.47 6.54) (xy 10.299 6.82) (xy 10.47 7.1) (xy 10.554 7.074399) (xy 10.638 7.053599) (xy 10.722 7.0376)
				(xy 10.806 7.0264) (xy 10.89 7.02)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.15 18) (xy 8.017123 18.279416) (xy 7.884247 18.522074) (xy 7.75137 18.727974) (xy 7.618494 18.897116)
				(xy 7.485618 19.029501) (xy 8.35 21.601) (xy 9.23097 19.054329) (xy 9.114775 18.915691) (xy 8.998581 18.740939)
				(xy 8.882388 18.530073) (xy 8.766194 18.283093) (xy 8.65 18)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.89 10.52) (xy 10.816715 10.507731) (xy 10.74343 10.484662) (xy 10.670145 10.450794) (xy 10.59686 10.406125)
				(xy 10.523576 10.350657) (xy 10.299 10.62) (xy 10.523576 10.889343) (xy 10.59686 10.833874) (xy 10.670145 10.789205)
				(xy 10.74343 10.755337) (xy 10.816715 10.732268) (xy 10.89 10.72)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/T_SET")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.35 8.5212) (xy 21.411 8.544083) (xy 21.472 8.578404) (xy 21.532999 8.624164) (xy 21.593999 8.681363)
				(xy 21.655 8.75) (xy 21.961 8.445) (xy 21.655 8.14) (xy 21.593999 8.208636) (xy 21.532999 8.265835)
				(xy 21.472 8.311595) (xy 21.411 8.345916) (xy 21.35 8.3688)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 6.925 14.375) (xy 7.070865 14.406111) (xy 7.216731 14.462264) (xy 7.362597 14.543458) (xy 7.508463 14.649693)
				(xy 7.654329 14.78097) (xy 8.401 14.225) (xy 7.654329 13.66903) (xy 7.508463 13.800306) (xy 7.362597 13.906541)
				(xy 7.216731 13.987735) (xy 7.070865 14.043888) (xy 6.925 14.075)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.849369 7.032212) (xy 10.934773 7.125558) (xy 10.988378 7.198102) (xy 11.031384 7.263713)
				(xy 11.08499 7.336258) (xy 11.170395 7.429605) (xy 11.350707 7.250707) (xy 11.529605 7.070395) (xy 11.436258 6.98499)
				(xy 11.363713 6.931384) (xy 11.298102 6.888378) (xy 11.225558 6.834773) (xy 11.132212 6.749369)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 26.89 15.305) (xy 26.861321 15.403428) (xy 26.832643 15.492556) (xy 26.803964 15.572384) (xy 26.775286 15.642912)
				(xy 26.746608 15.704141) (xy 27.04 16.556) (xy 27.333392 15.704141) (xy 27.304713 15.642912) (xy 27.276035 15.572384)
				(xy 27.247356 15.492556) (xy 27.218678 15.403428) (xy 27.19 15.305)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 8.65 18.325) (xy 8.714999 18.170999) (xy 8.779999 18.036499) (xy 8.845 17.9215) (xy 8.91 17.826)
				(xy 8.975 17.75) (xy 8.4 17.174) (xy 7.825 17.75) (xy 7.889999 17.826) (xy 7.954999 17.9215) (xy 8.02 18.036499)
				(xy 8.085 18.170999) (xy 8.15 18.325)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.875 13.95) (xy 9.729134 13.932805) (xy 9.583268 13.896111) (xy 9.437402 13.839918) (xy 9.291536 13.764224)
				(xy 9.145671 13.66903) (xy 8.399 14.225) (xy 9.145671 14.78097) (xy 9.291536 14.675776) (xy 9.437402 14.590082)
				(xy 9.583268 14.523887) (xy 9.729134 14.477193) (xy 9.875 14.45)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.582939 8.359299) (xy 27.535351 8.332256) (xy 27.487763 8.295166) (xy 27.440175 8.248029)
				(xy 27.392587 8.190845) (xy 27.345 8.123614) (xy 27.039293 8.445707) (xy 27.345 8.734516) (xy 27.41414 8.6548)
				(xy 27.48328 8.588196) (xy 27.55242 8.534705) (xy 27.62156 8.494327) (xy 27.690701 8.467061)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.895978 10.72) (xy 11.000696 10.724161) (xy 11.074243 10.73707) (xy 11.136114 10.759364) (xy 11.205801 10.791683)
				(xy 11.302798 10.834665) (xy 11.401 10.6) (xy 11.302798 10.365335) (xy 11.204176 10.413398) (xy 11.135417 10.455752)
				(xy 11.075285 10.489541) (xy 11.00255 10.511909) (xy 10.895978 10.52)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/T_SET")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.15 4.15) (xy 10.126 4.22491) (xy 10.102 4.29262) (xy 10.078 4.353131) (xy 10.054 4.406441)
				(xy 10.03 4.452552) (xy 10.3 4.691) (xy 10.57 4.452552) (xy 10.546 4.406441) (xy 10.522 4.353131)
				(xy 10.498 4.29262) (xy 10.474 4.22491) (xy 10.45 4.15)
			)
		)
	)
	(zone
		(net 11)
		(net_name "OP_STBL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 6.483293 13.558944) (xy 6.215929 13.713918) (xy 5.99952 13.627258) (xy 5.787492 13.396688) (xy 5.53327 13.119928)
				(xy 5.190281 12.894702) (xy 4.864293 13.680707) (xy 5.190281 14.465298) (xy 5.567254 14.318498)
				(xy 5.840943 14.215093) (xy 6.066224 14.105229) (xy 6.29797 13.939052) (xy 6.591056 13.666707)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VDC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.992421 8.370422) (xy 10.077132 8.298737) (xy 10.161844 8.231853) (xy 10.246556 8.169768) (xy 10.331268 8.112484)
				(xy 10.41598 8.06) (xy 10.300707 7.779293) (xy 9.99 7.694021) (xy 9.933915 7.782332) (xy 9.877831 7.865844)
				(xy 9.821746 7.944555) (xy 9.765662 8.018467) (xy 9.709578 8.087579)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.418388 13.893743) (xy 27.475538 13.909072) (xy 27.532689 13.933702) (xy 27.589839 13.967632)
				(xy 27.64699 14.010862) (xy 27.704141 14.063392) (xy 28.555707 13.769293) (xy 27.703769 13.476856)
				(xy 27.604266 13.536407) (xy 27.504764 13.586658) (xy 27.405261 13.627609) (xy 27.305759 13.65926)
				(xy 27.206257 13.681612)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.783639 11.657781) (xy 9.842196 11.6751) (xy 9.900753 11.702916) (xy 9.95931 11.741229) (xy 10.017867 11.790037)
				(xy 10.076424 11.849343) (xy 10.300707 11.579293) (xy 10.076424 11.310657) (xy 9.989583 11.373397)
				(xy 9.902742 11.425338) (xy 9.815901 11.466479) (xy 9.72906 11.49682) (xy 9.642219 11.516361)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(U1-REFZ_S)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.195 11.3062) (xy 19.274828 11.322374) (xy 19.354656 11.35218) (xy 19.434484 11.395619) (xy 19.514312 11.452689)
				(xy 19.594141 11.523392) (xy 20.446 11.23) (xy 19.594141 10.936608) (xy 19.514312 11.00731) (xy 19.434484 11.06438)
				(xy 19.354656 11.107819) (xy 19.274828 11.137625) (xy 19.195 11.1538)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.671231 6.438388) (xy 9.554894 6.38266) (xy 9.438557 6.308932) (xy 9.32222 6.217205) (xy 9.205883 6.107477)
				(xy 9.089547 5.97975) (xy 8.399293 6.349293) (xy 8.970671 6.83097) (xy 9.054214 6.783108) (xy 9.137757 6.748204)
				(xy 9.221301 6.726256) (xy 9.304844 6.717265) (xy 9.388388 6.721231)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/T_SET")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 20.236853 8.3738) (xy 20.12542 8.371586) (xy 20.046427 8.366308) (xy 19.978246 8.360008) (xy 19.899253 8.35473)
				(xy 19.787821 8.352517) (xy 19.786821 8.606517) (xy 19.967426 8.786122) (xy 20.028302 8.708264)
				(xy 20.065534 8.63745) (xy 20.09927 8.579573) (xy 20.14966 8.540525) (xy 20.236853 8.5262)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.805 11.13) (xy 29.725171 11.115921) (xy 29.645343 11.089543) (xy 29.565515 11.050864) (xy 29.485687 10.999886)
				(xy 29.405859 10.936608) (xy 28.554 11.23) (xy 29.405859 11.523392) (xy 29.485687 11.460113) (xy 29.565515 11.409135)
				(xy 29.645343 11.370456) (xy 29.725171 11.344078) (xy 29.805 11.33)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.806474 17.085764) (xy 9.690534 17.045945) (xy 9.574595 16.984782) (xy 9.458655 16.902274)
				(xy 9.342716 16.798421) (xy 9.226777 16.673223) (xy 8.399293 17.175707) (xy 9.226777 17.676777)
				(xy 9.364268 17.529707) (xy 9.50176 17.407848) (xy 9.639252 17.311198) (xy 9.776744 17.239757) (xy 9.914236 17.193526)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 7.175 10.25) (xy 7.305865 10.280764) (xy 7.436731 10.334244) (xy 7.567597 10.410438) (xy 7.698463 10.509346)
				(xy 7.829329 10.63097) (xy 8.401 10.15) (xy 7.829329 9.66903) (xy 7.698463 9.790653) (xy 7.567597 9.889561)
				(xy 7.436731 9.965755) (xy 7.305865 10.019235) (xy 7.175 10.05)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 1.373224 21.635355) (xy 1.568579 21.72441) (xy 1.763934 21.851915) (xy 1.959289 22.017868) (xy 2.154644 22.222271)
				(xy 2.35 22.465124) (xy 3.250707 21.600707) (xy 2.35 20.663663) (xy 2.19707 20.880241) (xy 2.044141 21.064487)
				(xy 1.891213 21.216399) (xy 1.738284 21.335978) (xy 1.585355 21.423224)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 21.70934 10.001577) (xy 21.640096 9.973058) (xy 21.570852 9.931269) (xy 21.501609 9.876211)
				(xy 21.432365 9.807884) (xy 21.363122 9.726287) (xy 20.444293 9.959293) (xy 21.295859 10.253392)
				(xy 21.357002 10.204304) (xy 21.418146 10.165355) (xy 21.479289 10.136545) (xy 21.540433 10.117873)
				(xy 21.601577 10.10934)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VDC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.89 7.68) (xy 10.816715 7.667731) (xy 10.74343 7.644662) (xy 10.670145 7.610794) (xy 10.59686 7.566125)
				(xy 10.523576 7.510657) (xy 10.299 7.78) (xy 10.523576 8.049343) (xy 10.59686 7.993874) (xy 10.670145 7.949205)
				(xy 10.74343 7.915337) (xy 10.816715 7.892268) (xy 10.89 7.88)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.15 6.26) (xy 10.124 6.343095) (xy 10.098 6.41839) (xy 10.071999 6.485884) (xy 10.045999 6.545579)
				(xy 10.02 6.597475) (xy 10.3 6.821) (xy 10.58 6.597475) (xy 10.554 6.545579) (xy 10.528 6.485884)
				(xy 10.501999 6.41839) (xy 10.475999 6.343095) (xy 10.45 6.26)
			)
		)
	)
	(zone
		(net 11)
		(net_name "OP_STBL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 25.6938 7.195) (xy 25.650361 7.302092) (xy 25.606923 7.395552) (xy 25.563484 7.47538) (xy 25.520046 7.541576)
				(xy 25.476608 7.594141) (xy 25.77 8.446) (xy 26.063392 7.594141) (xy 26.019953 7.541576) (xy 25.976515 7.47538)
				(xy 25.933076 7.395552) (xy 25.889638 7.302092) (xy 25.8462 7.195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.732825 12.425754) (xy 29.677326 12.408582) (xy 29.621828 12.381388) (xy 29.56633 12.34417)
				(xy 29.510832 12.296929) (xy 29.455334 12.239666) (xy 28.554293 12.500707) (xy 29.405859 12.793392)
				(xy 29.499536 12.723548) (xy 29.593213 12.666005) (xy 29.686891 12.620761) (xy 29.780568 12.587818)
				(xy 29.874246 12.567175)
			)
		)
	)
	(zone
		(net 9)
		(net_name "GNDREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.6312 15.65) (xy 28.67696 15.566123) (xy 28.72272 15.493684) (xy 28.768479 15.432684) (xy 28.814239 15.383123)
				(xy 28.86 15.345) (xy 28.555 15.039) (xy 28.25 15.345) (xy 28.29576 15.383123) (xy 28.34152 15.432684)
				(xy 28.387279 15.493684) (xy 28.433039 15.566123) (xy 28.4788 15.65)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 2.810075 17.615521) (xy 2.66997 17.402599) (xy 2.684726 17.216902) (xy 2.799556 17.030642) (xy 2.959675 16.81603)
				(xy 3.110298 16.545281) (xy 2.324293 16.219293) (xy 1.539702 16.545281) (xy 1.701999 16.936269)
				(xy 1.829969 17.211964) (xy 1.968471 17.434544) (xy 2.162368 17.666188) (xy 2.456521 17.969075)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 9.586153 6.918994) (xy 9.682613 6.942398) (xy 9.779074 6.970603) (xy 9.875535 7.003609) (xy 9.971996 7.041414)
				(xy 10.068457 7.084019) (xy 10.300707 6.820707) (xy 10.076424 6.550657) (xy 10.034938 6.577356)
				(xy 9.993452 6.599255) (xy 9.951965 6.616354) (xy 9.910479 6.628653) (xy 9.868994 6.636153)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.37 13.8462) (xy 27.436828 13.865727) (xy 27.503656 13.897209) (xy 27.570484 13.940648) (xy 27.637312 13.996042)
				(xy 27.704141 14.063392) (xy 28.556 13.77) (xy 27.704141 13.476608) (xy 27.637312 13.543957) (xy 27.570484 13.599351)
				(xy 27.503656 13.64279) (xy 27.436828 13.674272) (xy 27.37 13.6938)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 27.826718 7.1762) (xy 27.874842 7.191063) (xy 27.872596 7.231485) (xy 27.842772 7.291215) (xy 27.808164 7.364)
				(xy 27.791563 7.443589) (xy 28.046563 7.443589) (xy 28.142765 7.208924) (xy 28.062505 7.162758)
				(xy 28.011166 7.113484) (xy 27.968352 7.068779) (xy 27.913668 7.036324) (xy 27.826718 7.0238)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.5 14.1238) (xy 10.394024 14.115656) (xy 10.321758 14.093178) (xy 10.262047 14.059295) (xy 10.193736 14.016936)
				(xy 10.095671 13.96903) (xy 9.999 14.2) (xy 10.095671 14.43097) (xy 10.193736 14.383063) (xy 10.262047 14.340704)
				(xy 10.321758 14.306821) (xy 10.394024 14.284343) (xy 10.5 14.2762)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 29.069007 8.249816) (xy 29.066614 8.361545) (xy 29.060908 8.440735) (xy 29.054098 8.509079)
				(xy 29.048392 8.588269) (xy 29.046 8.7) (xy 29.3 8.701) (xy 29.479605 8.520395) (xy 29.401975 8.45943)
				(xy 29.331595 8.421883) (xy 29.27421 8.387762) (xy 29.235565 8.33707) (xy 29.221407 8.249816)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/T_SET")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 19.711621 8.098517) (xy 19.703228 8.206252) (xy 19.680104 8.279645) (xy 19.64533 8.340251) (xy 19.601987 8.409623)
				(xy 19.553156 8.509315) (xy 19.787821 8.607517) (xy 20.022486 8.509315) (xy 19.973654 8.409623)
				(xy 19.93031 8.340251) (xy 19.895536 8.279645) (xy 19.872413 8.206252) (xy 19.864021 8.098517)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/T_SET")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 10.3762 4.508) (xy 10.384592 4.400264) (xy 10.407715 4.32687) (xy 10.442489 4.266264) (xy 10.485833 4.196893)
				(xy 10.534665 4.097202) (xy 10.3 3.999) (xy 10.065335 4.097202) (xy 10.114166 4.196893) (xy 10.157509 4.266264)
				(xy 10.192283 4.32687) (xy 10.215407 4.400264) (xy 10.2238 4.508)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDPWR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 11.6 7.703386) (xy 11.600416 7.590943) (xy 11.601408 7.511148) (xy 11.602592 7.442236) (xy 11.603584 7.362441)
				(xy 11.604 7.25) (xy 11.35 7.249) (xy 11.170395 7.429605) (xy 11.242784 7.489437) (xy 11.30579 7.529096)
				(xy 11.355561 7.566217) (xy 11.388248 7.618435) (xy 11.4 7.703386)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 11.908 10.5) (xy 11.801444 10.493935) (xy 11.727533 10.47642) (xy 11.66582 10.448471) (xy 11.595858 10.411103)
				(xy 11.497202 10.365335) (xy 11.399 10.6) (xy 11.497202 10.834665) (xy 11.595858 10.788895) (xy 11.66582 10.751528)
				(xy 11.727533 10.723579) (xy 11.801444 10.706064) (xy 11.908 10.7)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.532627 7.571443) (xy 28.456376 7.495192) (xy 28.402264 7.44108) (xy 28.35553 7.394346) (xy 28.301417 7.340233)
				(xy 28.225168 7.263984) (xy 28.044856 7.442882) (xy 28.045563 7.697589) (xy 28.145032 7.682788)
				(xy 28.222435 7.65245) (xy 28.288033 7.627675) (xy 28.352089 7.62956) (xy 28.424865 7.679205)
			)
		)
	)
)
