(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 69)
    (no_connects 3)
    (area 122.860999 66.472999 186.518051 117.430051)
    (thickness 1.6)
    (drawings 42)
    (tracks 229)
    (zones 0)
    (modules 28)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 7.4 7.4)
    (pad_drill 3.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GPIO14_IN_DB)
  (net 2 GND)
  (net 3 3V3)
  (net 4 GPIO14_IN)
  (net 5 GPIO4)
  (net 6 GPIO5)
  (net 7 GPIO13)
  (net 8 GPIO2_OUT)
  (net 9 GPIO2)
  (net 10 GPIO2_IN_ST)
  (net 11 "Net-(P4-Pad1)")
  (net 12 "Net-(P5-Pad1)")
  (net 13 RESET_SER)
  (net 14 TXD)
  (net 15 RXD)
  (net 16 "Net-(P6-Pad4)")
  (net 17 "Net-(P6-Pad5)")
  (net 18 RESET)
  (net 19 BATT)
  (net 20 ADC)
  (net 21 "Net-(R9-Pad2)")
  (net 22 "Net-(R11-Pad1)")
  (net 23 GPIO12)
  (net 24 GPIO12_OUT)
  (net 25 GPIO14)
  (net 26 GPIO2_IN)
  (net 27 GPIO2_OUT_ST)
  (net 28 "Net-(U1-Pad10)")
  (net 29 "Net-(U1-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3V3)
    (add_net ADC)
    (add_net BATT)
    (add_net GND)
    (add_net GPIO12)
    (add_net GPIO12_OUT)
    (add_net GPIO13)
    (add_net GPIO14)
    (add_net GPIO14_IN)
    (add_net GPIO14_IN_DB)
    (add_net GPIO2)
    (add_net GPIO2_IN)
    (add_net GPIO2_IN_ST)
    (add_net GPIO2_OUT)
    (add_net GPIO2_OUT_ST)
    (add_net GPIO4)
    (add_net GPIO5)
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad5)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net RESET)
    (add_net RESET_SER)
    (add_net RXD)
    (add_net TXD)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5758AFE4)
    (at 164.084 76.708)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 4.572 0) (layer F.SilkS))
    (fp_text value C (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GPIO14_IN_DB))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57583936)
    (at 135.128 110.744 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.572 -0.254 270) (layer F.SilkS))
    (fp_text value C (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 5758B01A)
    (at 157.226 76.708 180)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D1 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value D (at 0.05 -2 180) (layer F.Fab))
    (fp_text user A (at 3.81 -1.778 180) (layer Cmts.User))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 4 GPIO14_IN))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GPIO14_IN_DB))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5758B233)
    (at 181.864 100.33 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GPIO4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GPIO5))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GPIO13))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 575B5817)
    (at 182.118 81.28 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 8.001 360) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 GPIO2_OUT))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 GPIO2))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 GPIO2_IN_ST))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5758458B)
    (at 164.338 99.06 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -0.762 5.588 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5758B230)
    (at 177.8 90.17)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 15.494) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GPIO13))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GPIO5))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GPIO4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 3V3))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5758B0AA)
    (at 141.478 112.014 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at -0.254 15.494 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 RESET_SER))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 TXD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 RXD))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5758B805)
    (at 164.338 112.014 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 5.334 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 RESET))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 RESET_SER))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 575838B9)
    (at 165.862 102.362 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -4.572 0 180) (layer F.SilkS))
    (fp_text value R (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 GPIO2))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5758AFE1)
    (at 164.084 80.264)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 4.572 0) (layer F.SilkS))
    (fp_text value R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GPIO14_IN))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 575838B6)
    (at 165.862 92.71 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.572 0 180) (layer F.SilkS))
    (fp_text value R (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 GPIO4))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5758B102)
    (at 155.448 80.264 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 4.572 0 180) (layer F.SilkS))
    (fp_text value R (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GPIO14_IN_DB))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GPIO14_IN))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 575838DD)
    (at 165.862 89.916 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -4.572 -0.254 180) (layer F.SilkS))
    (fp_text value R (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 GPIO5))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 57583934)
    (at 130.302 104.648)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -4.572 0) (layer F.SilkS))
    (fp_text value R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 GPIO13))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 57583952)
    (at 130.302 92.964)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at -4.572 0) (layer F.SilkS))
    (fp_text value R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 BATT))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 ADC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 57583956)
    (at 130.302 95.758 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 4.572 0 180) (layer F.SilkS))
    (fp_text value R (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 ADC))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5758392F)
    (at 130.302 98.552)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -4.572 0) (layer F.SilkS))
    (fp_text value R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5758396F)
    (at 130.302 90.17)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at -5.08 0) (layer F.SilkS))
    (fp_text value R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 RESET))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5758389C)
    (at 165.862 105.156)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 5.08 0.254) (layer F.SilkS))
    (fp_text value R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 575839B5)
    (at 165.862 95.504 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value R (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 575B55A9)
    (at 144.526 79.756 180)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 4.826 -0.127 180) (layer F.SilkS))
    (fp_text value 74HC7014 (at 0 5.375 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 GPIO12))
    (pad 2 smd rect (at -2.7 -2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 GPIO12_OUT))
    (pad 3 smd rect (at -2.7 -1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GPIO14_IN_DB))
    (pad 4 smd rect (at -2.7 0 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 GPIO14))
    (pad 5 smd rect (at -2.7 1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 GPIO2_IN))
    (pad 6 smd rect (at -2.7 2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GPIO2_IN_ST))
    (pad 7 smd rect (at -2.7 3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 GPIO2_OUT_ST))
    (pad 9 smd rect (at 2.7 2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GPIO2_OUT))
    (pad 10 smd rect (at 2.7 1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 2.7 0 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2.7 -1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 2.7 -2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.7 -3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:ESP07 (layer F.Cu) (tedit 57562EB8)
    (at 147.828 96.266)
    (fp_text reference U2 (at 0 11.684) (layer F.SilkS))
    (fp_text value ESP07 (at 0 -11.684) (layer F.Fab))
    (fp_text user VCC (at -10.85 9.1) (layer F.SilkS))
    (fp_text user GPIO13 (at -11.85 7.1) (layer F.SilkS))
    (fp_text user GPIO12 (at -11.85 5.1) (layer F.SilkS))
    (fp_text user GPIO14 (at -11.85 3.1) (layer F.SilkS))
    (fp_text user GPIO16 (at -11.85 1.1) (layer F.SilkS))
    (fp_text user CH_PD (at -11.5 -1.1) (layer F.SilkS))
    (fp_text user ADC (at -10.85 -3.1) (layer F.SilkS))
    (fp_text user RESET (at -11.5 -5.1) (layer F.SilkS))
    (fp_text user TXD (at 10.85 -5.1) (layer F.SilkS))
    (fp_text user RXD (at 10.95 -3.1) (layer F.SilkS))
    (fp_text user GPIO5 (at 11.5 -1.1) (layer F.SilkS))
    (fp_text user GPIO4 (at 11.5 1.1) (layer F.SilkS))
    (fp_text user GPIO0 (at 11.5 3.1) (layer F.SilkS))
    (fp_text user GPIO2 (at 11.5 5.1) (layer F.SilkS))
    (fp_text user GPIO15 (at 11.85 7.1) (layer F.SilkS))
    (fp_text user GND (at 11 9.1) (layer F.SilkS))
    (pad 1 smd rect (at 8 9.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 8 7.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R11-Pad1)"))
    (pad 3 smd rect (at 8 5.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 9 GPIO2))
    (pad 4 smd rect (at 8 3.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad1)"))
    (pad 5 smd rect (at 8 1.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 5 GPIO4))
    (pad 6 smd rect (at 8 -1.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 6 GPIO5))
    (pad 7 smd rect (at 8 -3.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 15 RXD))
    (pad 8 smd rect (at 8 -5.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 14 TXD))
    (pad 9 smd rect (at -8 -5.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 18 RESET))
    (pad 10 smd rect (at -8 -3.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 20 ADC))
    (pad 11 smd rect (at -8 -1.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R9-Pad2)"))
    (pad 12 smd rect (at -8 1.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 18 RESET))
    (pad 13 smd rect (at -8 3.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 25 GPIO14))
    (pad 14 smd rect (at -8 5.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 23 GPIO12))
    (pad 15 smd rect (at -8 7.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 7 GPIO13))
    (pad 16 smd rect (at -8 9.1) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 3V3))
  )
  (module footprints:Adafruit_3.5mm_Terminal_Block (layer F.Cu) (tedit 5758AFED)
    (at 154.94 70.104)
    (fp_text reference P1 (at 18.796 0 90) (layer F.SilkS))
    (fp_text value CONN_01X10 (at 0 -4.826) (layer F.Fab))
    (pad 5 thru_hole circle (at -1.75 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 26 GPIO2_IN))
    (pad 4 thru_hole circle (at -5.25 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 20 ADC))
    (pad 3 thru_hole circle (at -8.75 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 19 BATT))
    (pad 2 thru_hole circle (at -12.25 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 3V3))
    (pad 1 thru_hole circle (at -15.75 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at 1.75 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 27 GPIO2_OUT_ST))
    (pad 7 thru_hole circle (at 5.25 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 24 GPIO12_OUT))
    (pad 8 thru_hole circle (at 8.75 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 4 GPIO14_IN))
    (pad 9 thru_hole circle (at 12.25 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 18 RESET))
    (pad 10 thru_hole circle (at 15.75 -0.1) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.7mm_Pad (layer F.Cu) (tedit 5758AF7D)
    (at 128.016 71.628)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (fp_text reference P8 (at 0 -4.7) (layer Cmts.User))
    (fp_text value CONN_01X01 (at 0 4.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.7mm_Pad (layer F.Cu) (tedit 5758AF70)
    (at 181.356 71.628)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (fp_text reference P9 (at 0 -4.7) (layer Cmts.User))
    (fp_text value CONN_01X01 (at 0 4.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.7mm_Pad (layer F.Cu) (tedit 5758AF87)
    (at 128.016 112.268)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (fp_text reference P10 (at 0 -4.7) (layer Cmts.User))
    (fp_text value CONN_01X01 (at 0 4.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.7mm_Pad (layer F.Cu) (tedit 5758AF8F)
    (at 181.356 112.268)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (fp_text reference P11 (at -5.842 0.762) (layer Cmts.User))
    (fp_text value CONN_01X01 (at 0 4.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_text N/C (at 175.26 90.17 90) (layer F.SilkS))
  (gr_text GND (at 175.133 102.87 90) (layer F.SilkS))
  (gr_text 3V3 (at 175.133 100.33 90) (layer F.SilkS))
  (gr_text SDA (at 175.133 97.79 90) (layer F.SilkS))
  (gr_text SCL (at 175.26 95.25 90) (layer F.SilkS))
  (gr_text INT (at 175.26 92.71 90) (layer F.SilkS))
  (gr_text 3V3 (at 184.785 100.33 90) (layer F.SilkS))
  (gr_text SDA (at 184.785 97.79 90) (layer F.SilkS))
  (gr_text SCL (at 184.785 95.25 90) (layer F.SilkS))
  (gr_text INT (at 184.785 92.71 90) (layer F.SilkS))
  (gr_text GND (at 184.785 90.17 90) (layer F.SilkS))
  (gr_text "ESP8266 ESP-07\nCarrier Board v1.0\nJune 2016\nRobert Liesenfeld AK6L\nxunil@xunil.net\n" (at 124.841 81.915) (layer F.SilkS))
  (gr_text GND (at 170.688 74.422) (layer F.SilkS))
  (gr_text RESET (at 167.259 74.422) (layer F.SilkS))
  (gr_text "GPIO14\n IN" (at 163.703 74.549) (layer F.SilkS))
  (gr_text "GPIO12\n OUT" (at 160.147 74.549) (layer F.SilkS))
  (gr_text "GPIO2\n OUT" (at 156.591 74.549) (layer F.SilkS))
  (gr_text "GPIO2\n IN" (at 152.908 74.549) (layer F.SilkS))
  (gr_text ADC (at 149.479 74.422) (layer F.SilkS))
  (gr_text BATT (at 146.177 74.422) (layer F.SilkS))
  (gr_text 3V3 (at 142.621 74.422) (layer F.SilkS))
  (gr_text GND (at 139.192 74.422) (layer F.SilkS))
  (gr_text "ESP8266\nESP-07" (at 147.828 89.916) (layer F.SilkS))
  (gr_arc (start 181.864 112.776) (end 186.436 112.522) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.762 117.348) (end 182.118 117.348) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.936 71.12) (end 122.936 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.508 66.548) (end 181.864 66.548) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.436 71.12) (end 186.436 112.522) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 181.864 71.12) (end 181.864 66.548) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127.508 112.776) (end 127.762 117.348) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127.508 71.12) (end 122.936 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text OUT (at 177.038 83.947) (layer F.SilkS))
  (gr_text IN (at 182.118 83.947) (layer F.SilkS))
  (gr_text GPIO2 (at 179.578 78.359) (layer F.SilkS))
  (gr_text BOOT (at 170.942 98.298) (layer F.SilkS))
  (gr_text "SER RST" (at 165.608 115.316) (layer F.SilkS))
  (gr_text SERIAL (at 148.082 115.316) (layer F.SilkS))
  (gr_text RTC (at 179.832 87.249) (layer F.SilkS))
  (zone (net 3) (net_name 3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.928 71.12) (xy 185.928 113.03) (xy 182.118 116.84) (xy 127.762 116.84) (xy 123.444 112.776)
        (xy 123.444 70.866) (xy 127.254 67.056) (xy 181.864 67.056) (xy 185.928 71.12)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.928 71.12) (xy 185.928 113.03) (xy 182.118 116.84) (xy 127.762 116.84) (xy 123.444 112.776)
        (xy 123.444 70.866) (xy 127.254 67.056) (xy 181.864 67.056) (xy 185.928 71.12)
      )
    )
  )
)
