(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+BATT")
  (net 3 "unconnected-(J2-Pad2)")
  (net 4 "Net-(J2-Pad4)")
  (net 5 "Net-(J2-Pad5)")
  (net 6 "Net-(J2-Pad6)")
  (net 7 "Net-(J2-Pad7)")
  (net 8 "Net-(J2-Pad8)")
  (net 9 "Net-(J2-Pad9)")
  (net 10 "unconnected-(J2-Pad10)")
  (net 11 "Net-(J2-Pad11)")
  (net 12 "Net-(J2-Pad12)")
  (net 13 "unconnected-(J2-Pad13)")
  (net 14 "Net-(J3-Pad2)")
  (net 15 "Net-(R2-Pad1)")
  (net 16 "Net-(C2-Pad2)")
  (net 17 "unconnected-(U1-Pad1)")
  (net 18 "unconnected-(U1-Pad2)")
  (net 19 "unconnected-(U1-Pad7)")
  (net 20 "unconnected-(U1-Pad8)")
  (net 21 "unconnected-(U1-Pad14)")
  (net 22 "unconnected-(U1-Pad19)")
  (net 23 "unconnected-(U1-Pad22)")
  (net 24 "Net-(R3-Pad1)")
  (net 25 "unconnected-(U1-Pad27)")
  (net 26 "unconnected-(U1-Pad28)")
  (net 27 "unconnected-(U1-Pad30)")
  (net 28 "unconnected-(U1-Pad31)")
  (net 29 "unconnected-(U1-Pad32)")
  (net 30 "unconnected-(U2-Pad4)")
  (net 31 "Net-(C1-Pad2)")
  (net 32 "Net-(R4-Pad1)")
  (net 33 "Net-(R1-Pad1)")
  (footprint "Inductor_SMD:L_1210_3225Metric_Pad1.42x2.65mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 130.2512 69.6976)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at -3.5052 0) (layer "F.SilkS"))
    (fp_text value "10uH" (at 0 2.3876) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0) (size 1.425 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 2 "+BATT") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0) (size 1.425 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 31 "Net-(C1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A430)
    (at 129.057 65.253 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "ISP" (at 0 15.7738) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+BATT") (pinfunction "VCC") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad2)") (pinfunction "RESET") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad4)") (pinfunction "SCK") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad5)") (pinfunction "MISO") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad6)") (pinfunction "MOSI") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B7745C6)
    (at 121.5992 69.7092 180)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1 -2.55 180) (layer "F.SilkS"))
    (fp_text value "Battery" (at 1 7.45 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 2.5 180) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 2 "+BATT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 138.3792 84.8868)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TH1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "NTC 100k 0.1°C" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 15 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 24 "Net-(R3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x13_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A421)
    (at 126.4666 60.7568 90)
    (descr "Through hole straight socket strip, 1x13, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x13 2.54mm single row")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Display" (at 0 35.0266) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 15.24) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+BATT") (pinfunction "VIN") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J2-Pad2)") (pinfunction "3V3") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad4)") (pinfunction "SCK") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad5)") (pinfunction "MISO") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad6)") (pinfunction "MOSI") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad7)") (pinfunction "ECS") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad8)") (pinfunction "D/C") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad9)") (pinfunction "SRCS") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J2-Pad10)") (pinfunction "SDCS") (pintype "passive+no_connect"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad11)") (pinfunction "RST") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad12)") (pinfunction "BUSY") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J2-Pad13)") (pinfunction "ENA") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x13_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 153.416 73.914 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -0.0508 -1.8288 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at -0.0508 1.9304 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "+BATT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HIH-5030-001:HONEYWELL_HIH-5030-001" (layer "F.Cu")
    (tedit 63D95453)
    (at 158.4492 84.836 -90)
    (property "AVAILABILITY" "Good")
    (property "MF" "Honeywell")
    (property "MP" "HIH-5030-001")
    (property "PACKAGE" "None")
    (property "PRICE" "$6.78 USD")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -3.2512 0.004) (layer "F.SilkS"))
    (fp_text value "HIH-5030" (at -4.7752 0.004) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.27 5.335) (size 1.78 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "-VE") (pintype "power_in"))
    (pad "2" smd rect locked (at 0 5.335) (size 1.78 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(R4-Pad1)") (pinfunction "OUT") (pintype "output"))
    (pad "3" smd rect locked (at 1.27 5.335) (size 1.78 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(R2-Pad1)") (pinfunction "+VE") (pintype "power_in"))
    (pad "4" smd rect locked (at 0 -5.59 270) (size 2.54 2.29) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "unconnected-(U2-Pad4)") (pinfunction "TAB") (pintype "passive+no_connect"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 169.1132 86.3092)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (clearance 1.4)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H4" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "M2" (at 0 -3.1496) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.668 78.4192 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.5748 -0.0508) (layer "F.SilkS"))
    (fp_text value "1.2M" (at -2.6068 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 15 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 33 "Net-(R1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 136.3472 69.6976)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.8288) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.9812) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 31 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 169.1132 61.468)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (clearance 1.4)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H2" (at -0.0508 3.302) (layer "F.SilkS") hide)
    (fp_text value "M2" (at -3.6068 0.1016) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm" (layer "F.Cu")
    (tedit 5A02F146)
    (at 145.4404 73.9648 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -6.05) (layer "F.SilkS"))
    (fp_text value "ATmega328P" (at 0 5.9944) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(U1-Pad1)") (pinfunction "PD3") (pintype "bidirectional+no_connect"))
    (pad "2" smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(U1-Pad2)") (pinfunction "PD4") (pintype "bidirectional+no_connect"))
    (pad "3" smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+BATT") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "6" smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+BATT") (pinfunction "VCC") (pintype "passive"))
    (pad "7" smd rect (at -4.25 2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(U1-Pad7)") (pinfunction "XTAL1/PB6") (pintype "bidirectional+no_connect"))
    (pad "8" smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(U1-Pad8)") (pinfunction "XTAL2/PB7") (pintype "bidirectional+no_connect"))
    (pad "9" smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(J2-Pad12)") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "10" smd rect (at -2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(J2-Pad11)") (pinfunction "PD6") (pintype "bidirectional"))
    (pad "11" smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(J2-Pad9)") (pinfunction "PD7") (pintype "bidirectional"))
    (pad "12" smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J2-Pad8)") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "13" smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J2-Pad7)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(U1-Pad14)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "15" smd rect (at 2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J2-Pad6)") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "16" smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J2-Pad5)") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "17" smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J2-Pad4)") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "18" smd rect (at 4.25 2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(C1-Pad2)") (pinfunction "AVCC") (pintype "power_in"))
    (pad "19" smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(U1-Pad19)") (pinfunction "ADC6") (pintype "input+no_connect"))
    (pad "20" smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(C2-Pad2)") (pinfunction "AREF") (pintype "passive"))
    (pad "21" smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "22" smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "unconnected-(U1-Pad22)") (pinfunction "ADC7") (pintype "input+no_connect"))
    (pad "23" smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(R1-Pad1)") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "24" smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(R2-Pad1)") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "25" smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(R3-Pad1)") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "26" smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(R4-Pad1)") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "27" smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(U1-Pad27)") (pinfunction "PC4") (pintype "bidirectional+no_connect"))
    (pad "28" smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(U1-Pad28)") (pinfunction "PC5") (pintype "bidirectional+no_connect"))
    (pad "29" smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J3-Pad2)") (pinfunction "~{RESET}/PC6") (pintype "bidirectional"))
    (pad "30" smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(U1-Pad30)") (pinfunction "PD0") (pintype "bidirectional+no_connect"))
    (pad "31" smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "unconnected-(U1-Pad31)") (pinfunction "PD1") (pintype "bidirectional+no_connect"))
    (pad "32" smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(U1-Pad32)") (pinfunction "PD2") (pintype "bidirectional+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 114.2492 61.468)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (clearance 1.4)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H1" (at 0.0508 3.302) (layer "F.SilkS") hide)
    (fp_text value "M2" (at 0 3.2512) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.1788 78.4192 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -2.524 0) (layer "F.SilkS"))
    (fp_text value "300K" (at 2.6576 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 33 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 143.6624 84.8868)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100k 0.1%" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 24 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 136.3472 73.5584)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 16 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 114.3 86.3092)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (clearance 1.4)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H3" (at 0.0508 -3.1496) (layer "F.SilkS") hide)
    (fp_text value "M2" (at 0 -3.1496) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 148.8948 84.8868 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "thermidity.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -0.0348 1.6764) (layer "F.SilkS"))
    (fp_text value "65k" (at -0.0508 -1.778) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 32 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 111.7 58.9) (end 171.7 88.9) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Dode's Thermidity" (at 156.972 64.7192) (layer "F.SilkS"))
  (gr_text "https://luniks.net/thermidity.jsp" (at 156.972 66.9544) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.704 88.9)
        (xy 111.76 88.9)
        (xy 111.7092 58.928)
        (xy 171.704 58.928)
      )
    )
  )
)
