(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6002)
    (drawings 17)
    (tracks 33)
    (zones 0)
    (modules 21)
    (nets 7)
  )
  (page A4)
  (title_block
    (title "IPSS Lower 043022")
    (date 2020-04-20)
    (rev A)
    (company Criterion)
    (comment 1 "Kevin Vermeer")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.635)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.27 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.6 3.6)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 152.4 101.6)
    (grid_origin 152.4 101.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VBATT)
  (net 2 GND)
  (net 3 Prox_18V)
  (net 4 Prox_Signal)
  (net 5 /SW2_B11)
  (net 6 /B12_B21)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net /B12_B21)
    (add_net /SW2_B11)
    (add_net GND)
    (add_net Prox_18V)
    (add_net Prox_Signal)
    (add_net VBATT)
  )
  (net_class Minimum ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class Power ""
    (clearance 0.635)
    (trace_width 0.635)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.635)
    (diff_pair_gap 0.635)
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer B.Cu) (tedit 5E9E0C39)
    (at 155.575 117.475)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J14 (at 2.921 2.413) (layer B.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 -2.55) (layer B.Fab))
    (fp_text user %R (at 0 2.4) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer B.Cu) (tedit 5E9E0C39)
    (at 149.225 117.475)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J13 (at -2.667 2.413) (layer B.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 -2.55) (layer B.Fab))
    (fp_text user %R (at 0 2.4) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Prox_Signal))
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer B.Cu) (tedit 5E9E0C39)
    (at 149.225 111.125)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J12 (at -2.921 -2.413) (layer B.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 -2.55) (layer B.Fab))
    (fp_text user %R (at 0 2.4) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 Prox_18V))
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer B.Cu) (tedit 5E9E0C39)
    (at 155.575 111.125)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J11 (at 2.667 -2.413) (layer B.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 -2.55) (layer B.Fab))
    (fp_text user %R (at 0 2.4) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 VBATT))
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer F.Cu) (tedit 5E9E0C39)
    (at 155.575 85.725)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J4 (at 2.413 -2.159) (layer F.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer F.Cu) (tedit 5E9E0C39)
    (at 149.225 85.725)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J3 (at -2.413 -2.413) (layer F.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Prox_Signal))
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer F.Cu) (tedit 5E9E0C39)
    (at 149.225 92.075)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J2 (at -2.413 2.413) (layer F.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 Prox_18V))
  )
  (module 0926-1-15-20-75-14-11-0:1946_or_S70-332 (layer F.Cu) (tedit 5E9E0C39)
    (at 155.575 92.075)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J1 (at 2.413 2.413) (layer F.SilkS))
    (fp_text value 0926-1-15-20-75-14-11-0 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 VBATT))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 141.732 99.06)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference B11 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 /SW2_B11))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 167.386 99.06)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference P3 (at 2.286 -2.032 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 171.704 101.6)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference P2 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Prox_Signal))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 167.386 104.14)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference P1 (at 2.54 2.032 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 Prox_18V))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 141.732 104.14)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference B22 (at 0 2.794 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 163.068 104.14)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference B21 (at 0 2.794 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 /B12_B21))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 163.068 99.06)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference B12 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 /B12_B21))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 137.414 101.6 90)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference SW2 (at -2.794 0) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 /SW2_B11))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 133.096 101.6 90)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference SW1 (at -2.794 0) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 VBATT))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer B.Cu) (tedit 56D1B4CB)
    (at 137.668 109.22)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H2 (at 0 3.5) (layer B.SilkS) hide)
    (fp_text value MountingHole (at 0 -3.5) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer B.Cu) (tedit 56D1B4CB)
    (at 137.668 93.98)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H1 (at 0 3.5) (layer B.SilkS) hide)
    (fp_text value MountingHole (at 0 -3.5) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 167.132 93.98)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 167.132 109.22)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (gr_text P2 (at 171.704 98.806) (layer B.SilkS))
  (gr_text P3 (at 169.672 97.028) (layer B.SilkS))
  (gr_text P1 (at 169.672 106.172) (layer B.SilkS))
  (gr_text B21 (at 162.814 106.934) (layer B.SilkS))
  (gr_text B12 (at 163.068 96.266) (layer B.SilkS))
  (gr_text B11 (at 141.732 96.266) (layer B.SilkS))
  (gr_text B22 (at 141.732 106.934) (layer B.SilkS))
  (gr_text SW2 (at 137.414 104.394) (layer B.SilkS))
  (gr_text SW1 (at 133.096 104.394) (layer B.SilkS))
  (gr_text "043022 A\nCriterion MS\n6652 2020 04" (at 158.496 88.138) (layer F.SilkS))
  (gr_circle (center 152.4 101.6) (end 159.5501 101.6) (layer Edge.Cuts) (width 0.254))
  (gr_circle (center 152.4 101.6) (end 174.625 101.6) (layer Edge.Cuts) (width 0.254))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.26 101.6) (xy 175.26 78.74) (xy 129.54 78.74) (xy 129.54 124.46) (xy 175.26 124.46)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.895 125.095) (xy 175.895 78.105) (xy 128.905 78.105) (xy 128.905 125.095)
      )
    )
  )
)
