<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="3.81" y1="0" x2="46.99" y2="0" width="0.254" layer="20"/>
<wire x1="50.8" y1="3.81" x2="50.8" y2="40.64" width="0.254" layer="20"/>
<wire x1="46.99" y1="44.45" x2="3.81" y2="44.45" width="0.254" layer="20"/>
<wire x1="0" y1="40.64" x2="0" y2="3.81" width="0.254" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0.254" layer="20" curve="90"/>
<text>HALT</text>
<text>RESET</text>
<text>CH A</text>
<text>OPTION</text>
<text>STATUS</text>
<text>ICSP</text>
<text>MoCk68K SBC KD0GLS 2020</text>
<wire x1="46.99" y1="0" x2="50.8" y2="3.81" width="0.254" layer="20" curve="90"/>
<wire x1="50.8" y1="40.64" x2="46.99" y2="44.45" width="0.254" layer="20" curve="90"/>
<wire x1="3.81" y1="44.45" x2="0" y2="40.64" width="0.254" layer="20" curve="90"/>
<text>TP</text>
<text>MoCk68K</text>
<text>CH B</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="LED_3MM">
</package>
<package name="CONN_BREAKAWAY_1X6_100">
</package>
<package name="TIL311">
</package>
<package name="TQFP64">
</package>
<package name="SWITCH_DIP_4POS">
</package>
<package name="MOUNTING_HOLE">
</package>
<package name="SWITCH_CK_PTS635">
<description>C&amp;K P/N PTS635SL50 LFS
Digi-Key P/N CKN9102-ND</description>
</package>
<package name="0805">
</package>
<package name="CONN_ICSP_TH">
<description>Molex PicoBlade 5-pin connector</description>
</package>
<package name="TO-92">
</package>
<package name="CAPACITOR_ELECTROLYTIC_2MM">
</package>
<package name="TEST_POINT">
<description>Keystone 5007
Digi-Key P/N 36-5007-ND</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="kd0gls" package="LED_3MM" value="HALT"/>
<element name="J1" library="kd0gls" package="CONN_BREAKAWAY_1X6_100" value="CONN_BREAKAWAY_1X6_100"/>
<element name="J2" library="kd0gls" package="CONN_BREAKAWAY_1X6_100" value="CONN_BREAKAWAY_1X6_100"/>
<element name="DPY1" library="kd0gls" package="TIL311" value="TIL311"/>
<element name="DPY2" library="kd0gls" package="TIL311" value="TIL311"/>
<element name="U1" library="kd0gls" package="TQFP64" value="PIC32MZ2048EFH064-I/PT"/>
<element name="SW2" library="kd0gls" package="SWITCH_DIP_4POS" value="SWITCH_DIP_4POS"/>
<element name="MH1" library="kd0gls" package="MOUNTING_HOLE" value="MOUNTING_HOLE"/>
<element name="MH2" library="kd0gls" package="MOUNTING_HOLE" value="MOUNTING_HOLE"/>
<element name="MH3" library="kd0gls" package="MOUNTING_HOLE" value="MOUNTING_HOLE"/>
<element name="MH4" library="kd0gls" package="MOUNTING_HOLE" value="MOUNTING_HOLE"/>
<element name="SW1" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="C4" library="kd0gls" package="0805" value="0.1uF"/>
<element name="C5" library="kd0gls" package="0805" value="0.1uF"/>
<element name="C6" library="kd0gls" package="0805" value="0.1uF"/>
<element name="C7" library="kd0gls" package="0805" value="0.1uF"/>
<element name="R1" library="kd0gls" package="0805" value="10K"/>
<element name="C2" library="kd0gls" package="0805" value="10uF"/>
<element name="C3" library="kd0gls" package="0805" value="10uF"/>
<element name="J3" library="kd0gls" package="CONN_ICSP_TH" value="CONN_ICSP_TH"/>
<element name="IC2" library="kd0gls" package="TO-92" value="MCP1700"/>
<element name="C1" library="kd0gls" package="CAPACITOR_ELECTROLYTIC_2MM" value="100uF"/>
<element name="TP" library="kd0gls" package="TEST_POINT" value="TEST_POINT"/>
</elements>
<signals>
<signal name="VCAP">
</signal>
<signal name="GND">
<contactref element="DPY1" pad="7"/>
<contactref element="DPY2" pad="7"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="40"/>
<contactref element="U1" pad="55"/>
<contactref element="U1" pad="59"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="MH1" pad="1"/>
<contactref element="MH2" pad="1"/>
<contactref element="MH3" pad="1"/>
<contactref element="MH4" pad="1"/>
<contactref element="SW1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW2" pad="3"/>
<contactref element="SW2" pad="4"/>
<contactref element="DPY1" pad="5"/>
<contactref element="DPY1" pad="8"/>
<contactref element="DPY2" pad="5"/>
<contactref element="DPY2" pad="8"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J3" pad="VSS"/>
<contactref element="U1" pad="34"/>
<contactref element="IC2" pad="1"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="39"/>
<contactref element="U1" pad="54"/>
<contactref element="U1" pad="60"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J3" pad="VDD"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="VPP">
<contactref element="SW1" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="R1" pad="2"/>
<contactref element="J3" pad="VPP"/>
</signal>
<signal name="5V">
<contactref element="DPY1" pad="14"/>
<contactref element="DPY1" pad="1"/>
<contactref element="DPY2" pad="14"/>
<contactref element="DPY2" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="D7">
<contactref element="DPY1" pad="12"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="D6">
<contactref element="DPY1" pad="13"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="D5">
<contactref element="DPY1" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="D4">
<contactref element="DPY1" pad="3"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="D3">
<contactref element="DPY2" pad="12"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="D2">
<contactref element="DPY2" pad="13"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="D1">
<contactref element="DPY2" pad="2"/>
<contactref element="U1" pad="15"/>
<contactref element="J3" pad="CLK"/>
</signal>
<signal name="D0">
<contactref element="DPY2" pad="3"/>
<contactref element="U1" pad="16"/>
<contactref element="J3" pad="DAT"/>
</signal>
<signal name="S3">
<contactref element="SW2" pad="8"/>
<contactref element="U1" pad="63"/>
</signal>
<signal name="S2">
<contactref element="SW2" pad="7"/>
<contactref element="U1" pad="62"/>
</signal>
<signal name="S1">
<contactref element="SW2" pad="6"/>
<contactref element="U1" pad="61"/>
</signal>
<signal name="S0">
<contactref element="SW2" pad="5"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="HALT">
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="TXA">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="42"/>
</signal>
<signal name="RXA">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="41"/>
</signal>
<signal name="TXB">
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="RXB">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="43"/>
</signal>
<signal name="TP">
<contactref element="U1" pad="32"/>
<contactref element="TP" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
