(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 21)
    (no_connects 3)
    (area 129.489999 93.929999 154.990001 142.290001)
    (thickness 1.6)
    (drawings 96)
    (tracks 89)
    (zones 0)
    (modules 13)
    (nets 11)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.9144)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.254)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 "Net-(BT1-Pad1)")
  (net 4 "Net-(D4-Pad2)")
  (net 5 "Net-(IC1-Pad2)")
  (net 6 "Net-(IC1-Pad3)")
  (net 7 "Net-(CON1-Pad1)")
  (net 8 "Net-(CON1-Pad5)")
  (net 9 "Net-(CON1-Pad4)")
  (net 10 "Net-(CON1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON1-Pad5)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
  )
  (net_class PWR ""
    (clearance 0.6096)
    (trace_width 0.6096)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module footprints:BATT_CR2032_SMD (layer F.Cu) (tedit 56CFB5D2)
    (at 142.24 132.08)
    (tags battery)
    (fp_text reference BT1 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value BATTERY (at 0 -2.54) (layer F.SilkS) hide)
    (pad 2 smd circle (at 0 0) (size 17.78 17.78) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -11.43 0) (size 2.54 5.08) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at 11.43 0) (size 2.54 5.08) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
  )
  (module window3 (layer B.Cu) (tedit 54A5C3A0)
    (at 132.08 102.87)
    (fp_text reference LOGO (at 0 -5) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0) (layer B.SilkS))
  )
  (module 078hole (layer F.Cu) (tedit 5AE15CCA)
    (at 142.24 101.6)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference HOLE_2 (at 0 -0.254) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 0.254) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 0.5) (layers *.Cu F.Paste F.SilkS F.Mask))
  )
  (module window3 (layer B.Cu) (tedit 54A5C3A0)
    (at 142.24 102.87)
    (fp_text reference LOGO (at 0 -5) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0) (layer B.SilkS))
  )
  (module sign (layer B.Cu) (tedit 54A5C85E)
    (at 146.05 112.395)
    (fp_text reference LOGO (at 0 -5) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0) (layer B.SilkS))
  )
  (module footprints:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AE012CD)
    (at 148.59 102.87)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference CON1 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 0.635) (layers *.Cu F.Mask)
      (net 7 "Net-(CON1-Pad1)"))
    (pad 2 smd oval (at 2.54 0) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd oval (at 0 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CON1-Pad3)"))
    (pad 4 smd oval (at 2.54 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CON1-Pad4)"))
    (pad 5 smd oval (at 0 5.08) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CON1-Pad5)"))
    (pad 6 smd oval (at 2.54 5.08) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:DIP-8__300 (layer F.Cu) (tedit 5AE1424C)
    (at 135.89 115.57 270)
    (descr "8 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference IC1 (at -1.27 1.27 270) (layer F.SilkS) hide)
    (fp_text value ATTINY85 (at 0.635 -0.635 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(CON1-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON1-Pad4)"))
    (pad 6 thru_hole circle (at 1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(CON1-Pad3)"))
    (pad 8 thru_hole circle (at -3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +BATT))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R3-LARGE_PADS (layer F.Cu) (tedit 544AD9F5)
    (at 142.24 97.79 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D4-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SPEAKER (layer F.Cu) (tedit 54A5B18B)
    (at 148.59 116.84 90)
    (descr "Switch inverseur")
    (tags "SWITCH DEV")
    (fp_text reference SP1 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text value SPEAKER (at -3.81 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON1-Pad4)"))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module footprints:SW_PUSH_TOUCH (layer B.Cu) (tedit 5AE13C33)
    (at 136.525 132.08 90)
    (fp_text reference SW1 (at -2.286 4.318 90) (layer B.SilkS) hide)
    (fp_text value TOUCH (at 5.715 0.127 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 3.302 3.175 90) (size 1.016 1.016) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(CON1-Pad3)"))
    (pad 2 smd rect (at 3.175 -3.175 90) (size 1.016 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.048 3.175 90) (size 1.016 1.016) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(CON1-Pad3)"))
    (pad 2 smd rect (at -3.048 -3.175 90) (size 1.016 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.127 0 90) (size 6.858 6.858) (layers B.Paste B.Mask))
  )
  (module footprints:SW_SPST (layer F.Cu) (tedit 5AE141D8)
    (at 135.89 105.41)
    (descr "Switch inverseur")
    (tags "SWITCH DEV")
    (fp_text reference SW2 (at -1.651 2.032 90) (layer F.SilkS) hide)
    (fp_text value ON (at -4.318 -4.826) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.54) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 1 +BATT))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -3.302 -2.54) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -3.302 0) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -3.302 2.54) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
  )
  (module footprints:C1 (layer F.Cu) (tedit 5AE14233)
    (at 133.35 123.19)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C1 (at -1.905 -1.905) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 1.27 -1.905 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED-3MM (layer F.Cu) (tedit 5AE13899)
    (at 142.24 95.25 180)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (fp_text reference D4 (at 0.381 -2.667 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 -0.889 180) (layer F.SilkS) hide)
    (fp_text user + (at -2.54 -0.508 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D4-Pad2)"))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ISP +" (at 151.13 100.965) (layer F.SilkS))
  (gr_text "TARDIS\nREV 0.1\nApr 2018" (at 139.065 107.315) (layer F.SilkS))
  (gr_text "POLICE       BOX" (at 142.875 100.33) (layer B.SilkS))
  (gr_arc (start 133.35 95.25) (end 134.62 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 153.67 97.79) (end 153.67 99.06) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.89 93.98) (end 148.59 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 140.97) (end 129.54 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.67 142.24) (end 130.81 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.94 100.33) (end 154.94 140.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.13 95.25) (end 151.13 96.52) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 130.81 97.79) (end 132.08 97.79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.13 97.79) (end 151.13 96.52) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 148.59 95.25) (end 148.59 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 135.89 95.25) (end 134.62 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133.35 97.79) (end 132.08 97.79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 130.81 100.33) (end 129.54 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 153.67 100.33) (end 153.67 99.06) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 130.81 140.97) (end 130.81 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 153.67 140.97) (end 154.94 140.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text SWITCH (at 134.366 105.41 90) (layer F.SilkS))
  (gr_text "OFF       ON" (at 130.81 104.775 90) (layer F.SilkS))
)
