(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 22)
    (no_connects 0)
    (area 157.658999 77.394999 167.715001 120.725001)
    (thickness 1.6)
    (drawings 6)
    (tracks 89)
    (zones 0)
    (modules 14)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(R1-Pad2)")
  (net 4 "Net-(R2-Pad2)")
  (net 5 GND)
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(C1-Pad2)")
  (net 8 "Net-(R3-Pad1)")
  (net 9 "Net-(R3-Pad2)")
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(R7-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net VDD)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5ABB0EF9)
    (at 163.576 110.49 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at -3.175 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 5A769F72)
    (at 162.56 78.74 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABB102A)
    (at 165.735 82.55 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.175 0.635 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABB102F)
    (at 162.56 82.55 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.508 1.524 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABB1021)
    (at 161.925 90.17 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.175 -0.635 270) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABB1026)
    (at 164.465 90.17 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABB1008)
    (at 159.512 100.584 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.302 0 270) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5A769F48)
    (at 166.116 110.49 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.302 0 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5A769F39)
    (at 164.846 104.14 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U1 (at -0.508 2.286 270) (layer F.SilkS))
    (fp_text value LTC6992 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R7-Pad1)"))
    (pad 5 smd rect (at 1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomFP:USBC_breakout (layer B.Cu) (tedit 5A769FFA)
    (at 165.1 120.015 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 4.318 -2.286 180) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 3.302 -2.286 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 5 0 180) (size 1.8 2) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 1 smd rect (at 0 0 180) (size 1.8 2) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad1)"))
  )
  (module CustomFP:SWITCH_SPDT_PTH (layer F.Cu) (tedit 5A769F4E)
    (at 159.258 110.236)
    (descr "SPDT PTH SLIDE SWITCH")
    (tags "SPDT PTH SLIDE SWITCH")
    (attr virtual)
    (fp_text reference SW1 (at 2.54 -0.762 90) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 0.254 90) (layer F.SilkS))
    (pad "" smd rect (at 1.1 -4 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad "" smd rect (at -1.1 -4 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad "" smd rect (at 1.1 3.9 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 2.1 2.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 2.1 0.7) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad1)") (solder_mask_margin 0.1016))
    (pad "" smd rect (at -1.1 3.9 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 smd rect (at 2.1 -2.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.1016))
  )
  (module CustomFP:slidingPot (layer F.Cu) (tedit 5ABB0DBC)
    (at 162.56 99.314 90)
    (descr "SLIDE POTENTIOMETER - PTH, 30MM TRAVEL")
    (tags "SLIDE POTENTIOMETER - PTH, 30MM TRAVEL")
    (attr virtual)
    (fp_text reference VR1 (at 0 -5.461 90) (layer F.SilkS))
    (fp_text value POT_SLIDE-30MM (at -0.381 6.35 90) (layer F.SilkS))
    (pad BOTT thru_hole circle (at 17.5 -2.625 90) (size 2.2479 2.2479) (drill 1.4986) (layers *.Cu *.Mask)
      (net 4 "Net-(R2-Pad2)") (solder_mask_margin 0.1016))
    (pad TOP thru_hole circle (at -17.5 -2.75 90) (size 2.2479 2.2479) (drill 1.4986) (layers *.Cu *.Mask)
      (net 5 GND) (solder_mask_margin 0.1016))
    (pad WIPE thru_hole circle (at -15.5 2.75 90) (size 2.2479 2.2479) (drill 1.4986) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (model C:/Users/Scott/Documents/KiCad/Models3D/slidingPot.wrl
      (at (xyz -1 0 -0.3))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5ABB100D)
    (at 159.512 95.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.556 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABB1013)
    (at 161.925 95.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Scott Co. USB Light V2" (at 166.37 94.615 90) (layer F.SilkS))
  (gr_line (start 167.64 120.65) (end 167.64 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 120.65) (end 157.734 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.386 77.47) (end 167.64 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.734 77.47) (end 167.386 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.734 120.65) (end 157.734 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 120.65) (xy 157.734 120.65) (xy 157.734 77.47) (xy 167.64 77.47)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 120.65) (xy 157.734 120.65) (xy 157.734 77.47) (xy 167.64 77.47)
      )
    )
  )
)
