(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 0.8)
    (drawings 13)
    (tracks 198)
    (zones 0)
    (modules 14)
    (nets 47)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 /K1)
  (net 2 /Ag)
  (net 3 /Ae)
  (net 4 /Ad)
  (net 5 /Ac)
  (net 6 /Af)
  (net 7 /K3)
  (net 8 /K2)
  (net 9 /A.)
  (net 10 /Ab)
  (net 11 /K4)
  (net 12 /Aa)
  (net 13 "Net-(R1-Pad1)")
  (net 14 "Net-(R2-Pad1)")
  (net 15 "Net-(R3-Pad1)")
  (net 16 "Net-(R4-Pad1)")
  (net 17 "Net-(R5-Pad1)")
  (net 18 "Net-(R6-Pad2)")
  (net 19 "Net-(R7-Pad2)")
  (net 20 "Net-(R8-Pad2)")
  (net 21 +3V3)
  (net 22 GND)
  (net 23 "Net-(U1-Pad10)")
  (net 24 "Net-(U1-Pad9)")
  (net 25 "Net-(U1-Pad2)")
  (net 26 "Net-(U1-Pad38)")
  (net 27 "Net-(U1-Pad28)")
  (net 28 "Net-(U1-Pad27)")
  (net 29 "Net-(U1-Pad26)")
  (net 30 "Net-(U1-Pad23)")
  (net 31 "Net-(U1-Pad22)")
  (net 32 "Net-(U1-Pad21)")
  (net 33 "Net-(U1-Pad20)")
  (net 34 "Net-(U1-Pad19)")
  (net 35 "Net-(U1-Pad18)")
  (net 36 "Net-(U1-Pad17)")
  (net 37 "Net-(U1-Pad16)")
  (net 38 "Net-(U1-Pad15)")
  (net 39 "Net-(U1-Pad14)")
  (net 40 "Net-(U1-Pad41)")
  (net 41 "Net-(U1-Pad40)")
  (net 42 "Net-(U1-Pad25)")
  (net 43 "Net-(SW1-Pad2)")
  (net 44 /swdio)
  (net 45 /swdck)
  (net 46 /trst)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /A.)
    (add_net /Aa)
    (add_net /Ab)
    (add_net /Ac)
    (add_net /Ad)
    (add_net /Ae)
    (add_net /Af)
    (add_net /Ag)
    (add_net /K1)
    (add_net /K2)
    (add_net /K3)
    (add_net /K4)
    (add_net /swdck)
    (add_net /swdio)
    (add_net /trst)
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad9)")
  )
  (module Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA (layer F.Cu) (tedit 5A02FC95)
    (at 113.55 98.3)
    (descr http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf)
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (attr smd)
    (fp_text reference SW1 (at 0.05 -1.25) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.625 0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at -2.625 0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -2.625 -0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 1 smd rect (at 2.625 -0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC164FB)
    (at 104.2 81.28 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.9 -0.02 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /Aa))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC164EA)
    (at 104.2 84.1 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0.3 -1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R2-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /Ab))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC164DC)
    (at 104 88.9 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -0.8 0.9 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /Af))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC164C6)
    (at 104 91.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -1 0.9 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 /Ad))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC164B6)
    (at 104.1 93.6 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0.1 1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /Ag))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC1652C)
    (at 106.5 84.2 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -0.1 1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /Ae))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC16513)
    (at 106.68 86.4 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -0.42 1.2 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /Ac))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5BC16541)
    (at 106.68 91.44 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -0.52 0.94 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /A.))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MDBT42Q:MDBT42Q (layer F.Cu) (tedit 5A4EE07B)
    (at 105.41 87.63)
    (attr smd)
    (fp_text reference U1 (at -6.71 -8.43) (layer F.Fab))
    (fp_text value MDBT42Q (at 0 10) (layer F.SilkS))
    (fp_text user "Top layer no ground" (at 1.7 -2.5) (layer Cmts.User))
    (fp_text user "No ground pad" (at 0 -6) (layer Cmts.User))
    (pad 11 smd rect (at -4.7 5.5) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 +3V3))
    (pad 10 smd rect (at -4.7 4.8) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -4.7 4.1) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -4.7 3.4) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R5-Pad1)"))
    (pad 7 smd rect (at -4.7 2.7) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R4-Pad1)"))
    (pad 6 smd rect (at -4.7 2) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R3-Pad1)"))
    (pad 5 smd rect (at -4.7 1.3) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /K2))
    (pad 4 smd rect (at -4.7 0.6) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -4.7 -0.1) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -4.7 -0.8) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad2)"))
    (pad 38 smd rect (at 4.7 -2.9 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad38)"))
    (pad 37 smd rect (at 4.7 -2.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 /swdio))
    (pad 36 smd rect (at 4.7 -1.5 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 /swdck))
    (pad 35 smd rect (at 4.7 -0.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 /trst))
    (pad 34 smd rect (at 4.7 -0.1 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /K1))
    (pad 33 smd rect (at 4.7 0.6 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 32 smd rect (at 4.7 1.3 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R7-Pad2)"))
    (pad 31 smd rect (at 4.7 2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /K3))
    (pad 30 smd rect (at 4.7 2.7 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R8-Pad2)"))
    (pad 29 smd rect (at 4.7 3.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /K4))
    (pad 28 smd rect (at 4.7 4.1 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad28)"))
    (pad 27 smd rect (at 4.7 4.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad27)"))
    (pad 26 smd rect (at 4.7 5.5 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad26)"))
    (pad 24 smd rect (at 4.2 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 23 smd rect (at 3.5 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad23)"))
    (pad 22 smd rect (at 2.8 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad22)"))
    (pad 21 smd rect (at 2.1 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad21)"))
    (pad 20 smd rect (at 1.4 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad20)"))
    (pad 19 smd rect (at 0.7 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad19)"))
    (pad 18 smd rect (at 0 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at -0.7 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad17)"))
    (pad 16 smd rect (at -1.4 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at -2.1 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at -2.8 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at -3.5 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(SW1-Pad2)"))
    (pad 41 smd rect (at 2.9 -1.85 180) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad41)"))
    (pad 40 smd rect (at 2.9 -3.25 180) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad40)"))
    (pad 39 smd rect (at 4.7 -3.8 180) (size 1.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 25 smd rect (at 4.7 6.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad25)"))
    (pad 12 smd rect (at -4.2 7.7 90) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 1 smd rect (at -4.7 -3.8) (size 1.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
  )
  (module Package_DIP:DIP-12_W7.62mm_SMDSocket_SmallPads (layer B.Cu) (tedit 5A02E8C5)
    (at 105.41 87.63 180)
    (descr "12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads")
    (attr smd)
    (fp_text reference J1 (at 0 8.68 180) (layer B.SilkS))
    (fp_text value Conn_02x06_Counter_Clockwise (at 0 -8.68 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -3.81 6.35 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 /K1))
    (pad 7 smd rect (at 3.81 -6.35 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /Ag))
    (pad 2 smd rect (at -3.81 3.81 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /Ae))
    (pad 8 smd rect (at 3.81 -3.81 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /Ad))
    (pad 3 smd rect (at -3.81 1.27 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /Ac))
    (pad 9 smd rect (at 3.81 -1.27 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /Af))
    (pad 4 smd rect (at -3.81 -1.27 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 /K3))
    (pad 10 smd rect (at 3.81 1.27 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 /K2))
    (pad 5 smd rect (at -3.81 -3.81 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 9 /A.))
    (pad 11 smd rect (at 3.81 3.81 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 10 /Ab))
    (pad 6 smd rect (at -3.81 -6.35 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 /K4))
    (pad 12 smd rect (at 3.81 6.35 180) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 /Aa))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-12_W7.62mm_SMDSocket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 101.3 97.9)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x05_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 113.3 87.2 180)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (fp_text reference J2 (at 0.125 6.8 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Female (at 0 6.775 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 +3V3))
    (pad 2 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 44 /swdio))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 45 /swdck))
    (pad 4 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 46 /trst))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 112.975 91.675)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0.625 -2.475) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 3V3 (at 115.825 94.2) (layer F.SilkS))
  (gr_text GND (at 115.875 91.5) (layer F.SilkS))
  (gr_text SWDIO (at 115.775 85.975) (layer F.SilkS))
  (gr_text SWDCK (at 115.8 84.625) (layer F.SilkS))
  (gr_text RST (at 116.2 83.5) (layer F.SilkS))
  (gr_text 3V3 (at 115.9 87.375) (layer F.SilkS))
  (gr_text GND (at 116.35 82.025) (layer F.SilkS))
  (dimension 19.750016 (width 0.3) (layer F.SilkS)
    (gr_text "19.750 mm" (at 107.733284 108.132315 0.07252626444) (layer F.SilkS))
    (feature1 (pts (xy 117.6 101.575) (xy 117.606369 106.606238)))
    (feature2 (pts (xy 97.85 101.6) (xy 97.856369 106.631238)))
    (crossbar (pts (xy 97.855626 106.044817) (xy 117.605626 106.019817)))
    (arrow1a (pts (xy 117.605626 106.019817) (xy 116.479865 106.607663)))
    (arrow1b (pts (xy 117.605626 106.019817) (xy 116.478381 105.434823)))
    (arrow2a (pts (xy 97.855626 106.044817) (xy 98.982871 106.629811)))
    (arrow2b (pts (xy 97.855626 106.044817) (xy 98.981387 105.456971)))
  )
  (dimension 22.900218 (width 0.3) (layer F.SilkS)
    (gr_text "22.900 mm" (at 122.728381 88.872176 89.74980168) (layer F.SilkS))
    (feature1 (pts (xy 117.6 100.3) (xy 121.164816 100.315567)))
    (feature2 (pts (xy 117.7 77.4) (xy 121.264816 77.415567)))
    (crossbar (pts (xy 120.678401 77.413006) (xy 120.578401 100.313006)))
    (arrow1a (pts (xy 120.578401 100.313006) (xy 119.996905 99.183952)))
    (arrow1b (pts (xy 120.578401 100.313006) (xy 121.169735 99.189074)))
    (arrow2a (pts (xy 120.678401 77.413006) (xy 120.087067 78.536938)))
    (arrow2b (pts (xy 120.678401 77.413006) (xy 121.259897 78.54206)))
  )
  (gr_line (start 117.6 77.4) (end 97.85 77.4) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 117.6 101.575) (end 117.6 77.4) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 97.85 101.6) (end 117.6 101.58) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 97.85 77.45) (end 97.85 101.6) (layer Edge.Cuts) (width 0.2))
)
