<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.23" y2="0" width="0" layer="20"/>
<wire x1="35.23" y1="0" x2="35.23" y2="33.01" width="0" layer="20"/>
<wire x1="35.23" y1="33.01" x2="0" y2="33.01" width="0" layer="20"/>
<wire x1="0" y1="33.01" x2="0" y2="0" width="0" layer="20"/>
<text>0
1
2
3
4
5
6
7</text>
<text>R/B#
RE#
CE#
CLE
ALE
WE#
WP#</text>
<text>1</text>
<text>24</text>
<text>25</text>
<text>48</text>
<text>VSS</text>
<text>VCC</text>
</plain>
<libraries>
<library name="flashmemory">
<description>&lt;b&gt;K9F5608X0D &lt;/b&gt;&lt;p&gt;Offered in 32Mx8bit , the K9F5608X0D is 256M bit with spare 8M bit capacity. The device is offered in 1.8V, 2.65V, 3.3V Vcc. Its
NAND cell provides the most cost-effective solutIon for the solid state mass storage market. A program operation can be performed
in typical 200?s on a 528-byte page and an erase operation can be performed in typical 2ms on a 16K-byte block. Data in the page
can be read out at 50ns cycle time per byte. The I/O pins serve as the ports for address and data input/output as well as command
input. The on-chip write control automates all program and erase functions including pulse repetition, where required, and internal
verification and margining of data. Even the write-intensive systems can take advantage of the K9F5608X0D?s extended reliability of
100K program/erase cycles by providing ECC(Error Correcting Code) with real time mapping-out algorithm.
The K9F5608X0D is an optimum solution for large nonvolatile storage applications such as solid state file storage and other portable
applications requiring non-volatility.&lt;p&gt;
&lt;ul&gt;K9F5608U0D-J &lt;p&gt;
2.7 ~ 3.6V TSOP1&lt;p&gt;
10pc = 49 EURO + VAT(MwSt)&lt;p&gt;
RoHS&lt;p&gt;
&lt;/ul&gt;
CALL +49 5631 5046960&lt;p&gt;
info@schulte-universe.com&lt;p&gt;&lt;p&gt;</description>
<packages>
<package name="TSOP48">
<description>&lt;b&gt;Thin Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA07-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="70543-02">
<description>&lt;b&gt;C-Grid SL Connector&lt;/b&gt;&lt;p&gt;
 vertical, 2 pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="flashmemory" package="TSOP48" value="K9F5608"/>
<element name="I/O" library="con-lstb" package="MA08-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="COMMANDS" library="con-lstb" package="MA07-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X1" library="con-molex" package="70543-02" value="C-GRID-02-70543">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$7">
<contactref element="U$1" pad="7"/>
<contactref element="COMMANDS" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="8"/>
<contactref element="COMMANDS" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="16"/>
<contactref element="COMMANDS" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="29"/>
<contactref element="I/O" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="44"/>
<contactref element="I/O" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="43"/>
<contactref element="I/O" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="I/O" pad="2"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="31"/>
<contactref element="I/O" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="32"/>
<contactref element="I/O" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="42"/>
<contactref element="I/O" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="37"/>
<contactref element="X1" pad="2"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="39"/>
</signal>
<signal name="N$14">
<contactref element="X1" pad="1"/>
<contactref element="U$1" pad="13"/>
<contactref element="U$1" pad="25"/>
<contactref element="U$1" pad="48"/>
<contactref element="U$1" pad="36"/>
</signal>
<signal name="N$19">
<contactref element="COMMANDS" pad="5"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="N$20">
<contactref element="COMMANDS" pad="6"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="N$21">
<contactref element="COMMANDS" pad="7"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="9"/>
<contactref element="COMMANDS" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="I/O" pad="5"/>
<contactref element="U$1" pad="41"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
