(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~86~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 78)
    (zones 0)
    (modules 5)
    (nets 11)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/wormley/tmp/z/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /BMB2)
  (net 3 /BMA1)
  (net 4 /VCC_IO)
  (net 5 /BMB1)
  (net 6 "Net-(C1-Pad1)")
  (net 7 /+VM)
  (net 8 /EN)
  (net 9 /STEP)
  (net 10 /DIR)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+VM)
    (add_net /BMA1)
    (add_net /BMB1)
    (add_net /BMB2)
    (add_net /DIR)
    (add_net /EN)
    (add_net /STEP)
    (add_net /VCC_IO)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
  )
  (module Package_SO:TSSOP-14_4.4x5mm_P0.65mm (layer Top) (tedit 5A02F25C)
    (at 148.59 110.49)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -3.55) (layer F.SilkS) hide)
    (fp_text value SN74LV4T125 (at 0 3.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 13 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 12 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers Top F.Paste F.Mask))
    (pad 10 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 8 /EN))
    (pad 8 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 3 /BMA1))
    (pad 7 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 2 /BMB2))
    (pad 5 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 10 /DIR))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 5 /BMB1))
    (pad 2 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 9 /STEP))
    (pad 1 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer Top) (tedit 59FED5CC)
    (at 146.05 100.33 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x03_Odd_Even (at 2.54 20.32 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /+VM))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC_IO))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBE)
    (at 148.808 105.41 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.82) (layer F.SilkS) hide)
    (fp_text value CP (at 0 1.82) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SilentStepStick-TMC5160_v14:1X08-S (layer Bottom) (tedit 0)
    (at 142.151 105.024 90)
    (descr "<b>PIN HEADER</b> - 2.54")
    (fp_text reference P1 (at -10.2362 1.8288 90) (layer B.SilkS) hide)
    (fp_text value MA08-1 (at -10.16 -3.175 90) (layer B.Fab) hide)
    (pad 8 thru_hole circle (at 8.89 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /EN))
    (pad 7 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /STEP))
    (pad 1 thru_hole rect (at -8.89 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /DIR))
  )
  (module SilentStepStick-TMC5160_v14:1X08-S (layer Bottom) (tedit 0)
    (at 154.851 105.024 90)
    (descr "<b>PIN HEADER</b> - 2.54")
    (fp_text reference P2 (at -10.2362 1.8288 90) (layer B.SilkS) hide)
    (fp_text value MA08-1 (at -10.16 -3.175 90) (layer B.Fab) hide)
    (pad 8 thru_hole circle (at 8.89 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /+VM))
    (pad 7 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /BMA1))
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /BMB1))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /BMB2))
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /VCC_IO))
    (pad 1 thru_hole rect (at -8.89 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text G (at 148.51 102.13) (layer F.SilkS))
  (gr_text V (at 146.05 95.95) (layer F.SilkS))
  (gr_text 5 (at 148.66 95.89) (layer F.SilkS))
  (gr_text M (at 151.16 95.95) (layer F.SilkS))
  (gr_text G (at 153.01 113.91) (layer B.SilkS))
  (gr_text S (at 153.07 106.3) (layer F.SilkS))
  (gr_text D (at 153.07 108.8) (layer F.SilkS))
  (gr_text E (at 153.07 103.83) (layer F.SilkS))
  (gr_text G (at 153.1 101.25) (layer F.SilkS))
  (gr_text M (at 152.99 96.07) (layer F.SilkS))
  (gr_text G (at 153.07 98.61) (layer F.SilkS))
  (gr_text V (at 153.28 111.47) (layer F.SilkS))
  (gr_text G (at 153.13 113.94) (layer F.SilkS))
  (gr_text E (at 143.81 96.15) (layer F.SilkS))
  (gr_text D (at 144 113.9) (layer F.SilkS))
  (gr_text S (at 143.89 111.42) (layer F.SilkS))
  (gr_line (start 140.8811 115.1636) (end 156.1211 115.1636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.1211 115.1636) (end 156.1211 94.8436) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.1211 94.8436) (end 140.8811 94.8436) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.8811 94.8436) (end 140.8811 115.1636) (layer Edge.Cuts) (width 0.05))
)
