(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 206.924999 21.924999 270.575001 80.075001)
    (thickness 1.6)
    (drawings 31)
    (tracks 136)
    (zones 0)
    (modules 200)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.508 0.508)
    (pad_drill 0.3048)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 ePWM1A)
  (net 2 GND)
  (net 3 +5V)
  (net 4 ePWM1B)
  (net 5 eQEP2B)
  (net 6 eQEP2A)
  (net 7 GaN_VIN)
  (net 8 GaN_GND)
  (net 9 GaN_HS)
  (net 10 GaN_HB)
  (net 11 "Net-(C23-Pad1)")
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(D2-Pad2)")
  (net 14 "Net-(JP1-Pad1)")
  (net 15 "Net-(JP1-Pad3)")
  (net 16 "Net-(JP2-Pad1)")
  (net 17 GaN_SW)
  (net 18 +3V3)
  (net 19 "Net-(P1-Pad4)")
  (net 20 "Net-(P1-Pad5)")
  (net 21 "Net-(P1-Pad6)")
  (net 22 "Net-(P1-Pad7)")
  (net 23 "Net-(P1-Pad8)")
  (net 24 "Net-(P1-Pad9)")
  (net 25 "Net-(P1-Pad10)")
  (net 26 "Net-(P1-Pad11)")
  (net 27 "Net-(P1-Pad12)")
  (net 28 "Net-(P1-Pad13)")
  (net 29 "Net-(P1-Pad14)")
  (net 30 "Net-(P1-Pad15)")
  (net 31 "Net-(P1-Pad19)")
  (net 32 "Net-(P1-Pad20)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net GaN_GND)
    (add_net GaN_HB)
    (add_net GaN_HS)
    (add_net GaN_SW)
    (add_net GaN_VIN)
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad3)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net ePWM1A)
    (add_net ePWM1B)
    (add_net eQEP2A)
    (add_net eQEP2B)
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 263.7 26.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 264.9 26.7)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 264.85 25.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 263.65 25.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 263.65 24.3)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 264.8 24.25)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 246.7 63.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 246.7 62.35)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 246.7 61)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 246.7 59.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 245.75 59.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 245.75 63.6)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 245.75 62.35)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 218.6 65.35)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 218.6 63.9)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 219.9 63.9)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 219.9 62.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 218.55 62)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 218.55 60.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 219.8 60.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 219.75 57.9)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 218.6 57.9)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 218.6 55.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803DE31)
    (at 246 35.45)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 3 +5V) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803DE31)
    (at 244 35.45)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 3 +5V) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 219.7 75.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 219.75 76.8)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 222.7 77.8)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 221.75 77.8)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 220.75 77.95)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 220.75 76.8)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 220.75 75.6)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 220.75 74.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 229.3 77)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 229.3 77)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 229.45 75.85)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 229.45 74.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 229.4 73.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.3 73.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.3 77)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.3 75.9)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.3 74.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 230.65 63.7)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.75 63.7)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 227.55 63.7)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 227.55 62.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.7 62)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.7 60.25)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 227.55 60.25)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 227.55 57.95)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.65 57.9)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 228.65 55.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 227.55 55.75)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 230.45 55.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 230.45 54.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 231.25 54.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 231.25 55.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 232.15 55.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 232.15 54.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 233.05 54.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 233.05 55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 233.95 55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 233.95 54.15)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 234.85 54.15)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 234.85 55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 235.65 55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 235.65 54.15)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 236.65 55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 236.65 54.15)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D5E0)
    (at 236.65 53.3)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 227.7 46.3)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 228.5 46.3)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 228.5 46.3)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 227.65 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 228.5 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 231.1 46.35)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 230.3 46.35)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 229.4 46.35)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 229.4 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 230.3 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 231.15 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 231.95 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 232.8 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803D283)
    (at 233.65 45.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 233.6 42.3)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 233.65 43.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 240.2 42.35)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 233.65 43)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 234.35 43)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 234.35 43.7)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 235.15 43.7)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 235.95 43.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 236.85 43.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 237.6 43.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 238.3 43.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 239 43.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 239.7 43.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 240.2 43)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 230 39.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 228.9 39.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 228.05 39.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 227.1 39.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 226.05 39.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 225.15 39.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 224.15 39.55)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 224.15 38.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 225.15 38.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 226.1 38.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 227.05 38.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 228 38.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 228.9 38.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 230 38.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 212.7 38.25)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 213.55 40.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 213.55 39.85)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 213.55 39.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 213.55 38.25)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 212.7 40.65)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 212.7 39.85)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803CED2)
    (at 212.7 39.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 8 GaN_GND) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 211.05 32.5)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 214.55 32.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 213.75 33.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 213.7 32.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 211.9 33.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 211.95 32.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 212.8 33.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 212.8 32.05)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D59EBC)
    (at 246.5 45.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 10p (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 ePWM1A))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D59BD8)
    (at 243 34.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 4 0 90) (layer F.SilkS))
    (fp_text value 2.2u (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D59EBA)
    (at 246.5 41 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 2 90) (layer F.SilkS))
    (fp_text value 10p (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 ePWM1B))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D59C13)
    (at 245 34.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 4 0 90) (layer F.SilkS))
    (fp_text value 100p (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D59C30)
    (at 247 34.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 4 0 90) (layer F.SilkS))
    (fp_text value 2.2u (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D58C54)
    (at 255.81 69.85 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 100p (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 eQEP2B))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D58C50)
    (at 250.73 69.85)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -3.81 0) (layer F.SilkS))
    (fp_text value 100p (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 eQEP2A))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_2220_HandSoldering (layer B.Cu) (tedit 58028F10)
    (at 225 67.5)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C8 (at -6.5 0) (layer B.SilkS))
    (fp_text value 10u (at -0.5 -0.5) (layer B.Fab))
    (pad 1 smd rect (at -3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_2220_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5803D58E)
    (at 229 50 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at 4.5 -0.5 270) (layer F.SilkS))
    (fp_text value 2u2 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5803D4C0)
    (at 223.5 62.5)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C10 (at -5.5 -0.5) (layer F.SilkS))
    (fp_text value 2u2 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5803D4B9)
    (at 223.5 58.5)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C11 (at -5 -0.5) (layer F.SilkS))
    (fp_text value 2u2 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58028F21)
    (at 223.5 59)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C12 (at -5 0) (layer B.SilkS))
    (fp_text value 2u2 (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5803D595)
    (at 232 50 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at 5 0 270) (layer F.SilkS))
    (fp_text value 1u (at -0.5 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_2220_HandSoldering (layer F.Cu) (tedit 5803D4CA)
    (at 225 67.5)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C14 (at -7 -0.5) (layer F.SilkS))
    (fp_text value 10u (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.5 0) (size 2.4 5) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 3.5 0) (size 2.4 5) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_2220_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5803D49D)
    (at 236.4 50.35 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 4 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5803D496)
    (at 234.4 50.35 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 4 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58028F1A)
    (at 223.5 55.5)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C17 (at -5 -0.5) (layer B.SilkS))
    (fp_text value 2u2 (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58029011)
    (at 235.5 50 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C18 (at 5 0 270) (layer B.SilkS))
    (fp_text value 2u2 (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58029017)
    (at 239 50 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C19 (at 5 0 270) (layer B.SilkS))
    (fp_text value 1u (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5803D4B1)
    (at 223.5 55)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C20 (at -5 0) (layer F.SilkS))
    (fp_text value 1u (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5803D4A4)
    (at 238.4 50.35 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 4 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57D596C3)
    (at 242.55 47.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 GaN_HS))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GaN_HB))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5803CD6A)
    (at 219.6 34.3 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C23 (at 5 0 270) (layer F.SilkS))
    (fp_text value 47u (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5803CD5F)
    (at 224.2 34.3 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C24 (at -6 0 270) (layer F.SilkS))
    (fp_text value 47u (at -0.5 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5803CD64)
    (at 221.9 34.3 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C25 (at 5 0 270) (layer F.SilkS))
    (fp_text value 47u (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 580291C1)
    (at 226.8 34.6 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C26 (at -5 0 270) (layer B.SilkS))
    (fp_text value 22u (at -0.5 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5803CD59)
    (at 226.9 34.7 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C27 (at -6 0 270) (layer F.SilkS))
    (fp_text value 22u (at -0.5 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5803CD51)
    (at 229.4 34.15 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C28 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value 2u2 (at 0.5 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 580291DE)
    (at 229.5 34.5 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C29 (at -5 0 270) (layer B.SilkS))
    (fp_text value 47u (at -0.5 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 580291E6)
    (at 224.5 33.9 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at -3.5 0 270) (layer B.SilkS))
    (fp_text value 47u (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 236.5 68 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57D59B6B)
    (at 257 24)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at -3.5 0) (layer F.SilkS))
    (fp_text value LED (at 0 2) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57D59E7C)
    (at 262.5 42.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 0 -3) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 ePWM1A))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(JP1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57D59E8A)
    (at 262.5 31)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 0 -3) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(JP2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 ePWM1B))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(JP1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x22 (layer F.Cu) (tedit 57D59F04)
    (at 267.97 24.13)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -3.47 -0.13) (layer F.SilkS))
    (fp_text value CONN_01X22 (at 0.03 11.87 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 +3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(JP1-Pad1)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(JP1-Pad3)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(JP2-Pad1)"))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P1-Pad19)"))
    (pad 20 thru_hole oval (at 0 48.26) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P1-Pad20)"))
    (pad 21 thru_hole oval (at 0 50.8) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 eQEP2A))
    (pad 22 thru_hole oval (at 0 53.34) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 eQEP2B))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x22.wrl
      (at (xyz 0 -1.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module BuchananTerminalBlocks:TE282834-2 (layer F.Cu) (tedit 58028D74)
    (at 224.73 76)
    (fp_text reference P2 (at -5.23 3) (layer F.SilkS))
    (fp_text value CONN_VIN (at 0 1.8) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.77 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 GaN_GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.77 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module BuchananTerminalBlocks:TE282834-2 (layer F.Cu) (tedit 58029098)
    (at 211 37.23 270)
    (fp_text reference P3 (at 4.5 3.5 270) (layer F.SilkS))
    (fp_text value CONN_VOUT (at 0 1.8 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.77 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 GaN_GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.77 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57D58C57)
    (at 255.81 73.66 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 eQEP2B))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57D58C59)
    (at 250.73 73.66 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 eQEP2A))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 234.5 72 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 20k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 57D5A05C)
    (at 243.8 58)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 3.5 0) (layer B.SilkS))
    (fp_text value 0R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GaN_GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 57D5A0AB)
    (at 259.08 24.13)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -3.08 -0.13) (layer B.SilkS))
    (fp_text value 1k (at -0.08 -0.13) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Panasonic_Rotary_Encoders:EVQVV_Rotary_Encoder (layer F.Cu) (tedit 57D58C4C)
    (at 253.27 58.42)
    (fp_text reference SW1 (at -3.81 -8.89) (layer F.SilkS))
    (fp_text value rotary_encoder (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.5 8.1) (size 1.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 eQEP2B))
    (pad 3 smd rect (at -2.5 8.1) (size 1.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 eQEP2A))
    (pad 1 smd rect (at 0 -6.1) (size 3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" thru_hole oval (at -4 0) (size 1.3 1.1) (drill oval 1.3 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole oval (at 4 0) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole oval (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 smd rect (at 0 8.1) (size 1.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 57D5A752)
    (at 255.5 45 270)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference W1 (at 0 -2 270) (layer F.SilkS))
    (fp_text value TEST_HI (at 1.5 -2.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 ePWM1A))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 57D5A74F)
    (at 255.5 41.5 90)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference W2 (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text value TEST_LO (at 1.27 2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 ePWM1B))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 56C3646A)
    (at 234.79 76.5 180)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference W3 (at 1.27 -2 180) (layer F.SilkS))
    (fp_text value TEST_VIN (at 1.27 2 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GaN_VIN))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GaN_GND))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 57D5A732)
    (at 211.5 45.75)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference W4 (at 3 2.5) (layer F.SilkS))
    (fp_text value TEST_VOUT (at 1.27 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GaN_GND))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 56C3646A)
    (at 251 35.5 90)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference W5 (at 1.27 -2 90) (layer F.SilkS))
    (fp_text value TEST_VBIAS (at 1.27 2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module lmg5200:LMG5200 (layer F.Cu) (tedit 5803D0BC)
    (at 239.18 42.89 90)
    (descr LMG5200)
    (tags "GaN halfbridge")
    (solder_mask_margin 0.07)
    (fp_text reference U1 (at 0 5.1 90) (layer F.SilkS))
    (fp_text value LMG5200 (at 0 -0.5 90) (layer F.Fab))
    (pad 5 smd rect (at 0.9 3.55 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 ePWM1B) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 2.55 2.05 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 2.55 3.25 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.55 3.25 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 GaN_HS) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -2.55 -1.78 90) (size 0.7 4.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GaN_VIN) (solder_mask_margin 0.07) (zone_connect 2))
    (pad 8 smd rect (at 2.55 -1.78 90) (size 0.7 4.25) (layers F.Cu F.Paste F.Mask)
      (net 17 GaN_SW) (solder_mask_margin 0.07) (zone_connect 2))
    (pad 9 smd rect (at 0 -1.78 90) (size 1.05 4.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GaN_GND) (solder_mask_margin 0.07) (zone_connect 2))
    (pad 2 smd rect (at -2.55 2.05 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 GaN_HB) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -0.9 3.55 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 ePWM1A) (solder_mask_margin 0.07))
  )
  (module Mounting_Holes:MountingHole_3mm_Pad (layer F.Cu) (tedit 57D97EC9)
    (at 242.5 26.5)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference "" (at 0 -4) (layer F.SilkS))
    (fp_text value "" (at 0 4) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm_Pad (layer F.Cu) (tedit 57D5A5D6)
    (at 242.5 75.5)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference "" (at 0 -4) (layer F.SilkS))
    (fp_text value "" (at 0 4) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm_Pad (layer F.Cu) (tedit 57D5A5D1)
    (at 211.5 75.5)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference "" (at 0 -4) (layer F.SilkS))
    (fp_text value "" (at 8.5 3.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm_Pad (layer F.Cu) (tedit 57D97E68)
    (at 211.5 26.5)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference "" (at 0 -4) (layer F.SilkS))
    (fp_text value "" (at 0 4) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module coilcraft_incuctors:XAL8080 (layer F.Cu) (tedit 5803BF5B)
    (at 235.37 35.27 90)
    (fp_text reference L1 (at 0 5.6 90) (layer F.SilkS))
    (fp_text value 4µ7 (at -0.1 -0.3 270) (layer F.Fab))
    (pad 2 smd rect (at 2.58 0 90) (size 1.78 7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
    (pad 1 smd rect (at -2.58 0 90) (size 1.78 7) (layers F.Cu F.Paste F.Mask)
      (net 17 GaN_SW) (zone_connect 2))
  )
  (module vias:via_38_mil (layer F.Cu) (tedit 5803B016)
    (at 233.4 40.3)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 38 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.9652) (layers *.Cu)
      (net 17 GaN_SW) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C76F)
    (at 230 30.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C767)
    (at 230 29.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C75F)
    (at 229 30.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C759)
    (at 229 29.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C77C)
    (at 228.1 29.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C782)
    (at 228.1 30.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C74C)
    (at 227.3 29.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C752)
    (at 227.3 30.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C73E)
    (at 226.4 29.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C745)
    (at 226.4 30.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C732)
    (at 225.5 29.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C738)
    (at 225.5 30.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C723)
    (at 224.5 29.1)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803C72A)
    (at 224.5 30.2)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 11 "Net-(C23-Pad1)") (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803DE31)
    (at 242.1 35.45)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 3 +5V) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E5EE)
    (at 219.6 55.7)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 7 GaN_VIN) (zone_connect 2))
  )
  (module vias:via_12_mil (layer F.Cu) (tedit 5803E663)
    (at 245.75 61)
    (fp_text reference REF** (at 1.3 1.7) (layer F.SilkS) hide)
    (fp_text value "via 12 mil" (at -0.1 -1.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.3048) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (gr_text + (at 237.25 76.25) (layer F.SilkS))
  (gr_text + (at 211.5 48.5) (layer F.SilkS))
  (gr_text 3 (at 259.5 48) (layer F.SilkS))
  (gr_text 3 (at 259.5 36.5) (layer F.SilkS))
  (gr_text "jumpers\nTMS570LS12x/RM46x\nJP1 1-2\nJP2 1-2\nTMS570LC43x/RM57x\nJP1 2-3\nJP2 2-3" (at 264.5 68) (layer B.SilkS))
  (gr_text hi (at 252 45) (layer F.SilkS))
  (gr_text lo (at 252 41.5) (layer F.SilkS))
  (gr_line (start 207 22) (end 270.5 22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207 80) (end 207 22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 270.5 80) (end 207 80) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 270.5 22) (end 270.5 80) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "LMG5200 BoosterPack\nfor Hercules v1" (at 210.5 61.5 90) (layer F.SilkS))
  (gr_text in (at 229.5 78.5) (layer F.SilkS))
  (gr_text GND (at 229.4 72.8 90) (layer F.SilkS))
  (gr_text + (at 219.9 75.7) (layer F.SilkS))
  (gr_text in (at 233.5 67.5) (layer F.SilkS))
  (gr_text bias (at 257 27.5) (layer F.SilkS))
  (gr_text GND (at 212.5 42) (layer F.SilkS))
  (gr_text + (at 211 33) (layer F.SilkS))
  (gr_text out (at 209 44.5 90) (layer F.SilkS))
  (gr_text 1 (at 259.5 42) (layer F.SilkS))
  (gr_text 1 (at 259.5 30.5) (layer F.SilkS))
  (gr_text bias (at 255 35.5) (layer F.SilkS))
  (zone (net 8) (net_name GaN_GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.9 42.2) (xy 239.75 41.75) (xy 232.75 41.75) (xy 231.3 38.9) (xy 231.3 36.3)
        (xy 230 34.7) (xy 225.6 34.7) (xy 224.9 34.2) (xy 224.1 34.2) (xy 223.6 34)
        (xy 222.2 34) (xy 221.5 34) (xy 215.5 34) (xy 214.6 35) (xy 214.6 36.5)
        (xy 213.5 37.5) (xy 209.174613 37.5) (xy 208.8 37.9) (xy 208.8 41) (xy 209.75 41.75)
        (xy 212.5 41.75) (xy 213.25 42.5) (xy 213.25 46.75) (xy 214.25 47.5) (xy 215.5 47.5)
        (xy 216 46.5) (xy 216 45.4) (xy 217.5 44) (xy 239.75 44) (xy 240.9 43.6)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C23-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.5 35) (xy 239.1 35) (xy 239.8 34.1) (xy 239.8 29.4) (xy 238 27.9)
        (xy 217 27.9) (xy 214.4 31) (xy 208.7 31) (xy 208.7 36.4) (xy 209.2 36.9)
        (xy 212.8 36.9) (xy 213.9 36) (xy 213.9 34.4) (xy 215.2 33.3) (xy 221.2 33.3)
        (xy 221.8 33.3) (xy 223.7 33.3) (xy 224.1 33.6) (xy 230.3 33.6)
      )
    )
  )
  (zone (net 7) (net_name GaN_VIN) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 239.9 45) (xy 239.6 44.8) (xy 238.6 44.8) (xy 217.8 44.8) (xy 216.9 45.6)
        (xy 216.9 77.6) (xy 218 79) (xy 224.1 79) (xy 224.1 72.3) (xy 222.7 71)
        (xy 222.7 51.1) (xy 224 49.7) (xy 240.3 49.7) (xy 240.3 45.9)
      )
    )
  )
  (zone (net 8) (net_name GaN_GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 230.7 51) (xy 238.4 51) (xy 240.3 51) (xy 240.3 53.4) (xy 241.9 55)
        (xy 243.3 56.8) (xy 243.3 71) (xy 238 71) (xy 238 75) (xy 233.4 75)
        (xy 233.4 78) (xy 232.7 79) (xy 225.4 79) (xy 225.4 70.7) (xy 224.5 70)
        (xy 224.5 52.6) (xy 226 51) (xy 227.1 51)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.9 37.8) (xy 212.1 37.8) (xy 212.1 40.2) (xy 209.9 40.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.9 34.4) (xy 209.9 36.6) (xy 212.1 36.6) (xy 212.1 34.4)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 242 31) (xy 241 31.7) (xy 241 41) (xy 242 41.6) (xy 242 44)
        (xy 241 44.7) (xy 241 53) (xy 244 56.4) (xy 244 71) (xy 246 71)
        (xy 246 79) (xy 269.3 79) (xy 269.3 22.6) (xy 247.6 22.6) (xy 247 23.3)
        (xy 246.076063 24.447462) (xy 246 30) (xy 245 31)
      )
    )
  )
  (zone (net 17) (net_name GaN_SW) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.9 35.5) (xy 231.9 38.9) (xy 233 41) (xy 240.3 41) (xy 240.3 35.5)
      )
    )
  )
  (zone (net 17) (net_name GaN_SW) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.9 35.5) (xy 231.9 39) (xy 233 41) (xy 240.3 41) (xy 240.3 35.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 262.6 29.7) (xy 269.3 29.7) (xy 269.3 50) (xy 255.4 49.9) (xy 255.1 37.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.7 35.2) (xy 231.7 39.1) (xy 233 41.4) (xy 240.5 41.4) (xy 240.5 35.2)
      )
    )
  )
  (zone (net 8) (net_name GaN_GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 241.3 35.9) (xy 241.3 31) (xy 239.9 31) (xy 239.9 29.6) (xy 238.1 27.9)
        (xy 217.1 27.9) (xy 214.374432 31) (xy 209.3 31) (xy 208.7 31.5) (xy 208.6 78.5)
        (xy 209.1 79) (xy 239 79) (xy 239 71) (xy 244.5 71.1) (xy 244.5 56)
        (xy 242.3 53.5) (xy 242.3 41.75) (xy 241.3 39.8) (xy 241.3 35.7)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 243 37.25) (xy 243 38.8) (xy 243.1 39.9) (xy 243.1 52.9) (xy 245.2 55.3)
        (xy 245.2 71) (xy 246 71) (xy 246 79.2) (xy 266.3 79.3) (xy 266.3 32)
        (xy 249.45 31.9) (xy 249.45 37.25) (xy 244.25 37.25)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 247.6 22.7) (xy 245.9 24.6) (xy 245.9 29.984695) (xy 245.05 31.05) (xy 242.25 31)
        (xy 242.286409 34.968708) (xy 241.7 34.95) (xy 241.7 39.4) (xy 242.1 39.8) (xy 242.05 40.7)
        (xy 242.8 40.8) (xy 242.8 39.9) (xy 242.25 39.178493) (xy 242.25 36.45) (xy 248.95 36.45)
        (xy 248.943494 31) (xy 269.3 31) (xy 269.3 22.6) (xy 247.7 22.6)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C23-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 238.1 27.9) (xy 217.1 27.9) (xy 214.4 30.9) (xy 208.7 31) (xy 208.7 36.4)
        (xy 209.1 36.9) (xy 212.8 36.9) (xy 213.9 36) (xy 213.9 34.4) (xy 215.3 33.3)
        (xy 223.7 33.3) (xy 224.1 33.6) (xy 230.3 33.6) (xy 231.5 35) (xy 239.1 35)
        (xy 239.9 34.2) (xy 239.9 29.6)
      )
    )
  )
  (zone (net 8) (net_name GaN_GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.9 42.2) (xy 240.9 43.6) (xy 239.8 44) (xy 217.5 44) (xy 216 45.4)
        (xy 216 46.5) (xy 215.5 47.5) (xy 214.2 47.5) (xy 213.25 46.75) (xy 213.25 42.5)
        (xy 212.5 41.75) (xy 209.75 41.75) (xy 208.8 41) (xy 208.8 37.9) (xy 209.15 37.5)
        (xy 213.5 37.5) (xy 214.6 36.5) (xy 214.6 35) (xy 215.5 34) (xy 223.6 34)
        (xy 224.15 34.2) (xy 224.9 34.2) (xy 225.6 34.7) (xy 230 34.7) (xy 231.3 36.3)
        (xy 231.3 38.9) (xy 232.75 41.75) (xy 239.75 41.75)
      )
    )
  )
  (zone (net 7) (net_name GaN_VIN) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.3 45.85) (xy 239.9 45) (xy 239.65 44.8) (xy 217.8 44.8) (xy 216.9 45.6)
        (xy 216.9 77.65) (xy 218 79) (xy 224 79) (xy 224.1 78.9) (xy 224.1 72.3)
        (xy 222.7 71) (xy 222.7 51.1) (xy 224 49.7) (xy 240.2 49.7) (xy 240.3 49.6)
        (xy 240.3 49.6)
      )
    )
  )
  (zone (net 8) (net_name GaN_GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226 51) (xy 224.5 52.55) (xy 224.5 70.05) (xy 225.4 70.75) (xy 225.4 78.9)
        (xy 225.5 79) (xy 232.7 79) (xy 233.4 78) (xy 233.4 75) (xy 238.55 75)
        (xy 238.55 71) (xy 243.3 71) (xy 243.3 56.75) (xy 240.3 53.4) (xy 240.3 51)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 269.3 79) (xy 269.3 22.6) (xy 247.6 22.6) (xy 246 24.5) (xy 246 30)
        (xy 245 31) (xy 242 31) (xy 241 31.7) (xy 241 34.254327) (xy 248.5 34.25)
        (xy 248.45 36.65) (xy 241 36.651619) (xy 241 41) (xy 242 41.6) (xy 242 44)
        (xy 241 44.75) (xy 241 52.95) (xy 244 56.45) (xy 244 71) (xy 246 71)
        (xy 246 79)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 241.6 39.45) (xy 241.6 41) (xy 242.9 41) (xy 242.9 39.45)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 241 34.6) (xy 247.95 34.6) (xy 247.95 36.35) (xy 241 36.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 252 64.95) (xy 252.05 67.95) (xy 250.7 67.95) (xy 250.75 70.5) (xy 255.7 70.5)
        (xy 255.7 67.85) (xy 254.45 67.85) (xy 254.45 65) (xy 258.192576 65) (xy 258.2 70.4)
        (xy 269.3 70.43833) (xy 269.3 79.1) (xy 265 79.05) (xy 265 75.4) (xy 248.5 75.5)
        (xy 248.5 64.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 246 42.25) (xy 256 42.35) (xy 256 44.1) (xy 246 44.05)
      )
    )
  )
)
