(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 254)
    (no_connects 0)
    (area 35.56 15.748 153.162001 107.696001)
    (thickness 1.6)
    (drawings 5)
    (tracks 1803)
    (zones 0)
    (modules 126)
    (nets 85)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.905 1.905)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 GND)
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C4-Pad2)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 "Net-(C6-Pad2)")
  (net 11 "Net-(C7-Pad1)")
  (net 12 "Net-(C8-Pad1)")
  (net 13 "Net-(C9-Pad1)")
  (net 14 "Net-(C10-Pad1)")
  (net 15 "Net-(C10-Pad2)")
  (net 16 "Net-(C11-Pad1)")
  (net 17 "Net-(C12-Pad1)")
  (net 18 "Net-(C13-Pad1)")
  (net 19 "Net-(C14-Pad1)")
  (net 20 "Net-(C15-Pad1)")
  (net 21 "Net-(C16-Pad1)")
  (net 22 "Net-(C17-Pad1)")
  (net 23 "Net-(C18-Pad1)")
  (net 24 "Net-(C19-Pad1)")
  (net 25 "Net-(C21-Pad1)")
  (net 26 "Net-(C22-Pad1)")
  (net 27 "Net-(C22-Pad2)")
  (net 28 "Net-(C25-Pad2)")
  (net 29 "Net-(C26-Pad1)")
  (net 30 "Net-(C27-Pad2)")
  (net 31 "Net-(C29-Pad1)")
  (net 32 "Net-(C30-Pad1)")
  (net 33 "Net-(C31-Pad1)")
  (net 34 "Net-(C32-Pad1)")
  (net 35 "Net-(D1-Pad1)")
  (net 36 "Net-(R1-Pad2)")
  (net 37 "Net-(R4-Pad1)")
  (net 38 "Net-(R7-Pad2)")
  (net 39 "Net-(R8-Pad2)")
  (net 40 "Net-(R9-Pad2)")
  (net 41 "Net-(R10-Pad1)")
  (net 42 +3V3)
  (net 43 "Net-(R12-Pad1)")
  (net 44 "Net-(R15-Pad2)")
  (net 45 "Net-(R19-Pad2)")
  (net 46 "Net-(R21-Pad1)")
  (net 47 "Net-(R21-Pad2)")
  (net 48 "Net-(R23-Pad1)")
  (net 49 "Net-(U1-Pad1)")
  (net 50 +5V)
  (net 51 +12V)
  (net 52 "Net-(U14-Pad1)")
  (net 53 "Net-(C45-Pad1)")
  (net 54 "Net-(C36-Pad1)")
  (net 55 "Net-(C37-Pad1)")
  (net 56 "Net-(C49-Pad1)")
  (net 57 "Net-(C52-Pad1)")
  (net 58 5V4_filtered)
  (net 59 "Net-(R26-Pad2)")
  (net 60 "Net-(R28-Pad1)")
  (net 61 "Net-(R29-Pad1)")
  (net 62 "Net-(R32-Pad2)")
  (net 63 "Net-(R34-Pad2)")
  (net 64 13V5_filtered)
  (net 65 "Net-(U23-Pad1)")
  (net 66 "Net-(U30-Pad8)")
  (net 67 "Net-(U30-Pad1)")
  (net 68 "Net-(U21-Pad17)")
  (net 69 "Net-(U21-Pad9)")
  (net 70 "Net-(U23-Pad8)")
  (net 71 "Net-(U4-Pad2)")
  (net 72 "Net-(U4-Pad3)")
  (net 73 "Net-(U4-Pad4)")
  (net 74 "Net-(U4-Pad5)")
  (net 75 "Net-(U4-Pad6)")
  (net 76 "Net-(U4-Pad12)")
  (net 77 "Net-(U4-Pad13)")
  (net 78 "Net-(U4-Pad14)")
  (net 79 "Net-(U4-Pad15)")
  (net 80 "Net-(U4-Pad16)")
  (net 81 "Net-(U4-Pad17)")
  (net 82 "Net-(U4-Pad18)")
  (net 83 "Net-(U4-Pad19)")
  (net 84 "Net-(U4-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad2)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C37-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(C49-Pad1)")
    (add_net "Net-(C52-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R34-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U14-Pad1)")
    (add_net "Net-(U21-Pad17)")
    (add_net "Net-(U21-Pad9)")
    (add_net "Net-(U23-Pad1)")
    (add_net "Net-(U23-Pad8)")
    (add_net "Net-(U30-Pad1)")
    (add_net "Net-(U30-Pad8)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad17)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad19)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad20)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
  )
  (net_class POWER ""
    (clearance 0.508)
    (trace_width 1.27)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net 13V5_filtered)
    (add_net 5V4_filtered)
  )
  (module "Reference Parts:SMA_RT_ANG" (layer F.Cu) (tedit 5B7C2F9D)
    (at 129.54 36.957)
    (fp_text reference U6 (at 0 -4.318) (layer F.SilkS))
    (fp_text value SMA_Rt_Ang (at 1.27 6.35) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 2.54 2.54) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at -2.54 2.54) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at -2.54 -2.54) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(C10-Pad2)"))
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5B7C2FB8)
    (at 124.0155 56.3245)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C40 (at -4.0005 -0.3175 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5B7C2FB5)
    (at 124.0155 53.0225)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C41 (at -4.0005 -0.1905 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5B7C2FAF)
    (at 124.0155 49.7205)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C42 (at -4.1275 -0.1905 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5B7C2FAA)
    (at 124.0155 46.4185)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C43 (at -4.0005 -2.2225 90) (layer F.SilkS) hide)
    (fp_text value 100uF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 124.0155 43.1165)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C44 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5B7C3222)
    (at 71.12 40.64 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at -3.175 -1.143 360) (layer F.SilkS))
    (fp_text value NC7SZ04 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 4 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (pad 5 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5B7C2E9D)
    (at 81.28 42.545 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U14 (at -3.048 -1.651 360) (layer F.SilkS))
    (fp_text value NC7SZ04 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U14-Pad1)"))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C25-Pad2)"))
    (pad 3 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 4 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C22-Pad1)"))
    (pad 5 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C27-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Reference Parts:SMA_RT_ANG" (layer F.Cu) (tedit 5B7C320B)
    (at 53.594 41.275 90)
    (fp_text reference U2 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value SMA_Rt_Ang (at 1.27 6.35 90) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at -2.54 2.54 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at -2.54 -2.54 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 36 "Net-(R1-Pad2)"))
  )
  (module "Reference Parts:Bourns_3361P" (layer F.Cu) (tedit 5B7C2B0A)
    (at 80.391 52.578 180)
    (fp_text reference R23 (at -0.889 -6.223 180) (layer F.SilkS))
    (fp_text value 100K (at 0 6.35 180) (layer F.Fab))
    (pad 3 smd rect (at -2.54 3.2 180) (size 1.19 3.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at 0 -3.2 180) (size 1.19 3.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R19-Pad2)"))
    (pad 1 smd rect (at 2.54 3.2 180) (size 1.19 3.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R23-Pad1)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5B7C31C0)
    (at 101.092 51.816 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C50 (at 1.397 1.27 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C49-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5B7C314D)
    (at 96.774 73.66 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C53 (at -0.381 -2.032 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C52-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Reference Parts:TPS7A88" (layer B.Cu) (tedit 5B7C3049)
    (at 107.188 85.344)
    (fp_text reference U21 (at -3.683 5.334) (layer B.SilkS) hide)
    (fp_text value TPS7A88 (at 0 -3.81) (layer B.Fab))
    (pad 13 smd rect (at 1.975 0) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -1.975 1) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at -1.975 0.5) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C32-Pad1)"))
    (pad 4 smd rect (at -1.975 -0.5) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C31-Pad1)"))
    (pad 5 smd rect (at -1.975 -1) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C31-Pad1)"))
    (pad 3 smd rect (at -1.975 0) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 15 smd rect (at 1.975 1) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 50 +5V))
    (pad 12 smd rect (at 1.975 -0.5) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 42 +3V3))
    (pad 11 smd rect (at 1.975 -1) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 42 +3V3))
    (pad 17 smd rect (at 0.5 1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(U21-Pad17)"))
    (pad 10 smd rect (at 1 -1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R28-Pad1)"))
    (pad 18 smd rect (at 0 1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C32-Pad1)"))
    (pad 9 smd rect (at 0.5 -1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(U21-Pad9)"))
    (pad 6 smd rect (at -1 -1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C31-Pad1)"))
    (pad 14 smd rect (at 1.975 0.5) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 50 +5V))
    (pad 16 smd rect (at 1 1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R29-Pad1)"))
    (pad 7 smd rect (at -0.5 -1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(C37-Pad1)"))
    (pad 8 smd rect (at 0 -1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C31-Pad1)"))
    (pad 20 smd rect (at -1 1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C32-Pad1)"))
    (pad 19 smd rect (at -0.5 1.975) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(C36-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.7 2.7) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 5B7C2FDE)
    (at 109.728 74.422 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U20 (at -0.508 2.54 180) (layer B.SilkS) hide)
    (fp_text value TPS736 (at 0 -2.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C30-Pad1)"))
    (pad 4 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R26-Pad2)"))
    (pad 5 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 42 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5B7C2FD2)
    (at 114.3 74.93)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 2.286 -1.27) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5B7C327C)
    (at 102.489 82.931 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0.127 1.905 180) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5B7C3052)
    (at 103.886 89.154 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 0.635 -1.397 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5B7C2FFB)
    (at 106.426 90.424 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C36 (at 0.889 2.159 270) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5B7C3181)
    (at 105.664 79.502 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C37 (at 1.27 5.461 90) (layer B.SilkS) hide)
    (fp_text value 1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(C37-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-89-3_Handsoldering (layer F.Cu) (tedit 58CE4E7F)
    (at 100.965 33.274 90)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference U26 (at 0.45 -3.3 90) (layer F.SilkS))
    (fp_text value ADL5545 (at 0.5 3.15 90) (layer F.Fab))
    (fp_text user %R (at 0.38 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.98 -1.5) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at -1.98 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.98 1.5) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.98 0) (size 2 4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd trapezoid (at -0.37 0 180) (size 1.5 0.75) (rect_delta 0 0.5 ) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F67)
    (at 108.204 34.671 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value NI (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F89)
    (at 110.363 34.798 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -0.635 2.032 360) (layer F.SilkS))
    (fp_text value 1 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F62)
    (at 106.172 34.798 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value NI (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C3123)
    (at 93.472 79.248 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 2.667 0 180) (layer B.SilkS))
    (fp_text value 29.1K (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(R34-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C30E9)
    (at 94.488 83.439 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 1.397 -1.524 180) (layer B.SilkS))
    (fp_text value 98.8K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 5V4_filtered))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(R34-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 98.806 60.706 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R32-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C31E4)
    (at 102.108 61.214 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at -2.794 -1.651 180) (layer B.SilkS))
    (fp_text value 87.6K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 51 +12V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R32-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C3187)
    (at 108.204 79.756 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at -1.143 -2.794 360) (layer B.SilkS))
    (fp_text value 3.57K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R28-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C3284)
    (at 109.728 89.154 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 10.5K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R29-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C2FF2)
    (at 108.458 91.948 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at -0.254 -1.524 270) (layer B.SilkS))
    (fp_text value 2K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R29-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C2FE3)
    (at 111.125 81.661)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0.381 -1.397) (layer B.SilkS))
    (fp_text value 1.15K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R28-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C3177)
    (at 105.156 75.946 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 3.937 -0.254 180) (layer B.SilkS) hide)
    (fp_text value 13K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5B7C3160)
    (at 104.394 73.152 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at -2.794 0.381 360) (layer B.SilkS))
    (fp_text value 22K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R26-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F7F)
    (at 104.521 34.925 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 2.413 -1.016 360) (layer F.SilkS) hide)
    (fp_text value 1.0uH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F5A)
    (at 100.203 38.862)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C45 (at -1.778 -1.397) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2EA4)
    (at 80.899 38.1 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at -0.889 1.397 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C25-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2FC1)
    (at 123.7615 58.8645)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at 3.3655 -0.1905) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F4F)
    (at 84.074 42.926 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at -1.143 -2.032 360) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C27-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2FC5)
    (at 123.7615 60.3885)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at -3.1115 -0.0635) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2E6D)
    (at 78.486 42.545 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value 10pF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C25-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C31EF)
    (at 68.58 55.753 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 0 -1.25 360) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C31F8)
    (at 72.136 55.753 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2E8C)
    (at 74.803 47.498 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at -1.397 -2.032 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C22-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C31F3)
    (at 70.358 55.753 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2B52)
    (at 63.881 51.943 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at -7.112 4.445 270) (layer F.SilkS) hide)
    (fp_text value 4.7uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 69.088 51.816 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 -1.25 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2E85)
    (at 70.612 45.847)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value NI (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2B62)
    (at 65.405 51.943 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -7.239 6.096 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2B3C)
    (at 61.341 49.403 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 6.604 0.381 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D6F)
    (at 72.009 48.895)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value .01uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C3239)
    (at 73.2155 61.4045 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -2.3495 -0.0635 360) (layer F.SilkS) hide)
    (fp_text value 33pF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C276B)
    (at 59.182 61.468 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at -0.254 1.651 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.397 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2E81)
    (at 70.612 43.942)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F92)
    (at 112.141 32.639 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 2.413 1.905 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F5D)
    (at 104.521 38.608)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 3.175 -0.762) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C323C)
    (at 70.0405 61.5315 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.6035 -0.0635 360) (layer F.SilkS) hide)
    (fp_text value 33pF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C323F)
    (at 67.1195 61.4045 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.6035 -0.8255 360) (layer F.SilkS) hide)
    (fp_text value 33pF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2836)
    (at 64.1985 61.4045 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.7305 -0.9525 360) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 95.885 36.195)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.25) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2DE8)
    (at 68.453 41.021 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -5.08 -1.651 360) (layer F.SilkS) hide)
    (fp_text value 10pF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D44)
    (at 66.421 43.688)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.794 -0.127) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C3221)
    (at 74.168 41.148 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -3.556 0.127 360) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 86.614 36.703 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D24)
    (at 65.151 40.894 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.54 -1.778 360) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F47)
    (at 96.012 38.481 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 1500 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2E8F)
    (at 81.28 46.482 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0.762 -1.651 180) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R23-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2EA1)
    (at 83.693 37.465 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 2.159 1.905 180) (layer F.SilkS))
    (fp_text value 470 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2E92)
    (at 85.09 48.514 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -1.778 1.524 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2E5B)
    (at 76.962 44.7675 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C25-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 74.168 51.689)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D57)
    (at 71.12 51.689 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 1.397 -2.286 360) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D6A)
    (at 70.739 47.371 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 470 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C22-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2B0D)
    (at 76.6445 61.4045 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -0.0635 -4.0005 360) (layer F.SilkS))
    (fp_text value 470 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C324B)
    (at 74.7395 61.4045 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 2.9845 -3.7465 360) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2837)
    (at 62.103 61.468 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 100 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2CA5)
    (at 67.183 52.451 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 6.223 10.541 360) (layer F.SilkS) hide)
    (fp_text value 4.7K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C28A6)
    (at 71.5645 61.4045 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.1905 15.5575 270) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C28AB)
    (at 68.6435 61.2775 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.5715 13.2715 360) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F3E)
    (at 91.821 36.195 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.524 -2.921 180) (layer F.SilkS))
    (fp_text value 4.7 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2F40)
    (at 91.821 37.719)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.397 -3.048) (layer F.SilkS))
    (fp_text value 200 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 88.392 36.576 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 4.7 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D1F)
    (at 66.929 40.894 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.413 -1.905 180) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D19)
    (at 61.976 42.164 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.032 -1.524 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C2D17)
    (at 61.976 40.386 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.127 1.524 180) (layer F.SilkS))
    (fp_text value 200 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B7C28AE)
    (at 65.5955 61.2775 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.9685 9.4615 360) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 5B7C28B4)
    (at 75.5015 58.2295 180)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D1 (at 0.4445 1.3335 180) (layer F.SilkS))
    (fp_text value LED_ALT (at 0 1.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 114.808 76.708)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C30 (at 0 1.75) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C3280)
    (at 101.346 84.836 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C31 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C30D9)
    (at 101.854 87.122 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C32 (at 2.159 -1.778 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C3170)
    (at 106.426 72.644 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C46 (at 2.794 0.762 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C2FE6)
    (at 112.268 84.328)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C47 (at 3.429 -1.143) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C2FEA)
    (at 112.776 86.868)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C48 (at 3.81 0.889) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 50 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C31C4)
    (at 99.314 51.308 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C49 (at -0.508 -1.524 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C49-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C3154)
    (at 98.552 72.898 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C52 (at 1.524 -3.937 180) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C52-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C3141)
    (at 96.774 81.28 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C54 (at -3.302 2.032 270) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 58 5V4_filtered))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B7C31E1)
    (at 103.632 58.928)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C51 (at 2.921 -0.127 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 51 +12V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B7C3192)
    (at 87.757 77.724 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C55 (at 0.127 1.524 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Reference Parts:PIC_HEADER" (layer F.Cu) (tedit 5B7C3199)
    (at 78.74 70.358 270)
    (fp_text reference U4 (at 2.667 -2.032 270) (layer F.SilkS))
    (fp_text value PIC_daughterboard (at 5.08 19.05 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 -6.35 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 42 +3V3))
    (pad 2 thru_hole circle (at -3.81 -3.81 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 71 "Net-(U4-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 -1.27 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 72 "Net-(U4-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 1.27 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 73 "Net-(U4-Pad4)"))
    (pad 5 thru_hole circle (at -3.81 3.81 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 74 "Net-(U4-Pad5)"))
    (pad 6 thru_hole circle (at -3.81 6.35 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 75 "Net-(U4-Pad6)"))
    (pad 7 thru_hole circle (at -3.81 8.89 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 "Net-(R15-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 11.43 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 "Net-(R9-Pad2)"))
    (pad 9 thru_hole circle (at -3.81 13.97 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 "Net-(R8-Pad2)"))
    (pad 10 thru_hole circle (at -3.81 16.51 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 "Net-(R7-Pad2)"))
    (pad 11 thru_hole circle (at 16.51 -6.35 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 12 thru_hole circle (at 16.51 -3.81 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 76 "Net-(U4-Pad12)"))
    (pad 13 thru_hole circle (at 16.51 -1.27 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 77 "Net-(U4-Pad13)"))
    (pad 14 thru_hole circle (at 16.51 1.27 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 78 "Net-(U4-Pad14)"))
    (pad 15 thru_hole circle (at 16.51 3.81 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 79 "Net-(U4-Pad15)"))
    (pad 16 thru_hole circle (at 16.51 6.35 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 80 "Net-(U4-Pad16)"))
    (pad 17 thru_hole circle (at 16.51 8.89 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 81 "Net-(U4-Pad17)"))
    (pad 18 thru_hole circle (at 16.51 11.43 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 82 "Net-(U4-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 13.97 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 83 "Net-(U4-Pad19)"))
    (pad 20 thru_hole circle (at 16.51 16.51 270) (size 2.04 2.04) (drill 1.02) (layers *.Cu *.Mask)
      (net 84 "Net-(U4-Pad20)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer B.Cu) (tedit 5B7C3130)
    (at 102.743 81.026 180)
    (fp_text reference U17 (at 2.032 4.445 180) (layer B.SilkS) hide)
    (fp_text value BLM15HG102SN1 (at 0 -2.54 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0.6985 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 5V4_filtered))
    (pad 2 smd rect (at -0.6985 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C31-Pad1)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer B.Cu) (tedit 5B7C3145)
    (at 102.87 79.375 180)
    (fp_text reference U18 (at 1.27 1.524 180) (layer B.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 -2.54 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0.6985 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 5V4_filtered))
    (pad 2 smd rect (at -0.6985 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C30-Pad1)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer B.Cu) (tedit 5B7C31D2)
    (at 103.759 52.832)
    (fp_text reference U22 (at 1.143 1.651) (layer B.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 -2.54) (layer B.Fab) hide)
    (pad 1 smd rect (at 0.6985 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 64 13V5_filtered))
    (pad 2 smd rect (at -0.6985 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C49-Pad1)"))
  )
  (module "Reference Parts:ADF4113HV" (layer F.Cu) (tedit 5B7C31FF)
    (at 65.659 47.244 180)
    (fp_text reference U7 (at 3.683 2.032 180) (layer F.SilkS))
    (fp_text value ADF4113HV (at 1.27 3.81 180) (layer F.Fab) hide)
    (pad 5 smd rect (at -1.904 1 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C18-Pad1)"))
    (pad 15 smd rect (at 1.904 -1 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C14-Pad1)"))
    (pad 14 smd rect (at 1.904 -0.5 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (pad 13 smd rect (at 1.904 0 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 12 smd rect (at 1.904 0.5 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C7-Pad1)"))
    (pad 11 smd rect (at 1.904 1 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C13-Pad1)"))
    (pad 8 smd rect (at 0 1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 10 smd rect (at 1 1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 9 smd rect (at 0.5 1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 7 smd rect (at -0.5 1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad1)"))
    (pad 6 smd rect (at -1 1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad1)"))
    (pad 3 smd rect (at -1.904 0 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 4 smd rect (at -1.904 0.5 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at -1.904 -0.5 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -1.904 -1 180) (size 0.854 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 20 smd rect (at -1 -1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C19-Pad1)"))
    (pad 19 smd rect (at -0.5 -1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R10-Pad1)"))
    (pad 18 smd rect (at 0 -1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 17 smd rect (at 0.5 -1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C16-Pad1)"))
    (pad 16 smd rect (at 1 -1.904 180) (size 0.25 0.854) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C16-Pad1)"))
    (pad 21 smd rect (at 0 0 180) (size 2.1 2.1) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:TPS7A19" (layer B.Cu) (tedit 5B7C31D8)
    (at 99.822 56.388 90)
    (fp_text reference U23 (at 0.508 3.81 180) (layer B.SilkS))
    (fp_text value TPS7A19 (at 0 -5.08 90) (layer B.Fab))
    (pad 9 smd rect (at 0 -0.63 90) (size 1.47 1.06) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 5 smd rect (at 1.4 -0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 6 smd rect (at 1.4 -0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C49-Pad1)"))
    (pad 8 smd rect (at 1.4 0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(U23-Pad8)"))
    (pad 4 smd rect (at -1.4 -0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.4 -0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R32-Pad2)"))
    (pad 1 smd rect (at -1.4 0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(U23-Pad1)"))
    (pad 7 smd rect (at 1.4 0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C49-Pad1)"))
    (pad 2 smd rect (at -1.4 0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 51 +12V))
    (pad 9 smd rect (at 0 0.63 90) (size 1.47 1.06) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:TPS7A19" (layer B.Cu) (tedit 5B7C3139)
    (at 97.536 77.724 90)
    (fp_text reference U30 (at 1.143 2.159 90) (layer B.SilkS))
    (fp_text value TPS7A19 (at 0 -5.08 90) (layer B.Fab))
    (pad 9 smd rect (at 0 -0.63 90) (size 1.47 1.06) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 5 smd rect (at 1.4 -0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 6 smd rect (at 1.4 -0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C52-Pad1)"))
    (pad 8 smd rect (at 1.4 0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U30-Pad8)"))
    (pad 4 smd rect (at -1.4 -0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.4 -0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(R34-Pad2)"))
    (pad 1 smd rect (at -1.4 0.975 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(U30-Pad1)"))
    (pad 7 smd rect (at 1.4 0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C52-Pad1)"))
    (pad 2 smd rect (at -1.4 0.325 90) (size 0.6 0.3) (layers B.Cu B.Paste B.Mask)
      (net 58 5V4_filtered))
    (pad 9 smd rect (at 0 0.63 90) (size 1.47 1.06) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5B7C2F99)
    (at 105.918 29.21 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C38 (at 3.81 -0.254 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5B7C2F97)
    (at 109.474 29.21 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C39 (at 2.032 2.286 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Reference Parts:T97F108K010LSA" (layer F.Cu) (tedit 5B7C2F93)
    (at 118.237 33.528)
    (fp_text reference U12 (at 0 -3.302) (layer F.SilkS))
    (fp_text value T97F108K010LSA (at 0 3.81) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.95 0) (size 2.3 4.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2.95 0) (size 2.3 4.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C3535)
    (at 50.8 93.98)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U24 (at 1.397 -3.937) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C351D)
    (at 132.08 22.86)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U25 (at -4.191 1.016) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C3524)
    (at 91.44 22.86)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U27 (at 0.381 3.683) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C353D)
    (at 132.08 93.98)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U28 (at -1.524 -3.683) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C3517)
    (at 132.08 55.88)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U31 (at -1.397 3.683 180) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C3539)
    (at 91.44 93.98)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U32 (at 0.254 -3.81) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C352F)
    (at 50.8 55.88)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U33 (at 1.524 -3.937) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:MountingHole" (layer F.Cu) (tedit 5B7C3529)
    (at 50.8 22.86)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference U34 (at 1.397 3.556) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.54) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C2DF6)
    (at 75.819 41.148 90)
    (fp_text reference U3 (at 2.54 0.381 180) (layer F.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at -0.7874 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C2E05)
    (at 74.295 45.212)
    (fp_text reference U5 (at -0.127 -7.239) (layer F.SilkS) hide)
    (fp_text value BLM15HG102SN1 (at 0 2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at -0.7874 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad1)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C31AF)
    (at 112.903 37.592 180)
    (fp_text reference U8 (at -5.207 -0.127 180) (layer F.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at -0.7874 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 +5V))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C2B42)
    (at 60.579 52.197 270)
    (fp_text reference U9 (at -0.127 1.524 270) (layer F.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at -0.7874 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C16-Pad1)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C2B2F)
    (at 62.484 52.07 90)
    (fp_text reference U10 (at 0 -3.937 90) (layer F.SilkS) hide)
    (fp_text value BLM15HG102SN1 (at 0 2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at -0.7874 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 +12V))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C2FC8)
    (at 122.428 62.23 180)
    (fp_text reference U11 (at -3.302 0 180) (layer F.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 +12V))
    (pad 2 smd rect (at -0.7874 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C2F4E)
    (at 85.852 44.577 270)
    (fp_text reference U13 (at -0.889 -1.651 270) (layer F.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at -0.7874 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C27-Pad2)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer F.Cu) (tedit 5B7C2FCA)
    (at 122.428 64.389 180)
    (fp_text reference U15 (at -1.905 -1.397 180) (layer F.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 +12V))
    (pad 2 smd rect (at -0.7874 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C26-Pad1)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer B.Cu) (tedit 5B7C30DD)
    (at 97.917 84.582 90)
    (fp_text reference U19 (at -1.27 -1.524 90) (layer B.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 -2.54 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 5V4_filtered))
    (pad 2 smd rect (at -0.7874 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C32-Pad1)"))
  )
  (module "Reference Parts:BLM15HG102SN1" (layer B.Cu) (tedit 5B7C3167)
    (at 100.584 72.517 90)
    (fp_text reference U29 (at 2.54 0.127 180) (layer B.SilkS))
    (fp_text value BLM15HG102SN1 (at 0 -2.54 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0.7874 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 51 +12V))
    (pad 2 smd rect (at -0.7874 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C52-Pad1)"))
  )
  (module "Reference Parts:OX-2050-BEE-20744" (layer F.Cu) (tedit 5B7C48D9)
    (at 103.378 54.991 180)
    (fp_text reference U16 (at -8.255 -11.684 180) (layer F.SilkS))
    (fp_text value OX-2050-BEE-20744-100M00000 (at 0 15.24 180) (layer F.Fab))
    (pad 5 thru_hole circle (at -9.525 9.525 180) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(C26-Pad1)"))
    (pad 4 thru_hole circle (at 9.525 9.525 180) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "Net-(R21-Pad2)"))
    (pad 3 thru_hole circle (at 9.525 -9.525 180) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 0 -9.525 180) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at -9.525 -9.525 180) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (gr_text "100 MHz Reference PCB\nREV 1" (at 69.215 76.327) (layer B.SilkS))
  (gr_line (start 134.62 96.52) (end 134.62 20.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 96.52) (end 134.62 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 20.32) (end 48.26 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 20.32) (end 48.26 20.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 96.52) (xy 48.26 96.52) (xy 48.26 20.32) (xy 134.62 20.32)
      )
    )
    (polygon
      (pts        (xy 50.8 22.86) (xy 50.8 93.98) (xy 132.08 93.98) (xy 132.08 22.86)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.618 70.231) (xy 88.138 70.231) (xy 88.138 39.751) (xy 118.618 39.751)
      )
    )
    (polygon
      (pts        (xy 116.078 67.691) (xy 116.078 42.291) (xy 90.678 42.291) (xy 90.678 67.691)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 96.52) (xy 48.26 96.52) (xy 48.26 20.32) (xy 134.62 20.32)
      )
    )
    (polygon
      (pts        (xy 50.8 22.86) (xy 50.8 93.98) (xy 132.08 93.98) (xy 132.08 22.86)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.414 102.108) (xy 44.958 102.108) (xy 44.958 19.304) (xy 137.414 19.304)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.192 103.632) (xy 43.434 103.632) (xy 43.434 17.272) (xy 139.192 17.272)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.386 16.256) (xy 143.764 16.256) (xy 143.764 107.696) (xy 39.116 107.696) (xy 39.116 15.748)
        (xy 40.386 15.748)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.162 106.426) (xy 35.56 106.426) (xy 35.56 16.002) (xy 153.162 16.002)
      )
    )
  )
)
