<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="13.95" y2="0" width="0" layer="20"/>
<wire x1="13.95" y1="0" x2="13.95" y2="30.15" width="0" layer="20"/>
<wire x1="13.95" y1="30.15" x2="0" y2="30.15" width="0" layer="20"/>
<wire x1="0" y1="30.15" x2="0" y2="0" width="0" layer="20"/>
<text>SerialLinkV2</text>
<text>By TinLethax</text>
<text>Designed in Thailand</text>
</plain>
<libraries>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD80C">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="connect">
<packages>
<package name="D-09F/90">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="PJ-242">
<packages>
<package name="PJ-242">
<description>PJ-262</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diode" package="SOD80C" value="Zener 4.7v">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
</element>
<element name="D2" library="diode" package="SOD80C" value="Zener 4.7v">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
</element>
<element name="DB9FEMALE" library="connect" package="D-09F/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="REDLED1" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="PJ-242" package="PJ-242" value="PJ-242">
<attribute name="PARTNO" value="PJ-242 2.5mm headphone jack socket 6 pin"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="A"/>
<contactref element="R3" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="REDLED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="DB9FEMALE" pad="6"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="C"/>
<contactref element="R2" pad="1"/>
<contactref element="DB9FEMALE" pad="8"/>
<contactref element="U$2" pad="P$5"/>
</signal>
<signal name="N$4">
<contactref element="DB9FEMALE" pad="5"/>
<contactref element="REDLED1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="DB9FEMALE" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="2"/>
<contactref element="DB9FEMALE" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="DB9FEMALE" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
