(kicad_pcb (version 20171130) (host pcbnew "(5.1.8-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 597)
    (zones 0)
    (modules 71)
    (nets 100)
  )
  (page USLedger)
  (title_block
    (date 2019-12-29)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1778)
    (zone_clearance 0.4064)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.6604)
    (via_drill 0.4064)
    (via_min_size 0.4064)
    (via_min_drill 0.3556)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.07)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0254)
    (solder_mask_min_width 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FEFDBF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 ~RESET~)
  (net 4 +3.3VP)
  (net 5 GNDA)
  (net 6 "Net-(CN22-Pad2)")
  (net 7 "Net-(CNQ1-Pad1)")
  (net 8 "Net-(CNQ2-Pad1)")
  (net 9 "Net-(CNRD1-Pad1)")
  (net 10 GNDPWR)
  (net 11 "Net-(CNRX+1-Pad1)")
  (net 12 "Net-(CNRX+1-Pad2)")
  (net 13 "Net-(CNRX-1-Pad1)")
  (net 14 "Net-(CNRX-1-Pad2)")
  (net 15 "Net-(CNTCT1-Pad2)")
  (net 16 "Net-(RN1-Pad1)")
  (net 17 "Net-(RN2-Pad1)")
  (net 18 "Net-(RN3-Pad1)")
  (net 19 "Net-(RN4-Pad1)")
  (net 20 "Net-(RN5-Pad1)")
  (net 21 "Net-(RNEXR1-Pad2)")
  (net 22 "Net-(RNLACT1-Pad2)")
  (net 23 "Net-(RNLDUP1-Pad2)")
  (net 24 "Net-(RNLNK1-Pad2)")
  (net 25 "Net-(RNLSPEED1-Pad2)")
  (net 26 "Net-(RNSPD1-Pad1)")
  (net 27 "Net-(RNDMPR-1-Pad2)")
  (net 28 "Net-(RNDMPT-1-Pad2)")
  (net 29 "Net-(RNAUTO1-Pad1)")
  (net 30 "Net-(RNDUP1-Pad1)")
  (net 31 "Net-(RNINT1-Pad1)")
  (net 32 "Net-(J_RJ45-Pad14)")
  (net 33 "Net-(J_RJ45-Pad5)")
  (net 34 "Net-(J_RJ45-Pad6)")
  (net 35 "Net-(J_RJ45-Pad12)")
  (net 36 "Net-(U_W5500-Pad47)")
  (net 37 "Net-(U_W5500-Pad46)")
  (net 38 "Net-(U_W5500-Pad18)")
  (net 39 "Net-(U_W5500-Pad13)")
  (net 40 "Net-(U_W5500-Pad12)")
  (net 41 "Net-(U_W5500-Pad7)")
  (net 42 "Net-(CN20-Pad2)")
  (net 43 "Net-(RN6-Pad2)")
  (net 44 "Net-(RNDMPR+1-Pad2)")
  (net 45 "Net-(RNDMPT+1-Pad2)")
  (net 46 "Net-(L_NDUP1-Pad1)")
  (net 47 "Net-(L_NSPD1-Pad1)")
  (net 48 /NETRST)
  (net 49 /NET-MISO)
  (net 50 "Net-(SP_HARDRESET_1-Pad2)")
  (net 51 "Net-(SP_SOFTRESET_1-Pad2)")
  (net 52 MOSI)
  (net 53 NETINT)
  (net 54 MISO)
  (net 55 SCK)
  (net 56 NETRES)
  (net 57 NETCS)
  (net 58 "Net-(JL1-Pad2)")
  (net 59 "Net-(JL1-Pad3)")
  (net 60 "Net-(JL1-Pad5)")
  (net 61 "Net-(JL1-Pad6)")
  (net 62 "Net-(JL1-Pad8)")
  (net 63 "Net-(JL1-Pad9)")
  (net 64 "Net-(JL1-Pad10)")
  (net 65 "Net-(JL1-Pad11)")
  (net 66 "Net-(JL1-Pad12)")
  (net 67 "Net-(JL1-Pad13)")
  (net 68 "Net-(JL1-Pad14)")
  (net 69 "Net-(JL1-Pad15)")
  (net 70 "Net-(JL1-Pad16)")
  (net 71 "Net-(JL1-Pad17)")
  (net 72 "Net-(JL1-Pad18)")
  (net 73 "Net-(JL1-Pad19)")
  (net 74 "Net-(JL1-Pad20)")
  (net 75 "Net-(JL1-Pad21)")
  (net 76 "Net-(JL1-Pad22)")
  (net 77 "Net-(JR1-Pad24)")
  (net 78 "Net-(JR1-Pad19)")
  (net 79 "Net-(JR1-Pad18)")
  (net 80 "Net-(JR1-Pad17)")
  (net 81 "Net-(JR1-Pad16)")
  (net 82 "Net-(JR1-Pad15)")
  (net 83 "Net-(JR1-Pad14)")
  (net 84 "Net-(JR1-Pad13)")
  (net 85 "Net-(JR1-Pad12)")
  (net 86 "Net-(JR1-Pad11)")
  (net 87 "Net-(JR1-Pad10)")
  (net 88 "Net-(JR1-Pad9)")
  (net 89 "Net-(JR1-Pad8)")
  (net 90 "Net-(JR1-Pad7)")
  (net 91 "Net-(JR1-Pad6)")
  (net 92 "Net-(JR1-Pad5)")
  (net 93 "Net-(JR1-Pad4)")
  (net 94 "Net-(JR1-Pad3)")
  (net 95 "Net-(JL1-Pad7)")
  (net 96 "Net-(JL1-Pad23)")
  (net 97 "Net-(J_POE++1-Pad1)")
  (net 98 "Net-(J_POE--1-Pad1)")
  (net 99 "Net-(JL1-Pad24)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.2032)
    (via_dia 0.6604)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.25)
    (add_net +3.3VP)
    (add_net +3V3)
    (add_net /NET-MISO)
    (add_net /NETRST)
    (add_net GND)
    (add_net GNDA)
    (add_net GNDPWR)
    (add_net MISO)
    (add_net MOSI)
    (add_net NETCS)
    (add_net NETINT)
    (add_net NETRES)
    (add_net "Net-(CN20-Pad2)")
    (add_net "Net-(CN22-Pad2)")
    (add_net "Net-(CNQ1-Pad1)")
    (add_net "Net-(CNQ2-Pad1)")
    (add_net "Net-(CNRD1-Pad1)")
    (add_net "Net-(CNRX+1-Pad1)")
    (add_net "Net-(CNRX+1-Pad2)")
    (add_net "Net-(CNRX-1-Pad1)")
    (add_net "Net-(CNRX-1-Pad2)")
    (add_net "Net-(CNTCT1-Pad2)")
    (add_net "Net-(JL1-Pad10)")
    (add_net "Net-(JL1-Pad11)")
    (add_net "Net-(JL1-Pad12)")
    (add_net "Net-(JL1-Pad13)")
    (add_net "Net-(JL1-Pad14)")
    (add_net "Net-(JL1-Pad15)")
    (add_net "Net-(JL1-Pad16)")
    (add_net "Net-(JL1-Pad17)")
    (add_net "Net-(JL1-Pad18)")
    (add_net "Net-(JL1-Pad19)")
    (add_net "Net-(JL1-Pad2)")
    (add_net "Net-(JL1-Pad20)")
    (add_net "Net-(JL1-Pad21)")
    (add_net "Net-(JL1-Pad22)")
    (add_net "Net-(JL1-Pad23)")
    (add_net "Net-(JL1-Pad24)")
    (add_net "Net-(JL1-Pad3)")
    (add_net "Net-(JL1-Pad5)")
    (add_net "Net-(JL1-Pad6)")
    (add_net "Net-(JL1-Pad7)")
    (add_net "Net-(JL1-Pad8)")
    (add_net "Net-(JL1-Pad9)")
    (add_net "Net-(JR1-Pad10)")
    (add_net "Net-(JR1-Pad11)")
    (add_net "Net-(JR1-Pad12)")
    (add_net "Net-(JR1-Pad13)")
    (add_net "Net-(JR1-Pad14)")
    (add_net "Net-(JR1-Pad15)")
    (add_net "Net-(JR1-Pad16)")
    (add_net "Net-(JR1-Pad17)")
    (add_net "Net-(JR1-Pad18)")
    (add_net "Net-(JR1-Pad19)")
    (add_net "Net-(JR1-Pad24)")
    (add_net "Net-(JR1-Pad3)")
    (add_net "Net-(JR1-Pad4)")
    (add_net "Net-(JR1-Pad5)")
    (add_net "Net-(JR1-Pad6)")
    (add_net "Net-(JR1-Pad7)")
    (add_net "Net-(JR1-Pad8)")
    (add_net "Net-(JR1-Pad9)")
    (add_net "Net-(J_POE++1-Pad1)")
    (add_net "Net-(J_POE--1-Pad1)")
    (add_net "Net-(J_RJ45-Pad12)")
    (add_net "Net-(J_RJ45-Pad14)")
    (add_net "Net-(J_RJ45-Pad5)")
    (add_net "Net-(J_RJ45-Pad6)")
    (add_net "Net-(L_NDUP1-Pad1)")
    (add_net "Net-(L_NSPD1-Pad1)")
    (add_net "Net-(RN1-Pad1)")
    (add_net "Net-(RN2-Pad1)")
    (add_net "Net-(RN3-Pad1)")
    (add_net "Net-(RN4-Pad1)")
    (add_net "Net-(RN5-Pad1)")
    (add_net "Net-(RN6-Pad2)")
    (add_net "Net-(RNAUTO1-Pad1)")
    (add_net "Net-(RNDMPR+1-Pad2)")
    (add_net "Net-(RNDMPR-1-Pad2)")
    (add_net "Net-(RNDMPT+1-Pad2)")
    (add_net "Net-(RNDMPT-1-Pad2)")
    (add_net "Net-(RNDUP1-Pad1)")
    (add_net "Net-(RNEXR1-Pad2)")
    (add_net "Net-(RNINT1-Pad1)")
    (add_net "Net-(RNLACT1-Pad2)")
    (add_net "Net-(RNLDUP1-Pad2)")
    (add_net "Net-(RNLNK1-Pad2)")
    (add_net "Net-(RNLSPEED1-Pad2)")
    (add_net "Net-(RNSPD1-Pad1)")
    (add_net "Net-(SP_HARDRESET_1-Pad2)")
    (add_net "Net-(SP_SOFTRESET_1-Pad2)")
    (add_net "Net-(U_W5500-Pad12)")
    (add_net "Net-(U_W5500-Pad13)")
    (add_net "Net-(U_W5500-Pad18)")
    (add_net "Net-(U_W5500-Pad46)")
    (add_net "Net-(U_W5500-Pad47)")
    (add_net "Net-(U_W5500-Pad7)")
    (add_net SCK)
    (add_net ~RESET~)
  )
  (module Package_TO_SOT_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FA7A3ED)
    (at 68.29298 23.18258 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U_2G7RES1 (at -0.2921 -2.43078 90) (layer F.SilkS))
    (fp_text value SN74LVC2G07DBVR (at 0.0254 2.2098 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.3302 2.9972 270) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 6 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(SP_HARDRESET_1-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(SP_SOFTRESET_1-Pad2)"))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 56 NETRES))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 ~RESET~))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 600E2DC4)
    (at 73.66 29.21 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J_GND1 (at -0.0254 -2.2098) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 2.0574 1.0414 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 600E2DC4)
    (at 73.66 8.89)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J_3V1 (at -0.0254 -2.2098) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 2.0574 1.0414 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 600E2DC4)
    (at 22.86 7.62 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J_POE++1 (at 2.35966 1.10744) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.79832 0.97028) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(J_POE++1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(J_POE++1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 600E2DC4)
    (at 22.86 30.48 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J_POE--1 (at -2.40538 1.24968) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.79832 0.97028) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(J_POE--1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(J_POE--1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MiniNetCard:RJ45_Wuerth_7499211121A_Horizontal (layer F.Cu) (tedit 5FA5E31A)
    (at 5.842 18.3896 90)
    (descr "10/100Base-TX RJ45 ethernet magnetic transformer connector horizontal https://katalog.we-online.de/pbs/datasheet/7499010121A.pdf")
    (tags "RJ45 ethernet magnetic")
    (fp_text reference J_RJ45 (at -0.6223 12.43838 270) (layer F.SilkS))
    (fp_text value Wuerth_7499211121A (at 9.8 4.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.05 0.05 180) (layer F.Fab) hide)
    (pad 14 thru_hole circle (at -6.661 -4.08 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 "Net-(J_RJ45-Pad14)"))
    (pad 13 thru_hole circle (at -4.09 -4.08 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole roundrect (at 5.715 8.89 270) (size 1.2 1.6) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.155)
      (net 12 "Net-(CNRX+1-Pad2)"))
    (pad 2 thru_hole circle (at 4.445 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(CNRX-1-Pad1)"))
    (pad 3 thru_hole circle (at 3.175 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(CNRD1-Pad1)"))
    (pad 4 thru_hole circle (at 1.905 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(CNTCT1-Pad2)"))
    (pad 5 thru_hole circle (at 0.635 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(J_RJ45-Pad5)"))
    (pad 6 thru_hole circle (at -0.635 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 "Net-(J_RJ45-Pad6)"))
    (pad 7 thru_hole circle (at -1.905 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.175 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0 270) (size 3.250001 3.250001) (drill 3.250001) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.715 0 270) (size 3.250001 3.250001) (drill 3.250001) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -7.745 3.05 270) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad 16 thru_hole circle (at 7.745 3.05 270) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad 10 thru_hole circle (at -5.715 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 "Net-(J_POE--1-Pad1)"))
    (pad 11 thru_hole circle (at 6.661 -4.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 9 thru_hole circle (at -4.445 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 97 "Net-(J_POE++1-Pad1)"))
    (pad 12 thru_hole circle (at 4.09 -4.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(J_RJ45-Pad12)"))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Wuerth_7499010121A_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 39.2684 8.48868 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDUP1 (at 0.13716 -1.524 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 30 "Net-(RNDUP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 42.08018 8.46836 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNSPD1 (at 0.07874 -1.40716 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 26 "Net-(RNSPD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 44.90974 8.4328 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNAUTO1 (at 0.27686 -1.40462 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 29 "Net-(RNAUTO1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 47.50308 8.28548 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN1 (at 3.09626 0.07112 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 16 "Net-(RN1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 49.60874 8.28548 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN2 (at 3.0734 -0.0508 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 17 "Net-(RN2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 51.66868 8.26008 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN3 (at 2.99974 0.01016 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 18 "Net-(RN3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 53.74894 8.26008 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN4 (at 2.99974 0.03048 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 19 "Net-(RN4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 55.82158 8.2423 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN5 (at 2.93624 -0.0127 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 20 "Net-(RN5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 59.27852 8.1534 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRESET1 (at 0.29972 -1.56972 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 48 /NETRST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 61.4934 8.13816 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNINT1 (at -0.01524 1.57734 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 31 "Net-(RNINT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 69.4309 19.56562)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNOR1 (at -0.15748 -1.45288) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 59.52744 13.27912)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNQ2 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 8 "Net-(CNQ2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 71.3359 23.03526 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRES1 (at 0.0635 1.53924 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 56 NETRES))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 62.93612 17.399 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNQ1 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value 1Meg (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 "Net-(CNQ1-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 8 "Net-(CNQ2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 59.64936 22.3266 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNQ1 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 7 "Net-(CNQ1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 68.8467 8.3947)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNMISO1 (at -0.02794 -1.47066) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 68.58508 15.59052)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNCS1 (at -0.05334 1.51384) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 57 NETCS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 62.89548 26.4668)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C28B1 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 55.64378 27.81554 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN6 (at -2.86004 0.27178 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 43 "Net-(RN6-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 53.59146 27.82824 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN22 (at -3.2004 0.14732 90) (layer F.SilkS))
    (fp_text value 22nf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 6 "Net-(CN22-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 51.5747 27.84094 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN21 (at -3.17754 0.02032 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 49.56048 27.83332 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN20 (at -3.26136 0.02794 90) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 42 "Net-(CN20-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 47.42434 27.85364 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN17 (at -3.29184 0.05588 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 45.30598 27.83332 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN15 (at -3.0988 -0.08382 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 42.69486 27.86126 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNEXR1 (at 0.03556 -1.49606 90) (layer F.SilkS))
    (fp_text value "12.4K 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 21 "Net-(RNEXR1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 42.38752 23.4696)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN11 (at -0.11176 1.48336) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 41.62298 21.29282)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN8 (at -0.08636 -1.32334) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 42.0751 16.94434)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN4 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 38.66388 12.47902)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPT-1 (at -4.572 0.0254) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 28 "Net-(RNDMPT-1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 34 "Net-(J_RJ45-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 38.62578 14.51356)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPT+1 (at -4.51104 -0.08128) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 45 "Net-(RNDMPT+1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 33 "Net-(J_RJ45-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 36.92398 17.74444)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPR-1 (at 0.09398 -1.37414) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 27 "Net-(RNDMPR-1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 14 "Net-(CNRX-1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 36.92398 19.86026)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPR+1 (at -0.04826 1.45542) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 44 "Net-(RNDMPR+1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 11 "Net-(CNRX+1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5FA84C73)
    (at 38.59022 27.06624 270)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference CNW6 (at 0.04826 1.46558 90) (layer F.SilkS))
    (fp_text value "10uf TANT" (at -0.0254 1.4732 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 2.4384 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4375 0 270) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 5 GNDA))
    (pad 1 smd roundrect (at -1.4375 0 270) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 4 +3.3VP))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 34.19348 25.25268 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F_NBV1 (at 0.26416 -1.38938) (layer F.SilkS))
    (fp_text value "120 ohm Ferrite" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 +3.3VP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 33.45434 28.40228 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F_NBG1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value "42 ohm Ferrite" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 32.69234 17.78508 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRDN1 (at 0.1778 -1.51892 90) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 9 "Net-(CNRD1-Pad1)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 14 "Net-(CNRX-1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 32.56788 21.71446 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRDP1 (at -0.26162 -1.47066 90) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 11 "Net-(CNRX+1-Pad1)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 9 "Net-(CNRD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 29.04744 12.19962 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNTXN1 (at 0.12954 -1.48082 90) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 34 "Net-(J_RJ45-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 29.0957 16.10868 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNTXP1 (at -0.3556 -1.50368 90) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 33 "Net-(J_RJ45-Pad5)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 14.87932 31.10484)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLNK1 (at 0.06604 1.48844) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 24 "Net-(RNLNK1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 32 "Net-(J_RJ45-Pad14)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 14.44752 28.94076)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLACT1 (at 0.09398 -1.43002) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 22 "Net-(RNLACT1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 35 "Net-(J_RJ45-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder (layer F.Cu) (tedit 5FA84D0A)
    (at 20.72894 12.54252)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRJ1 (at 3.97256 -0.07112 90) (layer F.SilkS))
    (fp_text value "1nf 2KV" (at 0 1.85) (layer F.Fab) hide)
    (fp_text user %R (at 0.0254 2.921) (layer F.Fab))
    (pad 2 smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 10 GNDPWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 25.15616 19.55038)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRX-1 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value "6.8nf 100V" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 14 "Net-(CNRX-1-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 13 "Net-(CNRX-1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 25.14346 21.63064 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRX+1 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value "6.8nf 100V" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 12 "Net-(CNRX+1-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 11 "Net-(CNRX+1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 27.68854 25.31618 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRD1 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value "10nf 100V" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 9 "Net-(CNRD1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5FA7A380)
    (at 25.23236 26.2636 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNTCT1 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value "22nf 100V" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 15 "Net-(CNTCT1-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 21.49602 25.46858 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNTCT1 (at 0.36068 -1.40716 90) (layer F.SilkS))
    (fp_text value "10 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 15 "Net-(CNTCT1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 8.7503 29.87294)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLSPEED1 (at 0.85344 -1.4732) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 25 "Net-(RNLSPEED1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 47 "Net-(L_NSPD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A271)
    (at 8.84174 32.131)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLDUP1 (at 0.25654 1.54178) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 23 "Net-(RNLDUP1-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 46 "Net-(L_NDUP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_EuroQuartz_MJ-4Pin_5.0x3.2mm (layer F.Cu) (tedit 5FA84CAD)
    (at 59.63666 17.69618 90)
    (descr "SMD Crystal EuroQuartz MJ series http://cdn-reichelt.de/documents/datenblatt/B400/MJ.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference QN1 (at 0.4699 -2.65684 90) (layer F.SilkS))
    (fp_text value "25.00 MHz 18pf" (at 0 2.8 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.1016 3.9116 90) (layer F.Fab) hide)
    (pad 4 smd rect (at -1.85 -1.15 90) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.85 -1.15 90) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CNQ2-Pad1)"))
    (pad 2 smd rect (at 1.85 1.15 90) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.85 1.15 90) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CNQ1-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_EuroQuartz_MJ-4Pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A02C)
    (at 3.9624 32.36722 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference L_NDUP1 (at -0.18288 -1.59766) (layer F.SilkS))
    (fp_text value Red (at 0.3302 1.5494) (layer F.Fab) hide)
    (fp_text user %R (at 0.0254 2.2098) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 46 "Net-(L_NDUP1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5FA7A02C)
    (at 4.01574 29.6164 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference L_NSPD1 (at -0.31242 1.57988) (layer F.SilkS))
    (fp_text value Green (at 0.3302 1.5494) (layer F.Fab) hide)
    (fp_text user %R (at 0.0254 2.2098) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 47 "Net-(L_NSPD1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-48_7x7mm_P0.5mm (layer F.Cu) (tedit 5FA7B566)
    (at 50.42154 18.53438)
    (descr "48 LEAD TQFP 7x7mm (see MICREL TQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U_W5500 (at 0.0254 -5.715) (layer F.SilkS))
    (fp_text value W5500 (at 0 6) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 48 smd rect (at -2.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 47 smd rect (at -2.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U_W5500-Pad47)"))
    (pad 46 smd rect (at -1.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U_W5500-Pad46)"))
    (pad 45 smd rect (at -1.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(RNDUP1-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(RNSPD1-Pad1)"))
    (pad 43 smd rect (at -0.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(RNAUTO1-Pad1)"))
    (pad 42 smd rect (at 0.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(RN1-Pad1)"))
    (pad 41 smd rect (at 0.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(RN2-Pad1)"))
    (pad 40 smd rect (at 1.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(RN3-Pad1)"))
    (pad 39 smd rect (at 1.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(RN4-Pad1)"))
    (pad 38 smd rect (at 2.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(RN5-Pad1)"))
    (pad 37 smd rect (at 2.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /NETRST))
    (pad 36 smd rect (at 4.35 -2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(RNINT1-Pad1)"))
    (pad 35 smd rect (at 4.35 -2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 MOSI))
    (pad 34 smd rect (at 4.35 -1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 /NET-MISO))
    (pad 33 smd rect (at 4.35 -1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 SCK))
    (pad 32 smd rect (at 4.35 -0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 NETCS))
    (pad 31 smd rect (at 4.35 -0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CNQ2-Pad1)"))
    (pad 30 smd rect (at 4.35 0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CNQ1-Pad1)"))
    (pad 29 smd rect (at 4.35 0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 4.35 1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 27 smd rect (at 4.35 1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(RNLACT1-Pad2)"))
    (pad 26 smd rect (at 4.35 2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(RNLDUP1-Pad2)"))
    (pad 25 smd rect (at 4.35 2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(RNLNK1-Pad2)"))
    (pad 24 smd rect (at 2.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(RNLSPEED1-Pad2)"))
    (pad 23 smd rect (at 2.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(RN6-Pad2)"))
    (pad 22 smd rect (at 1.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CN22-Pad2)"))
    (pad 21 smd rect (at 1.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 20 smd rect (at 0.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(CN20-Pad2)"))
    (pad 19 smd rect (at 0.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 18 smd rect (at -0.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U_W5500-Pad18)"))
    (pad 17 smd rect (at -0.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 16 smd rect (at -1.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 15 smd rect (at -1.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 14 smd rect (at -2.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 13 smd rect (at -2.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U_W5500-Pad13)"))
    (pad 12 smd rect (at -4.35 2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U_W5500-Pad12)"))
    (pad 11 smd rect (at -4.35 2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 10 smd rect (at -4.35 1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(RNEXR1-Pad2)"))
    (pad 9 smd rect (at -4.35 1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 8 smd rect (at -4.35 0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 7 smd rect (at -4.35 0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U_W5500-Pad7)"))
    (pad 6 smd rect (at -4.35 -0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(RNDMPR+1-Pad2)"))
    (pad 5 smd rect (at -4.35 -0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(RNDMPR-1-Pad2)"))
    (pad 4 smd rect (at -4.35 -1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 3 smd rect (at -4.35 -1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 2 smd rect (at -4.35 -2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(RNDMPT+1-Pad2)"))
    (pad 1 smd rect (at -4.35 -2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(RNDMPT-1-Pad2)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 44.51096 6.98246 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_AUTO1 (at -4.31522 0.1016 90) (layer B.SilkS))
    (fp_text value S_AUTO (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 29 "Net-(RNAUTO1-Pad1)"))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 37.60216 6.99008 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_DUPLEX1 (at -5.12318 0.02794 90) (layer B.SilkS))
    (fp_text value S_DUPLEX (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 30 "Net-(RNDUP1-Pad1)"))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 41.18864 7.00786 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_SPEED1 (at -4.826 0.05334 90) (layer B.SilkS))
    (fp_text value S_SPEED (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 26 "Net-(RNSPD1-Pad1)"))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5FA84C73)
    (at 62.29858 28.66136)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C28A1 (at -0.45974 1.6256) (layer F.SilkS))
    (fp_text value "10uf TANT" (at -0.0254 1.4732) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 2.4384) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4375 0) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4375 0) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 49.80178 10.9601 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_NETINT1 (at 0 1.8 90) (layer B.SilkS))
    (fp_text value S_NETINT (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 31 "Net-(RNINT1-Pad1)"))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 53 NETINT))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 66.52768 20.13966 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_HARDRESET_1 (at 0.41148 -1.75514 270) (layer B.SilkS))
    (fp_text value S_HARDRESET (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 48 /NETRST))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 50 "Net-(SP_HARDRESET_1-Pad2)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A88B)
    (at 71.57466 20.1168 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_SOFTRESET_1 (at 0.43434 1.61036 270) (layer B.SilkS))
    (fp_text value S_SOFTRESET (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 48 /NETRST))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 51 "Net-(SP_SOFTRESET_1-Pad2)"))
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5FA7A44B)
    (at 68.69938 12.04468 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U_74G1NCS1 (at -0.1397 -2.35204 90) (layer F.SilkS))
    (fp_text value SN74LVC1G125DBVR (at 0.0254 2.3622 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 54 MISO))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 49 /NET-MISO))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 57 NETCS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 12.7 35.56 270)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference JL1 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x24 (at 0 -60.75 270) (layer B.Fab))
    (fp_text user %R (at 0 -29.21) (layer B.Fab))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(JL1-Pad24)"))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(JL1-Pad23)"))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(JL1-Pad22)"))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(JL1-Pad21)"))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JL1-Pad20)"))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JL1-Pad19)"))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JL1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JL1-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JL1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JL1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JL1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JL1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JL1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JL1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JL1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JL1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JL1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(JL1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JL1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JL1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 ~RESET~))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JL1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JL1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 12.7 2.54 270)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference JR1 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x24 (at 0 -60.75 270) (layer B.Fab))
    (fp_text user %R (at 0 -29.21) (layer B.Fab))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(JR1-Pad24)"))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 MOSI))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 SCK))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 MISO))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 NETINT))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(JR1-Pad19)"))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(JR1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(JR1-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(JR1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(JR1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(JR1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(JR1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(JR1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(JR1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(JR1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(JR1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(JR1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(JR1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(JR1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(JR1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(JR1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(JR1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A8C6)
    (at 61.73978 32.00146)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_MCS1 (at 0.0508 1.6256) (layer B.SilkS))
    (fp_text value SolderJumper_3_Open (at 0 -1.5748) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 65 "Net-(JL1-Pad11)"))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 57 NETCS))
    (pad 3 smd rect (at 1.3 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 83 "Net-(JR1-Pad14)"))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5FA7A8C6)
    (at 69.59092 32.07766)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_NRST1 (at 0.0508 1.6256) (layer B.SilkS))
    (fp_text value SolderJumper_3_Open (at 0 -1.5748) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 96 "Net-(JL1-Pad23)"))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 56 NETRES))
    (pad 3 smd rect (at 1.3 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 99 "Net-(JL1-Pad24)"))
  )
  (gr_text "RJ45 has PoE\ndiodes builtin" (at 16.02994 8.36676) (layer F.SilkS))
  (gr_text R20 (at 61.0743 4.40944) (layer F.SilkS))
  (gr_text "CPU21  CS  R14  D10\nCPU21  NRST L23 D8\n\nCPU51  CS  L11   D10\nCPU51  NRST L24  D5" (at 62.88786 26.40584) (layer B.SilkS))
  (gr_text L11 (at 38.27526 33.58896) (layer F.SilkS))
  (gr_text L24 (at 71.12508 33.5153) (layer F.SilkS))
  (gr_text CS (at 38.08984 37.45738) (layer F.SilkS))
  (gr_text NRES (at 71.72452 37.41674) (layer F.SilkS))
  (gr_text L11 (at 58.55208 32.4231) (layer B.SilkS))
  (gr_text L24 (at 72.81418 31.61792) (layer B.SilkS))
  (gr_text "3.3Volts ONLY" (at 74.74966 18.96364 90) (layer F.SilkS))
  (gr_text R14 (at 64.95542 32.4231) (layer B.SilkS))
  (gr_text L23 (at 66.4718 31.47822) (layer B.SilkS))
  (gr_text R14 (at 45.73778 4.47548) (layer F.SilkS))
  (gr_text L23 (at 68.40728 33.58896) (layer F.SilkS))
  (gr_text 3V (at 15.20698 0.62738) (layer F.SilkS))
  (gr_text GND (at 12.80922 0.65278) (layer F.SilkS))
  (gr_text GND (at 12.77366 37.56406) (layer F.SilkS))
  (gr_text ~RESET (at 20.39112 37.592) (layer F.SilkS))
  (gr_text NRES (at 68.5292 37.41674) (layer F.SilkS))
  (gr_text CS (at 45.73016 0.62992) (layer F.SilkS))
  (gr_text MOSI (at 68.76288 0.60198) (layer F.SilkS))
  (gr_text SCK (at 66.0781 0.60198) (layer F.SilkS))
  (gr_text MISO (at 63.3603 0.61722) (layer F.SilkS))
  (gr_text INT (at 60.77204 0.61722) (layer F.SilkS))
  (gr_text "W5500\nReset\nOptions" (at 69.03974 13.55598) (layer B.SilkS))
  (gr_text "Copyright S. Cooper 2021.\nYou may redistribute and modify this documentation under the terms of the CERN OHL v.1.2.\nThis documentation is distributed WITHOUT ANY EXPRESS OR IMPLIED WARRANTY, \nINCLUDING OF MERCHANTABILITY, SATISFACTORY QUALITY AND FITNESS FOR A PARTICULAR PURPOSE.\nPlease see the CERN OHL v.1.2 for applicable conditions. (http://ohwr.org/cernohl)." (at 34.6202 19.13128) (layer B.SilkS))
  (gr_line (start 0 38.1) (end 0 0) (layer Edge.Cuts) (width 0.05))
  (gr_text "MiniNetCard\nVersion 4b\n26 Feb 2021" (at 5.56514 5.51942) (layer F.SilkS))
  (gr_line (start 76.2 0) (end 76.2 38.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 0) (end 76.2 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.2 38.1) (end 0 38.1) (layer Edge.Cuts) (width 0.05))
  (gr_text "MiniNetCard\nVersion 4b\n26 Feb 2021" (at 35.51682 26.75636) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.454 38.354) (xy -0.254 38.354) (xy -0.254 -0.254) (xy 76.454 -0.254)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.454 38.354) (xy -0.254 38.354) (xy -0.254 -0.254) (xy 76.454 -0.254)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.256 26.67) (xy 10.922 26.67) (xy 10.922 21.844) (xy 16.256 21.844)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.432 32.512) (xy 20.828 32.512) (xy 20.828 28.448) (xy 27.432 28.448)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.388053 9.652) (xy 20.784053 9.652) (xy 20.784053 5.588) (xy 27.388053 5.588)
      )
    )
  )
)
