(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 97)
    (no_connects 0)
    (area 40.564999 116.129999 68.655001 143.585001)
    (thickness 1.6)
    (drawings 28)
    (tracks 564)
    (zones 0)
    (modules 32)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.325)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 2.2)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory grb-r2/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VIN)
  (net 3 +3V3)
  (net 4 "Net-(CON101-Pad1)")
  (net 5 "Net-(CON101-Pad3)")
  (net 6 "Net-(CON101-Pad4)")
  (net 7 "Net-(CON101-Pad5)")
  (net 8 "Net-(IC101-Pad21)")
  (net 9 "Net-(IC101-Pad22)")
  (net 10 "Net-(IC101-Pad23)")
  (net 11 "Net-(IC101-Pad24)")
  (net 12 /RLY_DRV)
  (net 13 /AUX_DRV)
  (net 14 /ADCH2)
  (net 15 /R10VL)
  (net 16 /FUELL)
  (net 17 /TEMPL)
  (net 18 /BACKLIGHTL)
  (net 19 /RPMD)
  (net 20 /ROADSPDD)
  (net 21 /ECULAMPD)
  (net 22 /DAUXD)
  (net 23 /MOSI)
  (net 24 /RES)
  (net 25 /SCL)
  (net 26 /SDA)
  (net 27 /CS)
  (net 28 /DC)
  (net 29 "Net-(J1-Pad1)")
  (net 30 "Net-(J1-Pad2)")
  (net 31 /R10V)
  (net 32 /FUEL)
  (net 33 /TEMP)
  (net 34 /BACKLIGHT)
  (net 35 /RPM)
  (net 36 /ROADSPD)
  (net 37 /ECULAMP)
  (net 38 /DAUX)
  (net 39 "Net-(IC101-Pad19)")
  (net 40 "Net-(IC101-Pad20)")
  (net 41 /DAC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /ADCH2)
    (add_net /AUX_DRV)
    (add_net /BACKLIGHT)
    (add_net /BACKLIGHTL)
    (add_net /CS)
    (add_net /DAC)
    (add_net /DAUX)
    (add_net /DAUXD)
    (add_net /DC)
    (add_net /ECULAMP)
    (add_net /ECULAMPD)
    (add_net /FUEL)
    (add_net /FUELL)
    (add_net /MOSI)
    (add_net /R10V)
    (add_net /R10VL)
    (add_net /RES)
    (add_net /RLY_DRV)
    (add_net /ROADSPD)
    (add_net /ROADSPDD)
    (add_net /RPM)
    (add_net /RPMD)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TEMP)
    (add_net /TEMPL)
    (add_net /VIN)
    (add_net GND)
    (add_net "Net-(CON101-Pad1)")
    (add_net "Net-(CON101-Pad3)")
    (add_net "Net-(CON101-Pad4)")
    (add_net "Net-(CON101-Pad5)")
    (add_net "Net-(IC101-Pad19)")
    (add_net "Net-(IC101-Pad20)")
    (add_net "Net-(IC101-Pad21)")
    (add_net "Net-(IC101-Pad22)")
    (add_net "Net-(IC101-Pad23)")
    (add_net "Net-(IC101-Pad24)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 592541C7)
    (at 66.04 117.475)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J6 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value DAC (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /DAC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Crystals:Crystal_DS26_d2.0mm_l6.0mm_Horizontal (layer F.Cu) (tedit 5925376E)
    (at 60.198 136.652 215)
    (descr "Crystal THT DS26 6.0mm length 2.0mm diameter http://www.microcrystal.com/images/_Product-Documentation/03_TF_metal_Packages/01_Datasheet/DS-Series.pdf")
    (tags ['DS26'])
    (fp_text reference Y1 (at -1.57 1.625 305) (layer F.SilkS) hide)
    (fp_text value 32k (at 3.47 1.625 305) (layer F.Fab))
    (fp_text user %R (at 1 4.75 305) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 215) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 "Net-(IC101-Pad20)"))
    (pad 2 thru_hole circle (at 1.9 0 215) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 "Net-(IC101-Pad19)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_DS26_d2.0mm_l6.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINHEAD1-2 (layer B.Cu) (tedit 5923741B)
    (at 65.405 122.555 90)
    (fp_text reference P1 (at 1.27 3.9 90) (layer B.SilkS) hide)
    (fp_text value PWR (at 1.27 -3.81 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VIN))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer B.Cu) (tedit 59236A21)
    (at 45.085 130.175 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference CON101 (at 1.27 2.33 180) (layer B.SilkS) hide)
    (fp_text value AVR-PDI-6 (at 1.27 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 1.27 2.33 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(CON101-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(CON101-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(CON101-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(CON101-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 59236A02)
    (at 55.88 137.795 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.25 270) (layer B.SilkS) hide)
    (fp_text value .1u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 18 /BACKLIGHTL))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 56E5A53C)
    (at 43.18 122.555)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q102 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value IRLML6344TRPBF (at 0 3.81) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 /AUX_DRV))
    (pad 2 smd rect (at 0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 56E41486)
    (at 53.086 123.825)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U101 (at 0 0.762) (layer B.SilkS) hide)
    (fp_text value NCP1117ST33T3G (at 0 -0.762) (layer B.Fab) hide)
    (pad 4 smd rect (at 0 3.302) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 2.286 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 /VIN))
    (pad 1 smd rect (at -2.286 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 56E414CC)
    (at 43.815 122.555 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q101 (at 0 3.81 180) (layer B.SilkS) hide)
    (fp_text value IRLML6344TRPBF (at 0 -3.81 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 -1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 12 /RLY_DRV))
    (pad 2 smd rect (at 0.95 -1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 56E4148B)
    (at 54.61 130.81 315)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC101 (at 0 -6.05 315) (layer F.SilkS) hide)
    (fp_text value ATXMEGA32E5-A (at 0 6.05 315) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.25 -2.8 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.25 -2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /R10VL))
    (pad 3 smd rect (at -4.25 -1.2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /DAC))
    (pad 4 smd rect (at -4.25 -0.4 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /FUELL))
    (pad 5 smd rect (at -4.25 0.4 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /TEMPL))
    (pad 6 smd rect (at -4.25 1.2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /BACKLIGHTL))
    (pad 7 smd rect (at -4.25 2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CON101-Pad1)"))
    (pad 8 smd rect (at -4.25 2.8 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CON101-Pad5)"))
    (pad 9 smd rect (at -2.8 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /RPMD))
    (pad 10 smd rect (at -2 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /ROADSPDD))
    (pad 11 smd rect (at -1.2 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /ECULAMPD))
    (pad 12 smd rect (at -0.4 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /DAUXD))
    (pad 13 smd rect (at 0.4 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /MOSI))
    (pad 14 smd rect (at 1.2 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /RES))
    (pad 15 smd rect (at 2 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /SCL))
    (pad 16 smd rect (at 2.8 4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /SDA))
    (pad 17 smd rect (at 4.25 2.8 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 18 smd rect (at 4.25 2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 4.25 1.2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(IC101-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(IC101-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC101-Pad21)"))
    (pad 22 smd rect (at 4.25 -1.2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC101-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC101-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 315) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC101-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CON101-Pad4)"))
    (pad 26 smd rect (at 2 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON101-Pad3)"))
    (pad 27 smd rect (at 1.2 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /AUX_DRV))
    (pad 28 smd rect (at 0.4 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /RLY_DRV))
    (pad 29 smd rect (at -0.4 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /ADCH2))
    (pad 30 smd rect (at -1.2 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /CS))
    (pad 31 smd rect (at -2 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /DC))
    (pad 32 smd rect (at -2.8 -4.25 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 56E41475)
    (at 54.61 138.43)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C104 (at 0 -2.1) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 56E414EC)
    (at 47.625 122.555 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C103 (at 0 2.7 90) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -2.7 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 56E414E8)
    (at 58.42 122.555 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C102 (at 0 2.7 270) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -2.7 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 /VIN))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 60.96 130.81 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.25 90) (layer B.SilkS))
    (fp_text value .1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 15 /R10VL))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 59236A16)
    (at 62.23 130.81 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.25 90) (layer B.SilkS) hide)
    (fp_text value .1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 16 /FUELL))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 57.15 137.795 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.25 270) (layer B.SilkS))
    (fp_text value .1u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 17 /TEMPL))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 59236A3C)
    (at 41.91 118.11 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value DRV (at 0 -4.87 270) (layer B.Fab))
    (fp_text user %R (at 0 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 592369E1)
    (at 58.42 142.24 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value OLED_I2C (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 59236A40)
    (at 46.99 117.475 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value OLED_SPI (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /MOSI))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /RES))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /DC))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /CS))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 59236A08)
    (at 59.055 139.7 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ADC (at 0 -9.95 270) (layer B.Fab))
    (fp_text user %R (at 0 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /R10V))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /FUEL))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /TEMP))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /BACKLIGHT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 592369F2)
    (at 42.545 139.7 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J5 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value PULSE (at 0 -9.95 270) (layer B.Fab))
    (fp_text user %R (at 0 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /RPM))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /ROADSPD))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /ECULAMP))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /DAUX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer B.Cu) (tedit 59236A12)
    (at 66.04 135.255)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P104 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 -12.49) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC101-Pad21)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(IC101-Pad22)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(IC101-Pad23)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(IC101-Pad24)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 592369E8)
    (at 46.355 142.24)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 2k2 (at -3.81 3.386999) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 592369ED)
    (at 53.34 139.065 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 2k2 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 59236A26)
    (at 43.18 127 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 4k7 (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at -1.1 -0.635 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 /RLY_DRV))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59236A24)
    (at 43.985 127)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R107 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 4k7 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /AUX_DRV))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 59236A45)
    (at 60.96 121.455 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R108 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 330k (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 /ADCH2))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 /VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 59236A19)
    (at 60.96 125.56 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R109 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 22k (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 /ADCH2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer B.Cu) (tedit 59236A0F)
    (at 57.785 128.905)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 2.6) (layer B.SilkS) hide)
    (fp_text value 22k (at 0 -2.6) (layer B.Fab))
    (fp_text user %R (at 0 0.87 270) (layer B.Fab))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 17 /TEMPL))
    (pad 3 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 16 /FUELL))
    (pad 1 smd rect (at -0.85 1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 18 /BACKLIGHTL))
    (pad 4 smd rect (at -0.85 -1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 15 /R10VL))
    (pad 8 smd rect (at 0.85 1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.85 -1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer B.Cu) (tedit 59236A0B)
    (at 62.865 136.525 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value 330k (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at -2.54 -0.211999 540) (layer B.Fab))
    (pad 2 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 16 /FUELL))
    (pad 3 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 17 /TEMPL))
    (pad 1 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 15 /R10VL))
    (pad 4 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 18 /BACKLIGHTL))
    (pad 8 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 31 /R10V))
    (pad 7 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 32 /FUEL))
    (pad 6 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 33 /TEMP))
    (pad 5 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 34 /BACKLIGHT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer B.Cu) (tedit 592369FE)
    (at 49.53 136.525 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0 2.6 180) (layer B.SilkS) hide)
    (fp_text value 22k (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at -0.42 1.67 360) (layer B.Fab))
    (pad 2 smd rect (at -0.85 0.4 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 37 /ECULAMP))
    (pad 3 smd rect (at -0.85 -0.4 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 36 /ROADSPD))
    (pad 1 smd rect (at -0.85 1.2 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 38 /DAUX))
    (pad 4 smd rect (at -0.85 -1.2 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 35 /RPM))
    (pad 8 smd rect (at 0.85 1.2 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 22 /DAUXD))
    (pad 7 smd rect (at 0.85 0.4 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 21 /ECULAMPD))
    (pad 6 smd rect (at 0.85 -0.4 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 20 /ROADSPDD))
    (pad 5 smd rect (at 0.85 -1.2 90) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 19 /RPMD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer B.Cu) (tedit 59236A04)
    (at 53.34 133.985)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 0 2.6) (layer B.SilkS) hide)
    (fp_text value 8k2 (at 0 -2.6) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 21 /ECULAMPD))
    (pad 3 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 20 /ROADSPDD))
    (pad 1 smd rect (at -0.85 1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 22 /DAUXD))
    (pad 4 smd rect (at -0.85 -1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 19 /RPMD))
    (pad 8 smd rect (at 0.85 1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.85 -1.2) (size 0.9 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59287DA3)
    (at 62.23 124.46)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.635 -1.820001) (layer F.SilkS) hide)
    (fp_text value .1u (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 /ADCH2))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text BTNS (at 63.5 128.905 270) (layer F.SilkS))
  (gr_text ADC (at 62.865 137.795 180) (layer F.SilkS))
  (gr_text PULSE (at 46.355 137.795 180) (layer F.SilkS))
  (gr_text VCC (at 55.88 140.335 180) (layer B.SilkS))
  (gr_text VIN (at 62.865 120.015 90) (layer B.SilkS))
  (gr_text GND (at 62.865 135.255 180) (layer F.SilkS))
  (gr_text CS (at 62.23 120.015) (layer F.SilkS))
  (gr_text DC (at 59.69 120.015) (layer F.SilkS))
  (gr_text RES (at 57.15 120.015) (layer F.SilkS))
  (gr_text SDA (at 54.61 120.015) (layer F.SilkS))
  (gr_text SCK (at 52.07 120.015) (layer F.SilkS))
  (gr_text VCC (at 49.53 120.015) (layer F.SilkS))
  (gr_text I2C (at 54.61 140.081 180) (layer F.SilkS))
  (gr_text GND (at 60.96 142.24 180) (layer B.SilkS))
  (gr_text GND (at 46.99 120.015) (layer F.SilkS))
  (dimension 27.305 (width 0.3) (layer Dwgs.User)
    (gr_text "27.305 mm" (at 32.94 129.8575 90) (layer Dwgs.User))
    (feature1 (pts (xy 39.37 116.205) (xy 31.59 116.205)))
    (feature2 (pts (xy 39.37 143.51) (xy 31.59 143.51)))
    (crossbar (pts (xy 34.29 143.51) (xy 34.29 116.205)))
    (arrow1a (pts (xy 34.29 116.205) (xy 34.876421 117.331504)))
    (arrow1b (pts (xy 34.29 116.205) (xy 33.703579 117.331504)))
    (arrow2a (pts (xy 34.29 143.51) (xy 34.876421 142.383496)))
    (arrow2b (pts (xy 34.29 143.51) (xy 33.703579 142.383496)))
  )
  (dimension 27.94 (width 0.3) (layer Dwgs.User)
    (gr_text "27.940 mm" (at 54.61 148.67) (layer Dwgs.User))
    (feature1 (pts (xy 40.64 144.78) (xy 40.64 150.02)))
    (feature2 (pts (xy 68.58 144.78) (xy 68.58 150.02)))
    (crossbar (pts (xy 68.58 147.32) (xy 40.64 147.32)))
    (arrow1a (pts (xy 40.64 147.32) (xy 41.766504 146.733579)))
    (arrow1b (pts (xy 40.64 147.32) (xy 41.766504 147.906421)))
    (arrow2a (pts (xy 68.58 147.32) (xy 67.453496 146.733579)))
    (arrow2b (pts (xy 68.58 147.32) (xy 67.453496 147.906421)))
  )
  (gr_text UR170528 (at 54.61 122.555) (layer F.SilkS))
  (gr_text PDI (at 47.625 132.715 90) (layer B.SilkS))
  (gr_line (start 40.64 116.84) (end 40.64 136.906) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.275 116.205) (end 40.64 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.945 116.205) (end 41.275 116.205) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 116.84) (end 67.945 116.205) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 142.875) (end 68.58 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.945 143.51) (end 68.58 142.875) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.275 143.51) (end 67.945 143.51) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.64 142.875) (end 41.275 143.51) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.64 136.906) (end 40.64 142.875) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.64 142.875) (xy 41.275 143.51) (xy 67.945 143.51) (xy 68.58 142.875) (xy 68.58 116.84)
        (xy 67.945 116.205) (xy 41.275 116.205) (xy 40.64 116.84)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.64 142.875) (xy 41.275 143.51) (xy 67.945 143.51) (xy 68.58 142.875) (xy 68.58 116.84)
        (xy 41.275 116.205) (xy 40.64 116.84)
      )
    )
  )
)
