<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0.9525" y1="0" x2="26.3525" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0.9525" x2="0" y2="28.8925" width="0" layer="20"/>
<wire x1="0.9525" y1="29.845" x2="26.3525" y2="29.845" width="0" layer="20"/>
<wire x1="0" y1="28.8925" x2="0.9525" y2="29.845" width="0" layer="20" curve="-90"/>
<wire x1="0.9525" y1="0" x2="0" y2="0.9525" width="0" layer="20" curve="-90"/>
<wire x1="26.3525" y1="0" x2="27.305" y2="0.9525" width="0" layer="20" curve="90"/>
<wire x1="27.305" y1="0.9525" x2="27.305" y2="28.8925" width="0" layer="20"/>
<wire x1="27.305" y1="28.8925" x2="26.3525" y2="29.845" width="0" layer="20" curve="90"/>
<text>Quantum Effects</text>
<text>Bismuth</text>
<text>Boost</text>
<text>v1.0</text>
<text>B</text>
<text>i</text>
</plain>
<libraries>
<library name="Eigene_Kreationen">
<packages>
<package name="OCTO-PAD">
</package>
<package name="DPDT-FOOTSW">
</package>
<package name="GND-PAD">
</package>
</packages>
</library>
<library name="capacitors-film">
<description>&lt;b&gt;Capacitors, Ceramic&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;very small capacitances: 1 - 1000pF
&lt;/ul&gt;</description>
<packages>
<package name="BOX_SMALL">
</package>
</packages>
</library>
<library name="capacitors-elec">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="3MM_A">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="PADS_SMALL">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;
&lt;p&gt;3 terminals for circuit board for wires connecting to 3 lugs of pot off-board</description>
</package>
</packages>
</library>
<library name="transistors">
<packages>
<package name="TO92-">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="9V" library="Eigene_Kreationen" package="OCTO-PAD" value="9V">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="capacitors-film" package="BOX_SMALL" value="150n"/>
<element name="C3" library="capacitors-elec" package="050_020_1" value="47u"/>
<element name="C4" library="capacitors-film" package="BOX_SMALL" value="220n"/>
<element name="C2" library="capacitors-film" package="BOX_SMALL" value="150n"/>
<element name="CLR" library="resistors" package="R0207/3" value="4k7"/>
<element name="D1" library="diodes" package="DO41-3" value="1N5817"/>
<element name="D2" library="diodes" package="3MM_A" value="LEDA"/>
<element name="DPDT" library="Eigene_Kreationen" package="DPDT-FOOTSW" value=""/>
<element name="H11F1" library="optocoupler" package="DIL06" value="H11F1">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IN" library="Eigene_Kreationen" package="OCTO-PAD" value="IN">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="OUT" library="Eigene_Kreationen" package="OCTO-PAD" value="OUT"/>
<element name="VOL" library="potentiometers" package="PADS_SMALL" value="100kA"/>
<element name="Q1" library="transistors" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="R5" library="resistors" package="R0207/3" value="33R"/>
<element name="R3" library="resistors" package="R0207/3" value="100k"/>
<element name="R4" library="resistors" package="R0207/3" value="360R"/>
<element name="R1" library="resistors" package="R0207/3" value="830k"/>
<element name="R2" library="resistors" package="R0207/3" value="10k"/>
<element name="U$1" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
<element name="U$2" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
<element name="U$3" library="Eigene_Kreationen" package="GND-PAD" value="GND-PAD"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="-"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="DPDT" pad="A2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="VOL" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="C"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D1" pad="A"/>
<contactref element="9V" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="DPDT" pad="B1"/>
<contactref element="VOL" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="H11F1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="CLR" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="H11F1" pad="4"/>
<contactref element="DPDT" pad="A3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="CLR" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="D2" pad="K"/>
<contactref element="DPDT" pad="A1"/>
</signal>
<signal name="N$14">
<contactref element="H11F1" pad="6"/>
<contactref element="DPDT" pad="B3"/>
<contactref element="IN" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="DPDT" pad="B2"/>
<contactref element="OUT" pad="P$1"/>
</signal>
<signal name="N$23">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="Q1" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="R2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="+"/>
<contactref element="R5" pad="2"/>
<contactref element="H11F1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="1"/>
<contactref element="VOL" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
