(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 208)
    (no_connects 0)
    (area 69.278379 102.742999 160.045401 152.654)
    (thickness 1.6002)
    (drawings 18)
    (tracks 779)
    (zones 0)
    (modules 26)
    (nets 97)
  )
  (page A4)
  (title_block
    (date "4 dec 2013")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.381)
    (edge_width 0.381)
    (via_size 1.2192)
    (via_drill 0.508)
    (via_min_size 1.2192)
    (via_min_drill 0.508)
    (uvia_size 1.2192)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 1.2192)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 1.524 1.524)
    (pad_drill 0.8128)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 +5V)
  (net 3 /bufAS)
  (net 4 /bufAddr1)
  (net 5 /bufAddr10)
  (net 6 /bufAddr11)
  (net 7 /bufAddr12)
  (net 8 /bufAddr13)
  (net 9 /bufAddr14)
  (net 10 /bufAddr15)
  (net 11 /bufAddr16)
  (net 12 /bufAddr17)
  (net 13 /bufAddr18)
  (net 14 /bufAddr19)
  (net 15 /bufAddr2)
  (net 16 /bufAddr20)
  (net 17 /bufAddr21)
  (net 18 /bufAddr22)
  (net 19 /bufAddr23)
  (net 20 /bufAddr3)
  (net 21 /bufAddr4)
  (net 22 /bufAddr5)
  (net 23 /bufAddr6)
  (net 24 /bufAddr7)
  (net 25 /bufAddr8)
  (net 26 /bufAddr9)
  (net 27 /bufDTACK)
  (net 28 /bufData0)
  (net 29 /bufData1)
  (net 30 /bufData10)
  (net 31 /bufData11)
  (net 32 /bufData12)
  (net 33 /bufData13)
  (net 34 /bufData14)
  (net 35 /bufData15)
  (net 36 /bufData2)
  (net 37 /bufData3)
  (net 38 /bufData4)
  (net 39 /bufData5)
  (net 40 /bufData6)
  (net 41 /bufData7)
  (net 42 /bufData8)
  (net 43 /bufData9)
  (net 44 /bufLDSW)
  (net 45 /bufOE)
  (net 46 /bufReset)
  (net 47 /bufUDSW)
  (net 48 /mdAS)
  (net 49 /mdAddr1)
  (net 50 /mdAddr10)
  (net 51 /mdAddr11)
  (net 52 /mdAddr12)
  (net 53 /mdAddr13)
  (net 54 /mdAddr14)
  (net 55 /mdAddr15)
  (net 56 /mdAddr16)
  (net 57 /mdAddr17)
  (net 58 /mdAddr18)
  (net 59 /mdAddr19)
  (net 60 /mdAddr2)
  (net 61 /mdAddr20)
  (net 62 /mdAddr21)
  (net 63 /mdAddr22)
  (net 64 /mdAddr23)
  (net 65 /mdAddr3)
  (net 66 /mdAddr4)
  (net 67 /mdAddr5)
  (net 68 /mdAddr6)
  (net 69 /mdAddr7)
  (net 70 /mdAddr8)
  (net 71 /mdAddr9)
  (net 72 /mdDTACK)
  (net 73 /mdData0)
  (net 74 /mdData1)
  (net 75 /mdData10)
  (net 76 /mdData11)
  (net 77 /mdData12)
  (net 78 /mdData13)
  (net 79 /mdData14)
  (net 80 /mdData15)
  (net 81 /mdData2)
  (net 82 /mdData3)
  (net 83 /mdData4)
  (net 84 /mdData5)
  (net 85 /mdData6)
  (net 86 /mdData7)
  (net 87 /mdData8)
  (net 88 /mdData9)
  (net 89 /mdLDSW)
  (net 90 /mdOE)
  (net 91 /mdReset)
  (net 92 /mdUDSW)
  (net 93 GND)
  (net 94 N-000051)
  (net 95 N-000114)
  (net 96 N-000115)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 1.2192)
    (via_drill 0.508)
    (uvia_dia 1.2192)
    (uvia_drill 0.508)
    (add_net +3.3V)
    (add_net /bufAS)
    (add_net /bufAddr1)
    (add_net /bufAddr10)
    (add_net /bufAddr11)
    (add_net /bufAddr12)
    (add_net /bufAddr13)
    (add_net /bufAddr14)
    (add_net /bufAddr15)
    (add_net /bufAddr16)
    (add_net /bufAddr17)
    (add_net /bufAddr18)
    (add_net /bufAddr19)
    (add_net /bufAddr2)
    (add_net /bufAddr20)
    (add_net /bufAddr21)
    (add_net /bufAddr22)
    (add_net /bufAddr23)
    (add_net /bufAddr3)
    (add_net /bufAddr4)
    (add_net /bufAddr5)
    (add_net /bufAddr6)
    (add_net /bufAddr7)
    (add_net /bufAddr8)
    (add_net /bufAddr9)
    (add_net /bufDTACK)
    (add_net /bufData0)
    (add_net /bufData1)
    (add_net /bufData10)
    (add_net /bufData11)
    (add_net /bufData12)
    (add_net /bufData13)
    (add_net /bufData14)
    (add_net /bufData15)
    (add_net /bufData2)
    (add_net /bufData3)
    (add_net /bufData4)
    (add_net /bufData5)
    (add_net /bufData6)
    (add_net /bufData7)
    (add_net /bufData8)
    (add_net /bufData9)
    (add_net /bufLDSW)
    (add_net /bufOE)
    (add_net /bufReset)
    (add_net /bufUDSW)
    (add_net /mdAS)
    (add_net /mdAddr1)
    (add_net /mdAddr10)
    (add_net /mdAddr11)
    (add_net /mdAddr12)
    (add_net /mdAddr13)
    (add_net /mdAddr14)
    (add_net /mdAddr15)
    (add_net /mdAddr16)
    (add_net /mdAddr17)
    (add_net /mdAddr18)
    (add_net /mdAddr19)
    (add_net /mdAddr2)
    (add_net /mdAddr20)
    (add_net /mdAddr21)
    (add_net /mdAddr22)
    (add_net /mdAddr23)
    (add_net /mdAddr3)
    (add_net /mdAddr4)
    (add_net /mdAddr5)
    (add_net /mdAddr6)
    (add_net /mdAddr7)
    (add_net /mdAddr8)
    (add_net /mdAddr9)
    (add_net /mdDTACK)
    (add_net /mdData0)
    (add_net /mdData1)
    (add_net /mdData10)
    (add_net /mdData11)
    (add_net /mdData12)
    (add_net /mdData13)
    (add_net /mdData14)
    (add_net /mdData15)
    (add_net /mdData2)
    (add_net /mdData3)
    (add_net /mdData4)
    (add_net /mdData5)
    (add_net /mdData6)
    (add_net /mdData7)
    (add_net /mdData8)
    (add_net /mdData9)
    (add_net /mdLDSW)
    (add_net /mdOE)
    (add_net /mdReset)
    (add_net /mdUDSW)
    (add_net N-000051)
    (add_net N-000114)
    (add_net N-000115)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 1.27)
    (via_dia 1.2192)
    (via_drill 0.508)
    (uvia_dia 1.2192)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net GND)
  )
  (module MS-NPTH-6.00 (layer Front) (tedit 529A6FBA)
    (at 153.5684 118.745)
    (fp_text reference DRL1 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value MS-NPTH (at 0 -4.445) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 5.99948) (layers *.Cu *.Mask F.SilkS))
  )
  (module MS-NPTH-6.00 (layer Front) (tedit 529A6FC2)
    (at 83.9724 118.745)
    (fp_text reference DRL2 (at 0.1524 4.445) (layer F.SilkS) hide)
    (fp_text value MS-NPTH (at 0.1524 -4.445) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 5.99948) (layers *.Cu *.Mask F.SilkS))
  )
  (module MS-0805 (layer Front) (tedit 529DDEDD)
    (at 89.535 130.175 270)
    (attr smd)
    (fp_text reference C1 (at 0.0127 2.159 360) (layer F.SilkS))
    (fp_text value C (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-SIL1 (layer Front) (tedit 529E6D62)
    (at 123.19 135.89)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value DTACK (at 0 -1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 /mdDTACK))
  )
  (module MS-EDGE80%2f2.00 (layer Front) (tedit 529E75AC)
    (at 79.121 104.521)
    (fp_text reference CONN2 (at -7.00024 1.00076) (layer F.SilkS) hide)
    (fp_text value LX9 (at 0.381 2.794) (layer F.SilkS))
    (pad 1 connect rect (at 0 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 25 /bufAddr8))
    (pad 2 connect rect (at 0 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 2 +5V))
    (pad 3 connect rect (at 1.99898 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 6 /bufAddr11))
    (pad 4 connect rect (at 1.99898 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 1 +3.3V))
    (pad 5 connect rect (at 4.0005 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 24 /bufAddr7))
    (pad 6 connect rect (at 4.0005 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 26 /bufAddr9))
    (pad 7 connect rect (at 5.99948 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 7 /bufAddr12))
    (pad 8 connect rect (at 5.99948 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 5 /bufAddr10))
    (pad 9 connect rect (at 8.001 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 23 /bufAddr6))
    (pad 10 connect rect (at 8.001 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 13 /bufAddr18))
    (pad 11 connect rect (at 9.99998 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 14 /bufAddr19))
    (pad 12 connect rect (at 9.99998 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 13 connect rect (at 11.99896 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 8 /bufAddr13))
    (pad 14 connect rect (at 11.99896 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 15 connect rect (at 14.00048 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 16 /bufAddr20))
    (pad 16 connect rect (at 14.00048 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 17 connect rect (at 15.99946 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 22 /bufAddr5))
    (pad 18 connect rect (at 15.99946 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 19 connect rect (at 18.00098 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 17 /bufAddr21))
    (pad 20 connect rect (at 18.00098 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 21 connect rect (at 19.99996 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 9 /bufAddr14))
    (pad 22 connect rect (at 19.99996 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 23 connect rect (at 21.99894 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 46 /bufReset))
    (pad 24 connect rect (at 21.99894 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 25 connect rect (at 24.00046 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 18 /bufAddr22))
    (pad 26 connect rect (at 24.00046 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 27 connect rect (at 25.99944 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 21 /bufAddr4))
    (pad 28 connect rect (at 25.99944 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 29 connect rect (at 28.00096 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 19 /bufAddr23))
    (pad 30 connect rect (at 28.00096 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 31 connect rect (at 29.99994 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 10 /bufAddr15))
    (pad 32 connect rect (at 29.99994 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 33 connect rect (at 31.99892 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 20 /bufAddr3))
    (pad 34 connect rect (at 31.99892 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 35 connect rect (at 34.00044 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 11 /bufAddr16))
    (pad 36 connect rect (at 34.00044 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 37 connect rect (at 35.99942 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 15 /bufAddr2))
    (pad 38 connect rect (at 35.99942 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 39 connect rect (at 38.00094 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 12 /bufAddr17))
    (pad 40 connect rect (at 38.00094 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 41 connect rect (at 39.99992 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 45 /bufOE))
    (pad 42 connect rect (at 39.99992 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 43 connect rect (at 41.9989 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 4 /bufAddr1))
    (pad 44 connect rect (at 41.9989 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 45 connect rect (at 44.00042 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 3 /bufAS))
    (pad 46 connect rect (at 44.00042 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 47 connect rect (at 45.9994 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 44 /bufLDSW))
    (pad 48 connect rect (at 45.9994 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 49 connect rect (at 48.00092 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 47 /bufUDSW))
    (pad 50 connect rect (at 48.00092 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 51 connect rect (at 49.9999 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 41 /bufData7))
    (pad 52 connect rect (at 49.9999 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 53 connect rect (at 51.99888 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 28 /bufData0))
    (pad 54 connect rect (at 51.99888 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 55 connect rect (at 54.0004 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 42 /bufData8))
    (pad 56 connect rect (at 54.0004 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 57 connect rect (at 55.99938 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 35 /bufData15))
    (pad 58 connect rect (at 55.99938 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 59 connect rect (at 58.0009 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 40 /bufData6))
    (pad 60 connect rect (at 58.0009 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 61 connect rect (at 59.99988 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 34 /bufData14))
    (pad 62 connect rect (at 59.99988 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 63 connect rect (at 61.99886 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 29 /bufData1))
    (pad 64 connect rect (at 61.99886 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 65 connect rect (at 64.00038 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 33 /bufData13))
    (pad 66 connect rect (at 64.00038 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 67 connect rect (at 65.99936 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 43 /bufData9))
    (pad 68 connect rect (at 65.99936 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 69 connect rect (at 68.00088 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 32 /bufData12))
    (pad 70 connect rect (at 68.00088 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 71 connect rect (at 69.99986 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 39 /bufData5))
    (pad 72 connect rect (at 69.99986 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 93 GND))
    (pad 73 connect rect (at 71.99884 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 36 /bufData2))
    (pad 74 connect rect (at 71.99884 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 30 /bufData10))
    (pad 75 connect rect (at 74.00036 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 38 /bufData4))
    (pad 76 connect rect (at 74.00036 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 37 /bufData3))
    (pad 77 connect rect (at 75.99934 0) (size 1.3335 3.048) (layers Front F.Mask))
    (pad 78 connect rect (at 75.99934 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 31 /bufData11))
    (pad 79 connect rect (at 78.00086 0) (size 1.3335 3.048) (layers Front F.Mask)
      (net 27 /bufDTACK))
    (pad 80 connect rect (at 78.00086 0) (size 1.3335 3.048) (layers Back B.Mask)
      (net 94 N-000051))
  )
  (module MS-0805 (layer Front) (tedit 529DDEEF)
    (at 109.22 130.175 270)
    (attr smd)
    (fp_text reference C2 (at 4.5593 0.2032 360) (layer F.SilkS))
    (fp_text value C (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-0805 (layer Front) (tedit 529DDF00)
    (at 127.635 130.175 270)
    (attr smd)
    (fp_text reference C3 (at 4.5593 0.4572 360) (layer F.SilkS))
    (fp_text value C (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-0805 (layer Front) (tedit 529DDF6F)
    (at 147.32 130.175 270)
    (attr smd)
    (fp_text reference C4 (at 0 -2.0955 360) (layer F.SilkS))
    (fp_text value C (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-C3528%2fT (layer Back) (tedit 529D028A)
    (at 80.01 139.5095 180)
    (descr "SMD CHIP TANT")
    (tags "SMD CHIP TANT")
    (attr smd)
    (fp_text reference C5 (at -4.11226 -0.0508 180) (layer B.SilkS))
    (fp_text value CP1 (at -0.11176 -0.0508 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.5875 0.00254) (size 1.99898 2.19964) (layers Back B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.5875 0.00254) (size 1.99898 2.19964) (layers Back B.Paste B.Mask)
      (net 93 GND))
  )
  (module MS-C3528%2fT (layer Back) (tedit 529D0276)
    (at 156.21 139.5095)
    (descr "SMD CHIP TANT")
    (tags "SMD CHIP TANT")
    (attr smd)
    (fp_text reference C6 (at -4.08686 0.0508) (layer B.SilkS))
    (fp_text value CP1 (at -0.0889 0.0508 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.5875 0.00254 180) (size 1.99898 2.19964) (layers Back B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.5875 0.00254 180) (size 1.99898 2.19964) (layers Back B.Paste B.Mask)
      (net 93 GND))
  )
  (module MS-0805 (layer Front) (tedit 529DDED1)
    (at 89.535 125.984 90)
    (attr smd)
    (fp_text reference C7 (at 0.0127 -2.159 180) (layer F.SilkS))
    (fp_text value C (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-0805 (layer Front) (tedit 529DDEE7)
    (at 109.22 125.984 90)
    (attr smd)
    (fp_text reference C8 (at -7.2771 -0.2032 180) (layer F.SilkS))
    (fp_text value C (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-0805 (layer Front) (tedit 529DDEF9)
    (at 127.635 125.984 90)
    (attr smd)
    (fp_text reference C9 (at -7.2771 -0.4572 180) (layer F.SilkS))
    (fp_text value C (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-0805 (layer Front) (tedit 529DDF65)
    (at 147.32 125.984 90)
    (attr smd)
    (fp_text reference C10 (at 0 2.6035 180) (layer F.SilkS))
    (fp_text value C (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-C3528%2fT (layer Back) (tedit 529DC6B3)
    (at 118.4275 122.428 90)
    (descr "SMD CHIP TANT")
    (tags "SMD CHIP TANT")
    (attr smd)
    (fp_text reference C11 (at 3.683 0 180) (layer B.SilkS))
    (fp_text value CP1 (at -0.127 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.5875 0.00254 270) (size 1.99898 2.19964) (layers Back B.Paste B.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.5875 0.00254 270) (size 1.99898 2.19964) (layers Back B.Paste B.Mask)
      (net 93 GND))
  )
  (module MS-0805 (layer Front) (tedit 529DDF7D)
    (at 149.86 139.065)
    (attr smd)
    (fp_text reference R1 (at 0 1.905) (layer F.SilkS))
    (fp_text value R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 94 N-000051))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-OSHW-7MM (layer Front) (tedit 529DEC1F)
    (at 82.423 139.065)
    (fp_text reference "OPEN-SOURCE HARDWARE" (at 14.0335 0.4445) (layer F.SilkS))
    (fp_text value OSHW (at 0 0) (layer F.SilkS) hide)
  )
  (module MS-SIL1 (layer Front) (tedit 529E6D82)
    (at 148.59 135.89)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value DTACK (at 0 -1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 N-000114))
  )
  (module MS-0805 (layer Front) (tedit 529E75E2)
    (at 80.01 127 270)
    (attr smd)
    (fp_text reference R2 (at -2.413 0 360) (layer F.SilkS))
    (fp_text value R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 46 /bufReset))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers Front F.Paste F.Mask)
      (net 96 N-000115))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MS-TESTPOINT (layer Front) (tedit 529E6D77)
    (at 120.65 137.16)
    (fp_text reference TP1 (at -0.1524 -2.0066) (layer F.SilkS) hide)
    (fp_text value AS (at 0 1.524) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers Front F.Paste F.Mask)
      (net 48 /mdAS))
  )
  (module MS-SSOP48 (layer Front) (tedit 529E7570)
    (at 130.81 132.715)
    (fp_text reference U3 (at 7.3025 -11.1125) (layer F.SilkS))
    (fp_text value 74ALVC164245 (at 7.239 -5.588) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 94 N-000051))
    (pad 2 smd rect (at 0.635 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 86 /mdData7))
    (pad 3 smd rect (at 1.27 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 73 /mdData0))
    (pad 4 smd rect (at 1.905 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 5 smd rect (at 2.54 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 87 /mdData8))
    (pad 6 smd rect (at 3.175 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 80 /mdData15))
    (pad 7 smd rect (at 3.81 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (pad 8 smd rect (at 4.445 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 85 /mdData6))
    (pad 9 smd rect (at 5.08 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 79 /mdData14))
    (pad 10 smd rect (at 5.715 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 11 smd rect (at 6.35 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 74 /mdData1))
    (pad 12 smd rect (at 6.985 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 78 /mdData13))
    (pad 13 smd rect (at 7.62 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 88 /mdData9))
    (pad 14 smd rect (at 8.255 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 77 /mdData12))
    (pad 15 smd rect (at 8.89 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 16 smd rect (at 9.525 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 84 /mdData5))
    (pad 17 smd rect (at 10.16 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 81 /mdData2))
    (pad 18 smd rect (at 10.795 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (pad 19 smd rect (at 11.43 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 75 /mdData10))
    (pad 20 smd rect (at 12.065 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 83 /mdData4))
    (pad 21 smd rect (at 12.7 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 22 smd rect (at 13.335 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 82 /mdData3))
    (pad 23 smd rect (at 13.97 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 76 /mdData11))
    (pad 24 smd rect (at 14.605 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 94 N-000051))
    (pad 25 smd rect (at 14.605 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 26 smd rect (at 13.97 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 31 /bufData11))
    (pad 27 smd rect (at 13.335 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 37 /bufData3))
    (pad 28 smd rect (at 12.7 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 29 smd rect (at 12.065 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 38 /bufData4))
    (pad 30 smd rect (at 11.43 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 30 /bufData10))
    (pad 31 smd rect (at 10.795 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 32 smd rect (at 10.16 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 36 /bufData2))
    (pad 33 smd rect (at 9.525 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 39 /bufData5))
    (pad 34 smd rect (at 8.89 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 35 smd rect (at 8.255 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 32 /bufData12))
    (pad 36 smd rect (at 7.62 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 43 /bufData9))
    (pad 37 smd rect (at 6.985 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 33 /bufData13))
    (pad 38 smd rect (at 6.35 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 29 /bufData1))
    (pad 39 smd rect (at 5.715 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 40 smd rect (at 5.08 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 34 /bufData14))
    (pad 41 smd rect (at 4.445 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 40 /bufData6))
    (pad 42 smd rect (at 3.81 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 43 smd rect (at 3.175 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 35 /bufData15))
    (pad 44 smd rect (at 2.54 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 42 /bufData8))
    (pad 45 smd rect (at 1.905 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 46 smd rect (at 1.27 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 28 /bufData0))
    (pad 47 smd rect (at 0.635 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 41 /bufData7))
    (pad 48 smd rect (at 0 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
  )
  (module MS-SOT23 (layer Front) (tedit 529E7731)
    (at 153.67 135.89 90)
    (fp_text reference Q2 (at 2.413 -0.889 180) (layer F.SilkS))
    (fp_text value BC848B (at 0 -4.1275 90) (layer F.SilkS) hide)
    (pad B smd rect (at -0.94996 0 90) (size 0.8001 1.00076) (layers Front F.Paste F.Mask)
      (net 27 /bufDTACK))
    (pad E smd rect (at 0.94996 0 90) (size 0.8001 1.00076) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad C smd rect (at 0 -2.4003 90) (size 0.8001 1.00076) (layers Front F.Paste F.Mask)
      (net 95 N-000114))
  )
  (module MS-SSOP48 (layer Front) (tedit 529E756A)
    (at 111.125 132.715)
    (fp_text reference U2 (at 7.3025 -11.1125) (layer F.SilkS))
    (fp_text value 74ALVC164245 (at 7.239 -5.588) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.635 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 63 /mdAddr22))
    (pad 3 smd rect (at 1.27 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 66 /mdAddr4))
    (pad 4 smd rect (at 1.905 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 5 smd rect (at 2.54 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 64 /mdAddr23))
    (pad 6 smd rect (at 3.175 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 55 /mdAddr15))
    (pad 7 smd rect (at 3.81 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (pad 8 smd rect (at 4.445 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 65 /mdAddr3))
    (pad 9 smd rect (at 5.08 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 56 /mdAddr16))
    (pad 10 smd rect (at 5.715 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 11 smd rect (at 6.35 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 60 /mdAddr2))
    (pad 12 smd rect (at 6.985 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 57 /mdAddr17))
    (pad 13 smd rect (at 7.62 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 90 /mdOE))
    (pad 14 smd rect (at 8.255 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 49 /mdAddr1))
    (pad 15 smd rect (at 8.89 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 16 smd rect (at 9.525 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 48 /mdAS))
    (pad 17 smd rect (at 10.16 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 18 smd rect (at 10.795 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (pad 19 smd rect (at 11.43 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 20 smd rect (at 12.065 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 21 smd rect (at 12.7 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 22 smd rect (at 13.335 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 89 /mdLDSW))
    (pad 23 smd rect (at 13.97 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 92 /mdUDSW))
    (pad 24 smd rect (at 14.605 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 25 smd rect (at 14.605 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 26 smd rect (at 13.97 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 47 /bufUDSW))
    (pad 27 smd rect (at 13.335 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 44 /bufLDSW))
    (pad 28 smd rect (at 12.7 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 29 smd rect (at 12.065 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask))
    (pad 30 smd rect (at 11.43 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask))
    (pad 31 smd rect (at 10.795 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 32 smd rect (at 10.16 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask))
    (pad 33 smd rect (at 9.525 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 3 /bufAS))
    (pad 34 smd rect (at 8.89 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 35 smd rect (at 8.255 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 4 /bufAddr1))
    (pad 36 smd rect (at 7.62 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 45 /bufOE))
    (pad 37 smd rect (at 6.985 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 12 /bufAddr17))
    (pad 38 smd rect (at 6.35 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 15 /bufAddr2))
    (pad 39 smd rect (at 5.715 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 40 smd rect (at 5.08 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 11 /bufAddr16))
    (pad 41 smd rect (at 4.445 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 20 /bufAddr3))
    (pad 42 smd rect (at 3.81 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 43 smd rect (at 3.175 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 10 /bufAddr15))
    (pad 44 smd rect (at 2.54 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 19 /bufAddr23))
    (pad 45 smd rect (at 1.905 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 46 smd rect (at 1.27 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 21 /bufAddr4))
    (pad 47 smd rect (at 0.635 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 18 /bufAddr22))
    (pad 48 smd rect (at 0 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
  )
  (module MS-SSOP48 (layer Front) (tedit 529E7562)
    (at 91.44 132.715)
    (fp_text reference U1 (at 7.3025 -11.1125) (layer F.SilkS))
    (fp_text value 74ALVC164245 (at 7.239 -5.588) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 2 smd rect (at 0.635 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 70 /mdAddr8))
    (pad 3 smd rect (at 1.27 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 51 /mdAddr11))
    (pad 4 smd rect (at 1.905 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 5 smd rect (at 2.54 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 71 /mdAddr9))
    (pad 6 smd rect (at 3.175 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 69 /mdAddr7))
    (pad 7 smd rect (at 3.81 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (pad 8 smd rect (at 4.445 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 50 /mdAddr10))
    (pad 9 smd rect (at 5.08 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 52 /mdAddr12))
    (pad 10 smd rect (at 5.715 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 11 smd rect (at 6.35 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 58 /mdAddr18))
    (pad 12 smd rect (at 6.985 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 68 /mdAddr6))
    (pad 13 smd rect (at 7.62 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 59 /mdAddr19))
    (pad 14 smd rect (at 8.255 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 53 /mdAddr13))
    (pad 15 smd rect (at 8.89 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 16 smd rect (at 9.525 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 61 /mdAddr20))
    (pad 17 smd rect (at 10.16 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 67 /mdAddr5))
    (pad 18 smd rect (at 10.795 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 2 +5V))
    (pad 19 smd rect (at 11.43 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 62 /mdAddr21))
    (pad 20 smd rect (at 12.065 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 54 /mdAddr14))
    (pad 21 smd rect (at 12.7 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 22 smd rect (at 13.335 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 23 smd rect (at 13.97 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 24 smd rect (at 14.605 0) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 25 smd rect (at 14.605 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 26 smd rect (at 13.97 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask))
    (pad 27 smd rect (at 13.335 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask))
    (pad 28 smd rect (at 12.7 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 29 smd rect (at 12.065 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 9 /bufAddr14))
    (pad 30 smd rect (at 11.43 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 17 /bufAddr21))
    (pad 31 smd rect (at 10.795 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 32 smd rect (at 10.16 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 22 /bufAddr5))
    (pad 33 smd rect (at 9.525 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 16 /bufAddr20))
    (pad 34 smd rect (at 8.89 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 35 smd rect (at 8.255 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 8 /bufAddr13))
    (pad 36 smd rect (at 7.62 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 14 /bufAddr19))
    (pad 37 smd rect (at 6.985 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 23 /bufAddr6))
    (pad 38 smd rect (at 6.35 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 13 /bufAddr18))
    (pad 39 smd rect (at 5.715 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 40 smd rect (at 5.08 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 7 /bufAddr12))
    (pad 41 smd rect (at 4.445 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 5 /bufAddr10))
    (pad 42 smd rect (at 3.81 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 43 smd rect (at 3.175 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 24 /bufAddr7))
    (pad 44 smd rect (at 2.54 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 26 /bufAddr9))
    (pad 45 smd rect (at 1.905 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad 46 smd rect (at 1.27 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 6 /bufAddr11))
    (pad 47 smd rect (at 0.635 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 25 /bufAddr8))
    (pad 48 smd rect (at 0 -9.2456) (size 0.3556 2.2606) (layers Front F.Paste F.Mask)
      (net 93 GND))
  )
  (module MS-MDCART (layer Front) (tedit 529E75A2)
    (at 78.74 148.59)
    (fp_text reference CONN1 (at -5.08 0) (layer F.SilkS) hide)
    (fp_text value MDCART (at 1.524 -4.191) (layer F.SilkS))
    (pad B1 connect rect (at 0 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B2 connect rect (at 2.54 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 91 /mdReset))
    (pad B3 connect rect (at 5.08 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B4 connect rect (at 7.62 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 71 /mdAddr9))
    (pad B5 connect rect (at 10.16 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 50 /mdAddr10))
    (pad B6 connect rect (at 12.7 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 58 /mdAddr18))
    (pad B7 connect rect (at 15.24 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 59 /mdAddr19))
    (pad B8 connect rect (at 17.78 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 61 /mdAddr20))
    (pad B9 connect rect (at 20.32 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 62 /mdAddr21))
    (pad B10 connect rect (at 22.86 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 63 /mdAddr22))
    (pad B11 connect rect (at 25.4 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 64 /mdAddr23))
    (pad B12 connect rect (at 27.94 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B13 connect rect (at 30.48 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B14 connect rect (at 33.02 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B15 connect rect (at 35.56 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B16 connect rect (at 38.1 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 90 /mdOE))
    (pad B17 connect rect (at 40.64 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B18 connect rect (at 43.18 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 48 /mdAS))
    (pad B19 connect rect (at 45.72 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B20 connect rect (at 48.26 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 72 /mdDTACK))
    (pad B21 connect rect (at 50.8 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B22 connect rect (at 53.34 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 80 /mdData15))
    (pad B23 connect rect (at 55.88 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 79 /mdData14))
    (pad B24 connect rect (at 58.42 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 78 /mdData13))
    (pad B25 connect rect (at 60.96 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 77 /mdData12))
    (pad B26 connect rect (at 63.5 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B27 connect rect (at 66.04 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B28 connect rect (at 68.58 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 89 /mdLDSW))
    (pad B29 connect rect (at 71.12 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 92 /mdUDSW))
    (pad B30 connect rect (at 73.66 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B31 connect rect (at 76.2 0.381) (size 1.67386 5.842) (layers Front F.Mask))
    (pad B32 connect rect (at 78.74 0.381) (size 1.67386 5.842) (layers Front F.Mask)
      (net 93 GND))
    (pad A1 connect rect (at 0 0.635) (size 1.67386 6.35) (layers Back B.Mask)
      (net 93 GND))
    (pad A2 connect rect (at 2.54 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 2 +5V))
    (pad A3 connect rect (at 5.08 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 70 /mdAddr8))
    (pad A4 connect rect (at 7.62 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 51 /mdAddr11))
    (pad A5 connect rect (at 10.16 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 69 /mdAddr7))
    (pad A6 connect rect (at 12.7 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 52 /mdAddr12))
    (pad A7 connect rect (at 15.24 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 68 /mdAddr6))
    (pad A8 connect rect (at 17.78 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 53 /mdAddr13))
    (pad A9 connect rect (at 20.32 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 67 /mdAddr5))
    (pad A10 connect rect (at 22.86 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 54 /mdAddr14))
    (pad A11 connect rect (at 25.4 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 66 /mdAddr4))
    (pad A12 connect rect (at 27.94 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 55 /mdAddr15))
    (pad A13 connect rect (at 30.48 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 65 /mdAddr3))
    (pad A14 connect rect (at 33.02 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 56 /mdAddr16))
    (pad A15 connect rect (at 35.56 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 60 /mdAddr2))
    (pad A16 connect rect (at 38.1 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 57 /mdAddr17))
    (pad A17 connect rect (at 40.64 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 49 /mdAddr1))
    (pad A18 connect rect (at 43.18 0.635) (size 1.67386 6.35) (layers Back B.Mask)
      (net 93 GND))
    (pad A19 connect rect (at 45.72 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 86 /mdData7))
    (pad A20 connect rect (at 48.26 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 73 /mdData0))
    (pad A21 connect rect (at 50.8 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 87 /mdData8))
    (pad A22 connect rect (at 53.34 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 85 /mdData6))
    (pad A23 connect rect (at 55.88 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 74 /mdData1))
    (pad A24 connect rect (at 58.42 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 88 /mdData9))
    (pad A25 connect rect (at 60.96 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 84 /mdData5))
    (pad A26 connect rect (at 63.5 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 81 /mdData2))
    (pad A27 connect rect (at 66.04 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 75 /mdData10))
    (pad A28 connect rect (at 68.58 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 83 /mdData4))
    (pad A29 connect rect (at 71.12 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 82 /mdData3))
    (pad A30 connect rect (at 73.66 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 76 /mdData11))
    (pad A31 connect rect (at 76.2 0.381) (size 1.67386 5.842) (layers Back B.Mask)
      (net 2 +5V))
    (pad A32 connect rect (at 78.74 0.635) (size 1.67386 6.35) (layers Back B.Mask)
      (net 93 GND))
  )
  (module MS-SOT23 (layer Front) (tedit 529E7715)
    (at 80.01 130.175 180)
    (fp_text reference Q1 (at -2.921 -1.016 180) (layer F.SilkS))
    (fp_text value BC848B (at 0 -4.1275 180) (layer F.SilkS) hide)
    (pad B smd rect (at -0.94996 0 180) (size 0.8001 1.00076) (layers Front F.Paste F.Mask)
      (net 96 N-000115))
    (pad E smd rect (at 0.94996 0 180) (size 0.8001 1.00076) (layers Front F.Paste F.Mask)
      (net 93 GND))
    (pad C smd rect (at 0 -2.4003 180) (size 0.8001 1.00076) (layers Front F.Paste F.Mask)
      (net 91 /mdReset))
  )
  (gr_text "KiCad Source:\nhttps://github.com/makestuff/umdkv2-lx9/archive/605a3f7.tar.gz" (at 118.745 110.236) (layer B.SilkS))
  (gr_text DTACK (at 136.525 135.89) (layer F.SilkS))
  (gr_text "USB MegaDrive DevKit V2\nUMDKv2-LX9 Copyright © 2013 MakeStuff (http://makestuff.eu)\nLicensed under CERN OHL v1.2 (http://ohwr.org/cernohl)\nContact: Chris McClelland (chris@makestuff.eu)\nhttp://google.com/+ChrisMcClelland" (at 120.12168 109.52226) (layer F.SilkS))
  (gr_text B (at 157.3022 129.413) (layer F.SilkS))
  (gr_text A (at 157.3276 127) (layer F.SilkS))
  (gr_line (start 158.75 152.4) (end 160.02 151.13) (angle 90) (layer Edge.Cuts) (width 0.0508))
  (gr_line (start 76.2 151.13) (end 77.47 152.4) (angle 90) (layer Edge.Cuts) (width 0.0508))
  (gr_line (start 76.2 102.87) (end 76.2 151.13) (angle 90) (layer Edge.Cuts) (width 0.0508))
  (gr_line (start 160.02 102.87) (end 76.2 102.87) (angle 90) (layer Edge.Cuts) (width 0.0508))
  (gr_line (start 160.02 151.13) (end 160.02 102.87) (angle 90) (layer Edge.Cuts) (width 0.0508))
  (gr_line (start 77.47 152.4) (end 158.75 152.4) (angle 90) (layer Edge.Cuts) (width 0.0508))
  (zone (net 93) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.385 146.05) (xy 159.385 103.505) (xy 76.835 103.505) (xy 76.835 146.05)
      )
    )
  )
  (zone (net 93) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.3048)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.385 146.05) (xy 159.385 103.505) (xy 76.835 103.505) (xy 76.835 146.05)
      )
    )
  )
)
