(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J15-Pad1)")
  (net 2 "Net-(J15-Pad2)")
  (net 3 "Net-(J14-Pad1)")
  (net 4 "Net-(J14-Pad2)")
  (net 5 "Net-(J13-Pad1)")
  (net 6 "Net-(J13-Pad2)")
  (net 7 "Net-(J12-Pad1)")
  (net 8 "Net-(J12-Pad2)")
  (net 9 "Net-(J11-Pad1)")
  (net 10 "Net-(J11-Pad2)")
  (net 11 "Net-(J10-Pad1)")
  (net 12 "Net-(J10-Pad2)")
  (net 13 "Net-(J8-Pad27)")
  (net 14 "Net-(J8-Pad28)")
  (net 15 "Net-(J1-Pad1)")
  (net 16 "Net-(J1-Pad2)")
  (net 17 "Net-(J2-Pad1)")
  (net 18 "Net-(J2-Pad2)")
  (net 19 "Net-(J3-Pad1)")
  (net 20 "Net-(J3-Pad2)")
  (net 21 "Net-(J4-Pad2)")
  (net 22 "Net-(J4-Pad1)")
  (net 23 "Net-(J5-Pad1)")
  (net 24 "Net-(J5-Pad2)")
  (net 25 "Net-(J6-Pad1)")
  (net 26 "Net-(J6-Pad2)")
  (net 27 "Net-(J7-Pad1)")
  (net 28 "Net-(J7-Pad2)")
  (footprint "Package_DIP:DIP-28_W15.24mm_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 78.74 69.85)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 7.62 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_02x14_Counter_Clockwise" (at 7.62 35.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 16.51) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-Pad2)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad1)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J5-Pad2)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J6-Pad1)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad1)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J7-Pad2)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 15.24 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J15-Pad1)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 15.24 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J15-Pad2)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 15.24 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J14-Pad1)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 15.24 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J14-Pad2)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 15.24 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J13-Pad1)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 15.24 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J13-Pad2)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 15.24 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J12-Pad1)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 15.24 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J12-Pad2)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 15.24 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 15.24 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J11-Pad2)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 15.24 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at 15.24 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J10-Pad2)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 15.24 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad27)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at 15.24 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J8-Pad28)") (pinfunction "Pin_28") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 106.68 50.8 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad27)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 14 "Net-(J8-Pad28)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 66.04 109.22 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 25 "Net-(J6-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 66.04 71.12 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 66.04 45.72 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 106.68 88.9 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J12" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 7 "Net-(J12-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 8 "Net-(J12-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 106.68 114.3 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J14" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "Net-(J14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 4 "Net-(J14-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 66.04 96.52 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 24 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 106.68 101.6 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J13" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 5 "Net-(J13-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 6 "Net-(J13-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 106.68 76.2 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 10 "Net-(J11-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 106.68 127 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J15" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 "Net-(J15-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 "Net-(J15-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 106.68 63.5 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 12 "Net-(J10-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 66.04 121.92 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 28 "Net-(J7-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 66.04 83.82 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB)
    (at 66.04 58.42 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "wzif-28-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 2.54 -5.08 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 58.42 40.64) (end 114.3 132.08) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "12" (at 60.96 114.3) (layer "F.SilkS"))
  (gr_text "15" (at 113.03 128.27) (layer "F.SilkS"))
  (gr_text "23" (at 113.03 76.2) (layer "F.SilkS"))
  (gr_text "28" (at 112.973525 45.704569) (layer "F.SilkS"))
  (gr_text "21" (at 113.03 88.9) (layer "F.SilkS"))
  (gr_text "14" (at 60.96 127) (layer "F.SilkS"))
  (gr_text "27" (at 113.03 50.8) (layer "F.SilkS"))
  (gr_text "5" (at 59.69 71.12) (layer "F.SilkS"))
  (gr_text "25" (at 113.03 63.5) (layer "F.SilkS"))
  (gr_text "2" (at 59.69 50.8) (layer "F.SilkS"))
  (gr_text "22" (at 113.03 83.82) (layer "F.SilkS"))
  (gr_text "26" (at 113.03 58.42) (layer "F.SilkS"))
  (gr_text "10" (at 60.96 101.6) (layer "F.SilkS"))
  (gr_text "19" (at 113.03 101.6) (layer "F.SilkS"))
  (gr_text "9" (at 59.69 96.52) (layer "F.SilkS"))
  (gr_text "13" (at 60.96 121.92) (layer "F.SilkS"))
  (gr_text "17" (at 113.03 114.3) (layer "F.SilkS"))
  (gr_text "1" (at 59.69 45.72) (layer "F.SilkS"))
  (gr_text "16" (at 113.03 121.92) (layer "F.SilkS"))
  (gr_text "11" (at 60.96 109.22) (layer "F.SilkS"))
  (gr_text "24" (at 113.03 71.12) (layer "F.SilkS"))
  (gr_text "18" (at 113.03 109.22) (layer "F.SilkS"))
  (gr_text "6" (at 59.69 76.2) (layer "F.SilkS"))
  (gr_text "8" (at 59.69 88.9) (layer "F.SilkS"))
  (gr_text "4" (at 59.69 63.5) (layer "F.SilkS"))
  (gr_text "3" (at 59.69 58.42) (layer "F.SilkS"))
  (gr_text "7" (at 59.69 83.82) (layer "F.SilkS"))
  (gr_text "20" (at 112.973525 96.178055) (layer "F.SilkS"))
)
