(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GNDREF")
  (net 2 "Net-(J1-Pin_1)")
  (net 3 "Net-(J2-Pin_1)")
  (net 4 "Net-(Q1-B)")
  (net 5 "Net-(Q1-C)")
  (net 6 "Net-(Q2-E)")
  (net 7 "Net-(Q2-B)")
  (net 8 "Net-(Q2-C)")
  (net 9 "Net-(U1-LBO)")
  (net 10 "Net-(U1-5Vo)")
  (net 11 "unconnected-(U1-USB-5V-Pad5V)")
  (net 12 "unconnected-(U1-USB-D--PadD-)")
  (net 13 "unconnected-(U1-USB-D+-PadD+)")
  (net 14 "unconnected-(U1-USB-GND-PadUG)")
  (net 15 "unconnected-(U1-BAT-Pad2)")
  (net 16 "unconnected-(U1-Vsh-Pad3)")
  (net 17 "unconnected-(U2-GND-Pad17)")
  (net 18 "unconnected-(U2-PROGRAM-Pad18)")
  (net 19 "unconnected-(U2-ON_OFF-Pad19)")
  (net 20 "Net-(U2-13_SCK_CRX1_LED)")
  (net 21 "unconnected-(U2-3V3-Pad16)")
  (net 22 "unconnected-(U2-VBAT-Pad15)")
  (net 23 "Net-(U2-12_MISO_MQSL)")
  (net 24 "Net-(U2-14_A0_TX3_SPDIF_OUT)")
  (net 25 "unconnected-(U2-15_A1_RX3_SPDIF_IN-Pad22)")
  (net 26 "unconnected-(U2-16_A2_RX4_SCL1-Pad23)")
  (net 27 "unconnected-(U2-17_A3_TX4_SDA1-Pad24)")
  (net 28 "Net-(U2-18_A4_SDA0)")
  (net 29 "Net-(U2-19_A5_SCL0)")
  (net 30 "unconnected-(U2-20_A6_TX5_LRCLK1-Pad27)")
  (net 31 "unconnected-(U2-21_A7_RX5_BCLK1-Pad28)")
  (net 32 "unconnected-(U2-22_A8_CTX1-Pad29)")
  (net 33 "unconnected-(U2-23_A9_CRX1_MCLK1-Pad30)")
  (net 34 "unconnected-(U2-VUSB-Pad34)")
  (net 35 "Net-(U2-11_MOSI_CTX1)")
  (net 36 "unconnected-(U2-10_CS_MQSR-Pad12)")
  (net 37 "Net-(U2-9_OUT1C)")
  (net 38 "unconnected-(U2-8_TX2_IN1-Pad10)")
  (net 39 "Net-(U2-6_OUT1D)")
  (net 40 "Net-(U2-7_RX2_OUT1A)")
  (net 41 "Net-(U2-5_IN2)")
  (net 42 "unconnected-(U2-3_LRCLK2-Pad5)")
  (net 43 "unconnected-(U2-2_OUT2-Pad4)")
  (net 44 "unconnected-(U2-1_TX1_CTX2_MISO1-Pad3)")
  (net 45 "unconnected-(U2-0_RX1_CRX2_CS1-Pad2)")
  (net 46 "unconnected-(U2-24_A10_TX6_SCL2-Pad35)")
  (net 47 "unconnected-(U2-25_A11_RX6_SDA2-Pad36)")
  (net 48 "unconnected-(U2-26_A12_MOSI1-Pad37)")
  (net 49 "unconnected-(U2-27_A13_SCK1-Pad38)")
  (net 50 "unconnected-(U2-28_RX7-Pad39)")
  (net 51 "unconnected-(U2-29_TX7-Pad40)")
  (net 52 "unconnected-(U2-30_CRX3-Pad41)")
  (net 53 "unconnected-(U2-31_CTX3-Pad42)")
  (net 54 "unconnected-(U2-32_OUT1B-Pad43)")
  (net 55 "unconnected-(U2-33_MCLK2-Pad44)")
  (net 56 "unconnected-(U4-T_IRQ-Pad14)")
  (net 57 "unconnected-(U4-SD_CS-Pad15)")
  (net 58 "unconnected-(U4-SD_MOSI-Pad16)")
  (net 59 "unconnected-(U4-SD_MISO-Pad17)")
  (net 60 "unconnected-(U4-SD_SCK-Pad18)")
  (net 61 "unconnected-(U3-ADR{slash}POCI-Pad5)")
  (net 62 "unconnected-(U3-INT1-Pad8)")
  (net 63 "unconnected-(U3-CS-Pad6)")
  (net 64 "unconnected-(U3-INT2-Pad7)")
  (net 65 "unconnected-(U5-IRQ-Pad8)")
  (footprint "MountingHole:MountingHole_2.7mm" (layer "F.Cu")
    (at 157.48 41.656)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "BATT-b" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.7mm" (layer "F.Cu")
    (at 157.48 82.296)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "BATT-d" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.7mm" (layer "F.Cu")
    (at 104.14 82.296)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "BATT-c" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MJC:BMA400" (layer "F.Cu")
    (at 144.272 101.6 180)
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "BMA400" (at 0 -2.286 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -6.35 11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -3.81 11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q2-E)") (pinfunction "3V3") (pintype "power_in"))
    (pad "3" thru_hole circle (at -1.27 11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(U2-18_A4_SDA0)") (pinfunction "SDA/PICO") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 1.27 11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U2-19_A5_SCL0)") (pinfunction "SCL/SCK") (pintype "input"))
    (pad "5" thru_hole circle (at 3.81 11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(U3-ADR{slash}POCI-Pad5)") (pinfunction "ADR/POCI") (pintype "input+no_connect"))
    (pad "6" thru_hole circle (at 6.35 11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(U3-CS-Pad6)") (pinfunction "CS") (pintype "input+no_connect"))
    (pad "7" thru_hole circle (at -1.27 -11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(U3-INT2-Pad7)") (pinfunction "INT2") (pintype "output+no_connect"))
    (pad "8" thru_hole circle (at 1.27 -11.43 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(U3-INT1-Pad8)") (pinfunction "INT1") (pintype "output+no_connect"))
    (pad "9" thru_hole circle (at -10.16 -10.16 180) (size 3 3) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole circle (at 10.16 -10.16 180) (size 3 3) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "11" thru_hole circle (at 10.16 10.16 180) (size 3 3) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "12" thru_hole circle (at -10.16 10.16 180) (size 3 3) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_TopBottom" (layer "F.Cu")
    (at 162.56 36.83)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "PCB-b" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "F.Cu" "F.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "B.Cu" "B.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_TopBottom" (layer "F.Cu")
    (at 99.06 113.03)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "PCB-c" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "F.Cu" "F.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "B.Cu" "B.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_TopBottom" (layer "F.Cu")
    (at 162.56 113.03)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "PCB-d" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "F.Cu" "F.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "B.Cu" "B.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_TopBottom" (layer "F.Cu")
    (at 99.06 36.83)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "PCB-a" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "F.Cu" "F.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "B.Cu" "B.Mask")
      (net 1 "GNDREF") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.7mm" (layer "F.Cu")
    (at 104.14 41.656)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "BATT-a" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MJC:ILI9341" (layer "F.Cu")
    (at 130.81 74.7776)
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0 5.7404 unlocked) (layer "F.SilkS"))
    (fp_text value "Teensy ILI9341" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -16.51 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-5Vo)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole circle (at -13.97 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at -11.43 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(U2-14_A0_TX3_SPDIF_OUT)") (pinfunction "CS") (pintype "input"))
    (pad "4" thru_hole circle (at -8.89 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q2-E)") (pinfunction "RESET") (pintype "input"))
    (pad "5" thru_hole circle (at -6.35 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U2-9_OUT1C)") (pinfunction "DC") (pintype "input"))
    (pad "6" thru_hole circle (at -3.81 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U2-11_MOSI_CTX1)") (pinfunction "SDI(MOSI)") (pintype "input"))
    (pad "7" thru_hole circle (at -1.27 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U2-13_SCK_CRX1_LED)") (pinfunction "SCK") (pintype "input"))
    (pad "8" thru_hole circle (at 1.27 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-5Vo)") (pinfunction "LED") (pintype "input"))
    (pad "9" thru_hole circle (at 3.81 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U2-12_MISO_MQSL)") (pinfunction "SDO(MISO)") (pintype "output"))
    (pad "10" thru_hole circle (at 6.35 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U2-13_SCK_CRX1_LED)") (pinfunction "T_CLK") (pintype "input"))
    (pad "11" thru_hole circle (at 8.89 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(U2-5_IN2)") (pinfunction "T_CS") (pintype "input"))
    (pad "12" thru_hole circle (at 11.43 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U2-11_MOSI_CTX1)") (pinfunction "T_DIN") (pintype "input"))
    (pad "13" thru_hole circle (at 13.97 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U2-12_MISO_MQSL)") (pinfunction "T_DO") (pintype "output"))
    (pad "14" thru_hole circle (at 16.51 42.7482) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(U4-T_IRQ-Pad14)") (pinfunction "T_IRQ") (pintype "output+no_connect"))
    (pad "15" thru_hole circle (at -3.81 -41.7576) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(U4-SD_CS-Pad15)") (pinfunction "SD_CS") (pintype "no_connect"))
    (pad "16" thru_hole circle (at -1.27 -41.7576) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(U4-SD_MOSI-Pad16)") (pinfunction "SD_MOSI") (pintype "no_connect"))
    (pad "17" thru_hole circle (at 1.27 -41.7576) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(U4-SD_MISO-Pad17)") (pinfunction "SD_MISO") (pintype "no_connect"))
    (pad "18" thru_hole circle (at 3.81 -41.7576) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "unconnected-(U4-SD_SCK-Pad18)") (pinfunction "SD_SCK") (pintype "no_connect"))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "B.Cu")
    (at 123.3497 99.568 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -6.35) (layer "B.SilkS"))
    (fp_text value "2N3904" (at 1.27 -2.79) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q1-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(Q1-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "B.Cu")
    (at 154.94 33.02 180)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 3.556 1.33) (layer "B.SilkS"))
    (fp_text value "USB VIN" (at 0 -2.33) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "B.Cu")
    (at 119.5397 89.408 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at -3.81 0.92) (layer "B.SilkS"))
    (fp_text value "2K2" (at 2.54 -1.92) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(Q1-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "B.Cu")
    (at 119.5397 112.014 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 8.636 0.92) (layer "B.SilkS"))
    (fp_text value "1M" (at 2.54 -1.92) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-LBO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-5Vo)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "B.Cu")
    (at 119.5397 107.442 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 8.636 0) (layer "B.SilkS"))
    (fp_text value "470K" (at 2.54 -1.92) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-LBO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MJC:PowerBoost1000C" (layer "B.Cu")
    (at 119.888 60.96 180)
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0 19.05) (layer "B.SilkS"))
    (fp_text value "Powerboost1000C" (at 0 -19.05) (layer "B.Fab"))
    (fp_text user "PowerBoost 1000C" (at -0.08 0) (layer "B.SilkS"))
    (pad "1" thru_hole rect (at -10.16 5.08 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_1)") (pinfunction "USB") (pintype "power_in"))
    (pad "2" thru_hole circle (at -10.16 2.54 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(U1-BAT-Pad2)") (pinfunction "BAT") (pintype "power_in+no_connect"))
    (pad "3" thru_hole circle (at -10.16 0 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(U1-Vsh-Pad3)") (pinfunction "Vsh") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at -10.16 -2.54 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J2-Pin_1)") (pinfunction "EN") (pintype "input"))
    (pad "5" thru_hole circle (at -10.16 -5.08 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "GND") (pintype "passive"))
    (pad "5V" thru_hole circle (at -3.81 -12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(U1-USB-5V-Pad5V)") (pinfunction "USB-5V") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at -10.16 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-LBO)") (pinfunction "LBO") (pintype "output"))
    (pad "7" thru_hole circle (at -10.16 -10.16 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "G") (pintype "passive"))
    (pad "8" thru_hole circle (at -10.16 -12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-5Vo)") (pinfunction "5Vo") (pintype "power_out"))
    (pad "D+" thru_hole circle (at 1.27 -12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(U1-USB-D+-PadD+)") (pinfunction "USB-D+") (pintype "passive+no_connect"))
    (pad "D-" thru_hole circle (at -1.27 -12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U1-USB-D--PadD-)") (pinfunction "USB-D-") (pintype "passive+no_connect"))
    (pad "UG" thru_hole circle (at 3.81 -12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(U1-USB-GND-PadUG)") (pinfunction "USB-GND") (pintype "passive+no_connect"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.0_Assembly.STEP"
      (offset (xyz 33 9.5 -11))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "B.Cu")
    (at 119.5397 84.328 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at -3.81 1.016) (layer "B.SilkS"))
    (fp_text value "2K2" (at 2.54 -1.92) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q2-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "B.Cu")
    (at 113.1897 99.674 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -6.244) (layer "B.SilkS"))
    (fp_text value "2N3906" (at 1.27 -2.79) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q2-E)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q2-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q2-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "B.Cu")
    (at 119.5397 94.488 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at -4.064 1.016) (layer "B.SilkS"))
    (fp_text value "22K" (at 2.54 -1.92) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(Q1-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q2-E)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (at 119.38 33.02 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 1.778 -6.604) (layer "B.SilkS"))
    (fp_text value "DISABLE SW" (at -3.302 -1.275) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RF_Module:nRF24L01_Breakout" (layer "B.Cu")
    (at 104.14 93.472 180)
    (descr "nRF24L01 breakout board")
    (tags "nRF24L01 adapter breakout")
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ultra low power 2.4GHz RF Transceiver, Carrier PCB")
    (property "ki_keywords" "Low Power RF Transceiver breakout carrier")
    (attr through_hole)
    (fp_text reference "U5" (at 0.508 4.064) (layer "B.SilkS"))
    (fp_text value "NRF24L01_Breakout" (at 13 -5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 12.5 -2.5) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q2-E)") (pinfunction "VCC") (pintype "power_in"))
    (pad "3" thru_hole circle (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(U2-7_RX2_OUT1A)") (pinfunction "CE") (pintype "input"))
    (pad "4" thru_hole circle (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(U2-6_OUT1D)") (pinfunction "~{CSN}") (pintype "input"))
    (pad "5" thru_hole circle (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U2-13_SCK_CRX1_LED)") (pinfunction "SCK") (pintype "input"))
    (pad "6" thru_hole circle (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U2-11_MOSI_CTX1)") (pinfunction "MOSI") (pintype "input"))
    (pad "7" thru_hole circle (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U2-12_MISO_MQSL)") (pinfunction "MISO") (pintype "output"))
    (pad "8" thru_hole circle (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(U5-IRQ-Pad8)") (pinfunction "IRQ") (pintype "output+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/RF_Module.3dshapes/nRF24L01_Breakout.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "teensy:Teensy40" (layer "B.Cu")
    (at 145.034 68.58 -90)
    (property "Sheetfile" "Teensy-RV-Leveling-Helper-Pair-Compact.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -22.86 9.398) (layer "B.SilkS"))
    (fp_text value "Teensy4.0" (at 0 -10.16 90) (layer "B.Fab"))
    (fp_text user "DVL6A" (at 1.778 0) (layer "B.SilkS"))
    (fp_text user "MIMXRT1062" (at 0.254 0) (layer "B.SilkS"))
    (pad "1" thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U2-0_RX1_CRX2_CS1-Pad2)") (pinfunction "0_RX1_CRX2_CS1") (pintype "bidirectional+no_connect"))
    (pad "3" thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U2-1_TX1_CTX2_MISO1-Pad3)") (pinfunction "1_TX1_CTX2_MISO1") (pintype "bidirectional+no_connect"))
    (pad "4" thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U2-2_OUT2-Pad4)") (pinfunction "2_OUT2") (pintype "bidirectional+no_connect"))
    (pad "5" thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U2-3_LRCLK2-Pad5)") (pinfunction "3_LRCLK2") (pintype "bidirectional+no_connect"))
    (pad "6" thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q2-C)") (pinfunction "4_BCLK2") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(U2-5_IN2)") (pinfunction "5_IN2") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(U2-6_OUT1D)") (pinfunction "6_OUT1D") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(U2-7_RX2_OUT1A)") (pinfunction "7_RX2_OUT1A") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U2-8_TX2_IN1-Pad10)") (pinfunction "8_TX2_IN1") (pintype "bidirectional+no_connect"))
    (pad "11" thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U2-9_OUT1C)") (pinfunction "9_OUT1C") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U2-10_CS_MQSR-Pad12)") (pinfunction "10_CS_MQSR") (pintype "bidirectional+no_connect"))
    (pad "13" thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U2-11_MOSI_CTX1)") (pinfunction "11_MOSI_CTX1") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U2-12_MISO_MQSL)") (pinfunction "12_MISO_MQSL") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 16.51 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(U2-VBAT-Pad15)") (pinfunction "VBAT") (pintype "power_in+no_connect"))
    (pad "16" thru_hole circle (at 16.51 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(U2-3V3-Pad16)") (pinfunction "3V3") (pintype "power_in+no_connect"))
    (pad "17" thru_hole circle (at 16.51 0 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(U2-GND-Pad17)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "18" thru_hole circle (at 16.51 2.54 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(U2-PROGRAM-Pad18)") (pinfunction "PROGRAM") (pintype "input+no_connect"))
    (pad "19" thru_hole circle (at 16.51 5.08 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(U2-ON_OFF-Pad19)") (pinfunction "ON_OFF") (pintype "input+no_connect"))
    (pad "20" thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U2-13_SCK_CRX1_LED)") (pinfunction "13_SCK_CRX1_LED") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(U2-14_A0_TX3_SPDIF_OUT)") (pinfunction "14_A0_TX3_SPDIF_OUT") (pintype "bidirectional"))
    (pad "22" thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U2-15_A1_RX3_SPDIF_IN-Pad22)") (pinfunction "15_A1_RX3_SPDIF_IN") (pintype "bidirectional+no_connect"))
    (pad "23" thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U2-16_A2_RX4_SCL1-Pad23)") (pinfunction "16_A2_RX4_SCL1") (pintype "bidirectional+no_connect"))
    (pad "24" thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(U2-17_A3_TX4_SDA1-Pad24)") (pinfunction "17_A3_TX4_SDA1") (pintype "bidirectional+no_connect"))
    (pad "25" thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(U2-18_A4_SDA0)") (pinfunction "18_A4_SDA0") (pintype "bidirectional"))
    (pad "26" thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U2-19_A5_SCL0)") (pinfunction "19_A5_SCL0") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U2-20_A6_TX5_LRCLK1-Pad27)") (pinfunction "20_A6_TX5_LRCLK1") (pintype "bidirectional+no_connect"))
    (pad "28" thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(U2-21_A7_RX5_BCLK1-Pad28)") (pinfunction "21_A7_RX5_BCLK1") (pintype "bidirectional+no_connect"))
    (pad "29" thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(U2-22_A8_CTX1-Pad29)") (pinfunction "22_A8_CTX1") (pintype "bidirectional+no_connect"))
    (pad "30" thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 33 "unconnected-(U2-23_A9_CRX1_MCLK1-Pad30)") (pinfunction "23_A9_CRX1_MCLK1") (pintype "bidirectional+no_connect"))
    (pad "31" thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q2-E)") (pinfunction "3V3") (pintype "power_out"))
    (pad "32" thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "33" thru_hole circle (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-5Vo)") (pinfunction "VIN") (pintype "power_in"))
    (pad "34" thru_hole circle (at -13.97 5.08 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U2-VUSB-Pad34)") (pinfunction "VUSB") (pintype "power_out+no_connect"))
    (pad "35" thru_hole circle (at 11.43 5.08 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(U2-24_A10_TX6_SCL2-Pad35)") (pinfunction "24_A10_TX6_SCL2") (pintype "bidirectional+no_connect"))
    (pad "36" thru_hole circle (at 8.89 5.08 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(U2-25_A11_RX6_SDA2-Pad36)") (pinfunction "25_A11_RX6_SDA2") (pintype "bidirectional+no_connect"))
    (pad "37" thru_hole circle (at 11.43 2.54 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(U2-26_A12_MOSI1-Pad37)") (pinfunction "26_A12_MOSI1") (pintype "bidirectional+no_connect"))
    (pad "38" thru_hole circle (at 8.89 2.54 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U2-27_A13_SCK1-Pad38)") (pinfunction "27_A13_SCK1") (pintype "bidirectional+no_connect"))
    (pad "39" thru_hole circle (at 11.43 0 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(U2-28_RX7-Pad39)") (pinfunction "28_RX7") (pintype "bidirectional+no_connect"))
    (pad "40" thru_hole circle (at 8.89 0 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(U2-29_TX7-Pad40)") (pinfunction "29_TX7") (pintype "bidirectional+no_connect"))
    (pad "41" thru_hole circle (at 11.43 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(U2-30_CRX3-Pad41)") (pinfunction "30_CRX3") (pintype "bidirectional+no_connect"))
    (pad "42" thru_hole circle (at 8.89 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(U2-31_CTX3-Pad42)") (pinfunction "31_CTX3") (pintype "bidirectional+no_connect"))
    (pad "43" thru_hole circle (at 11.43 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(U2-32_OUT1B-Pad43)") (pinfunction "32_OUT1B") (pintype "bidirectional+no_connect"))
    (pad "44" thru_hole circle (at 8.89 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(U2-33_MCLK2-Pad44)") (pinfunction "33_MCLK2") (pintype "bidirectional+no_connect"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.0_Assembly.STEP"
      (offset (xyz 33 9.5 -11))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_line (start 92.71 25.4) (end 168.91 25.4)
    (layer "Edge.Cuts"))
  (gr_line (start 168.91 121.92) (end 92.71 121.92)
    (layer "Edge.Cuts"))
  (gr_line (start 92.71 121.92) (end 92.71 25.4)
    (layer "Edge.Cuts"))
  (gr_line (start 168.91 25.4) (end 168.91 121.92)
    (layer "Edge.Cuts"))
  (gr_text "TEENSY 4.0" (at 140.716 48.768) (layer "B.SilkS"))
  (gr_text "470K" (at 112.681656 109.728) (layer "B.SilkS"))
  (gr_text "22K" (at 124.873656 96.012) (layer "B.SilkS"))
  (gr_text "Teensy-RV-Leveling-Helper-Pair - Mark J Culross (KD5RXT) 20231226" (at 167.894 28.702) (layer "B.SilkS"))
  (gr_text "USB VIN" (at 146.304 34.036) (layer "B.SilkS"))
  (gr_text "1M" (at 111.919656 113.792) (layer "B.SilkS"))
  (gr_text "BMA400\n(NOTE: this device is mounted with\nthe top of the device PCB facing\nthe bottom of the main PCB)" (at 144.78 105.156) (layer "B.SilkS"))
  (gr_text "2N3904" (at 125.381656 104.394) (layer "B.SilkS"))
  (gr_text "U3" (at 145.542 97.536) (layer "B.SilkS"))
  (gr_text "2N3906" (at 115.079656 104.648) (layer "B.SilkS"))
  (gr_text "	" (at 154.178 28.702) (layer "B.SilkS"))
  (gr_text "2K2" (at 124.873656 85.852) (layer "B.SilkS"))
  (gr_text "DISABLE SW" (at 113.284 33.528) (layer "B.SilkS"))
  (gr_text "2K2" (at 124.873656 90.932) (layer "B.SilkS"))
  (gr_text "NRF24L01" (at 101.6 89.916) (layer "B.SilkS"))
  (gr_text "Teensy-RV-Leveling-Helper-Pair - Mark J Culross (KD5RXT) 20231226" (at 93.726 28.702) (layer "F.SilkS"))
  (gr_text "ILI9341" (at 128.778 83.058) (layer "F.SilkS"))
)
