<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>20</text>
<text>CW Wound</text>
<wire x1="0" y1="0" x2="0" y2="10.0584" width="0.0254" layer="20"/>
<wire x1="0" y1="10.0584" x2="32.766" y2="10.0584" width="0.0254" layer="20"/>
<wire x1="32.766" y1="10.0584" x2="32.766" y2="0" width="0.0254" layer="20"/>
<wire x1="32.766" y1="0" x2="0" y2="0" width="0.0254" layer="20"/>
</plain>
<libraries>
<library name="CONRADS">
<packages>
<package name="HRS_U.FL-R-SMT-1(10)">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="CONRADS" package="HRS_U.FL-R-SMT-1(10)" value="U.FL-R-SMT-1(10)">
<attribute name="DESCRIPTION" value=" U.FL Series 6 Ghz 50 Ohm Ultra-small SMT Coaxial Cable Receptacle "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="H11891CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/hirose-electric-co-ltd/U.FL-R-SMT-1_10_/H11891CT-ND/2504612?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Hirose"/>
<attribute name="MP" value="U.FL-R-SMT-1_10_"/>
<attribute name="PACKAGE" value="None"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
