(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 211)
    (no_connects 0)
    (area 138.006667 62.065 162.469524 135.085)
    (thickness 1.6)
    (drawings 156)
    (tracks 1464)
    (zones 0)
    (modules 58)
    (nets 80)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.16)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.15)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFE7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 /Controller/VCAP1)
  (net 2 GND)
  (net 3 /Controller/VCAP2)
  (net 4 /Controller/PH0)
  (net 5 /Controller/PH1)
  (net 6 2V8)
  (net 7 VCC)
  (net 8 "Net-(Q1-Pad1)")
  (net 9 "Net-(Q1-Pad3)")
  (net 10 "Net-(Q2-Pad1)")
  (net 11 "Net-(Q2-Pad3)")
  (net 12 "Net-(JP1-Pad2)")
  (net 13 "Net-(JP2-Pad2)")
  (net 14 "Net-(R10-Pad2)")
  (net 15 "Net-(R11-Pad2)")
  (net 16 "Net-(D3-Pad1)")
  (net 17 /Controller/VDDA)
  (net 18 VBAT)
  (net 19 NRST)
  (net 20 PA13)
  (net 21 PA14)
  (net 22 PB3)
  (net 23 PA15)
  (net 24 PA10)
  (net 25 PA11)
  (net 26 PA12)
  (net 27 PC13)
  (net 28 PC14)
  (net 29 PC15)
  (net 30 PC0)
  (net 31 PC1)
  (net 32 PC2)
  (net 33 PC3)
  (net 34 PA0)
  (net 35 PA1)
  (net 36 PA2)
  (net 37 PA3)
  (net 38 PA4)
  (net 39 PA5)
  (net 40 PA6)
  (net 41 PA7)
  (net 42 PC4)
  (net 43 PC5)
  (net 44 PB0)
  (net 45 PB1)
  (net 46 PB2)
  (net 47 PB10)
  (net 48 PB11)
  (net 49 PB12)
  (net 50 PB13)
  (net 51 PB14)
  (net 52 PB15)
  (net 53 PC6)
  (net 54 PC7)
  (net 55 PC8)
  (net 56 PC9)
  (net 57 PA8)
  (net 58 PC10)
  (net 59 PC11)
  (net 60 PC12)
  (net 61 PD2)
  (net 62 PB4)
  (net 63 PB5)
  (net 64 PB6)
  (net 65 PB7)
  (net 66 BOOT0)
  (net 67 PB8)
  (net 68 PB9)
  (net 69 RAIL_R)
  (net 70 RAIL_L)
  (net 71 +5V)
  (net 72 PA9)
  (net 73 MOT+)
  (net 74 TRAIN_I)
  (net 75 MOT-)
  (net 76 "Net-(J7-Pad6)")
  (net 77 REAR-)
  (net 78 FRONT-)
  (net 79 "Net-(R13-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Controller/PH0)
    (add_net /Controller/PH1)
    (add_net /Controller/VCAP1)
    (add_net /Controller/VCAP2)
    (add_net BOOT0)
    (add_net FRONT-)
    (add_net NRST)
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net PA0)
    (add_net PA1)
    (add_net PA10)
    (add_net PA11)
    (add_net PA12)
    (add_net PA13)
    (add_net PA14)
    (add_net PA15)
    (add_net PA2)
    (add_net PA3)
    (add_net PA4)
    (add_net PA5)
    (add_net PA6)
    (add_net PA7)
    (add_net PA8)
    (add_net PA9)
    (add_net PB0)
    (add_net PB1)
    (add_net PB10)
    (add_net PB11)
    (add_net PB12)
    (add_net PB13)
    (add_net PB14)
    (add_net PB15)
    (add_net PB2)
    (add_net PB3)
    (add_net PB4)
    (add_net PB5)
    (add_net PB6)
    (add_net PB7)
    (add_net PB8)
    (add_net PB9)
    (add_net PC0)
    (add_net PC1)
    (add_net PC10)
    (add_net PC11)
    (add_net PC12)
    (add_net PC13)
    (add_net PC14)
    (add_net PC15)
    (add_net PC2)
    (add_net PC3)
    (add_net PC4)
    (add_net PC5)
    (add_net PC6)
    (add_net PC7)
    (add_net PC8)
    (add_net PC9)
    (add_net PD2)
    (add_net REAR-)
    (add_net TRAIN_I)
  )
  (net_class Motor ""
    (clearance 0.16)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net MOT+)
    (add_net MOT-)
    (add_net RAIL_L)
    (add_net RAIL_R)
  )
  (net_class Power ""
    (clearance 0.16)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /Controller/VDDA)
    (add_net 2V8)
    (add_net GND)
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad3)")
    (add_net VBAT)
    (add_net VCC)
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB7DC)
    (at 144.5 66 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 20 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 PC13))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB7CA)
    (at 154.75 76.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 16 (at 0 0 360) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 PB9))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_GH_BM04B-GHS-TBT_04x1.25mm_Straight (layer F.Cu) (tedit 58DDB8BC)
    (at 150 120)
    (descr "JST GH series connector, BM04B-GHS-TBT, top entry type")
    (tags "connector jst GH SMT top vertical entry 1.25mm pitch")
    (attr smd)
    (fp_text reference J8 (at 0 0.5) (layer F.SilkS))
    (fp_text value IR (at 0 4.575) (layer F.Fab))
    (fp_text user %R (at 0 1.825) (layer F.Fab))
    (pad 1 smd rect (at -1.875 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at -0.625 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 44 PB0))
    (pad 3 smd rect (at 0.625 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 45 PB1))
    (pad 4 smd rect (at 1.875 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" smd rect (at 3.6 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.6 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module bcan:USB_Micro-B_Amphenol_10118192 (layer F.Cu) (tedit 58DC8B98)
    (at 150 130.55)
    (fp_text reference J4 (at 0 -1.3) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 3.5) (layer F.Fab))
    (fp_text user "PCB END" (at 0 1.8) (layer Dwgs.User))
    (pad 3 smd rect (at 0 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 25 PA11))
    (pad 4 smd rect (at 0.65 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 26 PA12))
    (pad 2 smd rect (at -0.65 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 24 PA10))
    (pad 1 smd rect (at -1.3 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 71 +5V))
    (pad 5 smd rect (at 1.3 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -3.15 -2.55) (size 2.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.15 -2.55) (size 2.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1.2 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.2 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.8 0) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -3.8 0) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Housings_QFP:TQFP-64_10x10mm_Pitch0.5mm (layer F.Cu) (tedit 58DDB90B)
    (at 150 100 315)
    (descr "64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 0 315) (layer F.SilkS))
    (fp_text value STM32F405RGTx (at 0 7.45 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -3.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 VBAT))
    (pad 2 smd rect (at -5.7 -3.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 PC13))
    (pad 3 smd rect (at -5.7 -2.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 PC14))
    (pad 4 smd rect (at -5.7 -2.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 PC15))
    (pad 5 smd rect (at -5.7 -1.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /Controller/PH0))
    (pad 6 smd rect (at -5.7 -1.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /Controller/PH1))
    (pad 7 smd rect (at -5.7 -0.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 NRST))
    (pad 8 smd rect (at -5.7 -0.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 PC0))
    (pad 9 smd rect (at -5.7 0.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 PC1))
    (pad 10 smd rect (at -5.7 0.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 PC2))
    (pad 11 smd rect (at -5.7 1.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 PC3))
    (pad 12 smd rect (at -5.7 1.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -5.7 2.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Controller/VDDA))
    (pad 14 smd rect (at -5.7 2.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 PA0))
    (pad 15 smd rect (at -5.7 3.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 PA1))
    (pad 16 smd rect (at -5.7 3.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 PA2))
    (pad 17 smd rect (at -3.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 PA3))
    (pad 18 smd rect (at -3.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at -2.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 20 smd rect (at -2.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 PA4))
    (pad 21 smd rect (at -1.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 PA5))
    (pad 22 smd rect (at -1.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 PA6))
    (pad 23 smd rect (at -0.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 PA7))
    (pad 24 smd rect (at -0.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 PC4))
    (pad 25 smd rect (at 0.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 PC5))
    (pad 26 smd rect (at 0.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 PB0))
    (pad 27 smd rect (at 1.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 PB1))
    (pad 28 smd rect (at 1.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 PB2))
    (pad 29 smd rect (at 2.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 PB10))
    (pad 30 smd rect (at 2.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 PB11))
    (pad 31 smd rect (at 3.25 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /Controller/VCAP1))
    (pad 32 smd rect (at 3.75 5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 33 smd rect (at 5.7 3.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 PB12))
    (pad 34 smd rect (at 5.7 3.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 PB13))
    (pad 35 smd rect (at 5.7 2.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 PB14))
    (pad 36 smd rect (at 5.7 2.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 PB15))
    (pad 37 smd rect (at 5.7 1.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 PC6))
    (pad 38 smd rect (at 5.7 1.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 PC7))
    (pad 39 smd rect (at 5.7 0.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 PC8))
    (pad 40 smd rect (at 5.7 0.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 PC9))
    (pad 41 smd rect (at 5.7 -0.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 PA8))
    (pad 42 smd rect (at 5.7 -0.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 PA9))
    (pad 43 smd rect (at 5.7 -1.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 PA10))
    (pad 44 smd rect (at 5.7 -1.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 PA11))
    (pad 45 smd rect (at 5.7 -2.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 PA12))
    (pad 46 smd rect (at 5.7 -2.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 PA13))
    (pad 47 smd rect (at 5.7 -3.25 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /Controller/VCAP2))
    (pad 48 smd rect (at 5.7 -3.75 315) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 49 smd rect (at 3.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 PA14))
    (pad 50 smd rect (at 3.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 PA15))
    (pad 51 smd rect (at 2.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 PC10))
    (pad 52 smd rect (at 2.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 PC11))
    (pad 53 smd rect (at 1.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 PC12))
    (pad 54 smd rect (at 1.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 PD2))
    (pad 55 smd rect (at 0.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 PB3))
    (pad 56 smd rect (at 0.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 PB4))
    (pad 57 smd rect (at -0.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 PB5))
    (pad 58 smd rect (at -0.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 PB6))
    (pad 59 smd rect (at -1.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 PB7))
    (pad 60 smd rect (at -1.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 BOOT0))
    (pad 61 smd rect (at -2.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 67 PB8))
    (pad 62 smd rect (at -2.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 PB9))
    (pad 63 smd rect (at -3.25 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 64 smd rect (at -3.75 -5.7 45) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (model Housings_QFP.3dshapes/TQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D80199)
    (at 144.25 86.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 0 270) (layer F.SilkS))
    (fp_text value 13k3 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 PC2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D8019F)
    (at 144.25 87.75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2k8 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 PC2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58D803D2)
    (at 148.5 125)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at 0 0 180) (layer F.SilkS))
    (fp_text value SPX3819M5 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R13-Pad2)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB80F)
    (at 144 130.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 12 (at 0 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58D8065F)
    (at 144.75 69.75)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 0 180) (layer F.SilkS))
    (fp_text value MMBT2222A (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58D80662)
    (at 144.75 73.25 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference Q4 (at 0 0 180) (layer F.SilkS))
    (fp_text value DMG6601LVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 75 MOT-))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 75 MOT-))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB7CE)
    (at 156.25 76.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 15 (at 0 0 360) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 PB8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm_SMD (layer B.Cu) (tedit 58DB292C)
    (at 150 90 180)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J3 (at 0 0 180) (layer B.SilkS))
    (fp_text value JTAG (at 0 -4.235 180) (layer B.Fab))
    (fp_text user %R (at 0 4.235 180) (layer B.Fab))
    (pad 1 smd rect (at -1.95 2.54 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 1.95 2.54 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 20 PA13))
    (pad 3 smd rect (at -1.95 1.27 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.95 1.27 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 21 PA14))
    (pad 5 smd rect (at -1.95 0 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1.95 0 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 22 PB3))
    (pad 7 smd rect (at -1.95 -1.27 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 1.95 -1.27 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 23 PA15))
    (pad 9 smd rect (at -1.95 -2.54 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 1.95 -2.54 180) (size 2.4 0.75) (layers B.Cu B.Paste B.Mask)
      (net 19 NRST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch1.27mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-8_4.4x3mm_Pitch0.65mm (layer F.Cu) (tedit 58D8063B)
    (at 153 112 180)
    (descr "8-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 0 360) (layer F.SilkS))
    (fp_text value M95512-RDW6TP (at 0 2.55 180) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 PB12))
    (pad 2 smd rect (at -2.95 -0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 PB14))
    (pad 3 smd rect (at -2.95 0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R11-Pad2)"))
    (pad 4 smd rect (at -2.95 0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.95 0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 PB15))
    (pad 6 smd rect (at 2.95 0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 PB13))
    (pad 7 smd rect (at 2.95 -0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R10-Pad2)"))
    (pad 8 smd rect (at 2.95 -0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (model Housings_SSOP.3dshapes/TSSOP-8_4.4x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm (layer F.Cu) (tedit 58D80613)
    (at 147 90.25 135)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 0 405) (layer F.SilkS))
    (fp_text value 16MHz (at 0 2.45 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 135) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /Controller/PH0))
    (pad 2 smd rect (at 1.1 0.85 135) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.1 -0.85 135) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /Controller/PH1))
    (pad 4 smd rect (at -1.1 -0.85 135) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_3225-4pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58D80653)
    (at 151.75 71.5 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R17 (at 0 0 360) (layer F.SilkS))
    (fp_text value 100 (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.6 270) (layer F.Fab))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58D8064F)
    (at 148.25 71.5 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R18 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100 (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.6 90) (layer F.Fab))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58D80657)
    (at 155.25 73.25 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 0 360) (layer F.SilkS))
    (fp_text value MMBT2222A (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58D8065B)
    (at 155.25 69.75 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference Q3 (at 0 0 360) (layer F.SilkS))
    (fp_text value DMG6601LVT (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 73 MOT+))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 73 MOT+))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D805DE)
    (at 147.5 108.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2u2 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /Controller/VCAP1))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D805F3)
    (at 155.5 109)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2u2 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /Controller/VCAP2))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D8042A)
    (at 152 90.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D80624)
    (at 148.25 88.25 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 0 225) (layer F.SilkS))
    (fp_text value 10p (at 0 1.5 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 135) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /Controller/PH0))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D80619)
    (at 145 91.5 315)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 0 405) (layer F.SilkS))
    (fp_text value 10p (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /Controller/PH1))
    (pad 2 smd rect (at 0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D805FF)
    (at 143.75 104.5 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 0 225) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 135) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D805CF)
    (at 147.5 109.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D806A6)
    (at 156.25 107 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 0 360) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58DDB7C2)
    (at 152 92)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference 10 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58DDB7BB)
    (at 144 92.5 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference 11 (at 0 0 225) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 135) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /Controller/VDDA))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58DDB7B6)
    (at 145.75 93.5 45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference 12 (at 0 0 135) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /Controller/VDDA))
    (pad 2 smd rect (at 0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58DDB80A)
    (at 154.25 125.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference 13 (at 0 0 360) (layer F.SilkS))
    (fp_text value 2u2 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer F.Cu) (tedit 58D802FD)
    (at 145.5 125 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 0 360) (layer F.SilkS))
    (fp_text value CUS08F30 (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 +5V))
    (model Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D8062D)
    (at 154.75 78.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(JP1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D805E8)
    (at 149.5 115 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(JP2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D80431)
    (at 152 89 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 NRST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D80218)
    (at 147.5 115.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 0 270) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 PB10))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D80251)
    (at 147.5 114 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 PB11))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB799)
    (at 147.5 112.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 10 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB7EC)
    (at 156.25 104.5 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 11 (at 0 0 315) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB803)
    (at 151.25 125.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 13 (at 0 0 360) (layer F.SilkS))
    (fp_text value 33k2 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB805)
    (at 152.75 125.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 14 (at 0 0 180) (layer F.SilkS))
    (fp_text value 26k1 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R13-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58DDB7D5)
    (at 155.5 66 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 19 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 RAIL_R))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D85D19)
    (at 147.5 111)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 0 90) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm_SMD (layer B.Cu) (tedit 58CD4EC5)
    (at 150 71.5 90)
    (descr "surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x04 2.54mm double row")
    (attr smd)
    (fp_text reference J7 (at 0 0 180) (layer B.SilkS))
    (fp_text value TRAIN (at 0 -6.14 90) (layer B.Fab))
    (fp_text user %R (at 0 6.14 90) (layer B.Fab))
    (pad 1 smd rect (at -2.77 3.81 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 69 RAIL_R))
    (pad 2 smd rect (at 2.77 3.81 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 73 MOT+))
    (pad 3 smd rect (at -2.77 1.27 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 74 TRAIN_I))
    (pad 4 smd rect (at 2.77 1.27 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 77 REAR-))
    (pad 5 smd rect (at -2.77 -1.27 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 78 FRONT-))
    (pad 6 smd rect (at 2.77 -1.27 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J7-Pad6)"))
    (pad 7 smd rect (at -2.77 -3.81 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 75 MOT-))
    (pad 8 smd rect (at 2.77 -3.81 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 70 RAIL_L))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SOP-4_4.4x2.8mm_Pitch1.27mm (layer F.Cu) (tedit 58D9B96E)
    (at 149.25 66 180)
    (descr "4-Lead Plastic Small Outline http://www.vishay.com/docs/49633/sg2098.pdf")
    (tags "SOP 1.27")
    (attr smd)
    (fp_text reference U7 (at 0 0 180) (layer F.SilkS))
    (fp_text value TLP293 (at 1 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.4 180) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -0.64 180) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -3.15 0.64 180) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 70 RAIL_L))
    (pad 3 smd rect (at 3.15 0.64 180) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 3.15 -0.64 180) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 PC13))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D9A003)
    (at 143.75 95.5 45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 0 315) (layer F.SilkS))
    (fp_text value 600 (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at 0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /Controller/VDDA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-523 (layer F.Cu) (tedit 58D9B967)
    (at 154 66 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D3 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.7 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 70 RAIL_L))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D3-Pad1)"))
  )
  (module bcan:TO-269AA (layer F.Cu) (tedit 58DDB84D)
    (at 150 78)
    (fp_text reference D1 (at 0 0) (layer F.SilkS))
    (fp_text value CDBHM240L-HF (at 0 3.5) (layer F.Fab))
    (fp_text user ~~ (at 1.25 -1.25) (layer F.SilkS))
    (fp_text user ~~ (at 1.25 1.25) (layer F.SilkS))
    (fp_text user - (at -1.25 1.25) (layer F.SilkS))
    (fp_text user + (at -1.25 -1.25) (layer F.SilkS))
    (pad 1 smd rect (at -3 -1.275) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at -3 1.275) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 3 1.275) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 69 RAIL_R))
    (pad 4 smd rect (at 3 -1.275) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 70 RAIL_L))
  )
  (module bcan:Castellations_1x32_Pitch2.00mm (layer F.Cu) (tedit 58DB3A91)
    (at 142 69)
    (fp_text reference J1 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value PIN[1..32] (at 0 64) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 VBAT))
    (pad 2 thru_hole oval (at 0 2) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 PC13))
    (pad 3 thru_hole oval (at 0 4) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 PC14))
    (pad 4 thru_hole oval (at 0 6) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 PC15))
    (pad 5 thru_hole oval (at 0 8) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 FRONT-))
    (pad 6 thru_hole oval (at 0 10) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 REAR-))
    (pad 7 thru_hole oval (at 0 12) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 NRST))
    (pad 8 thru_hole oval (at 0 14) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 PC0))
    (pad 9 thru_hole oval (at 0 16) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 PC1))
    (pad 10 thru_hole oval (at 0 18) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 PC2))
    (pad 11 thru_hole oval (at 0 20) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 PC3))
    (pad 12 thru_hole oval (at 0 22) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 2V8))
    (pad 13 thru_hole oval (at 0 24) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 2V8))
    (pad 14 thru_hole oval (at 0 26) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 PA0))
    (pad 15 thru_hole oval (at 0 28) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 PA1))
    (pad 16 thru_hole oval (at 0 30) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 PA2))
    (pad 17 thru_hole oval (at 0 32) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 PA3))
    (pad 18 thru_hole oval (at 0 34) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 19 thru_hole oval (at 0 36) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at 0 38) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 PA4))
    (pad 21 thru_hole oval (at 0 40) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 PA5))
    (pad 22 thru_hole oval (at 0 42) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 PA6))
    (pad 23 thru_hole oval (at 0 44) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 PA7))
    (pad 24 thru_hole oval (at 0 46) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 PC4))
    (pad 25 thru_hole oval (at 0 48) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 PC5))
    (pad 26 thru_hole oval (at 0 50) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 PB0))
    (pad 27 thru_hole oval (at 0 52) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 PB1))
    (pad 28 thru_hole oval (at 0 54) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 PB2))
    (pad 29 thru_hole oval (at 0 56) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 PB10))
    (pad 30 thru_hole oval (at 0 58) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 PB11))
    (pad 31 thru_hole oval (at 0 60) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 32 thru_hole oval (at 0 62) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 +5V))
  )
  (module bcan:Castellations_1x32_Pitch2.00mm (layer F.Cu) (tedit 58DB3A96)
    (at 158 131 180)
    (fp_text reference J2 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value PIN[33..64] (at 0 64 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 PB12))
    (pad 2 thru_hole oval (at 0 2 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 PB13))
    (pad 3 thru_hole oval (at 0 4 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 PB14))
    (pad 4 thru_hole oval (at 0 6 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 PB15))
    (pad 5 thru_hole oval (at 0 8 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 PC6))
    (pad 6 thru_hole oval (at 0 10 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 PC7))
    (pad 7 thru_hole oval (at 0 12 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 PC8))
    (pad 8 thru_hole oval (at 0 14 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 PC9))
    (pad 9 thru_hole oval (at 0 16 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 PA8))
    (pad 10 thru_hole oval (at 0 18 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 PA9))
    (pad 11 thru_hole oval (at 0 20 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 PA10))
    (pad 12 thru_hole oval (at 0 22 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 PA11))
    (pad 13 thru_hole oval (at 0 24 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 PA12))
    (pad 14 thru_hole oval (at 0 26 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 PA13))
    (pad 15 thru_hole oval (at 0 28 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 2V8))
    (pad 16 thru_hole oval (at 0 30 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 2V8))
    (pad 17 thru_hole oval (at 0 32 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 PA14))
    (pad 18 thru_hole oval (at 0 34 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 PA15))
    (pad 19 thru_hole oval (at 0 36 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 PC10))
    (pad 20 thru_hole oval (at 0 38 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 PC11))
    (pad 21 thru_hole oval (at 0 40 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 PC12))
    (pad 22 thru_hole oval (at 0 42 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 PD2))
    (pad 23 thru_hole oval (at 0 44 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 PB3))
    (pad 24 thru_hole oval (at 0 46 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 PB4))
    (pad 25 thru_hole oval (at 0 48 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 PB5))
    (pad 26 thru_hole oval (at 0 50 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 PB6))
    (pad 27 thru_hole oval (at 0 52 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 PB7))
    (pad 28 thru_hole oval (at 0 54 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 BOOT0))
    (pad 29 thru_hole oval (at 0 56 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 PB8))
    (pad 30 thru_hole oval (at 0 58 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 PB9))
    (pad 31 thru_hole oval (at 0 60 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 32 thru_hole oval (at 0 62 180) (size 1.85 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module bcan:Solder_Jumper_NC (layer B.Cu) (tedit 58DC8F8D)
    (at 150 77.75 270)
    (fp_text reference JP1 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value BOOT0 (at 0 -1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 66 BOOT0))
    (pad 2 smd rect (at 0.75 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(JP1-Pad2)"))
    (pad "" smd rect (at 0 0 270) (size 2.5 1) (layers B.Paste B.Mask))
  )
  (module bcan:Solder_Jumper_NC (layer B.Cu) (tedit 58DC883C)
    (at 149 123.75 270)
    (fp_text reference JP2 (at 0 -1.5 270) (layer B.SilkS) hide)
    (fp_text value BOOT1 (at 0 -1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 46 PB2))
    (pad 2 smd rect (at 0.75 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(JP2-Pad2)"))
    (pad "" smd rect (at 0 0 270) (size 2.5 1) (layers B.Paste B.Mask))
  )
  (module bcan:Solder_Jumper_NO (layer B.Cu) (tedit 58DC8D67)
    (at 149.25 108 90)
    (fp_text reference JP3 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value VCAP1 (at 0 -1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 /Controller/VCAP1))
    (pad "" smd rect (at 0 0 90) (size 2.5 1) (layers B.Mask))
  )
  (module bcan:Solder_Jumper_NO (layer B.Cu) (tedit 58DC8D5F)
    (at 150.75 108 90)
    (fp_text reference JP4 (at 0 -1.5 90) (layer B.SilkS) hide)
    (fp_text value VCAP2 (at 0 -1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /Controller/VCAP2))
    (pad "" smd rect (at 0 0 90) (size 2.5 1) (layers B.Mask))
  )
  (module bcan:Solder_Jumper_NC (layer B.Cu) (tedit 58DC880E)
    (at 151 123.75 90)
    (fp_text reference JP5 (at 0 -1.5 90) (layer B.SilkS) hide)
    (fp_text value USB_VBUS (at 0 -1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 71 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 72 PA9))
    (pad "" smd rect (at 0 0 90) (size 2.5 1) (layers B.Paste B.Mask))
  )
  (module Connectors_JST:JST_GH_SM04B-GHS-TB_04x1.25mm_Angled (layer F.Cu) (tedit 58DDB856)
    (at 150 84 180)
    (descr "JST GH series connector, SM04B-GHS-TB, side entry type")
    (tags "connector jst GH SMT side horizontal entry 1.25mm pitch")
    (attr smd)
    (fp_text reference J9 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value TOF (at 0 4.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0.45 180) (layer F.Fab))
    (pad 1 smd rect (at -1.875 -1.6 180) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 2V8))
    (pad 2 smd rect (at -0.625 -1.6 180) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 48 PB11))
    (pad 3 smd rect (at 0.625 -1.6 180) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 47 PB10))
    (pad 4 smd rect (at 1.875 -1.6 180) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" smd rect (at 3.6 1.6 180) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.6 1.6 180) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module bcan:Castellations_1x02_Pitch2.00mm (layer F.Cu) (tedit 58DD6B7E)
    (at 142 65)
    (fp_text reference J5 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value RAILS (at 0 4) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 3 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 RAIL_L))
    (pad 2 thru_hole oval (at 0 2) (size 3 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 MOT-))
  )
  (module bcan:Castellations_1x02_Pitch2.00mm (layer F.Cu) (tedit 58DD6B81)
    (at 158 67 180)
    (fp_text reference J6 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value MOTOR (at 0 4 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 3 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 MOT+))
    (pad 2 thru_hole oval (at 0 2 180) (size 3 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 RAIL_R))
  )
  (gr_text JST-GH (at 150 122) (layer F.SilkS))
  (gr_text JST-GH (at 150 82) (layer F.SilkS))
  (gr_text MOTOR (at 150 66.75) (layer B.SilkS))
  (gr_text RAILS (at 150 65) (layer B.SilkS))
  (gr_text bcan.io (at 155.7 128.9 270) (layer F.SilkS))
  (gr_text "Locomotive\nRev 1.0" (at 144.75 107.75 270) (layer F.SilkS))
  (gr_text GND (at 156.25 70 270) (layer B.SilkS))
  (gr_text F- (at 143 77) (layer B.SilkS))
  (gr_text R- (at 143 79) (layer B.SilkS))
  (gr_text L (at 143.5 65) (layer B.SilkS))
  (gr_text R (at 156.5 65) (layer B.SilkS))
  (gr_text + (at 156.5 66.75) (layer B.SilkS))
  (gr_text - (at 143.5 66.75) (layer B.SilkS))
  (gr_text BOOT1 (at 149 119.75 270) (layer B.SilkS))
  (gr_text VCAP (at 150 105.75) (layer B.SilkS))
  (gr_text 2V8 (at 143.75 92 270) (layer B.SilkS))
  (gr_text 5V (at 143 131) (layer B.SilkS))
  (gr_text VCC (at 143 129) (layer B.SilkS))
  (gr_text TOF (at 145 82.5 270) (layer F.SilkS))
  (gr_text JTAG (at 150 86) (layer B.SilkS))
  (gr_text IR (at 145 121.25 270) (layer F.SilkS))
  (gr_text B9 (at 157 73) (layer B.SilkS))
  (gr_text B8 (at 157 75) (layer B.SilkS))
  (gr_text BOOT0 (at 157 77) (layer B.SilkS))
  (gr_text PB7 (at 157 79) (layer B.SilkS))
  (gr_text PB6 (at 157 81) (layer B.SilkS))
  (gr_text PB5 (at 157 83) (layer B.SilkS))
  (gr_text PB4 (at 157 85) (layer B.SilkS))
  (gr_text PB3 (at 157 87) (layer B.SilkS))
  (gr_text PD2 (at 157 89) (layer B.SilkS))
  (gr_text PC12 (at 157 91) (layer B.SilkS))
  (gr_text PC11 (at 157 93) (layer B.SilkS))
  (gr_text PC10 (at 157 95) (layer B.SilkS))
  (gr_text PA15 (at 157 97) (layer B.SilkS))
  (gr_text PA14 (at 157 99) (layer B.SilkS))
  (gr_text 2V8 (at 156.25 102 270) (layer B.SilkS))
  (gr_text PA13 (at 157 105) (layer B.SilkS))
  (gr_text PA12 (at 157 107) (layer B.SilkS))
  (gr_text PA11 (at 157 109) (layer B.SilkS))
  (gr_text PA10 (at 157 111) (layer B.SilkS))
  (gr_text PA9 (at 157 113) (layer B.SilkS))
  (gr_text PA8 (at 157 115) (layer B.SilkS))
  (gr_text PC9 (at 157 117) (layer B.SilkS))
  (gr_text PC8 (at 157 119) (layer B.SilkS))
  (gr_text PC7 (at 157 121) (layer B.SilkS))
  (gr_text PC6 (at 157 123) (layer B.SilkS))
  (gr_text PB15 (at 157 125) (layer B.SilkS))
  (gr_text PB14 (at 157 127) (layer B.SilkS))
  (gr_text PB13 (at 157 129) (layer B.SilkS))
  (gr_text PB12 (at 157 131) (layer B.SilkS))
  (gr_text PB11 (at 143 127) (layer B.SilkS))
  (gr_text PB10 (at 143 125) (layer B.SilkS))
  (gr_text PB2 (at 143 123) (layer B.SilkS))
  (gr_text PB1 (at 143 121) (layer B.SilkS))
  (gr_text PB0 (at 143 119) (layer B.SilkS))
  (gr_text PC5 (at 143 117) (layer B.SilkS))
  (gr_text PC4 (at 143 115) (layer B.SilkS))
  (gr_text PA7 (at 143 113) (layer B.SilkS))
  (gr_text PA6 (at 143 111) (layer B.SilkS))
  (gr_text PA5 (at 143 109) (layer B.SilkS))
  (gr_text PA4 (at 143 107) (layer B.SilkS))
  (gr_text GND (at 143.75 104 270) (layer B.SilkS))
  (gr_text PA3 (at 143 101) (layer B.SilkS))
  (gr_text PA2 (at 143 99) (layer B.SilkS))
  (gr_text PA1 (at 143 97) (layer B.SilkS))
  (gr_text PA0 (at 143 95) (layer B.SilkS))
  (gr_text PC3 (at 143 89) (layer B.SilkS))
  (gr_text PC2 (at 143 87) (layer B.SilkS))
  (gr_text PC1 (at 143 85) (layer B.SilkS))
  (gr_text PC0 (at 143 83) (layer B.SilkS))
  (gr_text NRST (at 143 81) (layer B.SilkS))
  (gr_text C15 (at 142.5 74) (layer B.SilkS))
  (gr_text C14 (at 142.5 72) (layer B.SilkS))
  (gr_text C13 (at 142.5 70) (layer B.SilkS))
  (gr_text VBAT (at 142.5 68.25) (layer B.SilkS))
  (gr_line (start 142 132) (end 142 64) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158 132) (end 142 132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158 64) (end 158 132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142 64) (end 158 64) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151 104) (xy 149 104) (xy 149 98) (xy 147.5 98) (xy 150 94.5)
        (xy 152.5 98) (xy 151 98)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 142 64) (xy 158 64) (xy 158 132) (xy 142 132)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 142 64) (xy 158 64) (xy 158 132) (xy 142 132)
      )
    )
  )
  (zone (net 6) (net_name 2V8) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 142 100) (xy 150 92) (xy 158 100) (xy 150 108)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156 94.25) (xy 154 94.25) (xy 154 88.25) (xy 152.5 88.25) (xy 155 84.75)
        (xy 157.5 88.25) (xy 156 88.25)
      )
    )
  )
)
