(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu14.04.1-stable)
  (general
    (links 435)
    (no_connects 0)
    (area 45.9 32.300001 248.85 146.05)
    (thickness 1.6)
    (drawings 80)
    (tracks 2475)
    (zones 0)
    (modules 186)
    (nets 147)
  )
  (page A4)
  (title_block
    (title "OpenTX Evo")
    (rev 1)
    (comment 1 "Copyright © 2015 R Kilvington (eclrpk @ leeds.ac.uk)")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.299)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.508)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 0.8 0.8)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.1)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 46 68.5)
    (grid_origin 136 101.5)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory production/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /open_evo_misc/SERIAL_IN)
  (net 3 ADC0)
  (net 4 ADC1)
  (net 5 ADC10)
  (net 6 ADC2)
  (net 7 ADC3)
  (net 8 ADC4)
  (net 9 ADC5)
  (net 10 ADC6)
  (net 11 ADC7)
  (net 12 ADC8)
  (net 13 ADC9)
  (net 14 BATT_CHG)
  (net 15 BATT_SW)
  (net 16 GND)
  (net 17 LCD_A0)
  (net 18 LCD_CS_P)
  (net 19 LCD_MOSI)
  (net 20 LCD_RST_N)
  (net 21 LCD_SCK_P)
  (net 22 MPX_RF_EN)
  (net 23 MPX_RX)
  (net 24 PB1/SCK)
  (net 25 PB2/MOSI)
  (net 26 PB3/MISO)
  (net 27 PE4)
  (net 28 PE5)
  (net 29 PE6)
  (net 30 PE7)
  (net 31 PJ4)
  (net 32 PJ5)
  (net 33 PJ6)
  (net 34 PJ7)
  (net 35 PK5)
  (net 36 PK6)
  (net 37 PK7)
  (net 38 RESET-)
  (net 39 TELEM_BL_RX)
  (net 40 TELEM_BL_TX)
  (net 41 TRIM_BUTT_0)
  (net 42 TRIM_BUTT_1)
  (net 43 TRIM_BUTT_2)
  (net 44 TRIM_BUTT_3)
  (net 45 TRIM_BUTT_4)
  (net 46 TRIM_BUTT_5)
  (net 47 TRIM_BUTT_6)
  (net 48 TRIM_BUTT_7)
  (net 49 uSD_NSS)
  (net 50 /open_evo_misc/MPX_ANT)
  (net 51 PWR_HOLD)
  (net 52 "Net-(C5-Pad1)")
  (net 53 "Net-(C8-Pad1)")
  (net 54 "Net-(C18-Pad1)")
  (net 55 "Net-(C28-Pad1)")
  (net 56 "Net-(C34-Pad1)")
  (net 57 "Net-(C35-Pad1)")
  (net 58 +3V3)
  (net 59 "Net-(C49-Pad1)")
  (net 60 "Net-(C50-Pad1)")
  (net 61 "Net-(P9-Pad3)")
  (net 62 "Net-(P9-Pad5)")
  (net 63 "Net-(P9-Pad7)")
  (net 64 "Net-(P11-Pad5)")
  (net 65 "Net-(P11-Pad7)")
  (net 66 "Net-(P11-Pad10)")
  (net 67 "Net-(R1-Pad1)")
  (net 68 "Net-(R3-Pad2)")
  (net 69 "Net-(R5-Pad2)")
  (net 70 "Net-(R6-Pad2)")
  (net 71 "Net-(R7-Pad2)")
  (net 72 "Net-(R10-Pad2)")
  (net 73 "Net-(R17-Pad1)")
  (net 74 "Net-(R36-Pad1)")
  (net 75 "Net-(U1-Pad1)")
  (net 76 "Net-(U1-Pad4)")
  (net 77 "Net-(U1-Pad5)")
  (net 78 /open_evo_cpu/dsc_activated_FA)
  (net 79 /open_evo_cpu/rf_activated_FA)
  (net 80 /open_evo_cpu/buzzer_FA)
  (net 81 /open_evo_cpu/ppm_out_FA)
  (net 82 "Net-(U1-Pad27)")
  (net 83 "Net-(U1-Pad28)")
  (net 84 "Net-(U1-Pad29)")
  (net 85 "Net-(U1-Pad35)")
  (net 86 "Net-(U1-Pad37)")
  (net 87 "Net-(U1-Pad41)")
  (net 88 /open_evo_cpu/I2C_SCL)
  (net 89 /open_evo_cpu/I2C_SDA)
  (net 90 "Net-(U1-Pad45)")
  (net 91 "Net-(U1-Pad46)")
  (net 92 "Net-(U1-Pad47)")
  (net 93 "Net-(U1-Pad48)")
  (net 94 "Net-(U1-Pad49)")
  (net 95 "Net-(U1-Pad50)")
  (net 96 "Net-(U1-Pad58)")
  (net 97 "Net-(U1-Pad59)")
  (net 98 "Net-(U1-Pad60)")
  (net 99 "Net-(U1-Pad66)")
  (net 100 "Net-(U1-Pad70)")
  (net 101 "Net-(U1-Pad85)")
  (net 102 "Net-(U1-Pad86)")
  (net 103 "Net-(X1-Pad4)")
  (net 104 "Net-(P9-Pad1)")
  (net 105 "Net-(P9-Pad8)")
  (net 106 CARD_DETECT_N)
  (net 107 PWR_SW_STATUS)
  (net 108 "Net-(D2-Pad1)")
  (net 109 "Net-(D8-Pad2)")
  (net 110 "Net-(SW23-Pad3)")
  (net 111 MPX_TX)
  (net 112 "Net-(C60-Pad1)")
  (net 113 "Net-(D8-Pad1)")
  (net 114 "Net-(D12-Pad1)")
  (net 115 Piezo_Speaker)
  (net 116 "Net-(Q1-Pad1)")
  (net 117 CPPM_IN)
  (net 118 "/open_evo_misc/CPPM_IO_(was_MPX_SERIAL_O)")
  (net 119 /open_evo_misc/BATT_7V2)
  (net 120 CPPM_OUT_A)
  (net 121 CPPM_OUT_B)
  (net 122 "Net-(R24-Pad2)")
  (net 123 "Net-(R26-Pad2)")
  (net 124 /open_evo_cpu/CPPM_OUT_C)
  (net 125 /open_evo_inputs/R_STICK_V)
  (net 126 /open_evo_inputs/R_STICK_H)
  (net 127 /open_evo_inputs/L_STICK_H)
  (net 128 /open_evo_inputs/L_STICK_V)
  (net 129 /open_evo_inputs/SW_R_DIGI_DIR)
  (net 130 /open_evo_inputs/SW_L_DIGI_DIR)
  (net 131 /open_evo_cpu/hold_power_FA)
  (net 132 /open_evo_cpu/PB7)
  (net 133 /open_evo_cpu/PWR_LED)
  (net 134 "Net-(D11-Pad2)")
  (net 135 "Net-(P9-Pad2)")
  (net 136 "Net-(D5-Pad3)")
  (net 137 Trainer_Master_N)
  (net 138 "Net-(U1-Pad42)")
  (net 139 /open_evo_inputs/SW_R_DIGI_CLK)
  (net 140 /open_evo_inputs/SW_L_DIGI_CLK)
  (net 141 /open_evo_cpu/TRN_FA)
  (net 142 /open_evo_cpu/P4_RESET-)
  (net 143 /open_evo_cpu/P4_A0)
  (net 144 /open_evo_cpu/P4_MOSI)
  (net 145 /open_evo_cpu/P4_CS+)
  (net 146 /open_evo_cpu/P4_CLK+)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /open_evo_cpu/CPPM_OUT_C)
    (add_net /open_evo_cpu/I2C_SCL)
    (add_net /open_evo_cpu/I2C_SDA)
    (add_net /open_evo_cpu/P4_A0)
    (add_net /open_evo_cpu/P4_CLK+)
    (add_net /open_evo_cpu/P4_CS+)
    (add_net /open_evo_cpu/P4_MOSI)
    (add_net /open_evo_cpu/P4_RESET-)
    (add_net /open_evo_cpu/PB7)
    (add_net /open_evo_cpu/PWR_LED)
    (add_net /open_evo_cpu/TRN_FA)
    (add_net /open_evo_cpu/buzzer_FA)
    (add_net /open_evo_cpu/dsc_activated_FA)
    (add_net /open_evo_cpu/hold_power_FA)
    (add_net /open_evo_cpu/ppm_out_FA)
    (add_net /open_evo_cpu/rf_activated_FA)
    (add_net /open_evo_inputs/L_STICK_H)
    (add_net /open_evo_inputs/L_STICK_V)
    (add_net /open_evo_inputs/R_STICK_H)
    (add_net /open_evo_inputs/R_STICK_V)
    (add_net /open_evo_inputs/SW_L_DIGI_CLK)
    (add_net /open_evo_inputs/SW_L_DIGI_DIR)
    (add_net /open_evo_inputs/SW_R_DIGI_CLK)
    (add_net /open_evo_inputs/SW_R_DIGI_DIR)
    (add_net "/open_evo_misc/CPPM_IO_(was_MPX_SERIAL_O)")
    (add_net /open_evo_misc/SERIAL_IN)
    (add_net ADC0)
    (add_net ADC1)
    (add_net ADC10)
    (add_net ADC2)
    (add_net ADC3)
    (add_net ADC4)
    (add_net ADC5)
    (add_net ADC6)
    (add_net ADC7)
    (add_net ADC8)
    (add_net ADC9)
    (add_net CARD_DETECT_N)
    (add_net CPPM_IN)
    (add_net CPPM_OUT_A)
    (add_net CPPM_OUT_B)
    (add_net GND)
    (add_net LCD_A0)
    (add_net LCD_CS_P)
    (add_net LCD_MOSI)
    (add_net LCD_RST_N)
    (add_net LCD_SCK_P)
    (add_net MPX_RF_EN)
    (add_net MPX_RX)
    (add_net MPX_TX)
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C34-Pad1)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C49-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(C60-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D5-Pad3)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(P11-Pad10)")
    (add_net "Net-(P11-Pad5)")
    (add_net "Net-(P11-Pad7)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad3)")
    (add_net "Net-(P9-Pad5)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(P9-Pad8)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R36-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(SW23-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad58)")
    (add_net "Net-(U1-Pad59)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad66)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad86)")
    (add_net "Net-(X1-Pad4)")
    (add_net PB1/SCK)
    (add_net PB2/MOSI)
    (add_net PB3/MISO)
    (add_net PE4)
    (add_net PE5)
    (add_net PE6)
    (add_net PE7)
    (add_net PJ4)
    (add_net PJ5)
    (add_net PJ6)
    (add_net PJ7)
    (add_net PK5)
    (add_net PK6)
    (add_net PK7)
    (add_net PWR_HOLD)
    (add_net PWR_SW_STATUS)
    (add_net Piezo_Speaker)
    (add_net RESET-)
    (add_net TELEM_BL_RX)
    (add_net TELEM_BL_TX)
    (add_net TRIM_BUTT_0)
    (add_net TRIM_BUTT_1)
    (add_net TRIM_BUTT_2)
    (add_net TRIM_BUTT_3)
    (add_net TRIM_BUTT_4)
    (add_net TRIM_BUTT_5)
    (add_net TRIM_BUTT_6)
    (add_net TRIM_BUTT_7)
    (add_net Trainer_Master_N)
    (add_net uSD_NSS)
  )
  (net_class 0.5 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
  )
  (net_class 0.6 ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /open_evo_misc/BATT_7V2)
    (add_net /open_evo_misc/MPX_ANT)
  )
  (net_class 0.7 ""
    (clearance 0.2)
    (trace_width 0.7)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net BATT_SW)
  )
  (net_class 1.0 ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net BATT_CHG)
  )
  (module modules:SOT-23-6 (layer B.Cu) (tedit 584EEB23)
    (at 63 88.75 90)
    (fp_text reference U6 (at -2.5 -1.9 90) (layer B.SilkS) hide)
    (fp_text value 74LVC1G3157 (at -0.25 2.75 270) (layer B.SilkS))
    (pad 5 smd rect (at 0 1.25 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0 -1.25 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 3 smd rect (at 0.95 -1.25 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 121 CPPM_OUT_B))
    (pad 4 smd rect (at 0.95 1.25 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 136 "Net-(D5-Pad3)"))
    (pad 6 smd rect (at -0.95 1.25 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 137 Trainer_Master_N))
    (pad 1 smd rect (at -0.95 -1.25 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 117 CPPM_IN))
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DA962)
    (at 89 99.75 180)
    (attr smd)
    (fp_text reference R30 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 30K (at 0 1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 58 +3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 22 MPX_RF_EN))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5589)
    (at 67.25 77.25)
    (attr smd)
    (fp_text reference R28 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 1K (at 2 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 135 "Net-(P9-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 49 uSD_NSS))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:JST_B6B-ZR-3.4 locked (layer F.Cu) (tedit 58503EE1)
    (at 48.5 77 90)
    (fp_text reference P1 (at -2.5 3.75 90) (layer F.SilkS) hide)
    (fp_text value SW-R (at 0 3.75 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.75 0.6 90) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at -2.25 0.6 90) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 3 thru_hole oval (at -0.75 0.6 90) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 12 ADC8))
    (pad 4 thru_hole oval (at 0.75 0.6 90) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 11 ADC7))
    (pad 5 thru_hole oval (at 2.25 0.6 90) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 129 /open_evo_inputs/SW_R_DIGI_DIR))
    (pad 6 thru_hole oval (at 3.75 0.6 90) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 139 /open_evo_inputs/SW_R_DIGI_CLK))
  )
  (module modules:JST_B6B-ZR-3.4 locked (layer F.Cu) (tedit 58503F0E)
    (at 223.5 77 270)
    (fp_text reference P6 (at -2.5 3.75 270) (layer F.SilkS) hide)
    (fp_text value SW-L (at 0 3.75 450) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.75 0.6 270) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at -2.25 0.6 270) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 3 thru_hole oval (at -0.75 0.6 270) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 ADC10))
    (pad 4 thru_hole oval (at 0.75 0.6 270) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 13 ADC9))
    (pad 5 thru_hole oval (at 2.25 0.6 270) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 130 /open_evo_inputs/SW_L_DIGI_DIR))
    (pad 6 thru_hole oval (at 3.75 0.6 270) (size 1.1 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 140 /open_evo_inputs/SW_L_DIGI_CLK))
  )
  (module modules:SOD-323 (layer B.Cu) (tedit 584DA41A)
    (at 167.6 95 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D11 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value RB751V40 (at 0 1.35 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.15 0 270) (size 0.8 0.8) (layers B.Cu B.Mask)
      (net 120 CPPM_OUT_A))
    (pad 2 smd rect (at 1.15 0 270) (size 0.8 0.8) (layers B.Cu B.Mask)
      (net 134 "Net-(D11-Pad2)"))
  )
  (module modules:SOD-323 (layer F.Cu) (tedit 584DA9E3)
    (at 125.1 107.7 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value RB751V40 (at -0.2 -1.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.15 0 270) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 119 /open_evo_misc/BATT_7V2))
    (pad 2 smd rect (at 1.15 0 270) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 16 GND))
  )
  (module modules:SOD-323 (layer F.Cu) (tedit 584C5E56)
    (at 95.75 90.75)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value RB751V40 (at 0 -1.25) (layer F.SilkS))
    (pad 1 smd rect (at -1.15 0) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 20 LCD_RST_N))
    (pad 2 smd rect (at 1.15 0) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 142 /open_evo_cpu/P4_RESET-))
  )
  (module modules:SOD-323 (layer F.Cu) (tedit 584DA890)
    (at 133 83.5 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value RB751V40 (at 0 -1.5 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.15 0 270) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 113 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.15 0 270) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 109 "Net-(D8-Pad2)"))
  )
  (module modules:SOD-323 (layer F.Cu) (tedit 58503CCE)
    (at 131 83.5 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D9 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value RB751V40 (at 0 2 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.15 0 270) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 113 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.15 0 270) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 107 PWR_SW_STATUS))
  )
  (module modules:SOD-323 (layer B.Cu) (tedit 584C4FF1)
    (at 147.5 81.5 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D12 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value RB751V40 (at 0 -1.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.15 0 90) (size 0.8 0.8) (layers B.Cu B.Mask)
      (net 114 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.15 0 90) (size 0.8 0.8) (layers B.Cu B.Mask)
      (net 59 "Net-(C49-Pad1)"))
  )
  (module modules:evo_battery_holder locked (layer F.Cu) (tedit 56D9E18B)
    (at 83 131.5)
    (fp_text reference batt_holder1 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value MISC_MECH (at 4 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad "" thru_hole circle (at 0 -14.5) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 0 12.35) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module modules:evo_battery_holder locked (layer F.Cu) (tedit 56D9E18B)
    (at 189 131.5)
    (fp_text reference batt_holder2 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value MISC_MECH (at 4 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad "" thru_hole circle (at 0 -14.5) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 0 12.35) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA3FD)
    (at 193 78.5 90)
    (attr smd)
    (fp_text reference R26 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 1.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA49C)
    (at 79.5 74 90)
    (attr smd)
    (fp_text reference R24 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 1.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:MPX_JR_Module locked (layer F.Cu) (tedit 55E48381)
    (at 159.5 80.5)
    (fp_text reference P11 (at 4.8 0) (layer F.SilkS) hide)
    (fp_text value MPX_JR_MODULE (at -0.2 25.8) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0) (size 3.8 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(C50-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 3.8 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(C49-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 3.8 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 BATT_SW))
    (pad 4 thru_hole oval (at 0 7.62) (size 3.8 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 3.8 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P11-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 3.8 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 50 /open_evo_misc/MPX_ANT))
    (pad 14 thru_hole oval (at 57.8 4.45) (size 2.2 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 57.8 6.99) (size 2.2 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 57.8 9.53) (size 2.2 1.524) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 3.3 23) (size 1.524 2.2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(P11-Pad7)"))
    (pad 8 thru_hole oval (at 5.84 23) (size 1.524 2.2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 9 thru_hole oval (at 8.38 23) (size 1.524 2.2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 BATT_SW))
    (pad 10 thru_hole oval (at 10.92 23) (size 1.524 2.2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(P11-Pad10)"))
    (pad 11 thru_hole oval (at 13.46 23) (size 1.524 2.2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(D11-Pad2)"))
  )
  (module modules:Socket_Strip_Straight_2x03 (layer F.Cu) (tedit 584EF155)
    (at 49.6 93.5 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 0.1 -2.5 180) (layer F.SilkS) hide)
    (fp_text value ICSP (at -3.15 -2.25 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 PB3/MISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at -2.54 0) (size 1.7272 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 24 PB1/SCK))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7272 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 PB2/MOSI))
    (pad 5 thru_hole oval (at -5.08 0) (size 1.7272 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 38 RESET-))
    (pad 6 thru_hole oval (at -5.08 2.54) (size 1.7272 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x03.wrl
      (at (xyz 0.1 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module modules:hole_1-6mm locked (layer F.Cu) (tedit 55E0A204)
    (at 81 101.5)
    (fp_text reference hole7 (at 0 -0.9) (layer F.SilkS) hide)
    (fp_text value 1.6mm (at 0 0.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module modules:hole_1-6mm locked (layer F.Cu) (tedit 55E0A204)
    (at 191 101.5)
    (fp_text reference hole8 (at 0 -0.9) (layer F.SilkS) hide)
    (fp_text value 1.6mm (at 0 0.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module modules:hole_2-0mm locked (layer F.Cu) (tedit 55E0A402)
    (at 185.5 87.5)
    (fp_text reference hole4 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value 2.0mm (at 0 0.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module modules:hole_2-0mm locked (layer F.Cu) (tedit 55E0A402)
    (at 152.5 101.5)
    (fp_text reference hole3 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value 2.0mm (at 0 0.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module modules:hole_2-0mm locked (layer F.Cu) (tedit 55E0A402)
    (at 119.5 101.5)
    (fp_text reference hole2 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value 2.0mm (at 0 0.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module modules:hole_2-0mm locked (layer F.Cu) (tedit 55E0A402)
    (at 86.5 87.5)
    (fp_text reference hole1 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value 2.0mm (at 0 0.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module modules:JST_B6B-ZR-SM4-TF locked (layer F.Cu) (tedit 58503E88)
    (at 83 71)
    (fp_text reference P2 (at -2.5 0) (layer F.SilkS) hide)
    (fp_text value SP (at 8.25 0) (layer F.SilkS))
    (pad 1 smd rect (at -3.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.25 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 3 smd rect (at -0.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 9 ADC5))
    (pad 4 smd rect (at 0.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at 2.25 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 6 smd rect (at 3.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 8 ADC4))
    (pad 7 smd rect (at 5.95 1) (size 1.8 2.2) (layers F.Cu F.Mask))
    (pad 8 smd rect (at -5.95 1) (size 1.8 2.2) (layers F.Cu F.Mask))
  )
  (module modules:JST_B6B-ZR-SM4-TF locked (layer F.Cu) (tedit 58503E74)
    (at 113 71)
    (fp_text reference P3 (at -2.5 0) (layer F.SilkS) hide)
    (fp_text value KN-R (at 9 0) (layer F.SilkS))
    (pad 1 smd rect (at -3.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.25 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 3 smd rect (at -0.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 126 /open_evo_inputs/R_STICK_H))
    (pad 4 smd rect (at 0.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at 2.25 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 6 smd rect (at 3.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 125 /open_evo_inputs/R_STICK_V))
    (pad 7 smd rect (at 5.95 1) (size 1.8 2.2) (layers F.Cu F.Mask))
    (pad 8 smd rect (at -5.95 1) (size 1.8 2.2) (layers F.Cu F.Mask))
  )
  (module modules:JST_B6B-ZR-SM4-TF locked (layer F.Cu) (tedit 58503EA0)
    (at 149.5 71)
    (fp_text reference P5 (at -2.5 0) (layer F.SilkS) hide)
    (fp_text value KN-L (at -9 0) (layer F.SilkS))
    (pad 1 smd rect (at -3.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.25 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 3 smd rect (at -0.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 127 /open_evo_inputs/L_STICK_H))
    (pad 4 smd rect (at 0.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at 2.25 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 6 smd rect (at 3.75 3) (size 0.7 4) (layers F.Cu F.Mask)
      (net 128 /open_evo_inputs/L_STICK_V))
    (pad 7 smd rect (at 5.95 1) (size 1.8 2.2) (layers F.Cu F.Mask))
    (pad 8 smd rect (at -5.95 1) (size 1.8 2.2) (layers F.Cu F.Mask))
  )
  (module modules:c_elec_6.3x7.7 (layer F.Cu) (tedit 584EF09E)
    (at 111.5 97)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (attr smd)
    (fp_text reference C61 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "100u 20V" (at 3 -4.25 180) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0) (size 3.59918 1.6002) (layers F.Cu F.Mask)
      (net 15 BATT_SW))
    (pad 2 smd rect (at -2.75082 0) (size 3.59918 1.6002) (layers F.Cu F.Mask)
      (net 16 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM1206POL (layer F.Cu) (tedit 584EF04E)
    (at 101 101.5 90)
    (attr smd)
    (fp_text reference C43 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 2.25 2 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Mask)
      (net 15 BATT_SW))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd/chip_cms_pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM1206POL (layer F.Cu) (tedit 584EF040)
    (at 93.75 101.5 270)
    (attr smd)
    (fp_text reference C44 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 2.25 2 450) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Mask)
      (net 58 +3V3))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd/chip_cms_pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM1206POL (layer B.Cu) (tedit 584DA713)
    (at 101.2 101.5 270)
    (attr smd)
    (fp_text reference C46 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10u (at -3.5 -0.8 360) (layer B.SilkS))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Mask)
      (net 15 BATT_SW))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd/chip_cms_pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM1206POL (layer B.Cu) (tedit 584EF032)
    (at 93.6 101.6 90)
    (attr smd)
    (fp_text reference C47 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 10u (at 3.6 -0.85 360) (layer B.SilkS))
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd/chip_cms_pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:XTAL_QTC5A (layer F.Cu) (tedit 55E07C9F)
    (at 56.8 109.5 270)
    (fp_text reference X1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 16MHz (at 0 2.8 270) (layer F.SilkS))
    (fp_text user 1 (at -3.3 2.7 540) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 1.4 270) (size 2 1.5) (layers F.Cu F.Mask)
      (net 56 "Net-(C34-Pad1)") (solder_mask_margin 0.06858))
    (pad 2 smd rect (at 2.2 1.4 270) (size 2 1.5) (layers F.Cu F.Mask)
      (net 16 GND) (solder_mask_margin 0.06858))
    (pad 3 smd rect (at 2.2 -1.4 270) (size 2 1.5) (layers F.Cu F.Mask)
      (net 57 "Net-(C35-Pad1)"))
    (pad 4 smd rect (at -2.2 -1.4 270) (size 2 1.5) (layers F.Cu F.Mask)
      (net 103 "Net-(X1-Pad4)"))
  )
  (module modules:SOT-23 (layer F.Cu) (tedit 584EE85C)
    (at 130 78.5 180)
    (fp_text reference D3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value BAT54S (at -3 -1 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0 -1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 107 PWR_SW_STATUS))
    (pad 1 smd rect (at -0.95 1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 16 GND))
  )
  (module modules:SOT-23 (layer B.Cu) (tedit 584EECC3)
    (at 108 106.75 180)
    (fp_text reference D5 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value BAT54S (at 0 -2.5 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 -1.1 180) (size 0.6 1) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0 1.1 180) (size 0.6 1) (layers B.Cu B.Mask)
      (net 136 "Net-(D5-Pad3)"))
    (pad 1 smd rect (at -0.95 -1.1 180) (size 0.6 1) (layers B.Cu B.Mask)
      (net 16 GND))
  )
  (module modules:SOT-23 (layer B.Cu) (tedit 584DA526)
    (at 68.5 122.5 90)
    (fp_text reference D7 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value BAT54S (at -2.5 1.5 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 -1.1 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0 1.1 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 39 TELEM_BL_RX))
    (pad 1 smd rect (at -0.95 -1.1 90) (size 0.6 1) (layers B.Cu B.Mask)
      (net 16 GND))
  )
  (module modules:SOT-23 (layer F.Cu) (tedit 584EE863)
    (at 139 78.5 180)
    (fp_text reference D10 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value BAT54S (at -2.75 -1 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0 -1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 23 MPX_RX))
    (pad 1 smd rect (at -0.95 1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 16 GND))
  )
  (module modules:SOT-23 (layer F.Cu) (tedit 584DA9C6)
    (at 118.7 107.9)
    (fp_text reference Q1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value BC817-40 (at 0.05 2.6 180) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 1.1) (size 0.6 1) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 3 smd rect (at 0 -1.1) (size 0.6 1) (layers F.Cu F.Mask)
      (net 109 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -0.95 1.1) (size 0.6 1) (layers F.Cu F.Mask)
      (net 116 "Net-(Q1-Pad1)"))
  )
  (module modules:SOT-23 (layer F.Cu) (tedit 584DAA09)
    (at 114 102.9)
    (fp_text reference Q2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TSM2307CX (at -2.5 0.35 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 1.1) (size 0.6 1) (layers F.Cu F.Mask)
      (net 119 /open_evo_misc/BATT_7V2))
    (pad 3 smd rect (at 0 -1.1) (size 0.6 1) (layers F.Cu F.Mask)
      (net 15 BATT_SW))
    (pad 1 smd rect (at -0.95 1.1) (size 0.6 1) (layers F.Cu F.Mask)
      (net 109 "Net-(D8-Pad2)"))
  )
  (module modules:SOT-23 (layer F.Cu) (tedit 584DA973)
    (at 97.4 101.5 180)
    (fp_text reference U4 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value MCP1703-33 (at 0.15 -3.5 360) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 58 +3V3))
    (pad 3 smd rect (at 0 -1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 15 BATT_SW))
    (pad 1 smd rect (at -0.95 1.1 180) (size 0.6 1) (layers F.Cu F.Mask)
      (net 16 GND))
  )
  (module modules:SOT-23 (layer B.Cu) (tedit 584DA6E2)
    (at 97.4 101.5 180)
    (fp_text reference U5 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value MCP1703-50 (at 0.15 3.5 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 -1.1 180) (size 0.6 1) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0 1.1 180) (size 0.6 1) (layers B.Cu B.Mask)
      (net 15 BATT_SW))
    (pad 1 smd rect (at -0.95 -1.1 180) (size 0.6 1) (layers B.Cu B.Mask)
      (net 16 GND))
  )
  (module modules:MOLEX_52808-0770 (layer F.Cu) (tedit 55E07A2E)
    (at 121 80.5)
    (fp_text reference P4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LCD (at -4.4 2.3 180) (layer F.SilkS))
    (pad 1 smd rect (at -3 1.8) (size 0.6 1.65) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 2 smd rect (at -2 -1.8) (size 0.6 1.65) (layers F.Cu F.Mask)
      (net 143 /open_evo_cpu/P4_A0))
    (pad 3 smd rect (at -1 1.8) (size 0.6 1.65) (layers F.Cu F.Mask)
      (net 144 /open_evo_cpu/P4_MOSI))
    (pad 4 smd rect (at 0 -1.8) (size 0.6 1.65) (layers F.Cu F.Mask)
      (net 145 /open_evo_cpu/P4_CS+))
    (pad 5 smd rect (at 1 1.8) (size 0.6 1.65) (layers F.Cu F.Mask)
      (net 146 /open_evo_cpu/P4_CLK+))
    (pad 6 smd rect (at 2 -1.8) (size 0.6 1.65) (layers F.Cu F.Mask)
      (net 142 /open_evo_cpu/P4_RESET-))
    (pad 7 smd rect (at 3 1.8) (size 0.6 1.65) (layers F.Cu F.Mask)
      (net 58 +3V3))
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 125 80 90)
    (attr smd)
    (fp_text reference C26 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.2 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 127 /open_evo_inputs/L_STICK_H))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 112.7 80.4 90)
    (attr smd)
    (fp_text reference R8 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 20K (at 0 1.2 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 55 "Net-(C28-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 117.25 84)
    (attr smd)
    (fp_text reference R10 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 39K (at 0 1.2) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 7 ADC3))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 72 "Net-(R10-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 125 83.5 270)
    (attr smd)
    (fp_text reference C32 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.2 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 128 /open_evo_inputs/L_STICK_V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA3E2)
    (at 150.25 74 270)
    (attr smd)
    (fp_text reference C42 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA4A4)
    (at 81.5 87 180)
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 48 TRIM_BUTT_7))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEBB3)
    (at 73.8 110 45)
    (attr smd)
    (fp_text reference C2 (at 0 0 45) (layer B.SilkS) hide)
    (fp_text value 100n (at -2.156676 -0.035355 315) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 45) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 45) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 585041A6)
    (at 55.25 75.75 90)
    (attr smd)
    (fp_text reference C3 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10n (at 2 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 11 ADC7))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C6194)
    (at 87.5 92.5 270)
    (attr smd)
    (fp_text reference C4 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 -1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 45 TRIM_BUTT_4))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA4F9)
    (at 70 118.5 270)
    (attr smd)
    (fp_text reference C5 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OC (at -2 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 52 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 5850419C)
    (at 55.25 79 270)
    (attr smd)
    (fp_text reference C6 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 2 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 12 ADC8))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C619A)
    (at 84.5 92.5 90)
    (attr smd)
    (fp_text reference C7 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 -1.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 46 TRIM_BUTT_5))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA4F5)
    (at 67.5 118.5 270)
    (attr smd)
    (fp_text reference C8 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at -2 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 53 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DA955)
    (at 86.5 79 270)
    (attr smd)
    (fp_text reference C9 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 2 -0.25 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 8 ADC4))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA4AF)
    (at 81.5 90)
    (attr smd)
    (fp_text reference C10 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 47 TRIM_BUTT_6))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DA94E)
    (at 82 79 270)
    (attr smd)
    (fp_text reference C11 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 2 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 9 ADC5))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EED61)
    (at 177 98)
    (attr smd)
    (fp_text reference C12 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 -1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 43 TRIM_BUTT_2))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA408)
    (at 180.5 93 180)
    (attr smd)
    (fp_text reference C13 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 42 TRIM_BUTT_1))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA404)
    (at 188 93 180)
    (attr smd)
    (fp_text reference C14 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 41 TRIM_BUTT_0))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 112.7 79.4 90)
    (attr smd)
    (fp_text reference C15 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 -1.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 125 /open_evo_inputs/R_STICK_V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EED51)
    (at 172.5 98 180)
    (attr smd)
    (fp_text reference C16 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 44 TRIM_BUTT_3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 109.9 79.4 90)
    (attr smd)
    (fp_text reference C17 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 -1.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 126 /open_evo_inputs/R_STICK_H))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 103 74 270)
    (attr smd)
    (fp_text reference C18 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 54 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 112.5 73.5 270)
    (attr smd)
    (fp_text reference C19 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.2 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 6 ADC2))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C6362)
    (at 209 80.5)
    (attr smd)
    (fp_text reference C20 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 -1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 13 ADC9))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C6369)
    (at 209 76.5 180)
    (attr smd)
    (fp_text reference C21 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 5 ADC10))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5322)
    (at 55 79.25 270)
    (attr smd)
    (fp_text reference C22 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 -1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 27 PE4))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C532D)
    (at 52.75 79.25 270)
    (attr smd)
    (fp_text reference C23 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 28 PE5))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C634F)
    (at 205.75 88.5)
    (attr smd)
    (fp_text reference C24 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 29 PE6))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C6358)
    (at 205.75 84.5)
    (attr smd)
    (fp_text reference C25 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 30 PE7))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DA8E3)
    (at 49.7 87.7)
    (attr smd)
    (fp_text reference C27 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 100n (at 0.05 -1.45) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 121.75 80 90)
    (attr smd)
    (fp_text reference C28 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.2 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 55 "Net-(C28-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 94 82 270)
    (attr smd)
    (fp_text reference C29 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 3 ADC0))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA498)
    (at 77 74 270)
    (attr smd)
    (fp_text reference C30 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 112.7 84.1 270)
    (attr smd)
    (fp_text reference C31 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.2 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 7 ADC3))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584D2117)
    (at 54.5 104.5 180)
    (attr smd)
    (fp_text reference C34 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 24p (at 0 1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 56 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584D2124)
    (at 59 104.5 180)
    (attr smd)
    (fp_text reference C35 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 24p (at -1 1.5 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 57 "Net-(C35-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584D1FDE)
    (at 55.75 100.5)
    (attr smd)
    (fp_text reference C36 (at 0 0) (layer F.SilkS) hide)
    (fp_text value O.C. (at 0 -1.5) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 38 RESET-))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 110.5 80.4 270)
    (attr smd)
    (fp_text reference C38 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 1.2 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 94 72 90)
    (attr smd)
    (fp_text reference C39 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 -1.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 4 ADC1))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA3C2)
    (at 214.5 73.5 180)
    (attr smd)
    (fp_text reference C45 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE888)
    (at 124.5 86.5 270)
    (attr smd)
    (fp_text reference C52 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 100n (at -2 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 58 +3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEDFB)
    (at 55.9 114 270)
    (attr smd)
    (fp_text reference C53 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at -2 0.15 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EED06)
    (at 71 94.5)
    (attr smd)
    (fp_text reference C54 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB15)
    (at 64 84 180)
    (attr smd)
    (fp_text reference C55 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 58 +3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584D1FAE)
    (at 54.25 97.75 45)
    (attr smd)
    (fp_text reference C56 (at 0 0 45) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.414214 45) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 45) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 45) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEC55)
    (at 119 125 90)
    (attr smd)
    (fp_text reference C57 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 -1.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 35 PK5))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEC47)
    (at 93.5 125 90)
    (attr smd)
    (fp_text reference C58 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 -1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 36 PK6))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEC39)
    (at 98 125 270)
    (attr smd)
    (fp_text reference C59 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 1n (at 0 1.5 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 37 PK7))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA4E5)
    (at 65 118.5 90)
    (attr smd)
    (fp_text reference L1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value s.c. (at 0 -1.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 53 "Net-(C8-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 124.25 74.5 270)
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 1.2 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 67 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 127 /open_evo_inputs/L_STICK_H))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA446)
    (at 116 72.5)
    (attr smd)
    (fp_text reference R2 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 39K (at 0 -1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 6 ADC2))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 67 "Net-(R1-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 58504275)
    (at 153 125 90)
    (attr smd)
    (fp_text reference R3 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 5K1 (at -2 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 31 PJ4))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 68 "Net-(R3-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 121.75 74.5 270)
    (attr smd)
    (fp_text reference R4 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 20K (at 0 1.2 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 55 "Net-(C28-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEC3D)
    (at 102 125 90)
    (attr smd)
    (fp_text reference R5 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 5K1 (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 32 PJ5))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 69 "Net-(R5-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEBF2)
    (at 98 138.5 180)
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 5K1 (at -2.5 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 33 PJ6))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEBF9)
    (at 152 138.5)
    (attr smd)
    (fp_text reference R7 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 5K1 (at 2.5 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 34 PJ7))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 71 "Net-(R7-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 121.5 84)
    (attr smd)
    (fp_text reference R9 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 1.2) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 72 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 128 /open_evo_inputs/L_STICK_V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5320)
    (at 55 76 270)
    (attr smd)
    (fp_text reference R11 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 139 /open_evo_inputs/SW_R_DIGI_CLK))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 27 PE4))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5329)
    (at 52.75 76 270)
    (attr smd)
    (fp_text reference R12 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 129 /open_evo_inputs/SW_R_DIGI_DIR))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 28 PE5))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C6352)
    (at 209 88.5 180)
    (attr smd)
    (fp_text reference R13 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 140 /open_evo_inputs/SW_L_DIGI_CLK))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 29 PE6))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C635D)
    (at 209 84.5 180)
    (attr smd)
    (fp_text reference R14 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 130 /open_evo_inputs/SW_L_DIGI_DIR))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 30 PE7))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 94 77 270)
    (attr smd)
    (fp_text reference R15 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 20K (at 0 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 54 "Net-(C18-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 58503CFC)
    (at 106 80.5)
    (attr smd)
    (fp_text reference R17 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.5) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 73 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 125 /open_evo_inputs/R_STICK_V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE9CA)
    (at 97.5 83)
    (attr smd)
    (fp_text reference R18 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 39K (at 2 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 3 ADC0))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 73 "Net-(R17-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB76)
    (at 60 125)
    (attr smd)
    (fp_text reference R23 (at 0 0) (layer B.SilkS) hide)
    (fp_text value O.C. (at -2 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 27 PE4))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB71)
    (at 58 122.5)
    (attr smd)
    (fp_text reference R25 (at 0 0) (layer B.SilkS) hide)
    (fp_text value O.C. (at -2 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 28 PE5))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB6A)
    (at 56 120)
    (attr smd)
    (fp_text reference R27 (at 0 0) (layer B.SilkS) hide)
    (fp_text value O.C. (at -2 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 29 PE6))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB59)
    (at 54 117.5)
    (attr smd)
    (fp_text reference R29 (at 0 0) (layer B.SilkS) hide)
    (fp_text value O.C. (at -2 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 30 PE7))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 103 79 90)
    (attr smd)
    (fp_text reference R31 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 20K (at 0 -1.2 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 54 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE945)
    (at 105.5 85.25)
    (attr smd)
    (fp_text reference R32 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 3K6 (at 2.5 -0.75 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 143 /open_evo_cpu/P4_A0))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE882)
    (at 119.5 86.5 270)
    (attr smd)
    (fp_text reference R33 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 3K6 (at -2 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 144 /open_evo_cpu/P4_MOSI))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C7CC6)
    (at 51.5 100.5 45)
    (attr smd)
    (fp_text reference R34 (at 0 0 45) (layer B.SilkS) hide)
    (fp_text value O.C. (at 0 -1.414214 45) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 45) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 38 RESET-))
    (pad 2 smd rect (at 0.762 0 45) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 106 78.3)
    (attr smd)
    (fp_text reference R36 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 74 "Net-(R36-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 126 /open_evo_inputs/R_STICK_H))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 98.5 71)
    (attr smd)
    (fp_text reference R37 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 39K (at 0 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 4 ADC1))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 74 "Net-(R36-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE949)
    (at 105.5 88.25)
    (attr smd)
    (fp_text reference R48 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 3K6 (at 2.5 -0.75 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 145 /open_evo_cpu/P4_CS+))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE885)
    (at 122 86.5 270)
    (attr smd)
    (fp_text reference R49 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 3K6 (at -2 0.25 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 146 /open_evo_cpu/P4_CLK+))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE950)
    (at 105.5 91.25 180)
    (attr smd)
    (fp_text reference R50 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 5K1 (at -2.5 1 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 58 +3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 142 /open_evo_cpu/P4_RESET-))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584C5E4C)
    (at 99.25 91.5 180)
    (attr smd)
    (fp_text reference R52 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1K8 (at 0 -1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 144 /open_evo_cpu/P4_MOSI))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 19 LCD_MOSI))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584C5E4A)
    (at 96 92.75 180)
    (attr smd)
    (fp_text reference R53 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1K8 (at 0 -1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 146 /open_evo_cpu/P4_CLK+))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 21 LCD_SCK_P))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584C5F53)
    (at 96.25 86 180)
    (attr smd)
    (fp_text reference R54 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1K8 (at 0 -1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 143 /open_evo_cpu/P4_A0))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 17 LCD_A0))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584C5F56)
    (at 99.5 87.25 180)
    (attr smd)
    (fp_text reference R55 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1K8 (at 0 -1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 145 /open_evo_cpu/P4_CS+))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 18 LCD_CS_P))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB31)
    (at 67.5 84)
    (attr smd)
    (fp_text reference R56 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 2K (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 135 "Net-(P9-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C556D)
    (at 64 75 180)
    (attr smd)
    (fp_text reference R57 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 2 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 61 "Net-(P9-Pad3)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 25 PB2/MOSI))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5579)
    (at 64 77.25 180)
    (attr smd)
    (fp_text reference R58 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 2 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 62 "Net-(P9-Pad5)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 24 PB1/SCK))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB2B)
    (at 60.5 84 180)
    (attr smd)
    (fp_text reference R59 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 63 "Net-(P9-Pad7)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 26 PB3/MISO))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5590)
    (at 67.25 75)
    (attr smd)
    (fp_text reference R60 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 2K (at 2 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 61 "Net-(P9-Pad3)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C557D)
    (at 64 79.5 180)
    (attr smd)
    (fp_text reference R61 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 2K (at 2 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 62 "Net-(P9-Pad5)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DA9BA)
    (at 113.4 106.8)
    (attr smd)
    (fp_text reference R63 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 2K (at 0.1 1.45) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 108 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 109 "Net-(D8-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C55F6)
    (at 127 107)
    (attr smd)
    (fp_text reference C33 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 330p (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 118 "/open_evo_misc/CPPM_IO_(was_MPX_SERIAL_O)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA50D)
    (at 65 122.5 270)
    (attr smd)
    (fp_text reference C37 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 330p (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 39 TELEM_BL_RX))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEB98)
    (at 72.5 118.5 90)
    (attr smd)
    (fp_text reference C40 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 10 ADC6))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EEFB0)
    (at 134.5 78 90)
    (attr smd)
    (fp_text reference C41 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10n (at -0.75 1.5 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 107 PWR_SW_STATUS))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DAB1D)
    (at 147.3 101.2 90)
    (attr smd)
    (fp_text reference C48 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100n (at -0.05 1.45 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 14 BATT_CHG))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5003)
    (at 151.75 81.5 90)
    (attr smd)
    (fp_text reference C49 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 330p (at -2 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 59 "Net-(C49-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5134)
    (at 155.5 76.5 270)
    (attr smd)
    (fp_text reference C50 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 330p (at -2 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 60 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EE840)
    (at 137.5 83.5 270)
    (attr smd)
    (fp_text reference C51 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330p (at 0 -1.5 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 23 MPX_RX))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA52A)
    (at 67.5 126.5 90)
    (attr smd)
    (fp_text reference C60 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 330p (at 0 1.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 112 "Net-(C60-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DA99E)
    (at 107 105.25)
    (attr smd)
    (fp_text reference R16 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10K (at 2 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 51 PWR_HOLD))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 116 "Net-(Q1-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 58503F61)
    (at 107 107.5 180)
    (attr smd)
    (fp_text reference R19 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 100K (at -2 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 116 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C55E8)
    (at 123.75 107)
    (attr smd)
    (fp_text reference R21 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 1.5) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 136 "Net-(D5-Pad3)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 118 "/open_evo_misc/CPPM_IO_(was_MPX_SERIAL_O)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584DA52C)
    (at 65 126.5 270)
    (attr smd)
    (fp_text reference R22 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 1.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 40 TELEM_BL_TX))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 112 "Net-(C60-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EF070)
    (at 103.75 107.5)
    (attr smd)
    (fp_text reference R38 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 30K (at -0.75 -1.5) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 10 ADC6))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 15 BATT_SW))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EF072)
    (at 100.5 107.5 180)
    (attr smd)
    (fp_text reference R39 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 10K (at 0.75 1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 10 ADC6))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584EEE21)
    (at 72 122.5 270)
    (attr smd)
    (fp_text reference R67 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 2 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 39 TELEM_BL_RX))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 2 /open_evo_misc/SERIAL_IN))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C500C)
    (at 149.5 81.5 270)
    (attr smd)
    (fp_text reference R69 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 2K (at 2 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 22 MPX_RF_EN))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 59 "Net-(C49-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C5123)
    (at 160 76.5 90)
    (attr smd)
    (fp_text reference R71 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 5K1 (at 2 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 60 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 120 CPPM_OUT_A))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 584C512C)
    (at 157.75 76.5 270)
    (attr smd)
    (fp_text reference R73 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 10K (at -2 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 60 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584DA888)
    (at 140.5 83.5 270)
    (attr smd)
    (fp_text reference R74 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 23 MPX_RX))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 64 "Net-(P11-Pad5)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer F.Cu) (tedit 55E07978)
    (at 91.5 77 270)
    (attr smd)
    (fp_text reference C62 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 -1.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SM0603 (layer B.Cu) (tedit 55E07978)
    (at 107.5 73.5 270)
    (attr smd)
    (fp_text reference C63 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 1.2 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Mask)
      (net 16 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:SOIC-8 (layer F.Cu) (tedit 58517A80)
    (at 98.5 77)
    (fp_text reference U2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MCP6002 (at 0 4.5) (layer F.SilkS))
    (fp_text user 1 (at -2.7 2.7) (layer F.SilkS))
    (pad 1 smd rect (at -1.9 2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 3 ADC0))
    (pad 2 smd rect (at -0.63 2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 73 "Net-(R17-Pad1)"))
    (pad 3 smd rect (at 0.64 2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 54 "Net-(C18-Pad1)"))
    (pad 4 smd rect (at 1.91 2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 5 smd rect (at 1.91 -2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 54 "Net-(C18-Pad1)"))
    (pad 6 smd rect (at 0.64 -2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 74 "Net-(R36-Pad1)"))
    (pad 7 smd rect (at -0.63 -2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 4 ADC1))
    (pad 8 smd rect (at -1.9 -2.667) (size 0.6 1.55) (layers F.Cu F.Mask)
      (net 1 +5V))
  )
  (module modules:SOIC-8 (layer B.Cu) (tedit 58517A2D)
    (at 117.25 78)
    (fp_text reference U3 (at 0 0) (layer B.SilkS) hide)
    (fp_text value MCP6002 (at 1 4.5) (layer B.SilkS))
    (fp_text user 1 (at -2.7 -2.7) (layer B.SilkS))
    (pad 1 smd rect (at -1.9 -2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 6 ADC2))
    (pad 2 smd rect (at -0.63 -2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 67 "Net-(R1-Pad1)"))
    (pad 3 smd rect (at 0.64 -2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 55 "Net-(C28-Pad1)"))
    (pad 4 smd rect (at 1.91 -2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 5 smd rect (at 1.91 2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 55 "Net-(C28-Pad1)"))
    (pad 6 smd rect (at 0.64 2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 72 "Net-(R10-Pad2)"))
    (pad 7 smd rect (at -0.63 2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 7 ADC3))
    (pad 8 smd rect (at -1.9 2.667) (size 0.6 1.55) (layers B.Cu B.Mask)
      (net 1 +5V))
  )
  (module modules:DIN_MAB-7-SV locked (layer F.Cu) (tedit 55E07880)
    (at 136 101.5)
    (fp_text reference P10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TRAINER (at 0 -1.1) (layer F.SilkS))
    (pad 4 thru_hole circle (at 0 -6) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 118 "/open_evo_misc/CPPM_IO_(was_MPX_SERIAL_O)"))
    (pad 6 thru_hole circle (at -6 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(C60-Pad1)"))
    (pad 5 thru_hole circle (at 6 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(D12-Pad1)"))
    (pad 7 thru_hole circle (at 0 6) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 /open_evo_misc/SERIAL_IN))
    (pad 1 thru_hole circle (at -4.24 -4.24) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 BATT_CHG))
    (pad 2 thru_hole circle (at 4.24 -4.24) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 BATT_SW))
    (pad 3 thru_hole circle (at 4.24 4.24) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 8 thru_hole circle (at -2.75 2.75) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module modules:STM_LQFP100 (layer B.Cu) (tedit 584EEDE4)
    (at 63.3 104.6 315)
    (solder_mask_margin 0.1)
    (clearance 0.19)
    (fp_text reference U1 (at 0 0 315) (layer B.SilkS) hide)
    (fp_text value ATmega2560 (at 2.015254 0.318198 405) (layer B.SilkS))
    (fp_text user 1 (at 6.9 7.7 495) (layer B.SilkS))
    (pad 1 smd rect (at 6 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 75 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at 5.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 39 TELEM_BL_RX))
    (pad 3 smd rect (at 5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 40 TELEM_BL_TX))
    (pad 4 smd rect (at 4.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 76 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 4 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 77 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 3.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 27 PE4))
    (pad 7 smd rect (at 3 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 28 PE5))
    (pad 8 smd rect (at 2.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 29 PE6))
    (pad 9 smd rect (at 2 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 30 PE7))
    (pad 10 smd rect (at 1.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 11 smd rect (at 1 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 12 smd rect (at 0.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 20 LCD_RST_N))
    (pad 13 smd rect (at 0 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 19 LCD_MOSI))
    (pad 14 smd rect (at -0.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 21 LCD_SCK_P))
    (pad 15 smd rect (at -1 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 115 Piezo_Speaker))
    (pad 16 smd rect (at -1.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 131 /open_evo_cpu/hold_power_FA))
    (pad 17 smd rect (at -2 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 78 /open_evo_cpu/dsc_activated_FA))
    (pad 18 smd rect (at -2.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 79 /open_evo_cpu/rf_activated_FA))
    (pad 19 smd rect (at -3 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 49 uSD_NSS))
    (pad 20 smd rect (at -3.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 24 PB1/SCK))
    (pad 21 smd rect (at -4 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 25 PB2/MOSI))
    (pad 22 smd rect (at -4.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 26 PB3/MISO))
    (pad 23 smd rect (at -5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 80 /open_evo_cpu/buzzer_FA))
    (pad 24 smd rect (at -5.5 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 141 /open_evo_cpu/TRN_FA))
    (pad 25 smd rect (at -6 7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 81 /open_evo_cpu/ppm_out_FA))
    (pad 26 smd rect (at -7.75 6 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 132 /open_evo_cpu/PB7))
    (pad 27 smd rect (at -7.75 5.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 82 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at -7.75 5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 83 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at -7.75 4.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 84 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at -7.75 4 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 38 RESET-))
    (pad 31 smd rect (at -7.75 3.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 32 smd rect (at -7.75 3 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 33 smd rect (at -7.75 2.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 56 "Net-(C34-Pad1)"))
    (pad 34 smd rect (at -7.75 2 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 57 "Net-(C35-Pad1)"))
    (pad 35 smd rect (at -7.75 1.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 85 "Net-(U1-Pad35)"))
    (pad 36 smd rect (at -7.75 1 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 117 CPPM_IN))
    (pad 37 smd rect (at -7.75 0.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 86 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at -7.75 0 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 120 CPPM_OUT_A))
    (pad 39 smd rect (at -7.75 -0.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 121 CPPM_OUT_B))
    (pad 40 smd rect (at -7.75 -1 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 124 /open_evo_cpu/CPPM_OUT_C))
    (pad 41 smd rect (at -7.75 -1.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 87 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at -7.75 -2 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 138 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -7.75 -2.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 88 /open_evo_cpu/I2C_SCL))
    (pad 44 smd rect (at -7.75 -3 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 89 /open_evo_cpu/I2C_SDA))
    (pad 45 smd rect (at -7.75 -3.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 90 "Net-(U1-Pad45)"))
    (pad 46 smd rect (at -7.75 -4 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 91 "Net-(U1-Pad46)"))
    (pad 47 smd rect (at -7.75 -4.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 92 "Net-(U1-Pad47)"))
    (pad 48 smd rect (at -7.75 -5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 93 "Net-(U1-Pad48)"))
    (pad 49 smd rect (at -7.75 -5.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 94 "Net-(U1-Pad49)"))
    (pad 50 smd rect (at -7.75 -6 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 95 "Net-(U1-Pad50)"))
    (pad 51 smd rect (at -6 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 137 Trainer_Master_N))
    (pad 52 smd rect (at -5.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 106 CARD_DETECT_N))
    (pad 53 smd rect (at -5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 18 LCD_CS_P))
    (pad 54 smd rect (at -4.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 17 LCD_A0))
    (pad 55 smd rect (at -4 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 51 PWR_HOLD))
    (pad 56 smd rect (at -3.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 107 PWR_SW_STATUS))
    (pad 57 smd rect (at -3 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 133 /open_evo_cpu/PWR_LED))
    (pad 58 smd rect (at -2.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 96 "Net-(U1-Pad58)"))
    (pad 59 smd rect (at -2 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 97 "Net-(U1-Pad59)"))
    (pad 60 smd rect (at -1.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 98 "Net-(U1-Pad60)"))
    (pad 61 smd rect (at -1 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 62 smd rect (at -0.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 63 smd rect (at 0 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 23 MPX_RX))
    (pad 64 smd rect (at 0.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 111 MPX_TX))
    (pad 65 smd rect (at 1 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 22 MPX_RF_EN))
    (pad 66 smd rect (at 1.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 99 "Net-(U1-Pad66)"))
    (pad 67 smd rect (at 2 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 31 PJ4))
    (pad 68 smd rect (at 2.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 32 PJ5))
    (pad 69 smd rect (at 3 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 33 PJ6))
    (pad 70 smd rect (at 3.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 100 "Net-(U1-Pad70)"))
    (pad 71 smd rect (at 4 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 48 TRIM_BUTT_7))
    (pad 72 smd rect (at 4.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 47 TRIM_BUTT_6))
    (pad 73 smd rect (at 5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 46 TRIM_BUTT_5))
    (pad 74 smd rect (at 5.5 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 45 TRIM_BUTT_4))
    (pad 75 smd rect (at 6 -7.75 315) (size 0.3 1.2) (layers B.Cu B.Mask)
      (net 44 TRIM_BUTT_3))
    (pad 76 smd rect (at 7.75 -6 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 43 TRIM_BUTT_2))
    (pad 77 smd rect (at 7.75 -5.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 42 TRIM_BUTT_1))
    (pad 78 smd rect (at 7.75 -5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 41 TRIM_BUTT_0))
    (pad 79 smd rect (at 7.75 -4.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 34 PJ7))
    (pad 80 smd rect (at 7.75 -4 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 81 smd rect (at 7.75 -3.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 82 smd rect (at 7.75 -3 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 37 PK7))
    (pad 83 smd rect (at 7.75 -2.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 36 PK6))
    (pad 84 smd rect (at 7.75 -2 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 35 PK5))
    (pad 85 smd rect (at 7.75 -1.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 101 "Net-(U1-Pad85)"))
    (pad 86 smd rect (at 7.75 -1 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 102 "Net-(U1-Pad86)"))
    (pad 87 smd rect (at 7.75 -0.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 5 ADC10))
    (pad 88 smd rect (at 7.75 0 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 13 ADC9))
    (pad 89 smd rect (at 7.75 0.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 12 ADC8))
    (pad 90 smd rect (at 7.75 1 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 11 ADC7))
    (pad 91 smd rect (at 7.75 1.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 10 ADC6))
    (pad 92 smd rect (at 7.75 2 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 9 ADC5))
    (pad 93 smd rect (at 7.75 2.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 8 ADC4))
    (pad 94 smd rect (at 7.75 3 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 7 ADC3))
    (pad 95 smd rect (at 7.75 3.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 6 ADC2))
    (pad 96 smd rect (at 7.75 4 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 4 ADC1))
    (pad 97 smd rect (at 7.75 4.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 3 ADC0))
    (pad 98 smd rect (at 7.75 5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 52 "Net-(C5-Pad1)"))
    (pad 99 smd rect (at 7.75 5.5 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 16 GND))
    (pad 100 smd rect (at 7.75 6 315) (size 1.2 0.3) (layers B.Cu B.Mask)
      (net 53 "Net-(C8-Pad1)"))
  )
  (module modules:SOD-123W (layer F.Cu) (tedit 55E0772C)
    (at 124.5 101.5 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value PMEG3010ER (at 0 2.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1.2 1.2) (layers F.Cu F.Mask)
      (net 119 /open_evo_misc/BATT_7V2))
    (pad 2 smd rect (at 1.5 0 90) (size 1.2 1.2) (layers F.Cu F.Mask)
      (net 14 BATT_CHG))
  )
  (module modules:HRS_uSD_DM3CS locked (layer F.Cu) (tedit 584EF1E0)
    (at 68.5 84)
    (fp_text reference P9 (at -3 -5) (layer F.SilkS) hide)
    (fp_text value u_SD_CARD (at -6.75 3.75 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 104 "Net-(P9-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 135 "Net-(P9-Pad2)"))
    (pad 3 smd rect (at -2.2 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 61 "Net-(P9-Pad3)"))
    (pad 4 smd rect (at -3.3 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 58 +3V3))
    (pad 5 smd rect (at -4.4 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 62 "Net-(P9-Pad5)"))
    (pad 6 smd rect (at -5.5 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 7 smd rect (at -6.6 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 63 "Net-(P9-Pad7)"))
    (pad 8 smd rect (at -7.7 0) (size 0.7 2) (layers F.Cu F.Mask)
      (net 105 "Net-(P9-Pad8)"))
    (pad 10 smd rect (at 3.55 -0.5) (size 1.5 2.6) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 10 smd rect (at 1.65 -12.8) (size 1.2 1.2) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 9 smd rect (at -1.4 -12.7) (size 2.7 1.4) (layers F.Cu F.Mask)
      (net 106 CARD_DETECT_N))
    (pad 10 smd rect (at -6.3 -12.7) (size 2.7 1.4) (layers F.Cu F.Mask)
      (net 16 GND))
    (pad 10 smd rect (at -9.8 -0.5) (size 1 2.6) (layers F.Cu F.Mask)
      (net 16 GND))
  )
  (module modules:Sounder_ABT-436-RC locked (layer B.Cu) (tedit 55E0769F)
    (at 136 73.5 180)
    (fp_text reference SP1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value PIEZO (at 0 -1.2 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -5 0 180) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 16 GND))
    (pad 2 thru_hole circle (at 5 0 180) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 115 Piezo_Speaker))
  )
  (module modules:JUMPER_2PAD (layer F.Cu) (tedit 584EEFDC)
    (at 64.9 101.2)
    (fp_text reference JP1 (at 0 -1.3) (layer F.SilkS) hide)
    (fp_text value MPX_SERIAL (at 2.1 -1.7) (layer F.SilkS))
    (pad 2 smd rect (at 0.6604 0) (size 1.00076 1.00076) (layers F.Cu F.Mask)
      (net 111 MPX_TX))
    (pad 1 smd rect (at -0.6604 0) (size 1.00076 1.00076) (layers F.Cu F.Mask)
      (net 120 CPPM_OUT_A))
  )
  (module modules:SW_COMAX6_SPDT locked (layer B.Cu) (tedit 584EF115)
    (at 136 89)
    (fp_text reference SW23 (at 0 -1.7) (layer B.SilkS) hide)
    (fp_text value Power (at 0 2.25) (layer B.SilkS) hide)
    (pad "" thru_hole circle (at -6 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask B.SilkS))
    (pad "" thru_hole circle (at 6 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 16 GND))
    (pad 1 thru_hole circle (at -3 0) (size 2 2) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 113 "Net-(D8-Pad1)"))
    (pad 3 thru_hole circle (at 3 0) (size 2 2) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 110 "Net-(SW23-Pad3)"))
  )
  (module modules:aerial_tag (layer F.Cu) (tedit 55E04327)
    (at 151.9 91.4 135)
    (fp_text reference P12 (at 0 -2.262742 135) (layer F.SilkS) hide)
    (fp_text value MPX_Aerial (at 0 2.1 135) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 135) (size 4.5 2.5) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 50 /open_evo_misc/MPX_ANT))
  )
  (module modules:LED-5MM locked (layer B.Cu) (tedit 55E0719A)
    (at 115.5 89)
    (descr "LED vertical 5mm")
    (tags "LED-5MM LED 5mm")
    (fp_text reference D2 (at 0 0) (layer B.SilkS) hide)
    (fp_text value POWER (at 0.08 3.75) (layer B.SilkS))
    (fp_text user K (at -3.1 0) (layer B.SilkS))
    (pad 1 thru_hole rect (at -1.27134 0 270) (size 1.69926 1.69926) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 108 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 1.26866 0) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 119 /open_evo_misc/BATT_7V2))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 -0.012))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 178.5 132 90)
    (fp_text reference SW21 (at -2 0 180) (layer B.SilkS) hide)
    (fp_text value DIGI (at -4.5 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 71 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 71 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
    (pad 2 smd rect (at 2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 161.5 132 90)
    (fp_text reference SW20 (at -2 0 180) (layer B.SilkS) hide)
    (fp_text value REV/CLR (at -4.5 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 71 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 71 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
    (pad 2 smd rect (at 2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 127.5 132)
    (fp_text reference SW18 (at -2 0 90) (layer B.SilkS) hide)
    (fp_text value ENTER (at -4.5 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
    (pad 2 smd rect (at 2.25 -4.2) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 144.5 132 180)
    (fp_text reference SW17 (at -2 0 270) (layer B.SilkS) hide)
    (fp_text value ENTER (at -4.5 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 180) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 180) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 180) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
    (pad 2 smd rect (at 2.25 -4.2 180) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 110.5 132 90)
    (fp_text reference SW16 (at -2 0 180) (layer B.SilkS) hide)
    (fp_text value UP (at -4.5 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
    (pad 2 smd rect (at 2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA326)
    (at 169 79.5 270)
    (fp_text reference SW15 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_LH_R (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 44 TRIM_BUTT_3))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 44 TRIM_BUTT_3))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 93.5 132 90)
    (fp_text reference SW14 (at -2 0 180) (layer B.SilkS) hide)
    (fp_text value DN (at -4.5 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 70 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
    (pad 2 smd rect (at 2.25 -4.2 90) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA31E)
    (at 184 79.5 270)
    (fp_text reference SW13 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_LH_L (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 41 TRIM_BUTT_0))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 41 TRIM_BUTT_0))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 93.5 118 270)
    (fp_text reference SW12 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value MEMORY (at -4.5 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 69 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 69 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA32B)
    (at 176.5 87 270)
    (fp_text reference SW11 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_LH_DN (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 42 TRIM_BUTT_1))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 42 TRIM_BUTT_1))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 110.5 118 270)
    (fp_text reference SW10 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TIMERS (at -4.5 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 69 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 69 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA319)
    (at 176.5 72 270)
    (fp_text reference SW9 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_LH_UP (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 123 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 43 TRIM_BUTT_2))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 43 TRIM_BUTT_2))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 127.5 118 270)
    (fp_text reference SW8 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value SERVOS (at -4.5 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 69 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 69 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA304)
    (at 88 79.5 270)
    (fp_text reference SW7 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_RH_R (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 47 TRIM_BUTT_6))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 47 TRIM_BUTT_6))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 144.5 118 270)
    (fp_text reference SW6 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value MIXERS (at -4.5 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 68 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 68 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 37 PK7))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA2FE)
    (at 103 79.5 270)
    (fp_text reference SW5 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_RH_L (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 46 TRIM_BUTT_5))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 46 TRIM_BUTT_5))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 161.5 118 270)
    (fp_text reference SW4 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value CONTROLS (at -4.5 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 68 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 68 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 36 PK6))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA310)
    (at 95.5 87 270)
    (fp_text reference SW3 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_RH_DN (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 45 TRIM_BUTT_4))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 45 TRIM_BUTT_4))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 55E01395)
    (at 178.5 118 270)
    (fp_text reference SW2 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value SETUP (at -4.5 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 68 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 68 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 35 PK5))
  )
  (module modules:sw_tact_6x6_smd locked (layer B.Cu) (tedit 584DA2EA)
    (at 95.5 72 270)
    (fp_text reference SW1 (at -2 0 360) (layer B.SilkS) hide)
    (fp_text value TRIM_RH_UP (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 1 smd rect (at -2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 122 "Net-(R24-Pad2)"))
    (pad 2 smd rect (at 2.25 4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 48 TRIM_BUTT_7))
    (pad 2 smd rect (at 2.25 -4.2 270) (size 1.3 2.1) (layers B.Cu B.Mask)
      (net 48 TRIM_BUTT_7))
  )
  (module modules:SM0603 (layer F.Cu) (tedit 584EF0C1)
    (at 122.5 107.5 270)
    (attr smd)
    (fp_text reference R20 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 100K (at -2 -0.25 540) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 119 /open_evo_misc/BATT_7V2))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Mask)
      (net 109 "Net-(D8-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:Logo_openTX_15mm (layer F.Cu) (tedit 55F0A611)
    (at 203.5 86.5)
    (fp_text reference LOGO1 (at 0 10) (layer F.SilkS) hide)
    (fp_text value OPEN_TX (at 0 -10) (layer F.SilkS) hide)
  )
  (module modules:Lumberg_732782 (layer F.Cu) (tedit 584EDA22)
    (at 149.25 109.25 90)
    (descr "Pin strip 2pin")
    (tags "CONN DEV")
    (fp_text reference P8 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BATT (at 0 -5 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.25 0 90) (size 1.524 2.19964) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 2 thru_hole oval (at 1.25 0 90) (size 1.524 2.19964) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 BATT_CHG))
  )
  (target plus (at 71 131.5) (size 5) (width 0.1) (layer Edge.Cuts))
  (target plus (at 208.5 101.5) (size 5) (width 0.1) (layer Edge.Cuts))
  (gr_text "Licensed under the TAPR OHL\n(www.tapr.org/OHL)" (at 210 111.5) (layer F.SilkS))
  (dimension 31.5 (width 0.3) (layer Cmts.User)
    (gr_text "31.500 mm" (at 204.35 129.75 270) (layer Cmts.User))
    (feature1 (pts (xy 153.75 145.5) (xy 205.7 145.5)))
    (feature2 (pts (xy 153.75 114) (xy 205.7 114)))
    (crossbar (pts (xy 203 114) (xy 203 145.5)))
    (arrow1a (pts (xy 203 145.5) (xy 202.413579 144.373496)))
    (arrow1b (pts (xy 203 145.5) (xy 203.586421 144.373496)))
    (arrow2a (pts (xy 203 114) (xy 202.413579 115.126504)))
    (arrow2b (pts (xy 203 114) (xy 203.586421 115.126504)))
  )
  (gr_text "PCB Layout Copyright © 2015 R Kilvington" (at 140.5 143.75) (layer B.Cu))
  (gr_text "PCB Layout Copyright © 2015 R Kilvington" (at 131.5 143.75) (layer F.Cu))
  (gr_text V1.002 (at 203.75 124.25) (layer F.Cu))
  (dimension 77 (width 0.3) (layer Cmts.User)
    (gr_text "77.000 mm" (at 242.35 107 270) (layer Cmts.User))
    (feature1 (pts (xy 226 145.5) (xy 243.7 145.5)))
    (feature2 (pts (xy 226 68.5) (xy 243.7 68.5)))
    (crossbar (pts (xy 241 68.5) (xy 241 145.5)))
    (arrow1a (pts (xy 241 145.5) (xy 240.413579 144.373496)))
    (arrow1b (pts (xy 241 145.5) (xy 241.586421 144.373496)))
    (arrow2a (pts (xy 241 68.5) (xy 240.413579 69.626504)))
    (arrow2b (pts (xy 241 68.5) (xy 241.586421 69.626504)))
  )
  (dimension 180 (width 0.3) (layer Cmts.User)
    (gr_text "180.000 mm" (at 136 33.650001) (layer Cmts.User))
    (feature1 (pts (xy 226 68.5) (xy 226 32.300001)))
    (feature2 (pts (xy 46 68.5) (xy 46 32.300001)))
    (crossbar (pts (xy 46 35.000001) (xy 226 35.000001)))
    (arrow1a (pts (xy 226 35.000001) (xy 224.873496 35.586422)))
    (arrow1b (pts (xy 226 35.000001) (xy 224.873496 34.41358)))
    (arrow2a (pts (xy 46 35.000001) (xy 47.126504 35.586422)))
    (arrow2b (pts (xy 46 35.000001) (xy 47.126504 34.41358)))
  )
  (gr_line (start 46 117.5) (end 74 145.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226 117.5) (end 198 145.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74 145.5) (end 198 145.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 46 68.5) (end 46 117.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226 68.5) (end 226 117.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 20.5 (width 0.3) (layer Cmts.User)
    (gr_text "20.500 mm" (at 125.35 78.75 90) (layer Cmts.User))
    (feature1 (pts (xy 115.5 68.5) (xy 126.7 68.5)))
    (feature2 (pts (xy 115.5 89) (xy 126.7 89)))
    (crossbar (pts (xy 124 89) (xy 124 68.5)))
    (arrow1a (pts (xy 124 68.5) (xy 124.586421 69.626504)))
    (arrow1b (pts (xy 124 68.5) (xy 123.413579 69.626504)))
    (arrow2a (pts (xy 124 89) (xy 124.586421 87.873496)))
    (arrow2b (pts (xy 124 89) (xy 123.413579 87.873496)))
  )
  (gr_line (start 46 68.5) (end 226 68.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.5 82) (xy 71.5 80.5) (xy 59.5 80.5) (xy 57.5 82) (xy 57.5 72)
        (xy 73.5 72)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 45.9 68.4) (xy 45.9 117.6) (xy 73.9 145.6) (xy 198.1 145.6) (xy 226.1 117.6)
        (xy 226.1 68.4)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 45.9 68.4) (xy 45.9 117.6) (xy 73.9 145.6) (xy 198.1 145.6) (xy 226.1 117.6)
        (xy 226.1 68.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 152 84) (xy 148 85) (xy 145 88.5) (xy 144 91.5) (xy 145 95.5)
        (xy 148 98.05) (xy 160.85 98.05) (xy 162.95 95.95) (xy 162.95 90.9) (xy 156.8 90.9)
        (xy 156.8 85.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 145.2 88.7) (xy 148.2 85.3) (xy 152 84.3) (xy 156.4 85.9) (xy 156.4 91.3)
        (xy 162.6 91.3) (xy 162.6 96.1) (xy 155.7 98.05) (xy 148 98.05) (xy 145.4 95.3)
        (xy 144.4 91.5)
      )
    )
  )
)
