(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 0)
    (no_connects 0)
    (area 107.391999 78.689999 176.072001 122.732001)
    (thickness 1.6)
    (drawings 7)
    (tracks 146)
    (zones 0)
    (modules 38)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(DISP1-Pad1)")
  (net 8 "Net-(DISP1-Pad2)")
  (net 9 "Net-(DISP1-Pad3)")
  (net 10 "Net-(DISP1-Pad4)")
  (net 11 "Net-(DISP1-Pad5)")
  (net 12 "Net-(DISP1-Pad6)")
  (net 13 "Net-(DISP1-Pad7)")
  (net 14 "Net-(DISP1-Pad8)")
  (net 15 "Net-(DISP1-Pad9)")
  (net 16 "Net-(DISP1-Pad10)")
  (net 17 "Net-(DISP1-Pad11)")
  (net 18 "Net-(DISP1-Pad12)")
  (net 19 "Net-(DISP1-Pad13)")
  (net 20 "Net-(DISP1-Pad14)")
  (net 21 "Net-(DISP1-Pad15)")
  (net 22 "Net-(DISP1-Pad16)")
  (net 23 "Net-(DISP1-Pad17)")
  (net 24 "Net-(DISP1-Pad18)")
  (net 25 "Net-(DISP1-Pad19)")
  (net 26 "Net-(DISP1-Pad20)")
  (net 27 "Net-(DISP1-Pad21)")
  (net 28 "Net-(DISP1-Pad22)")
  (net 29 "Net-(DISP1-Pad24)")
  (net 30 "Net-(DISP1-Pad25)")
  (net 31 "Net-(DISP1-Pad26)")
  (net 32 "Net-(DISP1-Pad27)")
  (net 33 "Net-(DISP1-Pad28)")
  (net 34 "Net-(DISP1-Pad29)")
  (net 35 "Net-(DISP1-Pad30)")
  (net 36 "Net-(DISP1-Pad33)")
  (net 37 "Net-(DISP1-Pad34)")
  (net 38 "Net-(DISP1-Pad35)")
  (net 39 "Net-(DISP1-Pad36)")
  (net 40 "Net-(Q1-Pad1)")
  (net 41 "Net-(Q1-Pad2)")
  (net 42 "Net-(R1-Pad1)")
  (net 43 "Net-(R17-Pad1)")
  (net 44 "Net-(R17-Pad2)")
  (net 45 "Net-(U1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(DISP1-Pad1)")
    (add_net "Net-(DISP1-Pad10)")
    (add_net "Net-(DISP1-Pad11)")
    (add_net "Net-(DISP1-Pad12)")
    (add_net "Net-(DISP1-Pad13)")
    (add_net "Net-(DISP1-Pad14)")
    (add_net "Net-(DISP1-Pad15)")
    (add_net "Net-(DISP1-Pad16)")
    (add_net "Net-(DISP1-Pad17)")
    (add_net "Net-(DISP1-Pad18)")
    (add_net "Net-(DISP1-Pad19)")
    (add_net "Net-(DISP1-Pad2)")
    (add_net "Net-(DISP1-Pad20)")
    (add_net "Net-(DISP1-Pad21)")
    (add_net "Net-(DISP1-Pad22)")
    (add_net "Net-(DISP1-Pad24)")
    (add_net "Net-(DISP1-Pad25)")
    (add_net "Net-(DISP1-Pad26)")
    (add_net "Net-(DISP1-Pad27)")
    (add_net "Net-(DISP1-Pad28)")
    (add_net "Net-(DISP1-Pad29)")
    (add_net "Net-(DISP1-Pad3)")
    (add_net "Net-(DISP1-Pad30)")
    (add_net "Net-(DISP1-Pad33)")
    (add_net "Net-(DISP1-Pad34)")
    (add_net "Net-(DISP1-Pad35)")
    (add_net "Net-(DISP1-Pad36)")
    (add_net "Net-(DISP1-Pad4)")
    (add_net "Net-(DISP1-Pad5)")
    (add_net "Net-(DISP1-Pad6)")
    (add_net "Net-(DISP1-Pad7)")
    (add_net "Net-(DISP1-Pad8)")
    (add_net "Net-(DISP1-Pad9)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(U1-Pad4)")
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 58FE9BE9)
    (at 112.649 84.836 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C4 (at -1.27 2.667 90) (layer F.SilkS))
    (fp_text value .47u (at 1.25 4.21 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58FE9B97)
    (at 115.824 108.966 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value .01u (at 2.5 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58FE9B5F)
    (at 172.974 108.331 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.54 -0.127 180) (layer F.SilkS))
    (fp_text value .01u (at 2.5 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Vertical (layer F.Cu) (tedit 58FE9BE3)
    (at 110.744 90.551)
    (descr "TO-220, Vertical, RM 2.54mm")
    (tags "TO-220 Vertical RM 2.54mm")
    (fp_text reference Q1 (at 2.794 2.921) (layer F.SilkS))
    (fp_text value "Power Transistor" (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.794 2.921) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(DISP1-Pad22)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58FE9B53)
    (at 173.609 94.361 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference BT1 (at -1.905 1.397 360) (layer F.SilkS))
    (fp_text value 9V (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at -1.905 1.397 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module AAA_Myfootprints:rad_cap (layer F.Cu) (tedit 58FE9B5C)
    (at 171.069 115.951)
    (fp_text reference C2 (at 0.127 0.127) (layer F.SilkS))
    (fp_text value 470u (at 0 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ../../../../../../Users/Jim/Downloads/rad_cap.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module AAA_Myfootprints:4Digit7SegmentLED (layer B.Cu) (tedit 58C36B46)
    (at 141.859 100.711)
    (fp_text reference DISP1 (at -17.78 10.16) (layer B.SilkS))
    (fp_text value CA56-11 (at 0 -10.16) (layer B.Fab))
    (pad 1 thru_hole rect (at -21.59 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(DISP1-Pad1)"))
    (pad 2 thru_hole circle (at -19.05 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(DISP1-Pad2)"))
    (pad 3 thru_hole circle (at -16.51 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(DISP1-Pad3)"))
    (pad 4 thru_hole circle (at -13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(DISP1-Pad4)"))
    (pad 5 thru_hole circle (at -11.43 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(DISP1-Pad5)"))
    (pad 6 thru_hole circle (at -8.89 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(DISP1-Pad6)"))
    (pad 7 thru_hole circle (at -6.35 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(DISP1-Pad7)"))
    (pad 8 thru_hole circle (at -3.81 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(DISP1-Pad8)"))
    (pad 9 thru_hole circle (at -1.27 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(DISP1-Pad9)"))
    (pad 10 thru_hole circle (at 1.27 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(DISP1-Pad10)"))
    (pad 11 thru_hole circle (at 3.81 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(DISP1-Pad11)"))
    (pad 12 thru_hole circle (at 6.35 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(DISP1-Pad12)"))
    (pad 13 thru_hole circle (at 8.89 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(DISP1-Pad13)"))
    (pad 14 thru_hole circle (at 11.43 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(DISP1-Pad14)"))
    (pad 15 thru_hole circle (at 13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(DISP1-Pad15)"))
    (pad 16 thru_hole circle (at 16.51 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(DISP1-Pad16)"))
    (pad 17 thru_hole circle (at 19.05 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(DISP1-Pad17)"))
    (pad 18 thru_hole circle (at 21.59 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(DISP1-Pad18)"))
    (pad 19 thru_hole circle (at 21.59 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(DISP1-Pad19)"))
    (pad 20 thru_hole circle (at 19.05 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(DISP1-Pad20)"))
    (pad 21 thru_hole circle (at 16.51 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(DISP1-Pad21)"))
    (pad 22 thru_hole circle (at 13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(DISP1-Pad22)"))
    (pad 23 thru_hole circle (at 11.43 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(DISP1-Pad22)"))
    (pad 24 thru_hole circle (at 8.89 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(DISP1-Pad24)"))
    (pad 25 thru_hole circle (at 6.35 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(DISP1-Pad25)"))
    (pad 26 thru_hole circle (at 3.81 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(DISP1-Pad26)"))
    (pad 27 thru_hole circle (at 1.27 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(DISP1-Pad27)"))
    (pad 28 thru_hole circle (at -1.27 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(DISP1-Pad28)"))
    (pad 29 thru_hole circle (at -3.81 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(DISP1-Pad29)"))
    (pad 30 thru_hole circle (at -6.35 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(DISP1-Pad30)"))
    (pad 31 thru_hole circle (at -8.89 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(DISP1-Pad22)"))
    (pad 32 thru_hole circle (at -11.43 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(DISP1-Pad22)"))
    (pad 33 thru_hole circle (at -13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(DISP1-Pad33)"))
    (pad 34 thru_hole circle (at -16.51 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(DISP1-Pad34)"))
    (pad 35 thru_hole circle (at -19.05 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(DISP1-Pad35)"))
    (pad 36 thru_hole circle (at -21.59 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(DISP1-Pad36)"))
    (model ../../../../../../Users/Jim/Documents/KiCad/555/segmentLED.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.368 0.388 0.375))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97FF)
    (at 163.449 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R1 (at 5.207 0.127 90) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "Net-(Q1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B94)
    (at 125.349 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R2 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(DISP1-Pad34)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97E5)
    (at 122.809 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R3 (at 5.207 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.207 1.905 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(DISP1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97E8)
    (at 120.269 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R4 (at 5.207 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(DISP1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B8D)
    (at 120.269 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R5 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(DISP1-Pad36)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B90)
    (at 122.809 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R6 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(DISP1-Pad35)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B6A)
    (at 155.194 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R7 (at 4.953 0 270) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B73)
    (at 138.049 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R8 (at 4.699 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(DISP1-Pad29)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B79)
    (at 140.589 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R9 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(DISP1-Pad28)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97F0)
    (at 138.049 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R10 (at 5.207 -0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(DISP1-Pad8)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97ED)
    (at 130.429 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R11 (at 5.207 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(DISP1-Pad5)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B6F)
    (at 135.509 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R12 (at 4.953 0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(DISP1-Pad30)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97F2)
    (at 135.509 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R13 (at 5.207 -0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(DISP1-Pad7)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B87)
    (at 148.209 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R14 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(DISP1-Pad25)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97F7)
    (at 148.209 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R15 (at 5.207 -0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(DISP1-Pad12)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE97FA)
    (at 145.669 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R16 (at 4.953 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(DISP1-Pad11)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B9B)
    (at 109.474 107.696 270)
    (tags "resistor, tht")
    (fp_text reference R17 (at 4.826 0 270) (layer F.SilkS))
    (fp_text value 200k (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(R17-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(R17-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9BA0)
    (at 112.649 117.856 90)
    (tags "resistor, tht")
    (fp_text reference R18 (at 5.08 0.127 90) (layer F.SilkS))
    (fp_text value 500k (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(R17-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B7C)
    (at 143.129 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R19 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(DISP1-Pad27)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B84)
    (at 145.669 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R20 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(DISP1-Pad26)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B64)
    (at 163.449 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R21 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(DISP1-Pad19)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9802)
    (at 160.909 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R22 (at 5.207 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(DISP1-Pad17)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9808)
    (at 155.829 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R23 (at 5.207 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(DISP1-Pad15)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9B67)
    (at 158.369 110.871 270)
    (tags "resistor, tht")
    (fp_text reference R24 (at 4.953 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(DISP1-Pad21)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:Resistor_THT (layer F.Cu) (tedit 58FE9806)
    (at 158.369 90.551 90)
    (tags "resistor, tht")
    (fp_text reference R25 (at 4.953 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(DISP1-Pad16)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.27 0.27 0.27))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:switch_sliding (layer F.Cu) (tedit 58FE9B26)
    (at 172.974 88.646 90)
    (fp_text reference SW1 (at 2.032 -3.81 90) (layer F.SilkS))
    (fp_text value SW_SPST (at 2.54 10.16 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 5.08 5.08) (drill 3.302) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 5.08 5.08) (drill 3.302) (layers *.Cu *.Mask)
      (net 41 "Net-(Q1-Pad2)"))
    (model ../../../../../../Users/Jim/Documents/KiCad/555/switch_slider.wrl
      (at (xyz 0.12 0 0))
      (scale (xyz 0.45 0.45 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58FE9B4B)
    (at 166.624 91.186)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference SW2 (at 0 -2.54) (layer F.SilkS))
    (fp_text value PushButton (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module AAA_Myfootprints:DIP8 (layer F.Cu) (tedit 58FE9BD5)
    (at 170.434 101.346)
    (fp_text reference U1 (at 0.254 -4.064) (layer F.SilkS))
    (fp_text value LM555N (at 0 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 "Net-(R1-Pad1)"))
    (pad 3 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(R17-Pad1)"))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 6 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 8 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "Net-(Q1-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz -0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AAA_Myfootprints:DIP8 (layer F.Cu) (tedit 58FE9BD0)
    (at 113.284 100.711)
    (fp_text reference U2 (at 0 -3.937) (layer F.SilkS))
    (fp_text value LM555N (at 0 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 3 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 "Net-(Q1-Pad1)"))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(R17-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 6 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 7 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(R17-Pad2)"))
    (pad 8 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(R17-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz -0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58FE9BB5)
    (at 116.332 118.618)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference FAS1 (at -1.524 3.048) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58FE9BC3)
    (at 167.386 81.28)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference FAS2 (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_text "EASY BUTTON PCB" (at 143.002 100.838 180) (layer F.SilkS))
  (gr_text "J DERVAY\n20170424\nREV1" (at 152.146 85.598 180) (layer B.SilkS))
  (gr_line (start 176.022 78.74) (end 163.576 78.74) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 176.022 122.682) (end 176.022 78.74) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.442 122.682) (end 176.022 122.682) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.442 78.74) (end 107.442 122.682) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.576 78.74) (end 107.442 78.74) (angle 90) (layer Edge.Cuts) (width 0.1))
)
