(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.89)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (42 "Eco1.User" user "User.Eco1")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.8) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
      (castellated_pads yes)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 0.15 0.15)
    (pcbplotparams
      (layerselection 0x0000080_7ffffffe)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits false)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Print/")
    )
  )
  (net 0 "")
  (net 1 "+BATT")
  (net 2 "GND")
  (net 3 "Net-(JP1-A)")
  (net 4 "Net-(D1-K)")
  (net 5 "Net-(D1-A)")
  (net 6 "Net-(U2-PROG)")
  (net 7 "ALERT")
  (net 8 "Net-(JP1-B)")
  (net 9 "Net-(JP2-B)")
  (net 10 "VBUS")
  (net 11 "/SCL_PMIC")
  (net 12 "/SDA_PMIC")
  (net 13 "unconnected-(J3-Pad2)")
  (net 14 "unconnected-(J3-SHIELD1-PadS1)")
  (net 15 "unconnected-(J3-SHIELD2-PadS2)")
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 90.856 88.238 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 3-pole, open")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr smd exclude_from_pos_files)
    (fp_text reference "JP1" (at 1.386 1.6312) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Open" (at 0 2) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(JP1-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 1 "+BATT") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(JP1-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 76.3 77.9)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 94.8485 83.772 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -0.0115 -1.232) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 87.9415 91.472)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0.1425 1.232 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/SDA_PMIC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(JP1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 81.034 85.774)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0.89 1.694) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 7 "ALERT") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(JP2-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 84.85 85.62)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -0.308 1.232) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(JP2-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 91.3065 83.772 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0.1425 -1.232) (layer "F.SilkS"))
    (fp_text value "2K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2-PROG)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 95.014 76.6975 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 2.0115 0) (layer "F.SilkS"))
    (fp_text value "0.01µ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Castellated_PinHeaders_1x04:Castellated_PinHeader_1x04_P2.54mm" (layer "F.Cu")
    (at 73.7 81.79)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 3.758 9.99) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 4.385 9.89) (layer "F.Fab"))
    (pad "" thru_hole circle (at 2 0) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 7 "ALERT"))
    (pad "" thru_hole circle (at 2 2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 10 "VBUS"))
    (pad "" thru_hole circle (at 2 5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 11 "/SCL_PMIC"))
    (pad "" thru_hole circle (at 2 7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 12 "/SDA_PMIC"))
    (pad "1" thru_hole rect (at 0 0) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 7 "ALERT") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "2" thru_hole rect (at 0 2.54) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 10 "VBUS") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "3" thru_hole rect (at 0 5.08) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 11 "/SCL_PMIC") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "4" thru_hole rect (at 0 7.62) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 12 "/SDA_PMIC") (pinfunction "Pin_4") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 97.016 76.8305 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at -2.1445 0.154) (layer "F.SilkS"))
    (fp_text value "4.7µ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MOLEX_5025850370:MOLEX_5025850370" (layer "F.Cu")
    (at 83.95 79.35 180)
    (property "Check_prices" "https://www.snapeda.com/parts/5025850370/Molex/view-part/?ref=eda")
    (property "Description" "\n1.50mm Pitch, CLIK-Mate PCB Receptacle, Single Row, Surface Mount, Right-Angle, Tin Plating, Positive Lock, 3 Circuits, Natural\n")
    (property "DigiKey_Part_Number" "WM12831TR-ND")
    (property "MANUFACTURER" "Molex")
    (property "MAXIMUM_PACKAGE_HEIGHT" "6.4 mm")
    (property "MF" "Molex")
    (property "MP" "5025850370")
    (property "PARTREV" "C")
    (property "Package" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3618758&manufacturer=Molex&part_name=5025850370&search_term=5025850370")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/5025850370/Molex/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "J3" (at -1.825 -8.235) (layer "F.SilkS"))
    (fp_text value "5025850370" (at 5.16 -6.735) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -3.6 180) (size 0.8 2.9) (layers "F.Cu" "F.Paste")
      (net 1 "+BATT") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 -3.6 180) (size 0.8 2.9) (layers "F.Cu" "F.Paste")
      (net 13 "unconnected-(J3-Pad2)") (pinfunction "2") (pintype "passive+no_connect"))
    (pad "3" smd rect (at 1.5 -3.6 180) (size 0.8 2.9) (layers "F.Cu" "F.Paste")
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (pad "S1" smd rect (at -4.1 1.1 180) (size 1.8 3.8) (layers "F.Cu" "F.Paste")
      (net 14 "unconnected-(J3-SHIELD1-PadS1)") (pinfunction "SHIELD1") (pintype "passive+no_connect"))
    (pad "S2" smd rect (at 4.1 1.1 180) (size 1.8 3.8) (layers "F.Cu" "F.Paste")
      (net 15 "unconnected-(J3-SHIELD2-PadS2)") (pinfunction "SHIELD2") (pintype "passive+no_connect"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 81.1 82.95)
          (xy 79.1 82.95)
          (xy 79.1 80.35)
          (xy 81.1 80.35)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 82.15 76.35)
          (xy 79.95 76.35)
          (xy 79.95 74.35)
          (xy 82.15 74.35)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 87.95 76.35)
          (xy 85.75 76.35)
          (xy 85.75 74.35)
          (xy 87.95 74.35)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 88.8 82.95)
          (xy 86.8 82.95)
          (xy 86.8 80.35)
          (xy 88.8 80.35)
        )
      )
    )
    (zone (net 0) (net_name "") (layers "*.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 81.1 82.95)
          (xy 79.1 82.95)
          (xy 79.1 80.35)
          (xy 81.1 80.35)
        )
      )
    )
    (zone (net 0) (net_name "") (layers "*.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 82.15 76.35)
          (xy 79.95 76.35)
          (xy 79.95 74.35)
          (xy 82.15 74.35)
        )
      )
    )
    (zone (net 0) (net_name "") (layers "*.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 87.95 76.35)
          (xy 85.75 76.35)
          (xy 85.75 74.35)
          (xy 87.95 74.35)
        )
      )
    )
    (zone (net 0) (net_name "") (layers "*.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 88.8 82.95)
          (xy 86.8 82.95)
          (xy 86.8 80.35)
          (xy 88.8 80.35)
        )
      )
    )
  )
  (footprint "Package_DFN_QFN:TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm" (layer "F.Cu")
    (at 81.25 90.7925 90)
    (descr "TDFN, 8 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0168.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "TDFN NoLead")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "MAX17048G+T10")
    (attr smd)
    (fp_text reference "U1" (at -2.2195 -1.174 180) (layer "F.SilkS"))
    (fp_text value "MAX17048G+T10" (at 0 1.95 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.2 -0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.2 0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.2 -0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.2 0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.9875 -0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "CTG") (pintype "unspecified"))
    (pad "2" smd roundrect (at -0.9875 -0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "CELL") (pintype "unspecified"))
    (pad "3" smd roundrect (at -0.9875 0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd roundrect (at -0.9875 0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 0.9875 0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "ALERT") (pinfunction "*ALRT") (pintype "output"))
    (pad "6" smd roundrect (at 0.9875 0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "QSTRT") (pintype "input"))
    (pad "7" smd roundrect (at 0.9875 -0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/SCL_PMIC") (pinfunction "SCL") (pintype "input"))
    (pad "8" smd roundrect (at 0.9875 -0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/SDA_PMIC") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "9" smd rect (at 0 0 90) (size 0.8 1.2) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "EPAD") (pintype "unspecified"))
    (model "C:/Users/viggi/Documents/GitHub/MINDER-BioDAQ---Hardware-repo/PCB and schematics/Component Libraries/3D footprints/MAX17048G_T10.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 95.6032 80.643 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D1" (at 1.953 0.1808) (layer "F.SilkS"))
    (fp_text value "LED_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 91.472 77.0075 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 2.0135 0.616) (layer "F.SilkS"))
    (fp_text value "4.7µ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Castellated_PinHeaders_1x04:Castellated_PinHeader_1x04_P2.54mm" (layer "F.Cu")
    (at 101.96 89.33 180)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 2.788 -2.604) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 4.385 9.89) (layer "F.Fab"))
    (pad "" thru_hole circle (at 2 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 12 "/SDA_PMIC"))
    (pad "" thru_hole circle (at 2 2.54 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 11 "/SCL_PMIC"))
    (pad "" thru_hole circle (at 2 5.08 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 1 "+BATT"))
    (pad "" thru_hole circle (at 2 7.62 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "GND"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 12 "/SDA_PMIC") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "2" thru_hole rect (at 0 2.54 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 11 "/SCL_PMIC") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "3" thru_hole rect (at 0 5.08 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 1 "+BATT") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "4" thru_hole rect (at 0 7.62 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 93.936 91.472 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0.154 -1.232 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/SCL_PMIC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(JP1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 91.8395 80.872 180)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Open-Drain Status Output, in SOT23-5 package")
    (property "ki_keywords" "battery charger lithium")
    (attr smd)
    (fp_text reference "U2" (at -1.1725 2.182) (layer "F.SilkS"))
    (fp_text value "MCP73832-2-OT" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-A)") (pinfunction "STAT") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "V_{SS}") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "V_{BAT}") (pintype "power_out"))
    (pad "4" smd roundrect (at 1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "VBUS") (pinfunction "V_{DD}") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2-PROG)") (pinfunction "PROG") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line locked (start 73.461553 93.428447) (end 73.4798 74.3608)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 73.4798 74.3608) (mid 73.626247 74.007247) (end 73.9798 73.8608)
    (layer "Edge.Cuts"))
  (gr_circle (center 74.84 92.704) (end 75.4 93.214)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc locked (start 101.6564 73.8608) (mid 102.009953 74.007247) (end 102.1564 74.3608)
    (layer "Edge.Cuts"))
  (gr_circle (center 100.69 75.05) (end 101.25 75.56)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc locked (start 102.136 93.474) (mid 101.989553 93.827553) (end 101.636 93.974)
    (layer "Edge.Cuts"))
  (gr_circle (center 74.94 75.052571) (end 75.5 75.562571)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 100.712 92.562571) (end 101.272 93.072571)
    (fill none) (layer "Edge.Cuts"))
  (gr_line locked (start 101.636 93.974) (end 73.916 93.936)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 73.916 93.936) (mid 73.591766 93.769083) (end 73.461553 93.428447)
    (layer "Edge.Cuts"))
  (gr_line locked (start 73.9798 73.8608) (end 101.6564 73.8608)
    (layer "Edge.Cuts"))
  (gr_line locked (start 102.1564 74.3608) (end 102.136 93.474)
    (layer "Edge.Cuts"))
  (gr_text "BATT" (at 90.24 90.24) (layer "F.SilkS"))
  (gr_text "LIPO CHARGER AND POWER MONITOR" (at 87.93 93.474) (layer "F.SilkS"))
  (gr_text "SDA" (at 98.71 89.778 90) (layer "F.SilkS"))
  (gr_text "PMIC" (at 98.248 78.074) (layer "F.SilkS"))
  (gr_text "SDA" (at 76.8986 88.9012 -90) (layer "F.SilkS"))
  (gr_text "SDA" (at 88.854 90.24) (layer "F.SilkS"))
  (gr_text "SCL" (at 91.78 90.24) (layer "F.SilkS"))
  (gr_text "SCL" (at 76.8986 86.539 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 98.71 82.386 90) (layer "F.SilkS"))
  (gr_text "(-)" (at 80.076 74.07 180) (layer "F.SilkS"))
  (gr_text "BATT" (at 98.71 85.004 90) (layer "F.SilkS"))
  (gr_text "(+)\n" (at 91.01 73.916 180) (layer "F.SilkS"))
  (gr_text "ALERT" (at 76.81 80.68 270) (layer "F.SilkS"))
  (gr_text "VBUS\n" (at 76.9 83.54 270) (layer "F.SilkS"))
  (gr_text "SCL" (at 98.71 87.468 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "+BATT") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 75.02 73.39)
        (xy 102.37 73.39)
        (xy 102.2326 93.782)
        (xy 73.454 93.782)
        (xy 73.31 73.47)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 73.302 73.5052)
        (xy 101.482 74.378)
        (xy 101.482 93.782)
        (xy 73.51 93.936)
      )
    )
  )
)
