(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 138.163095 82.275 161.836905 117.825)
    (thickness 0.8)
    (drawings 17)
    (tracks 43)
    (zones 0)
    (modules 5)
    (nets 13)
  )
  (page A4)
  (title_block
    (title "IR Receiver")
    (date 2017-03-21)
    (rev 1.0)
    (company "ECE 445")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory images))
  )
  (net 0 "")
  (net 1 +2V8)
  (net 2 /IR_R)
  (net 3 /IR_L)
  (net 4 GND)
  (net 5 "Net-(U1-Pad2)")
  (net 6 "Net-(U1-Pad3)")
  (net 7 "Net-(U1-Pad4)")
  (net 8 "Net-(U1-Pad7)")
  (net 9 "Net-(U2-Pad2)")
  (net 10 "Net-(U2-Pad3)")
  (net 11 "Net-(U2-Pad4)")
  (net 12 "Net-(U2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net /IR_L)
    (add_net /IR_R)
    (add_net GND)
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad7)")
  )
  (net_class Tight ""
    (clearance 0.16)
    (trace_width 0.16)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module bcan:TSOP572xx (layer F.Cu) (tedit 58D19224)
    (at 142.625 100)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value TSOP57238 (at 0 3) (layer F.Fab))
    (pad 1 smd rect (at -1.775 -1.5) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /IR_R))
    (pad 5 smd rect (at -1.775 1.5) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 6 smd rect (at 1.775 1.5) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 8 smd rect (at 1.775 -1.5) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.775 -0.75) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 5 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -1.775 0) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 6 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -1.775 0.75) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 7 smd rect (at 1.775 0) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 8 "Net-(U1-Pad7)"))
  )
  (module bcan:TSOP572xx (layer F.Cu) (tedit 58D19224)
    (at 157.375 100 180)
    (fp_text reference U2 (at 0 0 180) (layer F.SilkS))
    (fp_text value TSOP57238 (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.775 -1.5 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 /IR_L))
    (pad 5 smd rect (at -1.775 1.5 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 6 smd rect (at 1.775 1.5 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 8 smd rect (at 1.775 -1.5 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.775 -0.75 180) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 9 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -1.775 0 180) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 10 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -1.775 0.75 180) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 11 "Net-(U2-Pad4)"))
    (pad 7 smd rect (at 1.775 0 180) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 12 "Net-(U2-Pad7)"))
  )
  (module Connectors_JST:JST_GH_SM04B-GHS-TB_04x1.25mm_Angled (layer F.Cu) (tedit 58A22BB2)
    (at 150 97.5)
    (descr "JST GH series connector, SM04B-GHS-TB, side entry type")
    (tags "connector jst GH SMT side horizontal entry 1.25mm pitch")
    (attr smd)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS))
    (fp_text value IR (at 0 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0.45) (layer F.Fab))
    (pad 1 smd rect (at -1.875 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 2 smd rect (at -0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /IR_R))
    (pad 3 smd rect (at 0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /IR_L))
    (pad 4 smd rect (at 1.875 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad "" smd rect (at 3.6 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.6 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Mounting_Holes:MountingHole_5mm (layer F.Cu) (tedit 58D19499)
    (at 150 89.25)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (fp_text reference REF** (at 0 -6) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm (at 0 6) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_5mm (layer F.Cu) (tedit 58D194BA)
    (at 150 110.75)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (fp_text reference REF** (at 0 -6) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm (at 0 6) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (gr_text JST-GH (at 150 101.5) (layer F.SilkS))
  (gr_text "This\nSide\nDown" (at 143.75 106.25) (layer F.SilkS))
  (gr_text REAR (at 150 114.5) (layer F.SilkS))
  (gr_text FRONT (at 150 85.5) (layer F.SilkS))
  (gr_text IR (at 159 100) (layer B.SilkS))
  (gr_text "Rev 1.0" (at 159 103.5) (layer B.SilkS))
  (gr_text bcan.io (at 159 96.5) (layer B.SilkS))
  (gr_text L (at 157.5 96.5) (layer F.SilkS))
  (gr_text R (at 142.5 96.5) (layer F.SilkS))
  (gr_arc (start 158 86) (end 158 84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158 114) (end 160 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142 114) (end 142 116) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142 86) (end 140 86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 114) (end 140 86) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 116) (end 142 116) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160 86) (end 160 114) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142 84) (end 158 84) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 140 84) (xy 160 84) (xy 160 116) (xy 140 116)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 140 84) (xy 160 84) (xy 160 116) (xy 140 116)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155 115) (xy 155 108.5) (xy 153.25 108.5) (xy 156.25 103.5) (xy 159.25 108.5)
        (xy 157.5 108.5) (xy 157.5 115)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 159 106.5) (xy 159 115) (xy 141 115) (xy 141 106.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 159.028497 85) (xy 159.028497 93.5) (xy 141.028497 93.5) (xy 141.028497 85)
      )
    )
  )
)
