<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="10.16" x2="31.75" y2="10.16" width="0" layer="20"/>
<wire x1="31.75" y1="10.16" x2="31.75" y2="0" width="0" layer="20"/>
<wire x1="31.75" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="10.16" width="0" layer="20"/>
<text>LM1881 BREAKOUT REV1</text>
<text>TIM KOSTKA 2016-JUL-31</text>
<text>CSOUT</text>
<text>CVIN</text>
<text>VSOUT</text>
<text>GND</text>
<text>BPOUT</text>
<text>RSET</text>
<text>OEOUT</text>
<text>5-12V</text>
</plain>
<libraries>
<library name="kcl_ics">
<packages>
<package name="SOIC8N">
<description>SOIC8, 3.8mm (0.150") body.</description>
</package>
</packages>
</library>
<library name="kcl_passives">
<packages>
<package name="C0805R">
<description>Chip capacitor land pattern, reflow soldering, size 0805.</description>
</package>
<package name="RES0805R">
<description>Vishay MCU 0805 resistor footprint for reflow soldering.</description>
</package>
</packages>
</library>
<library name="kcl_connectors_auto">
<packages>
<package name="SAM-TSW-104-XX-X-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="kcl_ics" package="SOIC8N" value="LM1881SOIC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="LM1881MX/NOPB"/>
</element>
<element name="C1" library="kcl_passives" package="C0805R" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="C0805C104K5RACTU"/>
</element>
<element name="C2" library="kcl_passives" package="C0805R" value="0.1 uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="C0805C104K5RACTU"/>
</element>
<element name="R1" library="kcl_passives" package="RES0805R" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW0805680RFKEA"/>
</element>
<element name="J1" library="kcl_connectors_auto" package="SAM-TSW-104-XX-X-S" value="CONN4TSW-S">
<attribute name="PN" value="TSW-101-07-F-S"/>
</element>
<element name="J2" library="kcl_connectors_auto" package="SAM-TSW-104-XX-X-S" value="CONN4TSW-S">
<attribute name="PN" value="TSW-101-07-F-S"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="5"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="8"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
