(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 150.1267 96.36 172.739525 114.846101)
    (thickness 1.6002)
    (drawings 15)
    (tracks 4)
    (zones 0)
    (modules 6)
    (nets 4)
  )
  (page A4)
  (title_block
    (title "Interactive Rainbow - Extra LEDs")
    (date 2016-10-08)
    (rev 1.0.0)
    (company "Sembazuru Circuit (for Barrel of Makers)")
    (comment 1 "1.0.0 - First PWB layout.")
    (comment 2 "1.0.1 - Adjust Front Silkscreen for J1&J2 polarization.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7145 1.7145)
    (pad_drill 0.93)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 152.4 101.6)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x301f0_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.076200)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 +5V)
  (net 3 /~LED_On)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 1.27)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net /~LED_On)
    (add_net "Net-(D1-Pad2)")
  )
  (module ipc-7251TH-standard:HDRV2W64P254_1X2_508X254X1016A (layer F.Cu) (tedit 58712E4A)
    (at 163.83 107.95 270)
    (descr "Header Vertical 2Pin 0.100” Pitch 1X2 Fabrication Level A(Most)")
    (tags HDRV2W64P254_1X2_508X254X1016)
    (fp_text reference J2 (at -4.318 0 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -2.286 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 1.15062) (layers *.Cu *.Mask)
      (net 3 /~LED_On))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 2.032 2.032) (drill 1.15062) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:HDRV2W64P254_1X2_508X254X1016A (layer F.Cu) (tedit 58712E2C)
    (at 153.67 107.95 270)
    (descr "Header Vertical 2Pin 0.100” Pitch 1X2 Fabrication Level A(Most)")
    (tags HDRV2W64P254_1X2_508X254X1016)
    (fp_text reference J1 (at -4.318 0 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 1.15062) (layers *.Cu *.Mask)
      (net 3 /~LED_On))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 2.032 2.032) (drill 1.15062) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:OSHW_02mm_copper_noMask (layer B.Cu) (tedit 0)
    (at 163.576 103.251 180)
    (fp_text reference G*** (at 0 -1.17856 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 1.17856 180) (layer B.SilkS) hide)
  )
  (module ipc-7251TH-standard:LEDRD254W50D500H960P (layer B.Cu) (tedit 58712E76)
    (at 158.75 107.95 270)
    (descr "LED 5mm Vertical")
    (tags LED)
    (fp_text reference D1 (at -3.556 0 360) (layer B.SilkS))
    (fp_text value "RGB Slow Flashing" (at -5.08 0 360) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.7145 1.7145) (drill 0.93) (layers *.Cu *.Mask)
      (net 3 /~LED_On))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.7145 1.7145) (drill 0.93) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0 0 0.02))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:RESAD1016W56L681D259 (layer F.Cu) (tedit 57F90382)
    (at 158.75 113.03)
    (descr "Resistor, Axial; 400 mil C X 22 mil W 268 mil L X 102 mil Dia body - Standard 1/4W Resistor")
    (tags "RES 0.25 1/4")
    (fp_text reference R1 (at -2.032 0) (layer F.SilkS))
    (fp_text value 180Ω (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.08 0) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model discret/resistors/horizontal/r_h_180R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:crane_0.15in_silkscreen (layer B.Cu) (tedit 0)
    (at 156.718 111.633 180)
    (fp_text reference G*** (at 0 -1.36398 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 1.36398 180) (layer B.SilkS) hide)
  )
  (gr_text + (at 153.67 111.125) (layer F.SilkS))
  (gr_text - (at 153.67 104.775) (layer F.SilkS))
  (gr_text - (at 163.83 104.775) (layer F.SilkS))
  (gr_text + (at 163.83 111.125) (layer F.SilkS))
  (dimension 12.7 (width 0.0762) (layer F.Fab)
    (gr_text "0.5000 in" (at 168.99 107.95 270) (layer F.Fab))
    (feature1 (pts (xy 165.354 114.3) (xy 170.34 114.3)))
    (feature2 (pts (xy 165.354 101.6) (xy 170.34 101.6)))
    (crossbar (pts (xy 167.64 101.6) (xy 167.64 114.3)))
    (arrow1a (pts (xy 167.64 114.3) (xy 167.053579 113.173496)))
    (arrow1b (pts (xy 167.64 114.3) (xy 168.226421 113.173496)))
    (arrow2a (pts (xy 167.64 101.6) (xy 167.053579 102.726504)))
    (arrow2b (pts (xy 167.64 101.6) (xy 168.226421 102.726504)))
  )
  (dimension 12.7 (width 0.0762) (layer F.Fab)
    (gr_text "0.5000 in" (at 158.75 97.71) (layer F.Fab))
    (feature1 (pts (xy 165.1 101.346) (xy 165.1 96.36)))
    (feature2 (pts (xy 152.4 101.346) (xy 152.4 96.36)))
    (crossbar (pts (xy 152.4 99.06) (xy 165.1 99.06)))
    (arrow1a (pts (xy 165.1 99.06) (xy 163.973496 99.646421)))
    (arrow1b (pts (xy 165.1 99.06) (xy 163.973496 98.473579)))
    (arrow2a (pts (xy 152.4 99.06) (xy 153.526504 99.646421)))
    (arrow2b (pts (xy 152.4 99.06) (xy 153.526504 98.473579)))
  )
  (gr_text "Sch V2.0.0\nPcb V1.0.1" (at 156.464 108.458 90) (layer F.SilkS))
  (gr_text "DIY DE" (at 161.036 113.411) (layer B.SilkS))
  (gr_text BoM (at 161.036 112.141) (layer B.SilkS))
  (gr_text "Sembazuru\nCircuits" (at 156.718 113.538) (layer B.SilkS))
  (gr_text "TrippyRGB\nExtra LED" (at 158.75 103.632) (layer F.SilkS))
  (gr_line (start 152.4 114.3) (end 152.4 101.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.1 114.3) (end 152.4 114.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.1 101.6) (end 165.1 114.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.4 101.6) (end 165.1 101.6) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 1.27))
    (polygon
      (pts
        (xy 152.4 101.6) (xy 161.925 101.6) (xy 161.925 104.775) (xy 165.1 104.775) (xy 165.1 114.3)
        (xy 152.4 114.3)
      )
    )
  )
)
