(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber")
		)
	)
	(net 0 "")
	(net 1 "VCC_IN")
	(net 2 "GND")
	(net 3 "VCC_3V3")
	(net 4 "CHIP_EN")
	(net 5 "GPIO0")
	(net 6 "unconnected-(IC2-NC_2-Pad8)")
	(net 7 "unconnected-(IC2-NC_1-Pad5)")
	(net 8 "RX")
	(net 9 "TX")
	(net 10 "unconnected-(U1-IO36-Pad29)")
	(net 11 "unconnected-(U1-IO41-Pad34)")
	(net 12 "unconnected-(U1-IO46-Pad16)")
	(net 13 "unconnected-(U1-IO8-Pad12)")
	(net 14 "unconnected-(U1-IO37-Pad30)")
	(net 15 "unconnected-(U1-IO3-Pad15)")
	(net 16 "unconnected-(U1-IO17-Pad10)")
	(net 17 "unconnected-(U1-IO42-Pad35)")
	(net 18 "unconnected-(U1-IO45-Pad26)")
	(net 19 "unconnected-(U1-IO35-Pad28)")
	(net 20 "unconnected-(U1-IO18-Pad11)")
	(net 21 "unconnected-(U1-IO40-Pad33)")
	(net 22 "unconnected-(U1-IO38-Pad31)")
	(net 23 "unconnected-(U1-IO39-Pad32)")
	(net 24 "unconnected-(U1-IO7-Pad7)")
	(net 25 "Net-(D1-K)")
	(net 26 "USB-")
	(net 27 "USB+")
	(net 28 "unconnected-(J6-VCC-Pad2)")
	(net 29 "unconnected-(J7-VCC-Pad2)")
	(net 30 "Net-(D2-A)")
	(net 31 "GPIO2")
	(net 32 "Net-(D6-CANH)")
	(net 33 "GPIO48")
	(net 34 "Net-(C14-Pad2)")
	(net 35 "Net-(D6-CANL)")
	(net 36 "Net-(D4-A)")
	(net 37 "unconnected-(D3-NC_4-Pad10)")
	(net 38 "unconnected-(D3-IO2-Pad2)")
	(net 39 "unconnected-(D3-NC_3-Pad9)")
	(net 40 "Net-(D5-K)")
	(net 41 "GPIO9")
	(net 42 "GPIO10")
	(net 43 "GPIO1")
	(net 44 "Net-(J3-CC1)")
	(net 45 "unconnected-(J3-SBU1-PadA8)")
	(net 46 "unconnected-(J3-SBU2-PadB8)")
	(net 47 "Net-(J3-CC2)")
	(net 48 "GPIO21")
	(net 49 "GPIO47")
	(net 50 "Net-(J8-CANL)")
	(net 51 "Net-(J8-CANH)")
	(net 52 "GPIO11")
	(net 53 "unconnected-(U1-IO16-Pad9)")
	(net 54 "unconnected-(U1-IO12-Pad20)")
	(net 55 "unconnected-(U1-IO14-Pad22)")
	(net 56 "unconnected-(U1-IO5-Pad5)")
	(net 57 "unconnected-(U1-IO4-Pad4)")
	(net 58 "unconnected-(U1-IO13-Pad21)")
	(net 59 "unconnected-(U1-IO15-Pad8)")
	(net 60 "unconnected-(U1-IO6-Pad6)")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 133 120.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.304273 -0.054586 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C0603C106M9PAC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "VCC_IN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 158.5 85.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-10K-E3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "GPIO48")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ESP32-S3-WROOM-1-N8:XCVR_ESP32-S3-WROOM-1-N8"
		(layer "F.Cu")
		(at 139.5 97 90)
		(property "Reference" "U1"
			(at 0 10.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "ESP32-S3-WROOM-1-N8"
			(at 0.25 14.46 90)
			(layer "F.Fab")
		)
		(property "Footprint" "ESP32-S3-WROOM-1-N8:XCVR_ESP32-S3-WROOM-1-N8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bluetooth, WiFi 802.11b/g/n, Bluetooth v5.0 Transceiver Module 2.4GHz PCB Trace Surface Mount"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Espressif Systems"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" "Bluetooth, WiFi 802.11b/g/n, Bluetooth v5.0 Transceiver Module 2.4GHz PCB Trace Surface Mount"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "NON STANDARD Espressif Systems"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ESP32-S3-WROOM-1-N8/Espressif+Systems/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ESP32-S3-WROOM-1-N8/Espressif+Systems/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "ESP32-S3-WROOM-1-N8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=11020927&manufacturer=Espressif Systems&part_name=ESP32-S3-WROOM-1-N8&search_term=esp32-s3-wroom-1-n8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "\nWiFi 802.11a/b/g/n, Bluetooth v5.0 Transceiver Module 2.4GHz Antenna Not Included -\n"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PURCHASE-URL" "https://pricing.snapeda.com/search/part/ESP32-S3-WROOM-1-N8R8/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfr_Number" "356-ESP32-S3WROOM1N8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "356-ESP32-S3WROOM1N8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "ANTENNA"
			(at -4.5 -9.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -8.75 -5.26 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -8.75 -3.99 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VCC_3V3")
			(pinfunction "3V3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -8.75 -2.72 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "CHIP_EN")
			(pinfunction "EN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -8.75 -1.45 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "unconnected-(U1-IO4-Pad4)")
			(pinfunction "IO4")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -8.75 -0.18 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "unconnected-(U1-IO5-Pad5)")
			(pinfunction "IO5")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -8.75 1.09 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "unconnected-(U1-IO6-Pad6)")
			(pinfunction "IO6")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -8.75 2.36 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "unconnected-(U1-IO7-Pad7)")
			(pinfunction "IO7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -8.75 3.63 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "unconnected-(U1-IO15-Pad8)")
			(pinfunction "IO15")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -8.75 4.9 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "unconnected-(U1-IO16-Pad9)")
			(pinfunction "IO16")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at -8.75 6.17 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "unconnected-(U1-IO17-Pad10)")
			(pinfunction "IO17")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at -8.75 7.44 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "unconnected-(U1-IO18-Pad11)")
			(pinfunction "IO18")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at -8.75 8.71 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "unconnected-(U1-IO8-Pad12)")
			(pinfunction "IO8")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at -8.75 9.98 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "USB-")
			(pinfunction "IO19")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at -8.75 11.25 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "USB+")
			(pinfunction "IO20")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at -6.985 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "unconnected-(U1-IO3-Pad15)")
			(pinfunction "IO3")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at -5.715 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "unconnected-(U1-IO46-Pad16)")
			(pinfunction "IO46")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at -4.445 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "GPIO9")
			(pinfunction "IO9")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at -3.175 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "GPIO10")
			(pinfunction "IO10")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd rect
			(at -1.905 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "GPIO11")
			(pinfunction "IO11")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd rect
			(at -0.635 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "unconnected-(U1-IO12-Pad20)")
			(pinfunction "IO12")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd rect
			(at 0.635 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "unconnected-(U1-IO13-Pad21)")
			(pinfunction "IO13")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd rect
			(at 1.905 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "unconnected-(U1-IO14-Pad22)")
			(pinfunction "IO14")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd rect
			(at 3.175 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "GPIO21")
			(pinfunction "IO21")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd rect
			(at 4.445 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "GPIO47")
			(pinfunction "IO47")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "25" smd rect
			(at 5.715 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "GPIO48")
			(pinfunction "IO48")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "26" smd rect
			(at 6.985 12.5 90)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "unconnected-(U1-IO45-Pad26)")
			(pinfunction "IO45")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "27" smd rect
			(at 8.75 11.25 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "GPIO0")
			(pinfunction "IO0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "28" smd rect
			(at 8.75 9.98 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "unconnected-(U1-IO35-Pad28)")
			(pinfunction "IO35")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "29" smd rect
			(at 8.75 8.71 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "unconnected-(U1-IO36-Pad29)")
			(pinfunction "IO36")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "30" smd rect
			(at 8.75 7.44 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "unconnected-(U1-IO37-Pad30)")
			(pinfunction "IO37")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "31" smd rect
			(at 8.75 6.17 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "unconnected-(U1-IO38-Pad31)")
			(pinfunction "IO38")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "32" smd rect
			(at 8.75 4.9 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "unconnected-(U1-IO39-Pad32)")
			(pinfunction "IO39")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "33" smd rect
			(at 8.75 3.63 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(U1-IO40-Pad33)")
			(pinfunction "IO40")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "34" smd rect
			(at 8.75 2.36 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-IO41-Pad34)")
			(pinfunction "IO41")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "35" smd rect
			(at 8.75 1.09 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "unconnected-(U1-IO42-Pad35)")
			(pinfunction "IO42")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "36" smd rect
			(at 8.75 -0.18 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RX")
			(pinfunction "RXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "37" smd rect
			(at 8.75 -1.45 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "TX")
			(pinfunction "TXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "38" smd rect
			(at 8.75 -2.72 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "GPIO2")
			(pinfunction "IO2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "39" smd rect
			(at 8.75 -3.99 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "GPIO1")
			(pinfunction "IO1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "40" smd rect
			(at 8.75 -5.26 90)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_1" smd rect
			(at -1.5 2.46 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_2" smd rect
			(at -2.9 2.46 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_3" smd rect
			(at -0.1 2.46 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_4" smd rect
			(at -2.9 3.86 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_5" smd rect
			(at -1.5 3.86 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_6" smd rect
			(at -0.1 3.86 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_7" smd rect
			(at -2.9 1.06 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_8" smd rect
			(at -1.5 1.06 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_9" smd rect
			(at -0.1 1.06 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_10" thru_hole circle
			(at -1.5 1.76 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_11" thru_hole circle
			(at -2.9 1.76 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_12" thru_hole circle
			(at -0.1 1.76 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_13" thru_hole circle
			(at -2.9 3.16 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_14" thru_hole circle
			(at -1.5 3.16 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_15" thru_hole circle
			(at -0.1 3.16 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_16" thru_hole circle
			(at -2.2 1.06 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_17" thru_hole circle
			(at -0.8 1.06 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_18" thru_hole circle
			(at -2.2 2.46 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_19" thru_hole circle
			(at -0.8 2.46 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_20" thru_hole circle
			(at -2.2 3.86 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_21" thru_hole circle
			(at -0.8 3.86 90)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 126.75 106) (xy 126.75 88) (xy 132.75 88) (xy 132.75 106)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "*.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 126.75 106) (xy 126.75 88) (xy 132.75 88) (xy 132.75 106)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 126.75 106) (xy 126.75 88) (xy 132.75 88) (xy 132.75 106)
				)
			)
		)
		(model "C:/Users/paulr/Documents/KiCad/custom-parts/ESP32-S3-WROOM-1-N8/ESP32-S3-WROOM-1-N8.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_Pad"
		(layer "F.Cu")
		(at 170 77)
		(descr "Mounting Hole 2.2mm, M2")
		(tags "mounting hole 2.2mm m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.4 4.4)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 139 108)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 160.5 88 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at -0.74097 2.611693 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "CHIP_EN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "USB-C-data-connector:GCT_USB4105-GF-A"
		(layer "F.Cu")
		(at 158.5 125.8625)
		(property "Reference" "J3"
			(at 0 -3 0)
			(layer "F.SilkS")
		)
		(property "Value" "USB4105-GF-A"
			(at 0.17 -6.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "USB-C-data-connector:GCT_USB4105-GF-A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "B3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Global Connector Technology"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.31mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "640-USB4105-GF-A-120"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "PCB EDGE"
			(at 6.1775 3.3375 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -3.68)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -3.68)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1_B12" smd rect
			(at -3.2 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "A4_B9" smd rect
			(at -2.4 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(D2-A)")
			(pinfunction "VBUS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "A5" smd rect
			(at -1.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(J3-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A6" smd rect
			(at -0.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "USB+")
			(pinfunction "DP1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A7" smd rect
			(at 0.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "USB-")
			(pinfunction "DN1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A8" smd rect
			(at 1.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "unconnected-(J3-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "B1_A12" smd rect
			(at 3.2 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "B4_A9" smd rect
			(at 2.4 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(D2-A)")
			(pinfunction "VBUS__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "B5" smd rect
			(at 1.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "Net-(J3-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B6" smd rect
			(at 0.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "USB+")
			(pinfunction "DP2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B7" smd rect
			(at -0.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "USB-")
			(pinfunction "DN2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B8" smd rect
			(at -1.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "unconnected-(J3-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "SH1" thru_hole oval
			(at -4.32 -4.18)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHELL_GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH2" thru_hole oval
			(at 4.32 -4.18)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHELL_GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH3" thru_hole roundrect
			(at -4.32 0)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "SHELL_GND__2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH4" thru_hole roundrect
			(at 4.32 0)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "SHELL_GND__3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(model "C:/Users/paulr/Documents/KiCad/custom-parts/USB-C-data-connector/USB4105-GF-A.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DQA_R-PUSON-N10_"
		(layer "F.Cu")
		(at 157.25 118.492275)
		(descr "DQA (R-PUSON-N10)")
		(tags "Diode")
		(property "Reference" "D3"
			(at 0.09974 -1.648587 0)
			(layer "F.SilkS")
		)
		(property "Value" "TPD4E02B04DQAR"
			(at -0.34483 -1.37981 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SamacSys_Parts:DQA_R-PUSON-N10_"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tpd4e02b04"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Channel ESD Protection Diode for USB Type-C and HDMI 2.0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-TPD4E02B04DQAR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPD4E02B04DQAR?qs=8%2FmU9qzJpL%2FFVYtHO1iV9g%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TPD4E02B04DQAR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "595-TPD4E02B04DQAR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.34483 -1.37981 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1 0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(D2-A)")
			(pinfunction "IO1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "unconnected-(D3-IO2-Pad2)")
			(pinfunction "IO2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at 0 0.385)
			(size 0.4 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.5 0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "USB-")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1 0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "USB+")
			(pinfunction "IO4")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1 -0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "USB+")
			(pinfunction "NC_1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "USB-")
			(pinfunction "NC_2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0 -0.385)
			(size 0.4 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -0.5 -0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "unconnected-(D3-NC_3-Pad9)")
			(pinfunction "NC_3")
			(pintype "passive+no_connect")
		)
		(pad "10" smd rect
			(at -1 -0.385)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "unconnected-(D3-NC_4-Pad10)")
			(pinfunction "NC_4")
			(pintype "passive+no_connect")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\TPD4E02B04DQAR.stp"
			(offset
				(xyz 0 0 0.5299999634)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "SamacSys_Parts:LEDC1608X80N"
		(layer "F.Cu")
		(at 134.5 125.5 -90)
		(descr "WL-SMCW")
		(tags "LED")
		(property "Reference" "D1"
			(at 2.5 0.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "150060RS75000"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SamacSys_Parts:LEDC1608X80N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://katalog.we-online.de/led/datasheet/150060RS75000.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WURTH ELEKTRONIK - 150060RS75000 - LED, 0603, RED, 250MCD, 625NM"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.8"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "710-150060RS75000"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Wurth-Elektronik/150060RS75000?qs=LlUlMxKIyB3QnmZ3fw%2FVCA%3D%3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Wurth Elektronik"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "150060RS75000"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "710-150060RS75000"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0)
			(size 0.95 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0)
			(size 0.95 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\150060RS75000.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 135.5 108 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C0603C106M9PAC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.75 122.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -1 1.75 180)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-5.1K-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(J3-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:TSW-102-XX-YY-S"
		(layer "F.Cu")
		(at 128.8125 84.25 90)
		(descr "TSW-102-XX-YY-S")
		(tags "Connector")
		(property "Reference" "J1"
			(at -0.865071 2.324069 180)
			(layer "F.SilkS")
		)
		(property "Value" "EXT"
			(at -2.311707 -0.057316 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "TSW-102-XX-YY-S"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://suddendocs.samtec.com/prints/tsw-xxx-xx-xxx-x-xx-xxx-mkt.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2 Position, Single Row, Classic PCB Header Strips, 0.100&quot; pitch"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "200-TSW10207TS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Samtec/TSW-102-07-T-S?qs=hzq9O0YpnZuE%252BS9CaLPVlQ%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "SAMTEC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TSW-102-07-T-S"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "200-TSW10207TS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.55 1.55)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "GPIO1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.55 1.55)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\TSW-102-07-T-S.stp"
			(offset
				(xyz 1.279999952 -0.009999999626 -0.1099999978)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 131 120.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -2 180)
			(layer "F.SilkS")
		)
		(property "Value" "47"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-47-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:1719710103"
		(layer "F.Cu")
		(at 142.75 82.04 -90)
		(descr "171971-0103-2")
		(tags "Connector")
		(property "Reference" "J6"
			(at -2.54 -5.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "PWM1"
			(at 3.96 -0.75 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "SamacSys_Parts:1719710103"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://suddendocs.samtec.com/prints/tsw-xxx-xx-xxx-x-xx-xxx-mkt.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3 Position, Single Row, Classic PCB Header Strips, 0.100&quot; pitch"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "200-TSW10307TS"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Samtec/TSW-103-07-T-S?qs=hzq9O0YpnZs1xDByQQIs%2FQ%3D%3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "SAMTEC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TSW-103-07-T-S"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "538-171971-0103"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "GPIO21")
			(pinfunction "SIG")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -2.54 0 270)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J6-VCC-Pad2)")
			(pinfunction "VCC")
			(pintype "power_out+no_connect")
		)
		(pad "3" thru_hole circle
			(at -5.08 0 270)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\171971-0103.stp"
			(offset
				(xyz -2.539999924 0 11.90999967)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:LEDC1608X80N"
		(layer "F.Cu")
		(at 171.5 113.5 90)
		(descr "WL-SMCW")
		(tags "LED")
		(property "Reference" "D5"
			(at -2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "150060RS75000"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SamacSys_Parts:LEDC1608X80N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://katalog.we-online.de/led/datasheet/150060RS75000.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WURTH ELEKTRONIK - 150060RS75000 - LED, 0603, RED, 250MCD, 625NM"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "710-150060RS75000"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Wurth-Elektronik/150060RS75000?qs=LlUlMxKIyB3QnmZ3fw%2FVCA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Wurth Elektronik"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "150060RS75000"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "710-150060RS75000"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 180)
			(size 0.95 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 180)
			(size 0.95 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\150060RS75000.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:PTS636SKG25JSMTRLFS"
		(layer "F.Cu")
		(at 156.5 92.5 90)
		(descr "PTS636 SKG25J SMTR LFS-2")
		(tags "Switch")
		(property "Reference" "S3"
			(at 4 -2 180)
			(layer "F.SilkS")
		)
		(property "Value" "Reset"
			(at -5.5 0 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "PTS636SKG25JSMTRLFS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/2779/pts636.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tactile Switches Tact 50mA 12VDC, 6.0x3.5, 2.5mm H, 250gf, J leads, Ground pin, Red Actuator"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.7"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "611-PTS636SKG25JSMTR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CK/PTS636-SKG25J-SMTR-LFS?qs=vLWxofP3U2zmD1x5JCMkFg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "C & K COMPONENTS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PTS636 SKG25J SMTR LFS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "PTS636 SKG25J SMTR LFS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.775 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.775 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "CHIP_EN")
			(pinfunction "NO")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\PTS636_SKG25J_SMTR_LFS.stp"
			(offset
				(xyz -2422.229944 -680.0200093 0.3499999888)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:1719710103"
		(layer "F.Cu")
		(at 164.92 86.5 180)
		(descr "171971-0103-2")
		(tags "Connector")
		(property "Reference" "J8"
			(at -6.58 3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "TERM"
			(at -2.58 3.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "SamacSys_Parts:1719710103"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://suddendocs.samtec.com/prints/ssw-1xx-xx-xxx-x-xx-xxx-xx-mkt.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3 Position, .100&quot; Tiger Buy&trade; Socket Strip"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "8.51"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "200-SSW10301FS"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Samtec/SSW-103-01-F-S?qs=fnpEE5GccuPw9U6TKlPWnw%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "SAMTEC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SSW-103-01-F-S"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "538-171971-0103"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J8-CANH)")
			(pinfunction "CANH")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -2.54 0 180)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "NC")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.08 0 180)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J8-CANL)")
			(pinfunction "CANL")
			(pintype "bidirectional")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\171971-0103.stp"
			(offset
				(xyz -2.539999924 0 11.90999967)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 171.48384 118.19748 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 2.189163 -0.240494 0)
			(layer "F.SilkS")
		)
		(property "Value" "47"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-47-E3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(D5-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "GPIO11")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 160.5 98 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -2.159628 0.034589 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GPIO0")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 160.5 91.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0.296115 -1.691511 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-10K-E3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "CHIP_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 166 110.5 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 2 180)
			(layer "F.SilkS")
		)
		(property "Value" "60"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW120660R0KNAIF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 34 "Net-(C14-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 32 "Net-(D6-CANH)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:1190297"
		(layer "F.Cu")
		(at 140.08 114)
		(descr "1190297")
		(tags "Connector")
		(property "Reference" "J5"
			(at 7.92 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "5-12V"
			(at 2.92 6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "1190297"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://g.componentsearchengine.com/Datasheets/0/15169004.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PCB terminal block, nominal current: 24 A, rated voltage (III/2): 400 V, nominal cross section: 2.5 mm2, number of potentials: 2, number of rows: 1, number of positions per row: 2, product range: LPT 2,5/, pitch: 5 mm, connection method: Lever Push-in connection, mounting: Wave soldering, conductor/PCB connection direction: 0 , color: green, Pin layout: Linear pinning, Solder pin [P]: 3.5 mm, type of packaging: packed in cardboard"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "23.58"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "651-1190297"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Phoenix-Contact/1190297?qs=QNEnbhJQKvaBinyAO%252BdsFA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Phoenix Contact"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "1190297"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "651-1190297"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.92 6 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC_IN")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 8.2)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC_IN")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 5 8.2)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\1190297.stp"
			(offset
				(xyz -2.79999991 -13.39999942 0.05999999776)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_Pad"
		(layer "F.Cu")
		(at 130 125.5)
		(descr "Mounting Hole 2.2mm, M2")
		(tags "mounting hole 2.2mm m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.4 4.4)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 158.5 83.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -3.675096 0.418395 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "GPIO48")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DIONM5027X250N"
		(layer "F.Cu")
		(at 151.5 117 90)
		(descr "SMA ~ DO-214AC")
		(tags "Diode")
		(property "Reference" "D4"
			(at 0 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "SK14"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "DIONM5027X250N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.arrow.com/en/products/sk14/diotec-semiconductor-ag?region=europe"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky Diodes & Rectifiers Schottky, SMA, 40V, 1A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "637-SK14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diotec-Semiconductor/SK14?qs=OlC7AqGiEDkqBnpJlZ2UeA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diotec"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SK14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "637-SK14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.1 0 180)
			(size 1.55 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "VCC_IN")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.1 0 180)
			(size 1.55 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\SK14.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 137.438648 86.297991 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 2.594275 -0.008764 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "GPIO2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:FSM4JH"
		(layer "F.Cu")
		(at 162 79 180)
		(descr "FSM4JH")
		(tags "Switch")
		(property "Reference" "S4"
			(at -4.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "E-Stop"
			(at 0.141041 4.255585 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "SamacSys_Parts:FSM4JH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1825910%7FC9%7Fpdf%7FEnglish%7FENG_CD_1825910_C9.pdf%7F1825910-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "6x6mm tactile switch,5mm H 1.6N Black Button Tactile Switch, SPST-NO 50 mA@ 24 V dc 1.4mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "506-FSM4JH"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Alcoswitch/FSM4JH?qs=g%252BEszo6zu8OwVWrHD2r3Rw%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "TE Connectivity"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "FSM4JH"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "506-FSM4JH"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.45433 -0.00933 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -3.25 -2.25 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.25 -2.25 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "GPIO48")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -3.25 2.25 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 3.25 2.25 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "GPIO48")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\FSM4JH.stp"
			(offset
				(xyz -0.05999999776 0 7.269999872)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 167.5 122)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 3 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:PTS636SKG25JSMTRLFS"
		(layer "F.Cu")
		(at 136 79.225 -90)
		(descr "PTS636 SKG25J SMTR LFS-2")
		(tags "Switch")
		(property "Reference" "S1"
			(at -0.225 -3 180)
			(layer "F.SilkS")
		)
		(property "Value" "Test"
			(at 5.5 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "PTS636SKG25JSMTRLFS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/2779/pts636.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tactile Switches Tact 50mA 12VDC, 6.0x3.5, 2.5mm H, 250gf, J leads, Ground pin, Red Actuator"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.7"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "611-PTS636SKG25JSMTR"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CK/PTS636-SKG25J-SMTR-LFS?qs=vLWxofP3U2zmD1x5JCMkFg%3D%3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "C & K COMPONENTS"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PTS636 SKG25J SMTR LFS"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "PTS636 SKG25J SMTR LFS"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.775 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.775 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "GPIO2")
			(pinfunction "NO")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\PTS636_SKG25J_SMTR_LFS.stp"
			(offset
				(xyz -2422.229944 -680.0200093 0.3499999888)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOT230P700X180-4N"
		(layer "F.Cu")
		(at 131.5 114.5 90)
		(descr "DCY (R-PDSO-G4)")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 3 3 180)
			(layer "F.SilkS")
		)
		(property "Value" "LM1117MPX-3.3_NOPB"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SamacSys_Parts:SOT230P700X180-4N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Space saving 800-mA low-dropout linear regulator with internal current limit"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "926-LM1117MPX3.3NOPB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LM1117MPX-3.3-NOPB?qs=X1J7HmVL2ZHRbBIxXi4utg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LM1117MPX-3.3/NOPB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "926-LM1117MPX3.3NOPB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3 180)
			(size 0.95 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "ADJ/GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -3.15 0 180)
			(size 0.95 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VCC_3V3")
			(pinfunction "OUTPUT")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at -3.15 2.3 180)
			(size 0.95 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "VCC_IN")
			(pinfunction "INPUT")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at 3.15 0 90)
			(size 1.75 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VCC_3V3")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\LM1117MPX-3.3_NOPB.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOT96P237X111-3N"
		(layer "F.Cu")
		(at 167.5 103 90)
		(descr "SOT-23 (TO-236) CASE 318-08 ISSUE AR")
		(tags "Diode")
		(property "Reference" "D6"
			(at 0 -3 0)
			(layer "F.SilkS")
		)
		(property "Value" "SZNUP2105LT1G"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SOT96P237X111-3N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NUP2105L-D.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Bi-Directional TVS Diode, 350W peak, 3-pin SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.11"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "863-SZNUP2105LT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/onsemi/SZNUP2105LT1G?qs=PJJcWtbOkNWqqZbXH80dfQ%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "onsemi"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SZNUP2105LT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "863-SZNUP2105LT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.955 180)
			(size 0.6 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(D6-CANH)")
			(pinfunction "CANH")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.05 0.955 180)
			(size 0.6 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(D6-CANL)")
			(pinfunction "CANL")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.05 0 180)
			(size 0.6 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\SZNUP2105LT1G.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 165 106 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C0603C101J1GACLR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "Net-(D6-CANH)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 132 109)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -0.045824 -1.480748 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C0603C106M9PAC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 169 110.5 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -2.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "60"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW120660R0KNAIF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 34 "Net-(C14-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 35 "Net-(D6-CANL)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 132 82 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 2 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-10K-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "GPIO2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_Pad"
		(layer "F.Cu")
		(at 130 77)
		(descr "Mounting Hole 2.2mm, M2")
		(tags "mounting hole 2.2mm m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.4 4.4)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
	)
	(footprint "SamacSys_Parts:1719710103"
		(layer "F.Cu")
		(at 164.96 95.5 180)
		(descr "171971-0103-2")
		(tags "Connector")
		(property "Reference" "J4"
			(at -6.54 3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "CAN"
			(at -2.54 3.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "SamacSys_Parts:1719710103"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://suddendocs.samtec.com/prints/tsw-xxx-xx-xxx-x-xx-xxx-mkt.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3 Position, Single Row, Classic PCB Header Strips, 0.100&quot; pitch"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "200-TSW10307TS"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Samtec/TSW-103-07-T-S?qs=hzq9O0YpnZs1xDByQQIs%2FQ%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "SAMTEC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TSW-103-07-T-S"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "538-171971-0103"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D6-CANH)")
			(pinfunction "CANH")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 0 180)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "NC")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.08 0 180)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(D6-CANL)")
			(pinfunction "CANL")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\171971-0103.stp"
			(offset
				(xyz -2.539999924 0 11.90999967)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 128.5 109 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P600X175-8N"
		(layer "F.Cu")
		(at 167.5 117 90)
		(descr "D (R-PDSO-G8)")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at -2 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN65HVD232DR"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SOIC127P600X175-8N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn65hvd232"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3.3 V CAN Transceiver"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-SN65HVD232DR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/SN65HVD232DR?qs=QViXGNcIEAtY%252BrViRMr46w%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SN65HVD232DR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "595-SN65HVD232DR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.712 -1.905 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "GPIO9")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.712 -0.635 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.712 0.635 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VCC_3V3")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.712 1.905 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "GPIO10")
			(pinfunction "R")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.712 1.905 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(IC2-NC_1-Pad5)")
			(pinfunction "NC_1")
			(pintype "passive+no_connect")
		)
		(pad "6" smd rect
			(at 2.712 0.635 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(D6-CANL)")
			(pinfunction "CANL")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.712 -0.635 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(D6-CANH)")
			(pinfunction "CANH")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.712 -1.905 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "unconnected-(IC2-NC_2-Pad8)")
			(pinfunction "NC_2")
			(pintype "passive+no_connect")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\SN65HVD232DR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 135 120.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -2.317534 -0.012441 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C603C104K5RAC3121"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "VCC_IN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DIONM5027X250N"
		(layer "F.Cu")
		(at 151.5 124 -90)
		(descr "SMA ~ DO-214AC")
		(tags "Diode")
		(property "Reference" "D2"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SK14"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "DIONM5027X250N"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.arrow.com/en/products/sk14/diotec-semiconductor-ag?region=europe"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky Diodes & Rectifiers Schottky, SMA, 40V, 1A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.5"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "637-SK14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diotec-Semiconductor/SK14?qs=OlC7AqGiEDkqBnpJlZ2UeA%3D%3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diotec"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SK14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "637-SK14"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.1 0)
			(size 1.55 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "VCC_IN")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.1 0)
			(size 1.55 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\SK14.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 167.825 81 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -2.675 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-120-E3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "Net-(J8-CANL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "Net-(J8-CANH)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:1719710103"
		(layer "F.Cu")
		(at 151.75 82.08 -90)
		(descr "171971-0103-2")
		(tags "Connector")
		(property "Reference" "J7"
			(at -2.58 -5.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "PWM2"
			(at 3.92 -0.75 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "SamacSys_Parts:1719710103"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://suddendocs.samtec.com/prints/tsw-xxx-xx-xxx-x-xx-xxx-mkt.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3 Position, Single Row, Classic PCB Header Strips, 0.100&quot; pitch"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "200-TSW10307TS"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Samtec/TSW-103-07-T-S?qs=hzq9O0YpnZs1xDByQQIs%2FQ%3D%3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "SAMTEC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TSW-103-07-T-S"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "538-171971-0103"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "GPIO47")
			(pinfunction "SIG")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -2.54 0 270)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(J7-VCC-Pad2)")
			(pinfunction "VCC")
			(pintype "power_out+no_connect")
		)
		(pad "3" thru_hole circle
			(at -5.08 0 270)
			(size 1.635 1.635)
			(drill 1.09)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\171971-0103.stp"
			(offset
				(xyz -2.539999924 0 11.90999967)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.75 126 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.248636 0.003261 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-5.1K-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "Net-(J3-CC1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 167.5 106.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -2.5 -3.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7n"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C0603C472J5G"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(C14-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:PTS636SKG25JSMTRLFS"
		(layer "F.Cu")
		(at 156.5 104.225 90)
		(descr "PTS636 SKG25J SMTR LFS-2")
		(tags "Switch")
		(property "Reference" "S2"
			(at 4.225 -2 180)
			(layer "F.SilkS")
		)
		(property "Value" "Boot"
			(at -5.275 0 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "PTS636SKG25JSMTRLFS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/2779/pts636.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tactile Switches Tact 50mA 12VDC, 6.0x3.5, 2.5mm H, 250gf, J leads, Ground pin, Red Actuator"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.7"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "611-PTS636SKG25JSMTR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CK/PTS636-SKG25J-SMTR-LFS?qs=vLWxofP3U2zmD1x5JCMkFg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "C & K COMPONENTS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PTS636 SKG25J SMTR LFS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "PTS636 SKG25J SMTR LFS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.775 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.775 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "GPIO0")
			(pinfunction "NO")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\PTS636_SKG25J_SMTR_LFS.stp"
			(offset
				(xyz -2422.229944 -680.0200093 0.3499999888)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 160.5 101.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.230498 0.003543 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "71-CRCW0603-10K-E3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GPIO0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC_3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 170 106)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C0603C101J1GACLR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(D6-CANL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_Pad"
		(layer "F.Cu")
		(at 170 125.5)
		(descr "Mounting Hole 2.2mm, M2")
		(tags "mounting hole 2.2mm m2")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.4 4.4)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
	)
	(footprint "SamacSys_Parts:HDRV4W64P0X254_1X4_1016X254X889P"
		(layer "F.Cu")
		(at 161.5 116.04 90)
		(descr "M20-9990446")
		(tags "Connector")
		(property "Reference" "J2"
			(at 10.04 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "FTDI"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "HDRV4W64P0X254_1X4_1016X254X889P"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn.harwin.com/pdfs/M20-999.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "M20 Header, Pin, Sil, Vertical, 4 W HARWIN M20 Series, 2.54mm Pitch 4 Way 1 Row Straight Pin Header, Through Hole, Solder Termination"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "8.89"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "855-M20-9990446"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Harwin/M20-9990446?qs=ulE8k0yEMYaW%252BOM7jiG6%252Bw%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Harwin"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "M20-9990446"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "855-M20-9990446"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(D4-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "TX")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 7.62 0 90)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "RX")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "C:\\Users\\paulr\\Documents\\KiCad\\SamacSys_Parts.3dshapes\\M20-9990446.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 154.5 118 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier_Number" "80-C0603C106M9PAC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Mouser"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MRF_NUMBER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part_Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "motor_master.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "VCC_IN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 170.5 73.5)
		(end 129.5 73.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.5 76.5)
		(end 126.5 126)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.5 129)
		(mid 127.37868 128.12132)
		(end 126.5 126)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 173.5 126)
		(mid 172.62132 128.12132)
		(end 170.5 129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.5 129)
		(end 170.5 129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.5 126)
		(end 173.5 76.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.5 73.5)
		(mid 172.62132 74.37868)
		(end 173.5 76.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 126.5 76.5)
		(mid 127.37868 74.37868)
		(end 129.5 73.5)
		(layer "Edge.Cuts")
	)
	(gr_text "47x55.5mm"
		(at 138.272576 105 90)
		(layer "B.SilkS")
	)
	(gr_text "Robotics Academy 2024 v1"
		(at 135.5 86.5 90)
		(layer "B.SilkS")
	)
	(gr_text "MotorMaster"
		(at 138.5 88.5 90)
		(layer "B.SilkS")
	)
	(gr_text "G"
		(at 148 77 0)
		(layer "F.SilkS")
	)
	(gr_text "H"
		(at 164.5 100.5 0)
		(layer "F.SilkS")
	)
	(gr_text "L"
		(at 170.5 100.5 0)
		(layer "F.SilkS")
	)
	(gr_text "S"
		(at 148 82.5 0)
		(layer "F.SilkS")
	)
	(gr_text "5-12v"
		(at 140 110.5 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 149 128.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 135 128.5 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(locked yes)
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.5 73.5) (xy 173.5 73.5) (xy 173.5 129) (xy 126.5 129)
			)
		)
	)
)
