(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "/CXN")
  (net 4 "/CXP")
  (net 5 "REG")
  (net 6 "~{SHDN}")
  (footprint "footprints:MAX1595EUA50&plus_" (layer "F.Cu")
    (tedit 0)
    (at 148.3102 99.2974)
    (property "Sheetfile" "dev2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -2.54) (layer "F.SilkS"))
    (fp_text value "MAX1595EUA50+" (at 0 2.54) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at -1.1684 -1.4732) (layer "F.Fab"))
    (fp_text user "*" (at -1.1684 -1.4732) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2098 -0.97536) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "REG") (pinfunction "AOUT") (pintype "input"))
    (pad "2" smd rect (at -2.2098 -0.32512) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "~{SHDN}") (pinfunction "~{SHDN}") (pintype "input"))
    (pad "3" smd rect (at -2.2098 0.32512) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "IN") (pintype "power_in"))
    (pad "4" smd rect (at -2.2098 0.97536) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.2098 0.97536) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "PGND") (pintype "power_in"))
    (pad "6" smd rect (at 2.2098 0.32512) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/CXN") (pinfunction "CXN") (pintype "bidirectional"))
    (pad "7" smd rect (at 2.2098 -0.32512) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/CXP") (pinfunction "CXP") (pintype "bidirectional"))
    (pad "8" smd rect (at 2.2098 -0.97536) (size 1.3208 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "REG") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x02_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 147.574 102.87)
    (descr "Through hole straight pin header, 2x02, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 1.27mm double row")
    (property "Sheetfile" "dev2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0.7112 2.794) (layer "F.SilkS"))
    (fp_text value "Conn_02x02_Top_Bottom" (at 0.635 2.965) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.635 0.635 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "REG") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "~{SHDN}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x02_P1.27mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric_Pad0.64x0.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 152.4 99.314 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "dev2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -2.032 0 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.4325 0 90) (size 0.458 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.4325 0 90) (size 0.458 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.4075 0 90) (size 0.635 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/CXN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.4075 0 90) (size 0.635 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/CXP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 143.51 99.822 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "dev2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 154.178 99.2925 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "dev2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 3.0695 0 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 5 "REG") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 149.8611 100.9904 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "dev2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2.1" (at 2.9983 0.254) (layer "B.SilkS"))
    (fp_text value "C" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/CXN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/CXP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 140.97 95.885) (end 140.97 106.68) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 156.21 106.68) (end 156.21 95.885) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 140.97 106.68) (end 156.21 106.68) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 156.21 95.885) (end 140.97 95.885) (layer "Edge.Cuts") (width 0.1))
  (gr_text "dev2" (at 143.6624 101.2444 270) (layer "B.Mask"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.575 106.045)
        (xy 141.605 106.045)
        (xy 141.605 96.52)
        (xy 155.575 96.52)
      )
    )
  )
)
