(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 142.24 50.8 223.520001 106.680001)
    (thickness 1.6)
    (drawings 14)
    (tracks 40)
    (zones 0)
    (modules 22)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory svg/))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad2)")
  (net 2 "Net-(J2-Pad3)")
  (net 3 "Net-(J4-Pad2)")
  (net 4 "Net-(R1-Pad1)")
  (net 5 GND)
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J5-Pad2)")
  (net 9 "Net-(J5-Pad3)")
  (net 10 "Net-(J6-Pad2)")
  (net 11 "Net-(J6-Pad3)")
  (net 12 "Net-(R5-Pad1)")
  (net 13 "Net-(J3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Audio ""
    (clearance 0.38608)
    (trace_width 0.64008)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R5-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 157.48 57.658)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "CH 1 IN" (at -2.54 1.27 90) (layer F.Fab))
    (fp_text user %R (at -1.016 6.096 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59B0C0F2)
    (at 179.832 62.992 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value "ST IN" (at -3.048 7.874 360) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 149.098 74.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 4.826 0 90) (layer F.SilkS))
    (fp_text value 6k81 (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 161.29 61.214)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 0) (layer F.SilkS))
    (fp_text value 475 (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 185.928 62.992 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value "ST IN" (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 196.088 101.092 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "CH 2 OUT" (at 0 10.922 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 161.29 57.658)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 475 (at 5.334 -2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 171.45 64.77 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 20k (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 216.662 74.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 6k81 (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R5-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 204.47 57.658 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 475 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 204.47 61.214 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 475 (at 5.08 -2.286 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 194.31 64.77)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.08 0) (layer F.SilkS))
    (fp_text value 20k (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 164.592 101.092 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "CH 1 OUT" (at -0.254 11.176 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 208.28 57.658)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "CH 2 IN" (at 2.794 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 59C32805)
    (at 215.9 99.06)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (zone_connect 2)
    (fp_text reference REF** (at 0 -3.048) (layer F.Fab))
    (fp_text value 1pin (at 0 3 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 5 GND) (zone_connect 2))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 59C327DD)
    (at 149.86 99.06)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (zone_connect 2)
    (fp_text reference REF** (at 0 -3.048) (layer F.Fab))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 5 GND) (zone_connect 2))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 59C327D3)
    (at 149.86 58.42)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (zone_connect 2)
    (fp_text reference REF** (at 0 -3.048) (layer F.Fab))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 5 GND) (zone_connect 2))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 59C327C1)
    (at 215.9 58.42)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (zone_connect 2)
    (fp_text reference REF** (at 0 -3.048) (layer F.Fab))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 5 GND) (zone_connect 2))
  )
  (module NeutrikSnakeLib:JT-DB-EPC (layer F.Cu) (tedit 59F22CD3)
    (at 172.466 92.456 90)
    (fp_text reference T1 (at 8.89 0 90) (layer F.SilkS))
    (fp_text value JT-DB-EPC (at 8.89 -11.43 90) (layer F.SilkS))
    (pad 4 thru_hole circle (at 0 0 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 3 thru_hole circle (at 0 -3.81 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 0 -7.62 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -11.43 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 8 thru_hole circle (at 19.05 -11.43 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 7 thru_hole circle (at 19.05 -7.62 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole circle (at 19.05 -3.81 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole circle (at 19.05 0 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad1)"))
  )
  (module NeutrikSnakeLib:JT-DB-EPC (layer F.Cu) (tedit 59F22CD3)
    (at 204.724 92.456 90)
    (fp_text reference T2 (at 8.89 0 90) (layer F.SilkS))
    (fp_text value JT-DB-EPC (at 8.89 -11.43 90) (layer F.SilkS))
    (pad 4 thru_hole circle (at 0 0 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 11 "Net-(J6-Pad3)"))
    (pad 3 thru_hole circle (at 0 -3.81 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 0 -7.62 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -11.43 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 10 "Net-(J6-Pad2)"))
    (pad 8 thru_hole circle (at 19.05 -11.43 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 7 thru_hole circle (at 19.05 -7.62 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole circle (at 19.05 -3.81 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole circle (at 19.05 0 90) (size 1.9558 1.9558) (drill 1.27) (layers *.Cu *.Mask)
      (net 12 "Net-(R5-Pad1)"))
  )
  (module logo:TSC (layer F.Cu) (tedit 59B07D79)
    (at 182.88 93.98)
    (fp_text reference G*** (at 0 0) (layer F.Cu) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Cu) hide)
  )
  (module logo:TSCMask (layer F.Cu) (tedit 59B07D79)
    (at 182.88 93.98)
    (fp_text reference G*** (at 0 0) (layer F.Mask) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Mask) hide)
  )
  (gr_text "Stereo DI\n12.12.2017" (at 182.88 101.6) (layer F.SilkS))
  (gr_text "L\nR\nG" (at 182.88 60.452) (layer F.SilkS))
  (gr_text "G\n+" (at 210.82 58.42) (layer F.SilkS))
  (gr_text "G\n+" (at 154.94 58.42) (layer F.SilkS))
  (gr_text "G + -" (at 198.628 98.298) (layer F.SilkS))
  (gr_text "G + -" (at 167.132 98.298) (layer F.SilkS))
  (gr_line (start 149.86 104.14) (end 215.9 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 58.42) (end 144.78 99.06) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 53.34) (end 149.86 53.34) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 220.98 58.42) (end 220.98 99.06) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.86 99.06) (end 149.86 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 215.9 99.06) (end 220.98 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 215.9 58.42) (end 215.9 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.86 58.42) (end 144.78 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 50.8) (xy 223.52 50.8) (xy 223.52 106.68) (xy 142.24 106.68)
      )
    )
  )
)
