(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu16.04.1-stable)
  (general
    (links 0)
    (no_connects 8)
    (area -50.012701 -25.012701 50.012701 25.012701)
    (thickness 1.6)
    (drawings 153)
    (tracks 2056)
    (zones 0)
    (modules 196)
    (nets 228)
  )
  (page A)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.0254)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.0254)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.0508)
    (pad_size 0.79756 0.79756)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFF577F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.025400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 Vsupply)
  (net 3 3.3V_Reg)
  (net 4 "Net-(C103-Pad2)")
  (net 5 CPLD_3.3V)
  (net 6 CPLD_1.8V)
  (net 7 USB_5V)
  (net 8 USB_3.3V)
  (net 9 VCCIO1A)
  (net 10 VCCIO1B)
  (net 11 VCCA)
  (net 12 A_G)
  (net 13 A0)
  (net 14 A1)
  (net 15 A2)
  (net 16 A3)
  (net 17 A4)
  (net 18 A5)
  (net 19 VCC_ONE)
  (net 20 A6)
  (net 21 A7)
  (net 22 A8)
  (net 23 VCCIO)
  (net 24 "Net-(C139-Pad2)")
  (net 25 +BATT)
  (net 26 "Net-(D102-Pad2)")
  (net 27 "Net-(D104-Pad1)")
  (net 28 "Net-(D105-Pad2)")
  (net 29 "Net-(D106-Pad2)")
  (net 30 "Net-(D107-Pad2)")
  (net 31 /IO_021)
  (net 32 "Net-(D108-Pad2)")
  (net 33 /IO_022)
  (net 34 "Net-(D109-Pad2)")
  (net 35 /IO_024)
  (net 36 "Net-(D110-Pad2)")
  (net 37 /IO_025)
  (net 38 "Net-(D111-Pad2)")
  (net 39 /IO_026)
  (net 40 "Net-(D112-Pad2)")
  (net 41 /IO_027)
  (net 42 "Net-(D113-Pad2)")
  (net 43 /IO_028)
  (net 44 "Net-(D114-Pad2)")
  (net 45 /IO_029)
  (net 46 "Net-(P103-Pad1)")
  (net 47 "Net-(P104-Pad6)")
  (net 48 "Net-(P104-Pad7)")
  (net 49 "Net-(P104-Pad8)")
  (net 50 A_8)
  (net 51 A_7)
  (net 52 A_6)
  (net 53 A_5)
  (net 54 A_4)
  (net 55 A_3)
  (net 56 A_2)
  (net 57 A_1)
  (net 58 A_0)
  (net 59 CLK_24MHz)
  (net 60 "Net-(R102-Pad2)")
  (net 61 "Net-(R103-Pad2)")
  (net 62 "Net-(R104-Pad2)")
  (net 63 "Net-(R105-Pad2)")
  (net 64 "Net-(R106-Pad2)")
  (net 65 /J_en)
  (net 66 /J_TMS)
  (net 67 /J_TDI)
  (net 68 /D4)
  (net 69 /D2)
  (net 70 /D1)
  (net 71 /D7)
  (net 72 /D5)
  (net 73 /D6)
  (net 74 /D3)
  (net 75 /RD#)
  (net 76 /WR)
  (net 77 /TXE#)
  (net 78 /RXF#)
  (net 79 /D0)
  (net 80 "Net-(U104-Pad3)")
  (net 81 "Net-(U104-Pad4)")
  (net 82 "Net-(U104-Pad5)")
  (net 83 "Net-(U104-Pad9)")
  (net 84 /J_TDO)
  (net 85 "Net-(U104-Pad40)")
  (net 86 "Net-(U104-Pad43)")
  (net 87 "Net-(U105-Pad5)")
  (net 88 "Net-(U105-Pad17)")
  (net 89 "Net-(U105-Pad30)")
  (net 90 "Net-(U105-Pad32)")
  (net 91 "Net-(U105-Pad33)")
  (net 92 "Net-(U105-Pad48)")
  (net 93 "Net-(U105-Pad80)")
  (net 94 "Net-(U105-Pad96)")
  (net 95 "Net-(U105-Pad97)")
  (net 96 "Net-(U105-Pad98)")
  (net 97 "Net-(U105-Pad112)")
  (net 98 "Net-(U105-Pad123)")
  (net 99 "Net-(U105-Pad134)")
  (net 100 /IO_120)
  (net 101 /IO_119)
  (net 102 /IO_118)
  (net 103 /IO_114)
  (net 104 /IO_113)
  (net 105 /IO_111)
  (net 106 /IO_110)
  (net 107 /IO_106)
  (net 108 /IO_105)
  (net 109 /IO_102)
  (net 110 /IO_101)
  (net 111 /IO_100)
  (net 112 /IO_099)
  (net 113 /IO_093)
  (net 114 /IO_141)
  (net 115 /IO_140)
  (net 116 /IO_135)
  (net 117 /IO_132)
  (net 118 /IO_131)
  (net 119 /IO_130)
  (net 120 /IO_092)
  (net 121 /IO_091)
  (net 122 /IO_090)
  (net 123 /IO_088)
  (net 124 /IO_087)
  (net 125 /IO_086)
  (net 126 /IO_085)
  (net 127 /IO_084)
  (net 128 /IO_081)
  (net 129 /IO_079)
  (net 130 /IO_078)
  (net 131 /IO_077)
  (net 132 /IO_076)
  (net 133 /IO_075)
  (net 134 /IO_074)
  (net 135 "Net-(U105-Pad61)")
  (net 136 /IO_127)
  (net 137 /IO_124)
  (net 138 "Net-(D115-Pad1)")
  (net 139 "Net-(D115-Pad2)")
  (net 140 /IO_038)
  (net 141 /IO_041)
  (net 142 /IO_044)
  (net 143 /IO_046)
  (net 144 /IO_050)
  (net 145 /IO_054)
  (net 146 /IO_056)
  (net 147 /IO_058)
  (net 148 /IO_059)
  (net 149 /IO_057)
  (net 150 /IO_055)
  (net 151 /IO_052)
  (net 152 /IO_047)
  (net 153 /IO_045)
  (net 154 /IO_043)
  (net 155 /IO_039)
  (net 156 /IO_060)
  (net 157 /IO_062)
  (net 158 /IO_064)
  (net 159 /IO_065)
  (net 160 /IO_066)
  (net 161 /IO_069)
  (net 162 /IO_070)
  (net 163 /D-)
  (net 164 /D+)
  (net 165 /ID)
  (net 166 /USBDm)
  (net 167 /USBDp)
  (net 168 /C_P_TCK_a)
  (net 169 /C_P_TDO)
  (net 170 /C_P_TMS)
  (net 171 /C_P_TDI)
  (net 172 /J_TCK_b)
  (net 173 /J_TCK_a)
  (net 174 /J_TCK_c)
  (net 175 /C_P_TCK_b)
  (net 176 "Net-(U104-Pad7)")
  (net 177 "Net-(U104-Pad52)")
  (net 178 "Net-(U104-Pad56)")
  (net 179 "Net-(U104-Pad53)")
  (net 180 "Net-(U104-Pad54)")
  (net 181 "Net-(U104-Pad55)")
  (net 182 USB_1.8V)
  (net 183 /E_P_TCK_b)
  (net 184 /E_P_TDO)
  (net 185 /E_P_SEN_a)
  (net 186 /E_P_TMS)
  (net 187 /E_P_TDI)
  (net 188 /E_P_TCK_a)
  (net 189 /E_P_SEN_b)
  (net 190 "Net-(U104-Pad44)")
  (net 191 "Net-(U104-Pad45)")
  (net 192 "Net-(U104-Pad46)")
  (net 193 "Net-(U104-Pad47)")
  (net 194 "Net-(U104-Pad48)")
  (net 195 /USB_VCC)
  (net 196 CBUS5_6MHz)
  (net 197 /CBUS6)
  (net 198 /USB_RST)
  (net 199 /E_P_SEN_i)
  (net 200 "Net-(D116-Pad1)")
  (net 201 /e)
  (net 202 /d)
  (net 203 /f)
  (net 204 /g)
  (net 205 /c)
  (net 206 /a)
  (net 207 /b)
  (net 208 "Net-(D124-Pad1)")
  (net 209 "Net-(D132-Pad1)")
  (net 210 "Net-(D140-Pad1)")
  (net 211 /pt)
  (net 212 /cc_3)
  (net 213 /cc_2)
  (net 214 /cc_1)
  (net 215 /cc_0)
  (net 216 "Net-(U104-Pad1)")
  (net 217 "Net-(U104-Pad2)")
  (net 218 "Net-(U104-Pad10)")
  (net 219 "Net-(U104-Pad11)")
  (net 220 "Net-(U104-Pad12)")
  (net 221 "Net-(U104-Pad38)")
  (net 222 "Net-(U104-Pad49)")
  (net 223 "Net-(U104-Pad50)")
  (net 224 "Net-(U104-Pad51)")
  (net 225 "Net-(U104-Pad62)")
  (net 226 "Net-(U104-Pad63)")
  (net 227 "Net-(U104-Pad64)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net /CBUS6)
    (add_net /C_P_TCK_a)
    (add_net /C_P_TCK_b)
    (add_net /C_P_TDI)
    (add_net /C_P_TDO)
    (add_net /C_P_TMS)
    (add_net /D+)
    (add_net /D-)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /E_P_SEN_a)
    (add_net /E_P_SEN_b)
    (add_net /E_P_SEN_i)
    (add_net /E_P_TCK_a)
    (add_net /E_P_TCK_b)
    (add_net /E_P_TDI)
    (add_net /E_P_TDO)
    (add_net /E_P_TMS)
    (add_net /ID)
    (add_net /IO_021)
    (add_net /IO_022)
    (add_net /IO_024)
    (add_net /IO_025)
    (add_net /IO_026)
    (add_net /IO_027)
    (add_net /IO_028)
    (add_net /IO_029)
    (add_net /IO_038)
    (add_net /IO_039)
    (add_net /IO_041)
    (add_net /IO_043)
    (add_net /IO_044)
    (add_net /IO_045)
    (add_net /IO_046)
    (add_net /IO_047)
    (add_net /IO_050)
    (add_net /IO_052)
    (add_net /IO_054)
    (add_net /IO_055)
    (add_net /IO_056)
    (add_net /IO_057)
    (add_net /IO_058)
    (add_net /IO_059)
    (add_net /IO_060)
    (add_net /IO_062)
    (add_net /IO_064)
    (add_net /IO_065)
    (add_net /IO_066)
    (add_net /IO_069)
    (add_net /IO_070)
    (add_net /IO_074)
    (add_net /IO_075)
    (add_net /IO_076)
    (add_net /IO_077)
    (add_net /IO_078)
    (add_net /IO_079)
    (add_net /IO_081)
    (add_net /IO_084)
    (add_net /IO_085)
    (add_net /IO_086)
    (add_net /IO_087)
    (add_net /IO_088)
    (add_net /IO_090)
    (add_net /IO_091)
    (add_net /IO_092)
    (add_net /IO_093)
    (add_net /IO_099)
    (add_net /IO_100)
    (add_net /IO_101)
    (add_net /IO_102)
    (add_net /IO_105)
    (add_net /IO_106)
    (add_net /IO_110)
    (add_net /IO_111)
    (add_net /IO_113)
    (add_net /IO_114)
    (add_net /IO_118)
    (add_net /IO_119)
    (add_net /IO_120)
    (add_net /IO_124)
    (add_net /IO_127)
    (add_net /IO_130)
    (add_net /IO_131)
    (add_net /IO_132)
    (add_net /IO_135)
    (add_net /IO_140)
    (add_net /IO_141)
    (add_net /J_TCK_a)
    (add_net /J_TCK_b)
    (add_net /J_TCK_c)
    (add_net /J_TDI)
    (add_net /J_TDO)
    (add_net /J_TMS)
    (add_net /J_en)
    (add_net /RD#)
    (add_net /RXF#)
    (add_net /TXE#)
    (add_net /USBDm)
    (add_net /USBDp)
    (add_net /USB_RST)
    (add_net /USB_VCC)
    (add_net /WR)
    (add_net /a)
    (add_net /b)
    (add_net /c)
    (add_net /cc_0)
    (add_net /cc_1)
    (add_net /cc_2)
    (add_net /cc_3)
    (add_net /d)
    (add_net /e)
    (add_net /f)
    (add_net /g)
    (add_net /pt)
    (add_net 3.3V_Reg)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A_0)
    (add_net A_1)
    (add_net A_2)
    (add_net A_3)
    (add_net A_4)
    (add_net A_5)
    (add_net A_6)
    (add_net A_7)
    (add_net A_8)
    (add_net A_G)
    (add_net CBUS5_6MHz)
    (add_net CLK_24MHz)
    (add_net CPLD_1.8V)
    (add_net CPLD_3.3V)
    (add_net GND)
    (add_net "Net-(C103-Pad2)")
    (add_net "Net-(C139-Pad2)")
    (add_net "Net-(D102-Pad2)")
    (add_net "Net-(D104-Pad1)")
    (add_net "Net-(D105-Pad2)")
    (add_net "Net-(D106-Pad2)")
    (add_net "Net-(D107-Pad2)")
    (add_net "Net-(D108-Pad2)")
    (add_net "Net-(D109-Pad2)")
    (add_net "Net-(D110-Pad2)")
    (add_net "Net-(D111-Pad2)")
    (add_net "Net-(D112-Pad2)")
    (add_net "Net-(D113-Pad2)")
    (add_net "Net-(D114-Pad2)")
    (add_net "Net-(D115-Pad1)")
    (add_net "Net-(D115-Pad2)")
    (add_net "Net-(D116-Pad1)")
    (add_net "Net-(D124-Pad1)")
    (add_net "Net-(D132-Pad1)")
    (add_net "Net-(D140-Pad1)")
    (add_net "Net-(P103-Pad1)")
    (add_net "Net-(P104-Pad6)")
    (add_net "Net-(P104-Pad7)")
    (add_net "Net-(P104-Pad8)")
    (add_net "Net-(R102-Pad2)")
    (add_net "Net-(R103-Pad2)")
    (add_net "Net-(R104-Pad2)")
    (add_net "Net-(R105-Pad2)")
    (add_net "Net-(R106-Pad2)")
    (add_net "Net-(U104-Pad1)")
    (add_net "Net-(U104-Pad10)")
    (add_net "Net-(U104-Pad11)")
    (add_net "Net-(U104-Pad12)")
    (add_net "Net-(U104-Pad2)")
    (add_net "Net-(U104-Pad3)")
    (add_net "Net-(U104-Pad38)")
    (add_net "Net-(U104-Pad4)")
    (add_net "Net-(U104-Pad40)")
    (add_net "Net-(U104-Pad43)")
    (add_net "Net-(U104-Pad44)")
    (add_net "Net-(U104-Pad45)")
    (add_net "Net-(U104-Pad46)")
    (add_net "Net-(U104-Pad47)")
    (add_net "Net-(U104-Pad48)")
    (add_net "Net-(U104-Pad49)")
    (add_net "Net-(U104-Pad5)")
    (add_net "Net-(U104-Pad50)")
    (add_net "Net-(U104-Pad51)")
    (add_net "Net-(U104-Pad52)")
    (add_net "Net-(U104-Pad53)")
    (add_net "Net-(U104-Pad54)")
    (add_net "Net-(U104-Pad55)")
    (add_net "Net-(U104-Pad56)")
    (add_net "Net-(U104-Pad62)")
    (add_net "Net-(U104-Pad63)")
    (add_net "Net-(U104-Pad64)")
    (add_net "Net-(U104-Pad7)")
    (add_net "Net-(U104-Pad9)")
    (add_net "Net-(U105-Pad112)")
    (add_net "Net-(U105-Pad123)")
    (add_net "Net-(U105-Pad134)")
    (add_net "Net-(U105-Pad17)")
    (add_net "Net-(U105-Pad30)")
    (add_net "Net-(U105-Pad32)")
    (add_net "Net-(U105-Pad33)")
    (add_net "Net-(U105-Pad48)")
    (add_net "Net-(U105-Pad5)")
    (add_net "Net-(U105-Pad61)")
    (add_net "Net-(U105-Pad80)")
    (add_net "Net-(U105-Pad96)")
    (add_net "Net-(U105-Pad97)")
    (add_net "Net-(U105-Pad98)")
    (add_net USB_1.8V)
    (add_net USB_3.3V)
    (add_net USB_5V)
    (add_net VCCA)
    (add_net VCCIO)
    (add_net VCCIO1A)
    (add_net VCCIO1B)
    (add_net VCC_ONE)
    (add_net Vsupply)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579CCEA6)
    (at -33.00476 -6.53796)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L101 (at -0.53086 1.08966) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at -0.0007 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 CPLD_1.8V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_0603_4Pads (layer F.Cu) (tedit 57673F71)
    (at 20.955 16.637 270)
    (descr "Crystal, Quarz, SMD, 0603, 4 Pads,")
    (tags "Crystal Quarz SMD 0603 4 Pads")
    (attr smd)
    (fp_text reference X101 (at -2.286 3.302 540) (layer F.SilkS))
    (fp_text value "SG5032CAN 24.000000M-TJGA3" (at 0.127 -0.127 360) (layer F.Fab))
    (pad 1 smd rect (at -2.19964 1.19888 270) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C139-Pad2)"))
    (pad 2 smd rect (at 2.19964 1.19888 270) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.19964 -1.19888 270) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 59 CLK_24MHz))
    (pad 4 smd rect (at -2.19964 -1.19888 270) (size 1.80086 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C139-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57943F11)
    (at -32.97174 -19.80438 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R139 (at 0 1.1684 450) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 /C_P_TDI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 579777F7)
    (at -48.77308 19.05 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D105 (at -1.75006 -0.1397 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D105-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 578BB3F7)
    (at -37.25926 7.9502 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C115 (at 0 -1.12522 450) (layer F.SilkS))
    (fp_text value 47pF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 164 /D+))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AFE9)
    (at -28.0924 19.7104 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D123 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 207 /b))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C3E2)
    (at -28.0924 10.7696 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D134 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 202 /d))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C3FD)
    (at -28.0924 5.1562 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D142 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 202 /d))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5781C14C)
    (at -23.5839 14.9987 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q103 (at 0 -1.92024 90) (layer F.SilkS) hide)
    (fp_text value MMBT3904,215 (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 213 /cc_2))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C16D)
    (at -25.9334 18.0467 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D124 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 211 /pt))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C18A)
    (at -32.4104 16.383 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D125 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 201 /e))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C1C2)
    (at -32.4104 14.097 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D130 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 206 /a))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C1A0)
    (at -34.5694 15.24 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D127 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 203 /f))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C193)
    (at -28.0924 16.383 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D126 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 202 /d))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C1B5)
    (at -25.9334 15.24 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D129 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 205 /c))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C1CB)
    (at -28.0924 14.097 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D131 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 207 /b))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C1A9)
    (at -30.2514 15.24 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D128 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 204 /g))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D124-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5781C15A)
    (at -23.876 17.4498 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R170 (at -0.0381 1.1811 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 /IO_028))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 213 /cc_2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5781B044)
    (at -23.876 23.0632 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R169 (at -0.0381 1.1811 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /IO_029))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 212 /cc_3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AFC6)
    (at -30.2514 20.8534 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D120 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 204 /g))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AFD4)
    (at -25.9334 20.8534 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D121 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 205 /c))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AF94)
    (at -28.0924 21.9964 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D118 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 202 /d))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AFBB)
    (at -34.5694 20.8534 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D119 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 203 /f))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AFE0)
    (at -32.4104 19.7104 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D122 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 206 /a))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AF86)
    (at -32.4104 21.9964 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D117 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 201 /e))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781AF73)
    (at -25.9334 23.6601 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D116 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 211 /pt))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5781A6F8)
    (at -23.5839 20.6121 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q102 (at 0 -1.92024 90) (layer F.SilkS) hide)
    (fp_text value MMBT3904,215 (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 212 /cc_3))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D116-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5781C36E)
    (at -23.5839 9.3853 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q104 (at 0 -1.92024 90) (layer F.SilkS) hide)
    (fp_text value MMBT3904,215 (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 214 /cc_1))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C361)
    (at -25.9334 12.4333 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D132 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 211 /pt))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C445)
    (at -32.4104 10.7696 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D133 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 201 /e))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C44F)
    (at -32.4104 8.4836 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D138 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 206 /a))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C476)
    (at -34.5694 9.6266 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D135 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 203 /f))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C3A7)
    (at -25.9334 9.6266 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D137 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 205 /c))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C3F1)
    (at -28.0924 8.4836 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D139 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 207 /b))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C41F)
    (at -30.2514 9.6266 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D136 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 204 /g))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D132-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5781C355)
    (at -23.876 11.8364 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R171 (at -0.0381 1.1811 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 /IO_027))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 214 /cc_1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5781C386)
    (at -23.876 6.223 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R172 (at -0.0381 1.1811 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /IO_026))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 215 /cc_0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C42A)
    (at -30.2514 4.0132 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D144 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 204 /g))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C405)
    (at -28.0924 2.8702 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D147 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 207 /b))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C3D2)
    (at -25.9334 4.0132 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D145 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 205 /c))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C486)
    (at -34.5694 4.0132 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D143 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 203 /f))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C465)
    (at -32.4104 2.8702 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D146 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 206 /a))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C45B)
    (at -32.4104 5.1562 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D141 (at 0.0254 1.016 180) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 201 /e))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5781C3C5)
    (at -25.9334 6.8199 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D140 (at 0.0254 1.016 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 211 /pt))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5781C391)
    (at -23.5839 3.7719 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q105 (at 0 -1.92024 90) (layer F.SilkS) hide)
    (fp_text value MMBT3904,215 (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 215 /cc_0))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D140-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 placed (layer F.Cu) (tedit 5794FF6E)
    (at -44.96435 -13.12545 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P104 (at 4.2672 6.35 270) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 1.2446 5.0292 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 183 /E_P_TCK_b))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 184 /E_P_TDO))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 185 /E_P_SEN_a))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 186 /E_P_TMS))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P104-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P104-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P104-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 187 /E_P_TDI))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57768E27)
    (at -19.56054 -15.24)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R125 (at -1.57988 -0.0127 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /J_TDI))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57950BA9)
    (at -41.91635 -19.47545 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R109 (at -1.55702 0 450) (layer F.SilkS))
    (fp_text value 10k (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 186 /E_P_TMS))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-64_7x7mm_Pitch0.4mm (layer F.Cu) (tedit 579CD253)
    (at -27.35834 -13.10386 270)
    (descr "LQFP64: plastic low profile quad flat package; 64 leads; body 7 x 7 x 1.4 mm(see NXP sot414-1_po.pdf and sot414-1_fr.pdf)")
    (tags "QFP 0.4")
    (attr smd)
    (fp_text reference U104 (at -5.01904 -4.56184 540) (layer F.SilkS))
    (fp_text value 5M80ZE64C5N (at 2.30378 8.27786 540) (layer F.SilkS))
    (pad 1 smd rect (at -4.25 -3 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(U104-Pad1)"))
    (pad 2 smd rect (at -4.25 -2.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(U104-Pad2)"))
    (pad 3 smd rect (at -4.25 -2.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U104-Pad3)"))
    (pad 4 smd rect (at -4.25 -1.8 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U104-Pad4)"))
    (pad 5 smd rect (at -4.25 -1.4 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U104-Pad5)"))
    (pad 6 smd rect (at -4.25 -1 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 7 smd rect (at -4.25 -0.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U104-Pad7)"))
    (pad 8 smd rect (at -4.25 -0.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 6 CPLD_1.8V))
    (pad 9 smd rect (at -4.25 0.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U104-Pad9)"))
    (pad 10 smd rect (at -4.25 0.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(U104-Pad10)"))
    (pad 11 smd rect (at -4.25 1 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(U104-Pad11)"))
    (pad 12 smd rect (at -4.25 1.4 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(U104-Pad12)"))
    (pad 13 smd rect (at -4.25 1.8 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 199 /E_P_SEN_i))
    (pad 14 smd rect (at -4.25 2.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 170 /C_P_TMS))
    (pad 15 smd rect (at -4.25 2.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 171 /C_P_TDI))
    (pad 16 smd rect (at -4.25 3 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 175 /C_P_TCK_b))
    (pad 17 smd rect (at -3 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 169 /C_P_TDO))
    (pad 18 smd rect (at -2.6 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 187 /E_P_TDI))
    (pad 19 smd rect (at -2.2 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 186 /E_P_TMS))
    (pad 20 smd rect (at -1.8 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 184 /E_P_TDO))
    (pad 21 smd rect (at -1.4 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 189 /E_P_SEN_b))
    (pad 22 smd rect (at -1 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 188 /E_P_TCK_a))
    (pad 23 smd rect (at -0.6 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 24 smd rect (at -0.2 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 68 /D4))
    (pad 25 smd rect (at 0.2 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 69 /D2))
    (pad 26 smd rect (at 0.6 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 70 /D1))
    (pad 27 smd rect (at 1 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 71 /D7))
    (pad 28 smd rect (at 1.4 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 1.8 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 2.2 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 72 /D5))
    (pad 31 smd rect (at 2.6 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 73 /D6))
    (pad 32 smd rect (at 3 4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 74 /D3))
    (pad 33 smd rect (at 4.25 3 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 76 /WR))
    (pad 34 smd rect (at 4.25 2.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 75 /RD#))
    (pad 35 smd rect (at 4.25 2.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 77 /TXE#))
    (pad 36 smd rect (at 4.25 1.8 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 78 /RXF#))
    (pad 37 smd rect (at 4.25 1.4 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 79 /D0))
    (pad 38 smd rect (at 4.25 1 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(U104-Pad38)"))
    (pad 39 smd rect (at 4.25 0.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 40 smd rect (at 4.25 0.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U104-Pad40)"))
    (pad 41 smd rect (at 4.25 -0.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 6 CPLD_1.8V))
    (pad 42 smd rect (at 4.25 -0.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 196 CBUS5_6MHz))
    (pad 43 smd rect (at 4.25 -1 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U104-Pad43)"))
    (pad 44 smd rect (at 4.25 -1.4 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(U104-Pad44)"))
    (pad 45 smd rect (at 4.25 -1.8 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(U104-Pad45)"))
    (pad 46 smd rect (at 4.25 -2.2 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(U104-Pad46)"))
    (pad 47 smd rect (at 4.25 -2.6 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(U104-Pad47)"))
    (pad 48 smd rect (at 4.25 -3 270) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(U104-Pad48)"))
    (pad 49 smd rect (at 3 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(U104-Pad49)"))
    (pad 50 smd rect (at 2.6 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(U104-Pad50)"))
    (pad 51 smd rect (at 2.2 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(U104-Pad51)"))
    (pad 52 smd rect (at 1.8 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U104-Pad52)"))
    (pad 53 smd rect (at 1.4 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U104-Pad53)"))
    (pad 54 smd rect (at 1 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U104-Pad54)"))
    (pad 55 smd rect (at 0.6 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(U104-Pad55)"))
    (pad 56 smd rect (at 0.2 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U104-Pad56)"))
    (pad 57 smd rect (at -0.2 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 58 smd rect (at -0.6 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 84 /J_TDO))
    (pad 59 smd rect (at -1 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 67 /J_TDI))
    (pad 60 smd rect (at -1.4 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 173 /J_TCK_a))
    (pad 61 smd rect (at -1.8 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 66 /J_TMS))
    (pad 62 smd rect (at -2.2 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(U104-Pad62)"))
    (pad 63 smd rect (at -2.6 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(U104-Pad63)"))
    (pad 64 smd rect (at -3 -4.25) (size 1.2 0.24) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(U104-Pad64)"))
    (pad 65 smd rect (at 0 0 270) (size 4.5 4.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_QFP.3dshapes/LQFP-64_7x7mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-24_3.9x8.7mm_Pitch0.635mm placed (layer F.Cu) (tedit 579CCC99)
    (at -43.04284 -1.63068)
    (descr "SSOP24: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot556-1_po.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U103 (at 0.02032 5.04698 180) (layer F.SilkS))
    (fp_text value FT240XS (at 0.30226 -4.91998 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.6 -3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 /D4))
    (pad 2 smd rect (at -2.6 -2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 /D2))
    (pad 3 smd rect (at -2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 USB_3.3V))
    (pad 4 smd rect (at -2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 /D1))
    (pad 5 smd rect (at -2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 71 /D7))
    (pad 6 smd rect (at -2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 /D5))
    (pad 8 smd rect (at -2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 73 /D6))
    (pad 9 smd rect (at -2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 74 /D3))
    (pad 10 smd rect (at -2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -2.6 2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 75 /RD#))
    (pad 12 smd rect (at -2.6 3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 76 /WR))
    (pad 13 smd rect (at 2.6 3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 167 /USBDp))
    (pad 14 smd rect (at 2.6 2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 166 /USBDm))
    (pad 15 smd rect (at 2.6 2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 USB_3.3V))
    (pad 16 smd rect (at 2.6 1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 198 /USB_RST))
    (pad 17 smd rect (at 2.6 0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 182 USB_1.8V))
    (pad 18 smd rect (at 2.6 0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 USB_5V))
    (pad 19 smd rect (at 2.6 -0.3175) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 2.6 -0.9525) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 77 /TXE#))
    (pad 21 smd rect (at 2.6 -1.5875) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 78 /RXF#))
    (pad 22 smd rect (at 2.6 -2.2225) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 /CBUS6))
    (pad 23 smd rect (at 2.6 -2.8575) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 196 CBUS5_6MHz))
    (pad 24 smd rect (at 2.6 -3.4925) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 79 /D0))
    (model Housings_SSOP.3dshapes/SSOP-24_3.9x8.7mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_Mini-B locked (layer F.Cu) (tedit 57923302)
    (at -45.32122 9.59866)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P106 (at 0.5842 -4.3688) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 195 /USB_VCC))
    (pad 2 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 163 /D-))
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 164 /D+))
    (pad 4 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 165 /ID))
    (pad 5 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0.8509 -2.19964) (size 1.27 1.27) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0.8509 2.19964) (size 1.27 1.27) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Housings_QFP:LQFP-144_20x20mm_Pitch0.5mm (layer F.Cu) (tedit 579CF5EF)
    (at 10.16 0 315)
    (descr "144-Lead Plastic Low Profile Quad Flatpack (PL) - 20x20x1.40 mm Body [LQFP], 2.00 mm Footprint (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U105 (at -8.385763 -7.498514 405) (layer F.SilkS))
    (fp_text value 10M08SAE144C8G (at 12.1898 5.109766 405) (layer F.SilkS))
    (pad 1 smd rect (at -10.7 -8.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 2 smd rect (at -10.7 -8.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (pad 3 smd rect (at -10.7 -7.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 A0))
    (pad 4 smd rect (at -10.7 -7.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 5 smd rect (at -10.7 -6.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U105-Pad5)"))
    (pad 6 smd rect (at -10.7 -6.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 A1))
    (pad 7 smd rect (at -10.7 -5.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 A2))
    (pad 8 smd rect (at -10.7 -5.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 A3))
    (pad 9 smd rect (at -10.7 -4.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCCIO1A))
    (pad 10 smd rect (at -10.7 -4.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 A4))
    (pad 11 smd rect (at -10.7 -3.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 A5))
    (pad 12 smd rect (at -10.7 -3.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 A6))
    (pad 13 smd rect (at -10.7 -2.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 A7))
    (pad 14 smd rect (at -10.7 -2.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 A8))
    (pad 15 smd rect (at -10.7 -1.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 /J_en))
    (pad 16 smd rect (at -10.7 -1.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 /J_TMS))
    (pad 17 smd rect (at -10.7 -0.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U105-Pad17)"))
    (pad 18 smd rect (at -10.7 -0.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 174 /J_TCK_c))
    (pad 19 smd rect (at -10.7 0.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 67 /J_TDI))
    (pad 20 smd rect (at -10.7 0.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 /J_TDO))
    (pad 21 smd rect (at -10.7 1.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /IO_021))
    (pad 22 smd rect (at -10.7 1.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /IO_022))
    (pad 23 smd rect (at -10.7 2.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 VCCIO1B))
    (pad 24 smd rect (at -10.7 2.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /IO_024))
    (pad 25 smd rect (at -10.7 3.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /IO_025))
    (pad 26 smd rect (at -10.7 3.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /IO_026))
    (pad 27 smd rect (at -10.7 4.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /IO_027))
    (pad 28 smd rect (at -10.7 4.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /IO_028))
    (pad 29 smd rect (at -10.7 5.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /IO_029))
    (pad 30 smd rect (at -10.7 5.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U105-Pad30)"))
    (pad 31 smd rect (at -10.7 6.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 32 smd rect (at -10.7 6.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U105-Pad32)"))
    (pad 33 smd rect (at -10.7 7.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U105-Pad33)"))
    (pad 34 smd rect (at -10.7 7.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (pad 35 smd rect (at -10.7 8.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (pad 36 smd rect (at -10.7 8.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 37 smd rect (at -8.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 38 smd rect (at -8.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 140 /IO_038))
    (pad 39 smd rect (at -7.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 155 /IO_039))
    (pad 40 smd rect (at -7.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 41 smd rect (at -6.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 141 /IO_041))
    (pad 42 smd rect (at -6.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 43 smd rect (at -5.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 154 /IO_043))
    (pad 44 smd rect (at -5.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 142 /IO_044))
    (pad 45 smd rect (at -4.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 153 /IO_045))
    (pad 46 smd rect (at -4.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 143 /IO_046))
    (pad 47 smd rect (at -3.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 152 /IO_047))
    (pad 48 smd rect (at -3.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U105-Pad48)"))
    (pad 49 smd rect (at -2.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 50 smd rect (at -2.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 144 /IO_050))
    (pad 51 smd rect (at -1.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 52 smd rect (at -1.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 151 /IO_052))
    (pad 53 smd rect (at -0.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 54 smd rect (at -0.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 145 /IO_054))
    (pad 55 smd rect (at 0.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 150 /IO_055))
    (pad 56 smd rect (at 0.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 146 /IO_056))
    (pad 57 smd rect (at 1.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 149 /IO_057))
    (pad 58 smd rect (at 1.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 /IO_058))
    (pad 59 smd rect (at 2.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 /IO_059))
    (pad 60 smd rect (at 2.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /IO_060))
    (pad 61 smd rect (at 3.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(U105-Pad61)"))
    (pad 62 smd rect (at 3.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 157 /IO_062))
    (pad 63 smd rect (at 4.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 64 smd rect (at 4.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 158 /IO_064))
    (pad 65 smd rect (at 5.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 159 /IO_065))
    (pad 66 smd rect (at 5.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 160 /IO_066))
    (pad 67 smd rect (at 6.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 68 smd rect (at 6.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 69 smd rect (at 7.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 161 /IO_069))
    (pad 70 smd rect (at 7.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 162 /IO_070))
    (pad 71 smd rect (at 8.25 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (pad 72 smd rect (at 8.75 10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 73 smd rect (at 10.7 8.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 74 smd rect (at 10.7 8.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 134 /IO_074))
    (pad 75 smd rect (at 10.7 7.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 133 /IO_075))
    (pad 76 smd rect (at 10.7 7.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 132 /IO_076))
    (pad 77 smd rect (at 10.7 6.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 131 /IO_077))
    (pad 78 smd rect (at 10.7 6.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 /IO_078))
    (pad 79 smd rect (at 10.7 5.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 /IO_079))
    (pad 80 smd rect (at 10.7 5.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U105-Pad80)"))
    (pad 81 smd rect (at 10.7 4.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 /IO_081))
    (pad 82 smd rect (at 10.7 4.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 83 smd rect (at 10.7 3.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 84 smd rect (at 10.7 3.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 127 /IO_084))
    (pad 85 smd rect (at 10.7 2.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 126 /IO_085))
    (pad 86 smd rect (at 10.7 2.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 125 /IO_086))
    (pad 87 smd rect (at 10.7 1.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 124 /IO_087))
    (pad 88 smd rect (at 10.7 1.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 /IO_088))
    (pad 89 smd rect (at 10.7 0.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 CLK_24MHz))
    (pad 90 smd rect (at 10.7 0.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 /IO_090))
    (pad 91 smd rect (at 10.7 -0.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 121 /IO_091))
    (pad 92 smd rect (at 10.7 -0.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 120 /IO_092))
    (pad 93 smd rect (at 10.7 -1.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /IO_093))
    (pad 94 smd rect (at 10.7 -1.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 95 smd rect (at 10.7 -2.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 96 smd rect (at 10.7 -2.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U105-Pad96)"))
    (pad 97 smd rect (at 10.7 -3.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U105-Pad97)"))
    (pad 98 smd rect (at 10.7 -3.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U105-Pad98)"))
    (pad 99 smd rect (at 10.7 -4.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 112 /IO_099))
    (pad 100 smd rect (at 10.7 -4.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /IO_100))
    (pad 101 smd rect (at 10.7 -5.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /IO_101))
    (pad 102 smd rect (at 10.7 -5.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 109 /IO_102))
    (pad 103 smd rect (at 10.7 -6.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 104 smd rect (at 10.7 -6.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 105 smd rect (at 10.7 -7.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 108 /IO_105))
    (pad 106 smd rect (at 10.7 -7.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 /IO_106))
    (pad 107 smd rect (at 10.7 -8.25 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (pad 108 smd rect (at 10.7 -8.75 315) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 109 smd rect (at 8.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 110 smd rect (at 8.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 106 /IO_110))
    (pad 111 smd rect (at 7.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 105 /IO_111))
    (pad 112 smd rect (at 7.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U105-Pad112)"))
    (pad 113 smd rect (at 6.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 104 /IO_113))
    (pad 114 smd rect (at 6.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 103 /IO_114))
    (pad 115 smd rect (at 5.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 116 smd rect (at 5.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 117 smd rect (at 4.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 118 smd rect (at 4.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 102 /IO_118))
    (pad 119 smd rect (at 3.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 101 /IO_119))
    (pad 120 smd rect (at 3.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 100 /IO_120))
    (pad 121 smd rect (at 2.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R102-Pad2)"))
    (pad 122 smd rect (at 2.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R106-Pad2)"))
    (pad 123 smd rect (at 1.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U105-Pad123)"))
    (pad 124 smd rect (at 1.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 137 /IO_124))
    (pad 125 smd rect (at 0.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 126 smd rect (at 0.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P103-Pad1)"))
    (pad 127 smd rect (at -0.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 136 /IO_127))
    (pad 128 smd rect (at -0.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 129 smd rect (at -1.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R105-Pad2)"))
    (pad 130 smd rect (at -1.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 119 /IO_130))
    (pad 131 smd rect (at -2.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 118 /IO_131))
    (pad 132 smd rect (at -2.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 117 /IO_132))
    (pad 133 smd rect (at -3.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 134 smd rect (at -3.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U105-Pad134)"))
    (pad 135 smd rect (at -4.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /IO_135))
    (pad 136 smd rect (at -4.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R104-Pad2)"))
    (pad 137 smd rect (at -5.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 138 smd rect (at -5.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R103-Pad2)"))
    (pad 139 smd rect (at -6.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (pad 140 smd rect (at -6.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 115 /IO_140))
    (pad 141 smd rect (at -7.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 114 /IO_141))
    (pad 142 smd rect (at -7.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 143 smd rect (at -8.25 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (pad 144 smd rect (at -8.75 -10.7 45) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (pad 145 smd rect (at 0 0 315) (size 5.4 5.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_QFP.3dshapes/LQFP-144_20x20mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP2 locked (layer F.Cu) (tedit 57671838)
    (at 44.2722 12.6746 180)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW101 (at 1.524 0 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at 3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 1 smd rect (at -3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 2 smd rect (at -3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 110 /IO_101))
    (pad 2 smd rect (at 3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 110 /IO_101))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP2 locked (layer F.Cu) (tedit 57671858)
    (at 44.2722 -7.747 180)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW104 (at 1.524 0 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at 3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 1 smd rect (at -3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 2 smd rect (at -3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 102 /IO_118))
    (pad 2 smd rect (at 3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 102 /IO_118))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP2 locked (layer F.Cu) (tedit 57671866)
    (at 44.2722 -12.6746 180)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW105 (at 1.524 0 450) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at 3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 1 smd rect (at -3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 2 smd rect (at -3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 100 /IO_120))
    (pad 2 smd rect (at 3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 100 /IO_120))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP2 locked (layer F.Cu) (tedit 57671829)
    (at 44.2722 7.747 180)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW102 (at 1.524 0 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at 3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 1 smd rect (at -3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 2 smd rect (at -3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 108 /IO_105))
    (pad 2 smd rect (at 3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 108 /IO_105))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad locked (layer F.Cu) (tedit 57758585)
    (at -44.45 19.05)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference REF** (at -4.31292 4.57708 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at -5.08 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad locked (layer F.Cu) (tedit 57673FC2)
    (at 44.45 19.05)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 4.826 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad locked (layer F.Cu) (tedit 57675D67)
    (at 44.45 -19.05)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 4.9784 -0.0762 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 578E3F25)
    (at -31.6103 -4.02082 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C101 (at 0 1.03632 450) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 Vsupply))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57976F1A)
    (at -20.21586 -5.07746)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C102 (at -1.80594 -0.889 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57976A17)
    (at -35.90544 -5.8293)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C103 (at -1.6129 -0.87376) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5795B716)
    (at -25.60574 -19.65452 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C104 (at -0.08636 1.08204 450) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579CCE12)
    (at -35.76828 -13.02766)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C105 (at -0.1397 -1.04902) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579769C8)
    (at -20.83562 -7.67842 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C106 (at 1.71196 0.60198 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5795B70D)
    (at -27.89174 -19.65452 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C108 (at -0.35052 1.10998 450) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 CPLD_1.8V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579769F9)
    (at -28.79852 -6.53796)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C109 (at -1.50876 -0.87376 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 CPLD_1.8V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57922D54)
    (at -36.93668 10.59688)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C110 (at -0.06096 1.0922) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 USB_5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57959C1C)
    (at -41.35374 23.1648)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C111 (at 0.2921 1.32334) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 USB_5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579233A8)
    (at -48.79848 23.17242 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C112 (at 0 -1.1049 450) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 195 /USB_VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57923859)
    (at -47.244 -2.93624 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C113 (at 0 -1.07188 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 USB_3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 578BB3DC)
    (at -38.96106 7.9502 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C114 (at 0 1.07188 450) (layer F.SilkS))
    (fp_text value 47pF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 163 /D-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57609091)
    (at 2.6797 -12.8397)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C116 (at 0 1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 VCCIO1A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57777025)
    (at -6.3119 -7.13994)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C117 (at 0.02286 1.13538) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 VCCIO1B))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 13.97 -18.542 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C118 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5777701F)
    (at -7.5946 -3.0226 315)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C119 (at -1.048894 -1.084815 315) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5771592C)
    (at 5.334 14.4526)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C120 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57674688)
    (at 26.67 3.048 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C121 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575E1DBE)
    (at 8.89 -18.542 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C122 (at 0 -1.27 450) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 450) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 A0))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57715835)
    (at 6.35 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C123 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 A1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575ED644)
    (at 3.81 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C124 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 A2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575E120F)
    (at 1.27 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C125 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 A3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575E1218)
    (at -1.27 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C126 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 A4))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575E1247)
    (at -3.81 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C127 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 A5))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57777018)
    (at -9.8298 -3.0226 315)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C128 (at -1.066854 -1.081223 315) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579CD7F8)
    (at 6.5786 16.0274)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C129 (at 2.33934 0.7747) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57715559)
    (at 12.827 -16.256 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C130 (at 2.5908 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57673A67)
    (at 27.686 -0.762 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C131 (at 0 1.27 135) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575E1243)
    (at -6.35 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C132 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 A6))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575E1241)
    (at -8.89 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C133 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 A7))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575E1277)
    (at -11.43 -15.748 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C134 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 A8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 577155AF)
    (at 26.67 -7.62 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C135 (at 0 -1.1938 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5777702F)
    (at -5.0038 -3.7846)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C136 (at -0.381 -1.08966) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57673F52)
    (at 22.098 6.985 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C137 (at 0 -1.257236 135) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.089803 -0.089803 135) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 575FB695)
    (at 17.018 -15.24 225)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C138 (at 0 1.077631 225) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 225) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579CF3FE)
    (at 21.717 12.573)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C139 (at -2.48412 -0.6858) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.127 0.127) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C139-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57977FA3)
    (at -33.5788 0.3429 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D101 (at 2.44856 0.02286 360) (layer F.SilkS))
    (fp_text value CDBU0520 (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 25 +BATT))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 Vsupply))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 578BCDC5)
    (at -16.86052 -24.38654 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D102 (at -3.15468 0.19812 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D102-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57977F67)
    (at -33.5788 -1.15824 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D103 (at 2.44856 0.03048 360) (layer F.SilkS))
    (fp_text value CDBU0520 (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 USB_5V))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 Vsupply))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CBBE3)
    (at -10.668 0 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D107 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D107-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 140 /IO_038))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CBAEE)
    (at -10.668 2.54 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D108 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D108-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 141 /IO_041))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CBAE8)
    (at -10.668 5.08 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D109 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D109-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 142 /IO_044))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CBADA)
    (at -10.668 7.62 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D110 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D110-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 143 /IO_046))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CBAAE)
    (at -10.668 10.16 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D111 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D111-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 144 /IO_050))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CBA4F)
    (at -10.668 12.7 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D112 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D112-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 145 /IO_054))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CB9A5)
    (at -10.668 15.24 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D113 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D113-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 146 /IO_056))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 576CB992)
    (at -10.668 17.78 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D114 (at 0.0254 1.016 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D114-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 147 /IO_058))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5797692E)
    (at -23.7363 -6.59384)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L102 (at -1.56464 -0.87376) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 USB_3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57959C10)
    (at -45.7708 23.94712)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L103 (at 2.3368 0.54102 180) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 195 /USB_VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 USB_5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 576701CA)
    (at -0.8643 -12.8397)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L104 (at 0.0007 1.016) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0.0007 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 VCCIO1A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5777702A)
    (at -9.8933 -7.13994)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L105 (at 0.06096 1.12268) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 VCCIO1B))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 16.51 -18.542 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L106 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VCCA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57715745)
    (at 31.75 2.54 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L107 (at 1.1176 -1.1938 180) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 VCC_ONE))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57715776)
    (at 31.75 -7.62 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L108 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 VCCIO))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 579CF3F9)
    (at 21.717 11.049 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L109 (at 2.4384 0.64008 180) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at -0.127 -0.127 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C139-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 577158FC)
    (at -9.0424 -12.954 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L110 (at -1.257236 1.077631 135) (layer F.SilkS))
    (fp_text value MPZ1608S221ATA00 (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 A_G))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18 locked (layer F.Cu) (tedit 57675D60)
    (at 36.83 -21.59)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P101 (at 0 -2.3876) (layer F.SilkS))
    (fp_text value CONN_01X18 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 136 /IO_127))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 137 /IO_124))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 /IO_120))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 /IO_119))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 /IO_118))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 /IO_114))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 /IO_113))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 /IO_111))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 /IO_110))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 /IO_106))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 108 /IO_105))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 /IO_102))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 110 /IO_101))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 111 /IO_100))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 112 /IO_099))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 113 /IO_093))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 3.3V_Reg))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x18.wrl
      (at (xyz 0 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57922F1E)
    (at -37.06876 21.11248)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P102 (at 1.81102 2.79908 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 +BATT))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 575FBA2A)
    (at 27.432 -15.494 135)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P103 (at 1.778 2.54 225) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 1.27 225) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 135) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P103-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 135) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18 locked (layer F.Cu) (tedit 57675D4B)
    (at -11.43 -21.59 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P105 (at 0 -2.3876 270) (layer F.SilkS))
    (fp_text value CONN_01X18 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 A_8))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 A_7))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 A_6))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 A_5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 A_4))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 A_3))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 A_2))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 A_1))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 A_G))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 A_0))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 114 /IO_141))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 115 /IO_140))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 116 /IO_135))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 117 /IO_132))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 118 /IO_131))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 119 /IO_130))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 3.3V_Reg))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x18.wrl
      (at (xyz 0 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18 locked (layer F.Cu) (tedit 57675D5B)
    (at 31.75 21.59 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P107 (at 0 -2.4384 450) (layer F.SilkS))
    (fp_text value CONN_01X18 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 120 /IO_092))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 121 /IO_091))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 122 /IO_090))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 CLK_24MHz))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 123 /IO_088))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 124 /IO_087))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 125 /IO_086))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 126 /IO_085))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 127 /IO_084))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 128 /IO_081))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 129 /IO_079))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 130 /IO_078))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 131 /IO_077))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 132 /IO_076))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 133 /IO_075))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 134 /IO_074))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 3.3V_Reg))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x18.wrl
      (at (xyz 0 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18 locked (layer F.Cu) (tedit 57675D56)
    (at -16.51 21.59 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P109 (at 0 -2.4384 180) (layer F.SilkS))
    (fp_text value CONN_01X18 (at 0 -2.9718 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 148 /IO_059))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 149 /IO_057))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 150 /IO_055))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 151 /IO_052))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 152 /IO_047))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 153 /IO_045))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 154 /IO_043))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 155 /IO_039))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /IO_029))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IO_028))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IO_027))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IO_026))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /IO_025))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /IO_024))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /IO_022))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /IO_021))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 3.3V_Reg))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x18.wrl
      (at (xyz 0 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 578BCE28)
    (at -19.06016 -23.83536 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 0 -1.12268 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D102-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575FB97E)
    (at 25.908 -12.192 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at 0 -1.27 225) (layer F.SilkS))
    (fp_text value 10k (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R102-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575FB62B)
    (at 18.796 -18.542 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R103 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R103-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575FB654)
    (at 21.336 -18.542 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R104 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R104-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575FB8F9)
    (at 21.844 -12.7 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R105 (at 0 -1.27 225) (layer F.SilkS))
    (fp_text value 10k (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R105-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575FB94D)
    (at 23.622 -10.414 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R106 (at 0 -1.27 225) (layer F.SilkS))
    (fp_text value 10k (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R106-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575FB920)
    (at 23.876 -14.224 315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R107 (at 0 -1.27 315) (layer F.SilkS))
    (fp_text value 10k (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P103-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57950BC3)
    (at -41.91635 -22.01545 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R108 (at -1.55702 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 187 /E_P_TDI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 579CD0BB)
    (at -42.41673 -11.56843 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R110 (at 0.16891 -1.21285 450) (layer F.SilkS))
    (fp_text value 1k (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 183 /E_P_TCK_b))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57977E6A)
    (at -48.83404 16.09852)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R111 (at -0.06604 1.1684 180) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 195 /USB_VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D105-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57959F88)
    (at -36.94557 17.19961 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R112 (at -0.93599 1.16459 90) (layer F.SilkS))
    (fp_text value 499 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 USB_5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D104-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57950A18)
    (at -39.22776 -13.36548 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R113 (at 0 -1.10236 450) (layer F.SilkS))
    (fp_text value 27 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 /E_P_TCK_a))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 183 /E_P_TCK_b))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57950BD3)
    (at -41.91635 -14.39545 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R114 (at -1.55702 0 450) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 /E_P_SEN_b))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 /E_P_SEN_a))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5795B82F)
    (at -36.96208 -16.94942)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R115 (at 0.43688 -1.11506) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D106-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57977F84)
    (at -36.44392 -2.90322 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R116 (at 0.53594 1.15824 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 USB_3.3V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 196 CBUS5_6MHz))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57977F87)
    (at -38.79088 -2.90322 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R117 (at 0.75438 1.16332 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 197 /CBUS6))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5771B119)
    (at -38.29304 -0.04318 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R118 (at -0.0007 -1.1811 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 USB_3.3V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 198 /USB_RST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57950B87)
    (at -41.91635 -16.93545 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R119 (at -1.55702 0 450) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 /E_P_SEN_a))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 576DEC8E)
    (at -38.91026 4.81838 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R120 (at 0 1.1684 270) (layer F.SilkS))
    (fp_text value 27 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 166 /USBDm))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 /D-))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5775A563)
    (at -19.56054 -17.78 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R121 (at 1.54686 0.15748 270) (layer F.SilkS))
    (fp_text value 27 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 /J_TCK_b))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 173 /J_TCK_a))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 576DEC84)
    (at -37.31006 4.81838 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R122 (at 0 -1.2319 270) (layer F.SilkS))
    (fp_text value 27 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 167 /USBDp))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 /D+))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 577158BD)
    (at -9.7028 -10.922 135)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R123 (at 2.406709 0 135) (layer F.SilkS))
    (fp_text value 10k (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /J_en))
    (pad 2 smd rect (at 0.75 0 135) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57768E18)
    (at -19.56054 -20.32)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R124 (at -1.57226 -0.2032 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /J_TMS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 576751EC)
    (at -2.7432 -8.67664 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R126 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 /J_TCK_b))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 576C75D7)
    (at -0.127 -8.6106 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R127 (at 0 1.1684 180) (layer F.SilkS))
    (fp_text value 27 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 174 /J_TCK_c))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 /J_TCK_b))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5797805B)
    (at -39.67226 11.14806 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R128 (at -1.4859 -0.50292 360) (layer F.SilkS))
    (fp_text value 100k (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 /ID))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5769586D)
    (at -13.462 0)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R129 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D107-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57695863)
    (at -13.462 2.54)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R130 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D108-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57695850)
    (at -13.462 5.08)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R131 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D109-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5769583E)
    (at -13.462 7.62)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R132 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D110-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57695831)
    (at -13.462 10.16)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R133 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D111-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57695820)
    (at -13.462 12.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R134 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D112-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57943F41)
    (at -35.51174 -19.80438 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R135 (at 0 -1.1684 270) (layer F.SilkS))
    (fp_text value 27 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 /C_P_TCK_b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 168 /C_P_TCK_a))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57695810)
    (at -13.462 15.24)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R136 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D113-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57943EDA)
    (at -30.43174 -19.80438 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R137 (at 0 1.1684 450) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 CPLD_3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 170 /C_P_TMS))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57695806)
    (at -13.462 17.78)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R138 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D114-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57943FEA)
    (at -38.05174 -19.80438 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R140 (at 0 -1.1684 270) (layer F.SilkS))
    (fp_text value 1k (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 168 /C_P_TCK_a))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E1031)
    (at 11.43 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R141 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 5 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 A0))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 A_0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E102D)
    (at 6.35 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R142 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 5 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 A1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 A_1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E102B)
    (at 3.81 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R143 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 5 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 A2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 A_2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E10A1)
    (at 1.27 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R144 (at -0.002643 1.245566 90) (layer F.SilkS))
    (fp_text value 5 (at -0.002643 -0.024434 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 A3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 A_3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E1098)
    (at -1.27 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R145 (at -0.002644 1.245567 90) (layer F.SilkS))
    (fp_text value 5 (at -0.002644 -0.024433 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 A4))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 A_4))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E1093)
    (at -3.81 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R146 (at -0.002644 1.245567 90) (layer F.SilkS))
    (fp_text value 5 (at -0.002644 -0.024433 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 A5))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 A_5))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E1090)
    (at -6.35 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R147 (at -0.002643 1.245567 90) (layer F.SilkS))
    (fp_text value 5 (at -0.002643 -0.024433 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 A6))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 A_6))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E105F)
    (at -8.89 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R148 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 5 (at -0.002643 -0.024434 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 A7))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 A_7))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 575E1063)
    (at -11.43 -18.542 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R149 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 5 (at -0.002644 -0.024433 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 A8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 A_8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:SMD-8 locked placed (layer F.Cu) (tedit 576713E7)
    (at 44.2722 0 90)
    (descr "SMD-8 Surface Mount 300mil 8pin Dual In Line Package")
    (tags "Power Integrations G Package")
    (fp_text reference SW103 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value DIPS_04 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6322 4.318 90) (size 1.1684 2.032) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 2 smd rect (at -1.27 4.318 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 3 smd rect (at 1.27 4.318 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 4 smd rect (at 3.6322 4.318 90) (size 1.1684 2.032) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 5 smd rect (at 3.6322 -4.318 90) (size 1.1684 2.032) (layers F.Cu F.Paste F.Mask)
      (net 104 /IO_113))
    (pad 6 smd rect (at 1.27 -4.318 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 105 /IO_111))
    (pad 7 smd rect (at -1.27 -4.318 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 106 /IO_110))
    (pad 8 smd rect (at -3.6322 -4.318 90) (size 1.1684 2.032) (layers F.Cu F.Paste F.Mask)
      (net 107 /IO_106))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 578E3E93)
    (at -26.18994 -2.37744 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U101 (at 2.5527 5.01142 270) (layer F.SilkS))
    (fp_text value LD1117S33CTR (at 0 0.762 270) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 270) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (pad 3 smd rect (at 2.286 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 Vsupply))
    (pad 1 smd rect (at -2.286 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5771571B)
    (at 31.75 10.16 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R150 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 110 /IO_101))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5771572A)
    (at 31.75 7.62 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R151 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 108 /IO_105))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57715735)
    (at 31.75 5.08 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R152 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 107 /IO_106))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57715752)
    (at 31.75 0 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R153 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 /IO_110))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5771575E)
    (at 31.75 -2.54 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R154 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /IO_111))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5771576A)
    (at 31.75 -5.08 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R155 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 /IO_113))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57715786)
    (at 31.75 -10.16 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R156 (at 1.1176 -1.1938 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /IO_118))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57715792)
    (at 31.75 -12.7 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R157 (at 1.1176 -1.1938 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /IO_120))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57676A9C)
    (at 48.26 23.876 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R158 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57676AA6)
    (at 48.26 -23.876 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D115 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(D115-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(D115-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57676A91)
    (at 42.672 -23.876 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R159 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(D115-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V_Reg))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5795B82B)
    (at -34.26206 -16.99768 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D106 (at -0.45974 0.9906 180) (layer F.SilkS))
    (fp_text value Led_Small (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D106-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 199 /E_P_SEN_i))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5777571A)
    (at -39.04615 14.49959)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R160 (at 0 -1.17602) (layer F.SilkS))
    (fp_text value 499 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57775563)
    (at -39.39667 16.89989 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q101 (at 0 -1.92024 180) (layer F.SilkS))
    (fp_text value MMBT3904,215 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D104-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 7 USB_5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 57959FBA)
    (at -36.79571 14.39799 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D104 (at 1.27635 1.29159 90) (layer F.SilkS))
    (fp_text value PDZ2.4B,115 (at -0.02286 0.02286 90) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 90) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D104-Pad1)"))
    (pad 2 smd rect (at 1.055 0 90) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782A920)
    (at -19.558 2.5146 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R161 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 155 /IO_039))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 /a))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782A945)
    (at -19.558 5.0546 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R162 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 154 /IO_043))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 207 /b))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782AA14)
    (at -19.558 7.5946 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R163 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 153 /IO_045))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 205 /c))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782A9FB)
    (at -19.558 10.1346 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R164 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 152 /IO_047))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 202 /d))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782A9D3)
    (at -19.558 12.6746 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R165 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 /IO_052))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 201 /e))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782A9B0)
    (at -19.558 15.2146 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R166 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 150 /IO_055))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 /f))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782A961)
    (at -19.558 17.7546 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R167 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 149 /IO_057))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 204 /g))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782A522)
    (at -19.558 20.2946 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R168 (at 1.6256 0 270) (layer F.SilkS))
    (fp_text value 499 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 148 /IO_059))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 211 /pt))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5794FE99)
    (at -36.78174 -22.85492 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P108 (at 1.72466 12.97686 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at -0.00254 6.35762 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 169 /C_P_TDO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 168 /C_P_TCK_a))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 171 /C_P_TDI))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 170 /C_P_TMS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 CPLD_3.3V))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KMRH:neuron_silk_screen_graphic_2016-07-29 locked (layer B.Cu) (tedit 0)
    (at -0.0381 0)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module KMRH:SBL_logo_09p9x7p4_mm (layer F.Cu) (tedit 0)
    (at -3.30454 14.86408 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text 24MHz (at 17.28978 15.24) (layer F.SilkS))
  (gr_text "MAX 10 FPGA Dev Board\nCodename: \"Neuron\"\nDesign: Reg Holmes 2016-07-30\nSCH Rev: E0-1-0\nBRD Rev: E0-1-0" (at 26.59888 19.8374 90) (layer F.SilkS))
  (gr_text "MAX 10 FPGA" (at 15.0241 13.53312 45) (layer F.SilkS))
  (gr_text TDI (at -42.42435 -23.28545) (layer F.SilkS))
  (gr_text TMS (at -42.42435 -18.20545) (layer F.SilkS))
  (gr_text TDO (at -42.42435 -15.66545) (layer F.SilkS))
  (gr_text TCK (at -42.42435 -13.12545) (layer F.SilkS))
  (gr_text SENSE (at -49.58207 -15.66545 90) (layer F.SilkS))
  (gr_text TMS (at -26.6192 -24.54402) (layer F.SilkS))
  (gr_text TDI (at -31.70174 -24.5491) (layer F.SilkS))
  (gr_text TCK (at -34.24174 -24.54148) (layer F.SilkS))
  (gr_text TDO (at -36.00704 -24.54402) (layer F.SilkS))
  (gr_text 3.3V (at -29.16174 -24.5491) (layer F.SilkS))
  (gr_text CC0 (at -20.5994 -8.89) (layer F.SilkS))
  (gr_text CC1 (at -20.5994 -6.35) (layer F.SilkS))
  (gr_text CC2 (at -20.5994 -3.81) (layer F.SilkS))
  (gr_text CC3 (at -20.5994 -1.27) (layer F.SilkS))
  (gr_text a (at -20.3454 1.27) (layer F.SilkS))
  (gr_text b (at -20.3454 3.81) (layer F.SilkS))
  (gr_text c (at -20.3454 6.35) (layer F.SilkS))
  (gr_text d (at -20.3454 8.89) (layer F.SilkS))
  (gr_text e (at -20.3454 11.43) (layer F.SilkS))
  (gr_text f (at -20.3454 13.97) (layer F.SilkS))
  (gr_text g (at -20.3454 16.51) (layer F.SilkS))
  (gr_text pt (at -20.3454 19.05) (layer F.SilkS))
  (gr_text "FPGA Pwr" (at -16.20012 -23.33498) (layer F.SilkS))
  (gr_text "Auxiliary Power" (at -31.4325 24.41448) (layer F.SilkS))
  (gr_text U105 (at 11.56716 -15.05458) (layer F.SilkS))
  (gr_text "+5V\nto\n+15V" (at -39.77894 21.11248) (layer F.SilkS))
  (gr_text "Parallel\nto\nJTAG" (at -34.23412 -8.98906) (layer F.SilkS))
  (gr_text "External\nJTAG Programmer" (at -49.89322 -10.6553) (layer F.SilkS))
  (gr_text "CPLD JTAG Programmer" (at -30.89402 -24.37892) (layer B.SilkS))
  (gr_text "USB to Parallel" (at -43.48734 -7.48284) (layer F.SilkS))
  (gr_text Mini-USB (at -49.4538 3.28422 90) (layer F.SilkS))
  (gr_text 58 (at -8.6614 17.78) (layer F.SilkS))
  (gr_text 56 (at -8.6614 15.24) (layer F.SilkS))
  (gr_text 54 (at -8.6614 12.7) (layer F.SilkS))
  (gr_text 50 (at -8.6614 10.16) (layer F.SilkS))
  (gr_text 46 (at -8.6614 7.62) (layer F.SilkS))
  (gr_text 44 (at -8.6614 5.08) (layer F.SilkS))
  (gr_text 41 (at -8.6614 2.54) (layer F.SilkS))
  (gr_text 38 (at -8.6614 0) (layer F.SilkS))
  (gr_text GND (at -19.2786 21.59) (layer F.SilkS))
  (gr_text 59 (at -18.8214 19.05) (layer F.SilkS))
  (gr_text 57 (at -18.8214 16.51) (layer F.SilkS))
  (gr_text 55 (at -18.8214 13.97) (layer F.SilkS))
  (gr_text 52 (at -18.8214 11.43) (layer F.SilkS))
  (gr_text 47 (at -18.8214 8.89) (layer F.SilkS))
  (gr_text 45 (at -18.8214 6.35) (layer F.SilkS))
  (gr_text 43 (at -18.8214 3.81) (layer F.SilkS))
  (gr_text 39 (at -18.8214 1.27) (layer F.SilkS))
  (gr_text 29 (at -18.8214 -1.27) (layer F.SilkS))
  (gr_text 28 (at -18.8214 -3.81) (layer F.SilkS))
  (gr_text 27 (at -18.8214 -6.35) (layer F.SilkS))
  (gr_text 26 (at -18.8214 -8.89) (layer F.SilkS))
  (gr_text 25 (at -18.8214 -11.43) (layer F.SilkS))
  (gr_text 24 (at -18.8214 -13.97) (layer F.SilkS))
  (gr_text 22 (at -18.8214 -16.51) (layer F.SilkS))
  (gr_text 3.3V (at -19.2786 -21.59) (layer F.SilkS))
  (gr_text 21 (at -18.8214 -19.05) (layer F.SilkS))
  (gr_text "Switches Shorted" (at 49.022 -19.05 90) (layer F.SilkS))
  (gr_text 91 (at 26.67 24.13) (layer F.SilkS))
  (gr_text 92 (at 29.21 23.876) (layer F.SilkS))
  (gr_text 87 (at 16.51 24.13) (layer F.SilkS))
  (gr_text 88 (at 19.05 23.876) (layer F.SilkS))
  (gr_text 90 (at 24.13 23.876) (layer F.SilkS))
  (gr_text 89 (at 21.59 24.13) (layer F.SilkS))
  (gr_text 85 (at 11.43 24.13) (layer F.SilkS))
  (gr_text 86 (at 13.97 23.876) (layer F.SilkS))
  (gr_text 78 (at 1.27 24.13) (layer F.SilkS))
  (gr_text 79 (at 3.81 23.876) (layer F.SilkS))
  (gr_text 84 (at 8.89 23.876) (layer F.SilkS))
  (gr_text 81 (at 6.35 24.13) (layer F.SilkS))
  (gr_text 76 (at -3.81 24.13) (layer F.SilkS))
  (gr_text 77 (at -1.27 23.876) (layer F.SilkS))
  (gr_text 75 (at -6.35 23.876) (layer F.SilkS))
  (gr_text 74 (at -8.89 24.13) (layer F.SilkS))
  (gr_text 3.3V (at -11.43 23.876) (layer F.SilkS))
  (gr_text GND (at 31.75 24.13) (layer F.SilkS))
  (gr_text PB0 (at 34.036 12.192) (layer F.SilkS))
  (gr_text PB1 (at 34.036 7.112) (layer F.SilkS))
  (gr_text SW0 (at 34.036 4.572) (layer F.SilkS))
  (gr_text SW1 (at 34.036 2.032) (layer F.SilkS))
  (gr_text SW2 (at 34.036 -0.508) (layer F.SilkS))
  (gr_text SW3 (at 34.036 -3.048) (layer F.SilkS))
  (gr_text PB2 (at 34.036 -8.128) (layer F.SilkS))
  (gr_text PB3 (at 34.036 -13.208) (layer F.SilkS))
  (gr_text GND (at 39.751 -21.59) (layer F.SilkS))
  (gr_text 3.3V (at 39.8272 21.59) (layer F.SilkS))
  (gr_text 93 (at 33.9852 19.05) (layer F.SilkS))
  (gr_text 99 (at 33.9852 16.51) (layer F.SilkS))
  (gr_text 100 (at 33.9852 13.97) (layer F.SilkS))
  (gr_text 101 (at 33.9852 11.43) (layer F.SilkS))
  (gr_text 102 (at 33.9852 8.89) (layer F.SilkS))
  (gr_text 105 (at 33.9852 6.35) (layer F.SilkS))
  (gr_text 106 (at 33.9852 3.81) (layer F.SilkS))
  (gr_text 110 (at 33.9852 1.27) (layer F.SilkS))
  (gr_text 111 (at 33.9852 -1.27) (layer F.SilkS))
  (gr_text 113 (at 33.9852 -3.81) (layer F.SilkS))
  (gr_text 114 (at 33.9852 -6.35) (layer F.SilkS))
  (gr_text 118 (at 33.9852 -8.89) (layer F.SilkS))
  (gr_text 119 (at 33.9852 -11.43) (layer F.SilkS))
  (gr_text 120 (at 33.9852 -13.97) (layer F.SilkS))
  (gr_text 124 (at 33.9852 -16.51) (layer F.SilkS))
  (gr_text 127 (at 33.9852 -19.05) (layer F.SilkS))
  (gr_text "Profile\nSelect" (at 30.226 -14.478 45) (layer F.SilkS))
  (gr_text GND (at -11.43 -23.876) (layer F.SilkS))
  (gr_text 3.3V (at 31.75 -24.13) (layer F.SilkS))
  (gr_text 130 (at 29.21 -23.876) (layer F.SilkS))
  (gr_text 131 (at 26.67 -24.13) (layer F.SilkS))
  (gr_text 141 (at 16.51 -24.13) (layer F.SilkS))
  (gr_text 135 (at 21.59 -24.13) (layer F.SilkS))
  (gr_text 132 (at 24.13 -23.876) (layer F.SilkS))
  (gr_text 140 (at 19.05 -23.876) (layer F.SilkS))
  (gr_text A5 (at -1.27 -23.876) (layer F.SilkS))
  (gr_text A6 (at -3.81 -24.13) (layer F.SilkS))
  (gr_text A8 (at -8.89 -24.13) (layer F.SilkS))
  (gr_text A7 (at -6.35 -23.876) (layer F.SilkS))
  (gr_text A3 (at 3.81 -23.876) (layer F.SilkS))
  (gr_text A4 (at 1.27 -24.13) (layer F.SilkS))
  (gr_text A2 (at 6.35 -24.13) (layer F.SilkS))
  (gr_text A1 (at 8.89 -23.876) (layer F.SilkS))
  (gr_text A_GND (at 11.43 -24.13) (layer F.SilkS))
  (gr_text A0 (at 13.97 -23.876) (layer F.SilkS))
  (gr_line (start -50 25) (end -50 -25) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 50 25) (end -50 25) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 50 -25) (end 50 25) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start -50 -25) (end 50 -25) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (zone (net 3) (net_name 3.3V_Reg) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -19.90598 -25.146) (xy 47.752 -25.146) (xy 47.752 25.146) (xy -19.90598 25.146) (xy -19.90598 -4.2037)
        (xy -19.59356 -4.51612) (xy -19.59356 -5.6388) (xy -19.90598 -5.95122)
      )
    )
    (polygon
      (pts        (xy -12.1412 -19.812) (xy -12.1412 -14.5796) (xy -7.4422 -9.8806) (xy 2.9718 -9.8806) (xy 5.1308 -7.7216)
        (xy 9.5123 -12.1031) (xy 7.6708 -13.9446) (xy 7.6708 -14.7066) (xy 10.1092 -17.145) (xy 12.0142 -17.145)
        (xy 12.1412 -17.272) (xy 12.1412 -19.431) (xy 12.7127 -20.0025) (xy 14.6431 -20.0025) (xy 15.3289 -20.6756)
        (xy 15.3289 -23.368) (xy -10.414 -23.368) (xy -10.414 -20.574) (xy -11.176 -19.812)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 50.038 25.146) (xy -50.038 25.146) (xy -50.038 -25.146) (xy 50.038 -25.146) (xy 50.038 25.146)
      )
    )
    (polygon
      (pts        (xy -10.0076 -23.1902) (xy -10.2489 -22.9362) (xy -10.2489 -20.7772) (xy -11.2014 -19.812) (xy -12.1412 -19.812)
        (xy -12.1412 -14.5796) (xy -10.2108 -12.6492) (xy -6.8834 -12.6492) (xy -4.1148 -9.8806) (xy 2.9464 -9.8806)
        (xy 5.1308 -7.6962) (xy 9.525 -12.0904) (xy 7.6708 -13.9446) (xy 7.6708 -14.7066) (xy 10.1092 -17.145)
        (xy 12.0142 -17.145) (xy 12.1412 -17.272) (xy 12.1412 -19.431) (xy 12.7127 -20.0025) (xy 14.6431 -20.0025)
        (xy 15.3289 -20.6756) (xy 15.3289 -23.1902) (xy -10.0076 -23.1902)
      )
    )
  )
  (zone (net 138) (net_name "Net-(D115-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 50.038 25.146) (xy 48.514 25.146) (xy 48.514 -25.146) (xy 50.038 -25.146)
      )
    )
  )
  (zone (net 12) (net_name A_G) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -10.0711 -22.7965) (xy -9.8933 -22.9743) (xy 15.1511 -22.9743) (xy 15.1511 -20.8661) (xy 14.5415 -20.2565)
        (xy 12.573 -20.2565) (xy 11.8872 -19.5707) (xy 11.8872 -17.5387) (xy 11.7475 -17.399) (xy 10.0076 -17.399)
        (xy 7.4168 -14.8082) (xy 7.4168 -13.9192) (xy 8.8265 -12.5095) (xy 8.8265 -11.7729) (xy 5.461 -8.4074)
        (xy 4.7244 -8.4074) (xy 2.9845 -10.1473) (xy -3.6449 -10.1473) (xy -6.7691 -13.2715) (xy -10.4394 -13.2715)
        (xy -11.7983 -14.6304) (xy -11.8872 -14.6304) (xy -11.8872 -19.5834) (xy -11.1125 -19.5834) (xy -10.0711 -20.6248)
      )
    )
  )
  (zone (net 5) (net_name CPLD_3.3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy -30.47746 -9.44118) (xy -31.02102 -9.98474) (xy -31.02102 -16.22298) (xy -30.47746 -16.76654) (xy -24.23922 -16.76654)
        (xy -23.69566 -16.22298) (xy -23.69566 -9.98474) (xy -24.23922 -9.44118)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.29054 20.4216) (xy 18.29054 10.52322) (xy 18.288 9.6139) (xy 16.32712 7.65302) (xy 16.7513 7.22884)
        (xy 20.04568 10.52322) (xy 23.00478 10.52322) (xy 23.00478 20.4216) (xy 22.58314 21.96084) (xy 20.96262 21.96084)
        (xy 19.42338 20.4216)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.29054 20.4216) (xy 18.29054 10.52322) (xy 18.288 9.6139) (xy 16.32712 7.65302) (xy 16.7513 7.22884)
        (xy 20.04568 10.52322) (xy 23.00478 10.52322) (xy 23.00478 20.4216) (xy 22.58314 21.96084) (xy 20.96262 21.96084)
        (xy 19.42338 20.4216)
      )
    )
  )
)
