(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 13)
    (no_connects 0)
    (area 147.956499 103.068632 172.083501 141.443501)
    (thickness 1.6002)
    (drawings 7)
    (tracks 87)
    (zones 0)
    (modules 4)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 "Net-(J1-Pad3)")
  (net 6 /HV6)
  (net 7 /HV5)
  (net 8 /HV10)
  (net 9 /HV4)
  (net 10 /HV9)
  (net 11 /HV3)
  (net 12 /HV8)
  (net 13 /HV2)
  (net 14 /HV7)
  (net 15 /HV1)
  (net 16 "Net-(J1-Pad15)")
  (net 17 "Net-(J1-Pad5)")
  (net 18 "Net-(NX1-Pad12)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(NX1-Pad12)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5B2D8862)
    (at 170.18 136.84 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at -2.26 9.96 360) (layer F.SilkS) hide)
    (fp_text value Nixie (at 1.27 22.65 270) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV6))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV5))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV10))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV4))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV9))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV3))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV8))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV2))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV7))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV1))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 -0.12))
      (scale (xyz 1 1 -1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 170.72 126.48 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.1 1.5 270) (layer F.SilkS))
    (fp_text value 27K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(NX1-Pad12)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /Anode))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 164.82 132.38 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module .pretty:mynixies-GR10K (layer F.Cu) (tedit 5B2D85CB)
    (at 160.02 117.78)
    (attr virtual)
    (fp_text reference NX1 (at -0.381 -17.65046) (layer F.SilkS) hide)
    (fp_text value GR10K (at 22.3 -2.3) (layer F.SilkS) hide)
    (fp_text user 3 (at -7.747 9.271) (layer Dwgs.User))
    (fp_text user 9 (at -4.191 11.049) (layer Dwgs.User))
    (fp_text user 0 (at 4.318 11.176) (layer Dwgs.User))
    (fp_text user 7 (at 7.874 8.636) (layer Dwgs.User))
    (fp_text user 8 (at 10.16 5.842) (layer Dwgs.User))
    (fp_text user 6 (at 7.62 -9.144) (layer Dwgs.User))
    (fp_text user 5 (at 4.572 -10.795) (layer Dwgs.User))
    (fp_text user A (at 0 -11.811) (layer Dwgs.User))
    (fp_text user 1 (at -4.191 -11.176) (layer Dwgs.User))
    (fp_text user 2 (at -7.62 -9.271) (layer Dwgs.User))
    (fp_text user 4 (at -10.033 -6.096) (layer Dwgs.User))
    (pad 1 thru_hole circle (at -5.85978 6.985) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 11 /HV3))
    (pad 2 thru_hole circle (at -3.11658 8.56742) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 10 /HV9))
    (pad 4 thru_hole circle (at 3.11658 8.56742) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 8 /HV10))
    (pad 5 thru_hole circle (at 5.85978 6.985) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 14 /HV7))
    (pad 6 thru_hole circle (at 7.89686 4.5593) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 12 /HV8))
    (pad 10 thru_hole circle (at 5.85978 -6.985) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 6 /HV6))
    (pad 11 thru_hole circle (at 3.11658 -8.56742) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 7 /HV5))
    (pad 12 thru_hole circle (at 0 -9.1186) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 18 "Net-(NX1-Pad12)"))
    (pad 13 thru_hole circle (at -3.11658 -8.56742) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 15 /HV1))
    (pad 14 thru_hole circle (at -5.85978 -6.985) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 13 /HV2))
    (pad 15 thru_hole circle (at -7.89686 -4.5593) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 9 /HV4))
    (pad "" np_thru_hole circle (at 0 9.1186) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 8.9789 1.58242) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 8.9789 -1.58242) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.89686 -4.5593) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -8.9789 -1.58242) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -8.9789 1.58242) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 10.16 10.16) (drill 10.16) (layers *.Cu *.Mask))
  )
  (gr_text "nixies.us\nGR10K" (at 160.42 132.78) (layer B.Mask))
  (gr_arc (start 160.02 117.78) (end 148.02 109.38) (angle 110.0159606) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.02 134.38) (end 148.02 109.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.02 141.38) (end 148.02 134.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.02 134.38) (end 172.02 109.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.02 141.38) (end 172.02 134.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.02 141.38) (end 172.02 141.38) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 177.8 101.6) (xy 142.24 101.6) (xy 142.24 142.24) (xy 177.8 142.24)
      )
    )
  )
)
