(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6256)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "dielectric 1"
				(type "core")
				(color "FR4 natural")
				(thickness 1.524)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 110.16 49.71)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VDD")
	(net 2 "/BUZZ_NEG")
	(net 3 "/DAH_BASE")
	(net 4 "GND")
	(net 5 "/DIT_BASE")
	(net 6 "/UIO1")
	(net 7 "/UIO0")
	(net 8 "/AUX_DAH_EXT")
	(net 9 "/AUX_DIT_EXT")
	(net 10 "/LED_A")
	(net 11 "/LED_K")
	(net 12 "/DAH_EXT")
	(net 13 "/DIT_EXT")
	(net 14 "unconnected-(J1-PadTN)")
	(net 15 "unconnected-(J2-PadTN)")
	(net 16 "/UIO5")
	(net 17 "/UIO4")
	(net 18 "unconnected-(J3-Pin_9-Pad9)")
	(net 19 "unconnected-(J3-Pin_10-Pad10)")
	(net 20 "/UIO3")
	(net 21 "/UIO2")
	(net 22 "Net-(R7-Pad1)")
	(net 23 "Net-(R8-Pad1)")
	(net 24 "Net-(Q2A-B1)")
	(net 25 "Net-(Q2B-B2)")
	(net 26 "Net-(Q3A-B1)")
	(net 27 "Net-(Q3B-B2)")
	(footprint "LED_THT:LED_Oval_W5.2mm_H3.8mm"
		(layer "F.Cu")
		(at 110.26 80.085 90)
		(descr "LED_Oval, Oval,  Oval size 5.2x3.8mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-5603QBC-D(Ver.12B).pdf")
		(tags "LED_Oval Oval  Oval size 5.2x3.8mm^2 2 pins")
		(property "Reference" "D1"
			(at -1.925 -1.2 135)
			(layer "F.SilkS")
		)
		(property "Value" "C5SMF-RJF-CT0W0BB1"
			(at 1.27 2.96 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://downloads.cree-led.com/files/ds/h/HB-C5SMF-RJF-RJE-GJF-GJE-BJF-BJE.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Cree Oval 621nm Red LED C5SMF-RJF-CT0W0BB1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/LED_K")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/LED_A")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_Oval_W5.2mm_H3.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b-etz:PinHeader_2x06_P2.54mm_Horizontal_Flipped"
		(layer "F.Cu")
		(at 116.51 56.06 -90)
		(descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x06 2.54mm double row")
		(property "Reference" "J3"
			(at 1.65 1.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x06_PMOD"
			(at -7.54 6.51 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PMOD Connector, 90 Degrees"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.31 6.35 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/UIO0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/UIO1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/UIO2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/UIO3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at -2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/UIO4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at -2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/UIO5")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at -2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J3-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole oval
			(at -2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J3-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole oval
			(at -2.54 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at -2.54 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 -12.7 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 180)
			)
		)
	)
	(footprint "b-etz:TS11-674-55-BK-100-RA-D"
		(layer "F.Cu")
		(at 116.16 78.71 90)
		(descr "Same Sky TS11 Right-angle Tactile Switch, 5.5 mm Actuator, 100 grf")
		(tags "right-angle THT tactile switch")
		(property "Reference" "SW2"
			(at 0 2.25 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TS11-674-55-BK-100-RA-D"
			(at 0 4.65 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.sameskydevices.com/product/resource/ts11.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Double Pole Single Throw (DPST) Switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 2.25 1.25 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.25 1.25 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(R8-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 3.5 -1.25 90)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -3.5 -1.25 90)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/CUI_DEVICES_TS11-674-55-BK-100-RA-D/CUI_DEVICES_TS11-674-55-BK-100-RA-D.step"
			(offset
				(xyz 0 -3.25 4.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "b-etz:TS11-674-55-BK-100-RA-D"
		(layer "F.Cu")
		(at 104.16 78.71 -90)
		(descr "Same Sky TS11 Right-angle Tactile Switch, 5.5 mm Actuator, 100 grf")
		(tags "right-angle THT tactile switch")
		(property "Reference" "SW1"
			(at 0 2.95 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TS11-674-55-BK-100-RA-D"
			(at 0 4.65 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.sameskydevices.com/product/resource/ts11.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Double Pole Single Throw (DPST) Switch"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 2.25 1.25 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.25 1.25 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(R7-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 3.5 -1.25 270)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -3.5 -1.25 270)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/CUI_DEVICES_TS11-674-55-BK-100-RA-D/CUI_DEVICES_TS11-674-55-BK-100-RA-D.step"
			(offset
				(xyz 0 -3.25 4.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "b-etz:ASJ-200-B-HT"
		(layer "F.Cu")
		(at 104.16 90.21 90)
		(descr "3.5mm Stereo Phone Jack, Right Angle, THT")
		(property "Reference" "J1"
			(at 0 0.05 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ASJ-200-B-HT"
			(at 0 -0.05 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://app.adam-tech.com/products/download/data_sheet/203699/asj-200-x-ht-data-sheet.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Switched T Pole (Normalling)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr through_hole)
		(fp_text user "S"
			(at -2.1 2.9 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "R"
			(at -3.55 -1.65 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "T"
			(at 4.85 3.15 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -3 0 90)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 3 0 90)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
		)
		(pad "R" thru_hole oval
			(at -0.7 -2.4 90)
			(size 2.8 2.6)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/DAH_EXT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "S" thru_hole oval
			(at -3.6 2.6 90)
			(size 2.8 2.6)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "T" thru_hole oval
			(at 3.2 2.6 90)
			(size 2.8 2.6)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/DIT_EXT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "TN" thru_hole oval
			(at 5.1 -2.2 90)
			(size 2.2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J1-PadTN)")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/LIB_ASJ-200-B-HT/ASJ-200-B-HT_mirrored.step"
			(offset
				(xyz -5.5 0 2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "b-etz:ASJ-200-B-HT"
		(layer "F.Cu")
		(at 115.96 90.21 90)
		(descr "3.5mm Stereo Phone Jack, Right Angle, THT")
		(property "Reference" "J2"
			(at 0 0.05 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ASJ-200-B-HT"
			(at 0 -0.05 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://app.adam-tech.com/products/download/data_sheet/203699/asj-200-x-ht-data-sheet.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Switched T Pole (Normalling)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr through_hole)
		(fp_text user "S"
			(at -2.1 2.9 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "T"
			(at 4.85 3.15 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "R"
			(at -3.55 -1.65 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -3 0 90)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 3 0 90)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
		)
		(pad "R" thru_hole oval
			(at -0.7 -2.4 90)
			(size 2.8 2.6)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/AUX_DAH_EXT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "S" thru_hole oval
			(at -3.6 2.6 90)
			(size 2.8 2.6)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "T" thru_hole oval
			(at 3.2 2.6 90)
			(size 2.8 2.6)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/AUX_DIT_EXT")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "TN" thru_hole oval
			(at 5.1 -2.2 90)
			(size 2.2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J2-PadTN)")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/LIB_ASJ-200-B-HT/ASJ-200-B-HT_mirrored.step"
			(offset
				(xyz -5.5 0 2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "b-etz:Buzzer_TDK_PS1720P02"
		(layer "F.Cu")
		(at 110.16 65.91)
		(property "Reference" "BZ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PS1720P02"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://product.tdk.com/system/files/dam/doc/product/sw_piezo/sw_piezo/piezo-buzzer/catalog/piezoelectronic_buzzer_ps_en.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TDK PS1720P02 Piezo 17x8mm Buzzer Indicator"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Buzzer*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pinfunction "+")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BUZZ_NEG")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/CUI_DEVICES_CPE-1785/CUI_DEVICES_CPE-1785.step"
			(offset
				(xyz 0 0 0.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "B.Cu")
		(at 115.16 68.71 180)
		(descr "SOT-363, SC-70-6")
		(tags "SOT-363 SC-70-6")
		(property "Reference" "Q3"
			(at 0 -2.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "MBT3904DW1"
			(at 0 -2 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/mbt3904dw1t1-d.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?363*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "E1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.95 0 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(Q3A-B1)")
			(pinfunction "B1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BUZZ_NEG")
			(pinfunction "C2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "E2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 0.95 0 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(Q3B-B2)")
			(pinfunction "B2")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 0.95 0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/LED_K")
			(pinfunction "C1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 111.56 61.61 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 7 "/UIO0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 114.5 77.71)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 2.96 0.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "100n"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "KEMET C0805C104M5RACTU 100nF 20% X7R 50VDC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "/DAH_BASE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 107.66 74.51 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 2.99 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "/DIT_BASE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 116.56 61.61 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 3.1 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 26 "Net-(Q3A-B1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 17 "/UIO4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 103.86 61.61 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 3 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(Q2A-B1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 20 "/UIO3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 114.06 61.61 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 3.1 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(Q3B-B2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "/UIO5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 108.96 61.61 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at -2.6 -0.06 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 6 "/UIO1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 114.5 79.71 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at -2.96 0.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "220R"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/YAGEO_PYu_RC_Group_51_RoHS_L_12-3313492.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-13220RL 220 Ohm 5% 1/4W 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(R8-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "/DAH_BASE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 106 79.71 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 2.94 0.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "100n"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "KEMET C0805C104M5RACTU 100nF 20% X7R 50VDC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "/DIT_BASE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 110.26 74.51 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 2.8 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "220R"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/YAGEO_PYu_RC_Group_51_RoHS_L_12-3313492.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-13220RL 220 Ohm 5% 1/4W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 10 "/LED_A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "B.Cu")
		(at 116.96 90.21 -90)
		(descr "SOT-363, SC-70-6")
		(tags "SOT-363 SC-70-6")
		(property "Reference" "Q2"
			(at 0 -2.1 90)
			(layer "B.SilkS")
		)
		(property "Value" "MBT3904DW1"
			(at 0 -2 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/mbt3904dw1t1-d.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?363*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0.65 270)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "E1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.95 0 270)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(Q2A-B1)")
			(pinfunction "B1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 -0.65 270)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AUX_DIT_EXT")
			(pinfunction "C2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.95 -0.65 270)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "E2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 0.95 0 270)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(Q2B-B2)")
			(pinfunction "B2")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 0.95 0.65 270)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AUX_DAH_EXT")
			(pinfunction "C1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 112.06 65.91 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 3.4 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "/BUZZ_NEG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 106 77.71)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at -3.04 0.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "220R"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/YAGEO_PYu_RC_Group_51_RoHS_L_12-3313492.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-13220RL 220 Ohm 5% 1/4W 0805"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 22 "Net-(R7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "/DIT_BASE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 106.36 61.61 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 3.1 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(Q2B-B2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 21 "/UIO2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 110.16 91.51 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -3 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "220R"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/YAGEO_PYu_RC_Group_51_RoHS_L_12-3313492.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-13220RL 220 Ohm 5% 1/4W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "/DAH_EXT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "/DAH_BASE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 112.66 74.51 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 2.89 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/PYu_RC_Group_51_RoHS_L_11-1984063.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-102K2L 2.2 kOhm 5% 1/8W 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "/DAH_BASE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 106.86 89.91)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -2.9 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "220R"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/447/YAGEO_PYu_RC_Group_51_RoHS_L_12-3313492.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Yageo RC0805JR-13220RL 220 Ohm 5% 1/4W 0805"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 13 "/DIT_EXT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "/DIT_BASE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "B.Cu")
		(at 110.21 87.31 180)
		(descr "SOT-363, SC-70-6")
		(tags "SOT-363 SC-70-6")
		(property "Reference" "Q1"
			(at 0 0 270)
			(layer "B.SilkS")
		)
		(property "Value" "MBT3904DW1"
			(at 0 -2 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/mbt3904dw1t1-d.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "200mA IC, 40V Vce, Dual NPN/NPN Transistors, SOT-363"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?363*")
		(sheetname "/")
		(sheetfile "tt08_cw_keyer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "E1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.95 0 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/DAH_BASE")
			(pinfunction "B1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/UIO0")
			(pinfunction "C2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.95 -0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "E2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 0.95 0 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/DIT_BASE")
			(pinfunction "B2")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 0.95 0.65 180)
			(size 0.65 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/UIO1")
			(pinfunction "C1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 100 49.71)
		(end 120.32 95.96)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "I/O PMOD >>"
		(at 119.56 55.41 90)
		(layer "F.SilkS")
	)
	(gr_text "DIT/\nSK"
		(at 107.46 78.61 90)
		(layer "F.SilkS")
	)
	(gr_text "^ PADDLE IN ^"
		(at 109.86 90.11 90)
		(layer "F.SilkS")
	)
	(gr_text "DAH"
		(at 114.46 78.81 270)
		(layer "F.SilkS")
	)
	(gr_text "<< I/O PMOD"
		(at 100.86 55.51 270)
		(layer "F.SilkS")
	)
	(gr_text "^ AUX OUT ^"
		(at 110.66 89.91 270)
		(layer "F.SilkS")
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 99.66 49.21) (xy 120.66 49.21) (xy 120.66 96.21) (xy 99.66 96.21)
			)
		)
	)
	(zone
		(net 1)
		(net_name "VDD")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 99.66 49.21) (xy 120.66 49.21) (xy 120.66 96.21) (xy 99.66 96.21)
			)
		)
	)
	(embedded_fonts no)
)
