(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 140.792501 96.025)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J2-Pin_7)")
	(net 2 "Net-(J2-Pin_10)")
	(net 3 "Net-(J2-Pin_6)")
	(net 4 "Net-(J2-Pin_25)")
	(net 5 "Net-(J2-Pin_8)")
	(net 6 "Net-(J2-Pin_1)")
	(net 7 "Net-(J2-Pin_15)")
	(net 8 "Net-(J2-Pin_18)")
	(net 9 "Net-(J2-Pin_22)")
	(net 10 "Net-(J2-Pin_2)")
	(net 11 "Net-(J2-Pin_20)")
	(net 12 "Net-(J2-Pin_9)")
	(net 13 "Net-(J2-Pin_12)")
	(net 14 "Net-(J2-Pin_3)")
	(net 15 "Net-(J2-Pin_23)")
	(net 16 "Net-(J2-Pin_17)")
	(net 17 "Net-(J2-Pin_14)")
	(net 18 "Net-(J2-Pin_13)")
	(net 19 "Net-(J2-Pin_16)")
	(net 20 "Net-(J2-Pin_24)")
	(net 21 "Net-(J2-Pin_21)")
	(net 22 "Net-(J2-Pin_19)")
	(net 23 "Net-(J2-Pin_5)")
	(net 24 "Net-(J2-Pin_11)")
	(net 25 "Net-(J2-Pin_4)")
	(net 26 "Net-(J3-Pin_11)")
	(net 27 "Net-(J3-Pin_1)")
	(net 28 "Net-(J3-Pin_19)")
	(net 29 "Net-(J3-Pin_14)")
	(net 30 "Net-(J3-Pin_13)")
	(net 31 "Net-(J3-Pin_2)")
	(net 32 "Net-(J3-Pin_17)")
	(net 33 "Net-(J3-Pin_8)")
	(net 34 "Net-(J3-Pin_10)")
	(net 35 "Net-(J3-Pin_18)")
	(net 36 "Net-(J3-Pin_15)")
	(net 37 "Net-(J3-Pin_7)")
	(net 38 "Net-(J3-Pin_5)")
	(net 39 "Net-(J3-Pin_22)")
	(net 40 "Net-(J3-Pin_6)")
	(net 41 "Net-(J3-Pin_25)")
	(net 42 "Net-(J3-Pin_4)")
	(net 43 "Net-(J3-Pin_16)")
	(net 44 "Net-(J3-Pin_24)")
	(net 45 "Net-(J3-Pin_9)")
	(net 46 "Net-(J3-Pin_12)")
	(net 47 "Net-(J3-Pin_3)")
	(net 48 "Net-(J3-Pin_20)")
	(net 49 "Net-(J3-Pin_23)")
	(net 50 "Net-(J3-Pin_21)")
	(net 51 "Net-(J1-GND)")
	(net 52 "Net-(J1-GND__2)")
	(footprint "Benderlabs_Custom:SAMTEC_QTS-025-01-X-D-A-TR"
		(layer "F.Cu")
		(at 140.792501 96.025 -90)
		(property "Reference" "J1"
			(at -11.13 -0.01 180)
			(layer "F.SilkS")
		)
		(property "Value" "QTS-025-01-XXX-D"
			(at 9.71 4.865 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "C"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "4.347mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samtec"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Xineos1511LVDS-DebugHeader.kicad_sch")
		(attr smd)
		(pad "" np_thru_hole circle
			(at -9.24 -2.032 270)
			(size 1.016 1.016)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 9.24 -2.032 270)
			(size 1.016 1.016)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
		)
		(pad "01" smd rect
			(at -7.62 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(J3-Pin_1)")
			(pinfunction "01")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "02" smd rect
			(at -7.62 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J2-Pin_1)")
			(pinfunction "02")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "03" smd rect
			(at -6.985 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(J3-Pin_2)")
			(pinfunction "03")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "04" smd rect
			(at -6.985 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(J2-Pin_2)")
			(pinfunction "04")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "05" smd rect
			(at -6.35 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "Net-(J3-Pin_3)")
			(pinfunction "05")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "06" smd rect
			(at -6.35 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(J2-Pin_3)")
			(pinfunction "06")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "07" smd rect
			(at -5.715 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(J3-Pin_4)")
			(pinfunction "07")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "08" smd rect
			(at -5.715 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(J2-Pin_4)")
			(pinfunction "08")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "09" smd rect
			(at -5.08 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "Net-(J3-Pin_5)")
			(pinfunction "09")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at -5.08 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(J2-Pin_5)")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at -4.445 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Net-(J3-Pin_6)")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at -4.445 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(J2-Pin_6)")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at -3.81 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(J3-Pin_7)")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at -3.81 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(J2-Pin_7)")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at -3.175 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(J3-Pin_8)")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at -3.175 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(J2-Pin_8)")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at -2.54 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "Net-(J3-Pin_9)")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at -2.54 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(J2-Pin_9)")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd rect
			(at -1.905 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(J3-Pin_10)")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd rect
			(at -1.905 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(J2-Pin_10)")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd rect
			(at -1.27 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(J3-Pin_11)")
			(pinfunction "21")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd rect
			(at -1.27 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(J2-Pin_11)")
			(pinfunction "22")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd rect
			(at -0.635 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(J3-Pin_12)")
			(pinfunction "23")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd rect
			(at -0.635 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(J2-Pin_12)")
			(pinfunction "24")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "25" smd rect
			(at 0 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(J3-Pin_13)")
			(pinfunction "25")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "26" smd rect
			(at 0 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(J2-Pin_13)")
			(pinfunction "26")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "27" smd rect
			(at 0.635 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(J3-Pin_14)")
			(pinfunction "27")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "28" smd rect
			(at 0.635 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(J2-Pin_14)")
			(pinfunction "28")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "29" smd rect
			(at 1.27 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(J3-Pin_15)")
			(pinfunction "29")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "30" smd rect
			(at 1.27 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J2-Pin_15)")
			(pinfunction "30")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "31" smd rect
			(at 1.905 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(J3-Pin_16)")
			(pinfunction "31")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "32" smd rect
			(at 1.905 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(J2-Pin_16)")
			(pinfunction "32")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "33" smd rect
			(at 2.54 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "Net-(J3-Pin_17)")
			(pinfunction "33")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "34" smd rect
			(at 2.54 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(J2-Pin_17)")
			(pinfunction "34")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "35" smd rect
			(at 3.175 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(J3-Pin_18)")
			(pinfunction "35")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "36" smd rect
			(at 3.175 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(J2-Pin_18)")
			(pinfunction "36")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "37" smd rect
			(at 3.81 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(J3-Pin_19)")
			(pinfunction "37")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "38" smd rect
			(at 3.81 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(J2-Pin_19)")
			(pinfunction "38")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "39" smd rect
			(at 4.445 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "Net-(J3-Pin_20)")
			(pinfunction "39")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "40" smd rect
			(at 4.445 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(J2-Pin_20)")
			(pinfunction "40")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "41" smd rect
			(at 5.08 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "Net-(J3-Pin_21)")
			(pinfunction "41")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "42" smd rect
			(at 5.08 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(J2-Pin_21)")
			(pinfunction "42")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "43" smd rect
			(at 5.715 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(J3-Pin_22)")
			(pinfunction "43")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "44" smd rect
			(at 5.715 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(J2-Pin_22)")
			(pinfunction "44")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "45" smd rect
			(at 6.35 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(J3-Pin_23)")
			(pinfunction "45")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "46" smd rect
			(at 6.35 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(J2-Pin_23)")
			(pinfunction "46")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "47" smd rect
			(at 6.985 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(J3-Pin_24)")
			(pinfunction "47")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "48" smd rect
			(at 6.985 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(J2-Pin_24)")
			(pinfunction "48")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "49" smd rect
			(at 7.62 -3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "Net-(J3-Pin_25)")
			(pinfunction "49")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "50" smd rect
			(at 7.62 3.086 270)
			(size 0.406 1.448)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(J2-Pin_25)")
			(pinfunction "50")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "G1" smd rect
			(at -8.446 0 270)
			(size 2.54 0.635)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(J1-GND)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G2" smd rect
			(at -3.175 0 270)
			(size 4.699 0.635)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(J1-GND)")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G3" smd rect
			(at 3.175 0 270)
			(size 4.699 0.635)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(J1-GND__2)")
			(pinfunction "GND__2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G4" smd rect
			(at 8.446 0 270)
			(size 2.54 0.635)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(J1-GND__2)")
			(pinfunction "GND__3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3D_Models/QTS-025-01-F-D-A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(footprint "Benderlabs_Custom:7824c5a4_logo_15x4.5mm"
		(layer "B.Cu")
		(at 140.792501 93.265 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 140.792501 72.025)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J4"
			(at 0 2.33 180)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 0 -2.33 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Xineos1511LVDS-DebugHeader.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J1-GND)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 140.792501 120.025)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.33 180)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 0 -2.33 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Xineos1511LVDS-DebugHeader.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J1-GND__2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x25_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 121.5325 65.55 180)
		(descr "Through hole straight pin header, 1x25, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x25 2.54mm single row")
		(property "Reference" "J2"
			(at 0 2.33 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x25"
			(at 0 -63.29 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x25, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Xineos1511LVDS-DebugHeader.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.000001 -30.480002 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -0.000004 -5.079999 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0.000001 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -0.000005 -12.700001 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at -0.000002 -17.780003 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0.000001 -20.320005 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J2-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0.000007 -22.859999 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J2-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J2-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at -0.000001 -30.480002 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J2-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 -33.020002 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J2-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J2-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J2-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 0.000001 -43.180001 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_18)")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0.000003 -45.719997 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pin_19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_20)")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 -50.8 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_21)")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at -0.000006 -53.34 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_22)")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 0 -55.879999 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J2-Pin_23)")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 0 -58.42 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J2-Pin_24)")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 0 -60.96 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J2-Pin_25)")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x25_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x25_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 160.049999 65.550001 180)
		(descr "Through hole straight pin header, 1x25, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x25 2.54mm single row")
		(property "Reference" "J3"
			(at 0 2.33 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x25"
			(at 0 -63.29 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x25, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Xineos1511LVDS-DebugHeader.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.000001 -30.480002 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -0.000004 -5.079999 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0.000001 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -0.000005 -12.700001 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J3-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J3-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at -0.000002 -17.780003 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J3-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0.000001 -20.320005 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J3-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0.000007 -22.859999 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J3-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J3-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J3-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at -0.000001 -30.480002 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J3-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 -33.020002 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J3-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J3-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J3-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J3-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 0.000001 -43.180001 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J3-Pin_18)")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0.000003 -45.719997 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J3-Pin_19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J3-Pin_20)")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 -50.8 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J3-Pin_21)")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at -0.000006 -53.34 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J3-Pin_22)")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 0 -55.879999 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J3-Pin_23)")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 0 -58.42 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J3-Pin_24)")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 0 -60.96 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J3-Pin_25)")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x25_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 166.192501 127.774998)
		(mid 165.262563 130.020062)
		(end 163.017498 130.949998)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.567499 61.099998)
		(end 163.017501 61.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.192498 64.274999)
		(end 166.192501 127.774998)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.3925 127.775001)
		(end 115.392498 64.274999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.392498 64.274999)
		(mid 116.322441 62.029934)
		(end 118.567499 61.099998)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.567497 130.950002)
		(mid 116.322435 130.020064)
		(end 115.3925 127.775001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.017498 130.949998)
		(end 118.567497 130.950002)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 163.017501 61.1)
		(mid 165.262564 62.029936)
		(end 166.192498 64.274999)
		(layer "Edge.Cuts")
	)
	(gr_text "50"
		(at 136.492501 106.025 0)
		(layer "F.SilkS")
	)
	(gr_text "49"
		(at 145.092501 106.025 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 136.492501 86.025 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 145.092501 86.025 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 157.062501 65.545 0)
		(layer "B.SilkS")
	)
	(gr_text "37"
		(at 157.062505 111.264997 0)
		(layer "B.SilkS")
	)
	(gr_text "42"
		(at 124.522504 116.354999 0)
		(layer "B.SilkS")
	)
	(gr_text "36"
		(at 124.522503 108.734999 0)
		(layer "B.SilkS")
	)
	(gr_text "35"
		(at 157.062503 108.724999 0)
		(layer "B.SilkS")
	)
	(gr_text "24"
		(at 124.522503 93.494999 0)
		(layer "B.SilkS")
	)
	(gr_text "6"
		(at 124.522502 70.634999 0)
		(layer "B.SilkS")
	)
	(gr_text "29"
		(at 157.062503 101.104999 0)
		(layer "B.SilkS")
	)
	(gr_text "43"
		(at 157.0625 118.885 0)
		(layer "B.SilkS")
	)
	(gr_text "46"
		(at 124.522501 121.435 0)
		(layer "B.SilkS")
	)
	(gr_text "8"
		(at 124.522502 73.175001 0)
		(layer "B.SilkS")
	)
	(gr_text "22"
		(at 124.522505 90.955002 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 140.792501 122.525 0)
		(layer "B.SilkS")
	)
	(gr_text "QTS-025-01-XXX-D\nBreakout Board"
		(at 140.792501 97.935 0)
		(layer "B.SilkS")
	)
	(gr_text "34"
		(at 124.522505 106.194999 0)
		(layer "B.SilkS")
	)
	(gr_text "40"
		(at 124.522502 113.814999 0)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 157.062502 70.624999 0)
		(layer "B.SilkS")
	)
	(gr_text "7"
		(at 157.062502 73.165001 0)
		(layer "B.SilkS")
	)
	(gr_text "12"
		(at 124.522498 78.255001 0)
		(layer "B.SilkS")
	)
	(gr_text "18"
		(at 124.522504 85.875004 0)
		(layer "B.SilkS")
	)
	(gr_text "2"
		(at 124.522501 65.555 0)
		(layer "B.SilkS")
	)
	(gr_text "17"
		(at 157.062504 85.865004 0)
		(layer "B.SilkS")
	)
	(gr_text "44"
		(at 124.5225 118.895 0)
		(layer "B.SilkS")
	)
	(gr_text "48"
		(at 124.522505 123.975001 0)
		(layer "B.SilkS")
	)
	(gr_text "16"
		(at 124.522502 83.335002 0)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 157.062501 68.085002 0)
		(layer "B.SilkS")
	)
	(gr_text "11"
		(at 157.062498 78.245001 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 140.792501 69.525 0)
		(layer "B.SilkS")
	)
	(gr_text "13"
		(at 157.062505 80.785001 0)
		(layer "B.SilkS")
	)
	(gr_text "9"
		(at 157.062504 75.705001 0)
		(layer "B.SilkS")
	)
	(gr_text "33"
		(at 157.062505 106.184999 0)
		(layer "B.SilkS")
	)
	(gr_text "39"
		(at 157.062502 113.804999 0)
		(layer "B.SilkS")
	)
	(gr_text "47"
		(at 157.062505 123.965001 0)
		(layer "B.SilkS")
	)
	(gr_text "41"
		(at 157.062504 116.344999 0)
		(layer "B.SilkS")
	)
	(gr_text "21"
		(at 157.062505 90.945002 0)
		(layer "B.SilkS")
	)
	(gr_text "15\n"
		(at 157.062502 83.325002 0)
		(layer "B.SilkS")
	)
	(gr_text "25"
		(at 157.062504 96.025001 0)
		(layer "B.SilkS")
	)
	(gr_text "20"
		(at 124.522512 88.415 0)
		(layer "B.SilkS")
	)
	(gr_text "27"
		(at 157.062504 98.565002 0)
		(layer "B.SilkS")
	)
	(gr_text "4"
		(at 124.522501 68.095002 0)
		(layer "B.SilkS")
	)
	(gr_text "26"
		(at 124.522504 96.035001 0)
		(layer "B.SilkS")
	)
	(gr_text "14"
		(at 124.522505 80.795001 0)
		(layer "B.SilkS")
	)
	(gr_text "10"
		(at 124.522504 75.715001 0)
		(layer "B.SilkS")
	)
	(gr_text "31"
		(at 157.062502 103.645003 0)
		(layer "B.SilkS")
	)
	(gr_text "32"
		(at 124.522502 103.655003 0)
		(layer "B.SilkS")
	)
	(gr_text "38"
		(at 124.522505 111.274997 0)
		(layer "B.SilkS")
	)
	(gr_text "23\n"
		(at 157.062503 93.484999 0)
		(layer "B.SilkS")
	)
	(gr_text "30"
		(at 124.522503 101.114999 0)
		(layer "B.SilkS")
	)
	(gr_text "19"
		(at 157.062512 88.405 0)
		(layer "B.SilkS")
	)
	(gr_text "45"
		(at 157.062501 121.425 0)
		(layer "B.SilkS")
	)
	(gr_text "49"
		(at 157.062501 126.505 0)
		(layer "B.SilkS")
	)
	(gr_text "28"
		(at 124.522504 98.575002 0)
		(layer "B.SilkS")
	)
	(gr_text "50"
		(at 124.522501 126.515 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
