(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 14)
    (no_connects 3)
    (area 137.694999 101.880999 186.155001 134.085001)
    (thickness 1.6)
    (drawings 22)
    (tracks 47)
    (zones 0)
    (modules 8)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.5588)
    (user_trace_width 0.8128)
    (user_trace_width 1.2192)
    (user_trace_width 1.6256)
    (user_trace_width 2)
    (user_trace_width 2.54)
    (trace_clearance 0.2032)
    (zone_clearance 2.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.7366)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.9906 0.5842)
    (user_via 1.2446 0.8382)
    (user_via 1.4986 1.0922)
    (user_via 1.7526 1.3462)
    (user_via 2.0066 1.6002)
    (uvia_size 0.7366)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 1.19888)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(D1-Pad2)")
  (net 3 L_Wall)
  (net 4 "Net-(K1-Pad14)")
  (net 5 relay_on)
  (net 6 GND)
  (net 7 N_Wall)
  (net 8 L_Printer)
  (net 9 N_Printer)
  (net 10 "Net-(K1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.7366)
    (via_drill 0.3302)
    (uvia_dia 0.7366)
    (uvia_drill 0.3302)
    (add_net +5V)
    (add_net GND)
    (add_net L_Printer)
    (add_net L_Wall)
    (add_net N_Printer)
    (add_net N_Wall)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(K1-Pad14)")
    (add_net "Net-(K1-Pad3)")
    (add_net relay_on)
  )
  (module Relays_ThroughHole:Relay_DPDT_Schrack-RT2_RM5mm (layer F.Cu) (tedit 57D996A1)
    (at 145.415 121.285)
    (descr "Relay, DPST, Schrack-RT2, RM5mm,")
    (tags "Relay, DPST,  Schrack-RT1, RM5mm, Reais, 2 x um,")
    (fp_text reference K1 (at 13.97 -11.43) (layer F.SilkS))
    (fp_text value RELAY_2RT (at 12.7 5.08) (layer F.Fab))
    (pad 8 thru_hole circle (at 0 -7.62) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 9 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 15.24 0) (size 2.2 2.2) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(K1-Pad3)"))
    (pad 5 thru_hole circle (at 20.32 0) (size 2.2 2.2) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 7 N_Wall))
    (pad 1 thru_hole circle (at 25.4 0) (size 2.2 2.2) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 9 N_Printer))
    (pad 14 thru_hole circle (at 15.24 -7.62) (size 2.2 2.2) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(K1-Pad14)"))
    (pad 12 thru_hole circle (at 20.32 -7.62) (size 2.2 2.2) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 3 L_Wall))
    (pad 16 thru_hole circle (at 25.4 -7.62) (size 2.2 2.2) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 8 L_Printer))
  )
  (module Connect:AK300-2 (layer F.Cu) (tedit 54792136)
    (at 181.483 120.523 90)
    (descr CONNECTOR)
    (tags CONNECTOR)
    (attr virtual)
    (fp_text reference P3 (at -2.032 -7.112 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.779 7.747 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 9 N_Printer))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 8 L_Printer))
  )
  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 552FF239)
    (at 140.462 106.426 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value D_Small (at 0 4.3 90) (layer F.Fab))
    (fp_text user K (at -2.9 2.95 90) (layer F.SilkS))
    (fp_text user A (at 2.9 2.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 140.843 114.935)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -1.016 -2.413) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 relay_on))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 148.082 125.603 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.651 -2.3368 360) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 relay_on))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5418A00F)
    (at 140.716 122.809)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.6002) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 relay_on))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:AK300-2 (layer F.Cu) (tedit 54792136)
    (at 181.483 131.953 90)
    (descr CONNECTOR)
    (tags CONNECTOR)
    (attr virtual)
    (fp_text reference P2 (at 0 -7.366 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.779 7.747 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 7 N_Wall))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 7 N_Wall))
  )
  (module Connect:AK300-2 (layer F.Cu) (tedit 54792136)
    (at 181.483 109.093 90)
    (descr CONNECTOR)
    (tags CONNECTOR)
    (attr virtual)
    (fp_text reference P4 (at -2.032 -7.112 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.779 7.747 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 3 L_Wall))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 3 L_Wall))
  )
  (gr_circle (center 141.6012 130.1788) (end 140.0012 130.1788) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.795 101.981) (end 137.795 133.985) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 147.24 106.633) (end 145.64 106.633) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.94 116.205) (end 154.94 109.855) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 186.055 101.981) (end 137.795 101.981) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 186.055 133.985) (end 186.055 101.981) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.795 133.985) (end 186.055 133.985) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.94 118.745) (end 154.94 125.095) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 152.4 125.095) (end 152.4 109.855) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 153.67 125.095) (end 154.94 125.095) (angle 180) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 153.67 109.855) (end 152.4 109.855) (angle 180) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 172.085 117.475) (end 172.085 116.205) (angle 180) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.94 118.745) (end 172.085 118.745) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 172.085 116.205) (end 154.94 116.205) (layer Edge.Cuts) (width 0.2))
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.795 101.981) (xy 152.4 101.981) (xy 152.4 133.985) (xy 137.795 133.985)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.795 101.981) (xy 152.4 101.981) (xy 152.4 133.985) (xy 137.795 133.985)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 104.648) (xy 144.653 103.886) (xy 145.415 103.378) (xy 146.939 102.87) (xy 148.717 103.251)
        (xy 149.987 104.14) (xy 150.876 105.537) (xy 150.876 107.188) (xy 150.495 108.585) (xy 148.971 109.982)
        (xy 147.701 110.236) (xy 146.431 110.236) (xy 145.669 109.982) (xy 144.907 109.474) (xy 144.399 108.966)
        (xy 143.891 108.204) (xy 143.637 107.188) (xy 143.637 105.918)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 104.648) (xy 144.653 103.886) (xy 145.415 103.378) (xy 146.939 102.87) (xy 148.717 103.251)
        (xy 149.987 104.14) (xy 150.876 105.537) (xy 150.876 107.188) (xy 150.495 108.585) (xy 148.971 109.982)
        (xy 147.701 110.236) (xy 146.431 110.236) (xy 145.669 109.982) (xy 144.907 109.474) (xy 144.399 108.966)
        (xy 143.891 108.204) (xy 143.637 107.188) (xy 143.637 105.918)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 104.648) (xy 144.653 103.886) (xy 145.415 103.378) (xy 146.939 102.87) (xy 148.717 103.251)
        (xy 149.987 104.14) (xy 150.876 105.537) (xy 150.876 107.188) (xy 150.495 108.585) (xy 148.971 109.982)
        (xy 147.701 110.236) (xy 146.431 110.236) (xy 145.669 109.982) (xy 144.907 109.474) (xy 144.399 108.966)
        (xy 143.891 108.204) (xy 143.637 107.188) (xy 143.637 105.918)
      )
    )
  )
  (zone (net 7) (net_name N_Wall) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.211 121.158) (xy 164.211 133.985) (xy 186.055 133.985) (xy 186.055 124.079) (xy 169.926 124.079)
        (xy 167.259 121.158) (xy 167.132 120.65) (xy 166.878 120.269) (xy 166.37 119.888) (xy 165.862 119.761)
        (xy 165.481 119.761) (xy 165.1 119.888) (xy 164.719 120.142) (xy 164.465 120.396) (xy 164.211 120.777)
      )
    )
  )
  (zone (net 7) (net_name N_Wall) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.211 121.158) (xy 164.211 133.985) (xy 186.055 133.985) (xy 186.055 124.079) (xy 169.926 124.079)
        (xy 167.259 121.158) (xy 167.132 120.65) (xy 166.878 120.269) (xy 166.37 119.888) (xy 165.862 119.761)
        (xy 165.481 119.761) (xy 165.1 119.888) (xy 164.719 120.142) (xy 164.465 120.396) (xy 164.211 120.777)
      )
    )
  )
  (zone (net 9) (net_name N_Printer) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.055 124.079) (xy 186.055 119.507) (xy 169.418 119.507) (xy 169.418 123.5202) (xy 169.926 124.079)
      )
    )
  )
  (zone (net 9) (net_name N_Printer) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.055 124.079) (xy 186.055 119.507) (xy 169.418 119.507) (xy 169.418 123.5202) (xy 169.926 124.079)
      )
    )
  )
  (zone (net 3) (net_name L_Wall) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.211 113.792) (xy 164.211 101.981) (xy 186.055 101.981) (xy 186.055 110.871) (xy 169.926 110.871)
        (xy 167.259 113.792) (xy 167.132 114.3) (xy 166.878 114.681) (xy 166.37 115.062) (xy 165.862 115.189)
        (xy 165.481 115.189) (xy 165.1 115.062) (xy 164.719 114.808) (xy 164.465 114.554) (xy 164.211 114.173)
      )
    )
  )
  (zone (net 3) (net_name L_Wall) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.211 113.792) (xy 164.211 101.981) (xy 186.055 101.981) (xy 186.055 110.871) (xy 169.926 110.871)
        (xy 167.259 113.792) (xy 167.132 114.3) (xy 166.878 114.681) (xy 166.37 115.062) (xy 165.862 115.189)
        (xy 165.481 115.189) (xy 165.1 115.062) (xy 164.719 114.808) (xy 164.465 114.554) (xy 164.211 114.173)
      )
    )
  )
  (zone (net 8) (net_name L_Printer) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.055 110.871) (xy 186.055 116.459) (xy 169.418 116.459) (xy 169.418 111.4298) (xy 169.926 110.871)
      )
    )
  )
  (zone (net 8) (net_name L_Printer) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.055 110.871) (xy 186.055 116.459) (xy 169.418 116.459) (xy 169.418 111.4298) (xy 169.926 110.871)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.5062 128.1938) (xy 139.0142 127.4318) (xy 139.7762 126.9238) (xy 141.3002 126.4158) (xy 143.0782 126.7968)
        (xy 144.3482 127.6858) (xy 145.2372 129.0828) (xy 145.2372 130.7338) (xy 144.8562 132.1308) (xy 143.3322 133.5278)
        (xy 142.0622 133.7818) (xy 140.7922 133.7818) (xy 140.0302 133.5278) (xy 139.2682 133.0198) (xy 138.7602 132.5118)
        (xy 138.2522 131.7498) (xy 137.9982 130.7338) (xy 137.9982 129.4638)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.5062 128.1938) (xy 139.0142 127.4318) (xy 139.7762 126.9238) (xy 141.3002 126.4158) (xy 143.0782 126.7968)
        (xy 144.3482 127.6858) (xy 145.2372 129.0828) (xy 145.2372 130.7338) (xy 144.8562 132.1308) (xy 143.3322 133.5278)
        (xy 142.0622 133.7818) (xy 140.7922 133.7818) (xy 140.0302 133.5278) (xy 139.2682 133.0198) (xy 138.7602 132.5118)
        (xy 138.2522 131.7498) (xy 137.9982 130.7338) (xy 137.9982 129.4638)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.5062 128.1938) (xy 139.0142 127.4318) (xy 139.7762 126.9238) (xy 141.3002 126.4158) (xy 143.0782 126.7968)
        (xy 144.3482 127.6858) (xy 145.2372 129.0828) (xy 145.2372 130.7338) (xy 144.8562 132.1308) (xy 143.3322 133.5278)
        (xy 142.0622 133.7818) (xy 140.7922 133.7818) (xy 140.0302 133.5278) (xy 139.2682 133.0198) (xy 138.7602 132.5118)
        (xy 138.2522 131.7498) (xy 137.9982 130.7338) (xy 137.9982 129.4638)
      )
    )
  )
)
