(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 63)
    (zones 0)
    (modules 10)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad5)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J6-Pad1)")
  (net 6 "Net-(J7-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
  )
  (module Connector_USB:USB_Micro-B_Amphenol_10103594-0001LF_Horizontal (layer F.Cu) (tedit 5A1DC0BD)
    (at 22.733 50.673 270)
    (descr "Micro USB Type B 10103594-0001LF, http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10103594.pdf")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 6.223 0.381 270) (layer F.SilkS))
    (fp_text value USB_B_Micro (at -0.025 4.435 270) (layer F.Fab))
    (fp_text user "PCB edge" (at -0.025 2.235 270) (layer Dwgs.User))
    (fp_text user %R (at -0.025 -0.015 90) (layer F.Fab))
    (pad 6 smd rect (at 2.725 0.185 270) (size 1.35 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -2.755 0.185 270) (size 1.35 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -2.975 -0.565 270) (size 1.825 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 2.975 -0.565 270) (size 1.825 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -2.875 -1.865 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 2.875 -1.885 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 1 smd rect (at -1.325 -1.765) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -0.675 -1.765) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -0.025 -1.765) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.625 -1.765) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.275 -1.765) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at -2.445 -1.885) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.395 -1.885) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at -2.755 1.115) (size 1.7 1.35) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.705 1.115) (size 1.7 1.35) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -0.985 1.385) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 0.935 1.385) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10103594-0001LF_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC (layer F.Cu) (tedit 5A02FC95)
    (at 62.907 47.84)
    (descr http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf)
    (tags "SMD SMT SPST EVQPUL EVQPUC")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.625 0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J6-Pad1)"))
    (pad 2 smd rect (at -2.625 0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J6-Pad1)"))
    (pad 1 smd rect (at -2.625 -0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 1 smd rect (at 2.625 -0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad "" np_thru_hole circle (at 0 1.375 180) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -1.375 180) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUL_EVQPUC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC (layer F.Cu) (tedit 5A02FC95)
    (at 29.972 47.879)
    (descr http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf)
    (tags "SMD SMT SPST EVQPUL EVQPUC")
    (attr smd)
    (fp_text reference SW2 (at 0 -4.5) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -1.375 180) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 1.375 180) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 2.625 -0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 1 smd rect (at -2.625 -0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at -2.625 0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J7-Pad1)"))
    (pad 2 smd rect (at 2.625 0.85 180) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUL_EVQPUC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_3.0x3.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 27.432 53.848 90)
    (descr "SMD rectangular pad as test Point, square 3.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J2 (at -4.064 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.4 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3 3) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad5)"))
  )
  (module TestPoint:TestPoint_Pad_3.0x3.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 35.56 53.848)
    (descr "SMD rectangular pad as test Point, square 3.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J3 (at 0 4.064) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_3.0x3.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 31.496 53.848)
    (descr "SMD rectangular pad as test Point, square 3.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J4 (at 0 4.064) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Mask)
      (net 4 "Net-(J1-Pad3)"))
  )
  (module TestPoint:TestPoint_Pad_3.0x3.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 39.624 53.848)
    (descr "SMD rectangular pad as test Point, square 3.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J5 (at 0 4.064) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_3.0x3.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 54.864 53.848)
    (descr "SMD rectangular pad as test Point, square 3.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J6 (at 0 4.064) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Mask)
      (net 5 "Net-(J6-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_3.0x3.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 50.8 53.848)
    (descr "SMD rectangular pad as test Point, square 3.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J7 (at 0 4.064) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Mask)
      (net 6 "Net-(J7-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 56D1B4CB)
    (at 43.18 50.8)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "Designed by\nFredrik Hubinette" (at 55.372 52.324) (layer B.SilkS))
  (gr_text VBUS (at 39.624 49.276 90) (layer F.SilkS))
  (gr_text D+ (at 35.56 51.308) (layer F.SilkS))
  (gr_text D- (at 31.496 51.308) (layer F.SilkS))
  (gr_text GND (at 27.432 51.308) (layer F.SilkS))
  (gr_text "Buttons\n" (at 52.324 50.292) (layer F.SilkS))
  (gr_line (start 68.834 45.974) (end 20.066 45.974) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.834 55.626) (end 68.834 45.974) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.066 55.626) (end 68.834 55.626) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.066 45.974) (end 20.066 55.626) (layer Edge.Cuts) (width 0.15))
)
