(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 9)
    (no_connects 0)
    (area 93.904999 108.509999 146.760001 166.445001)
    (thickness 1.6)
    (drawings 10)
    (tracks 24)
    (zones 0)
    (modules 5)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (trace_clearance 0.5)
    (zone_clearance 2.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 4.5)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 104.775 133.985)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 "Net-(D1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
  )
  (net_class Power ""
    (clearance 1)
    (trace_width 4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net VCC)
  )
  (module TO_SOT_Packages_THT:TO-247-2_Vertical (layer F.Cu) (tedit 58A217F2)
    (at 132.08 126.365)
    (descr "TO-247-2, Vertical, RM 10.9mm")
    (tags "TO-247-2 Vertical RM 10.9mm")
    (fp_text reference D1 (at 5.45 -3.45) (layer F.SilkS))
    (fp_text value D (at 5.45 6.07) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-247-2_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-247-2_Vertical (layer F.Cu) (tedit 58A217F2)
    (at 142.875 148.59 180)
    (descr "TO-247-2, Vertical, RM 10.9mm")
    (tags "TO-247-2 Vertical RM 10.9mm")
    (fp_text reference D2 (at 5.45 -3.45 180) (layer F.SilkS))
    (fp_text value D (at 5.45 6.07 180) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.45 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 10.9 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-247-2_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer F.Cu) (tedit 58A217F2)
    (at 114.3 126.365)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (fp_text reference Q1 (at 5.45 -3.45) (layer F.SilkS))
    (fp_text value Q_NIGBT_GCE (at 5.45 6.07) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 2 thru_hole oval (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer F.Cu) (tedit 58A217F2)
    (at 125.095 148.59 180)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (fp_text reference Q2 (at 5.45 -3.45 180) (layer F.SilkS))
    (fp_text value Q_NIGBT_GCE (at 5.45 6.07 180) (layer F.Fab))
    (fp_text user %R (at 5.45 -3.45 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 5.45 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 10.9 0 180) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 104.775 141.605 180)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 4.315 -2.27 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 4.315 9.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 93.98 168.275) (end 93.98 166.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.98 106.68) (end 93.98 108.585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 106.68) (end 146.685 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 108.585) (end 148.59 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 168.275) (end 148.59 166.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.685 168.275) (end 148.59 168.275) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.98 166.37) (end 93.98 108.585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.685 168.275) (end 93.98 168.275) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 108.585) (end 148.59 166.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.98 106.68) (end 146.685 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(D1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.125 130.175) (xy 146.05 130.175) (xy 146.05 145.415) (xy 111.125 145.415)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.125 123.19) (xy 146.05 123.19) (xy 146.05 109.22) (xy 111.125 109.22)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.125 151.765) (xy 111.125 165.735) (xy 146.05 165.735) (xy 146.05 151.765)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 2.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.125 109.22) (xy 146.05 109.22) (xy 146.05 165.735) (xy 111.125 165.735)
      )
    )
  )
)
