<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.0">
<drawing>
<board>
<plain>
<hole x="33.1" y="40" drill="2.4"/>
<hole x="69.5" y="39.75" drill="2.4"/>
<hole x="51.5" y="22" drill="2.4"/>
<wire x1="63" y1="37" x2="63" y2="30" width="0.1524" layer="20"/>
<wire x1="63" y1="30" x2="52" y2="19" width="0.1524" layer="20" curve="-90"/>
<wire x1="40" y1="37" x2="40" y2="30" width="0.1524" layer="20"/>
<wire x1="40" y1="30" x2="51" y2="19" width="0.1524" layer="20" curve="90"/>
<wire x1="51" y1="19" x2="52" y2="19" width="0.1524" layer="20"/>
<wire x1="40" y1="50" x2="51" y2="61" width="0.1524" layer="20" curve="-90"/>
<wire x1="51" y1="61" x2="53" y2="61" width="0.1524" layer="20"/>
<wire x1="40" y1="43" x2="31" y2="43" width="0.1524" layer="20"/>
<wire x1="40" y1="37" x2="31" y2="37" width="0.1524" layer="20"/>
<wire x1="72" y1="43" x2="63" y2="43" width="0.1524" layer="20"/>
<wire x1="40" y1="50" x2="40" y2="43" width="0.1524" layer="20"/>
<wire x1="72" y1="37" x2="63" y2="37" width="0.1524" layer="20"/>
<wire x1="53" y1="61" x2="63" y2="51" width="0.1524" layer="20" curve="-90"/>
<wire x1="63" y1="51" x2="63" y2="43" width="0.1524" layer="20"/>
<wire x1="31" y1="43" x2="30" y2="42" width="0.1524" layer="20" curve="90"/>
<wire x1="31" y1="37" x2="30" y2="38" width="0.1524" layer="20" curve="-90"/>
<wire x1="30" y1="38" x2="30" y2="42" width="0.1524" layer="20"/>
<wire x1="72" y1="43" x2="73" y2="42" width="0.1524" layer="20" curve="-90"/>
<wire x1="72" y1="37" x2="73" y2="38" width="0.1524" layer="20" curve="90"/>
<wire x1="73" y1="38" x2="73" y2="42" width="0.1524" layer="20"/>
<hole x="51.75" y="58" drill="2.4"/>
<text>ESC</text>
<text>5VREG</text>
<text>G</text>
<text>SCL</text>
<text>SDA</text>
<text>5V</text>
<text>VB</text>
<text>G</text>
<text>SDA</text>
<text>SCL</text>
<text>M4</text>
<text>M3</text>
<text>M2</text>
<text>M1</text>
<text>3V3</text>
<text>5V</text>
<text>G</text>
<text>G</text>
<text>3V3</text>
<text>G</text>
<text>M1</text>
<text>M2</text>
<text>M3</text>
<text>M4</text>
<text>G</text>
<text>3V3</text>
<text>SCL</text>
<text>SDA</text>
<text>SDA</text>
<text>SCL</text>
<text>3V3</text>
<text>5V</text>
<text>G</text>
<text>VB</text>
<text>G</text>
<text>5V</text>
<text>V</text>
<text>G</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>USFS</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -10 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-6-SMD-HORI-1.0MM">
<description>&lt;h3&gt;JST SH Vertical 6-Pin SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 1 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;JST_6PIN_VERTICAL&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TP1" library="SparkFun-Connectors" package="1X10_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="TP2" library="SparkFun-Connectors" package="1X10_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VREG" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="USFS" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="ESC" library="SparkFun-Connectors" package="JST-6-SMD-HORI-1.0MM" value="BM06B-SRSS-TB">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="TP1" pad="2"/>
<contactref element="TP2" pad="10"/>
<contactref element="5VREG" pad="2"/>
<contactref element="USFS" pad="5"/>
<contactref element="ESC" pad="5"/>
</signal>
<signal name="5V">
<contactref element="TP1" pad="3"/>
<contactref element="5VREG" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="TP1" pad="4"/>
<contactref element="USFS" pad="4"/>
</signal>
<signal name="M3">
<contactref element="TP1" pad="8"/>
<contactref element="ESC" pad="2"/>
</signal>
<signal name="M2">
<contactref element="TP1" pad="9"/>
<contactref element="ESC" pad="3"/>
</signal>
<signal name="M1">
<contactref element="TP1" pad="10"/>
<contactref element="ESC" pad="4"/>
</signal>
<signal name="VBAT">
<contactref element="5VREG" pad="3"/>
<contactref element="ESC" pad="6"/>
</signal>
<signal name="M4">
<contactref element="TP1" pad="7"/>
<contactref element="ESC" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="USFS" pad="1"/>
<contactref element="TP2" pad="6"/>
</signal>
<signal name="SCL">
<contactref element="USFS" pad="2"/>
<contactref element="TP2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
