(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 43)
    (zones 0)
    (modules 5)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.1 3.1)
    (pad_drill 5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-PadTN4)")
  (net 2 "Net-(J1-PadRN3)")
  (net 3 "Net-(J1-PadR2)")
  (net 4 "Net-(J1-PadR22)")
  (net 5 "Net-(J1-PadTN24)")
  (net 6 "Net-(J1-PadRN23)")
  (net 7 "Net-(J2-PadRN23)")
  (net 8 "Net-(J2-PadTN24)")
  (net 9 "Net-(J2-PadR2)")
  (net 10 "Net-(J2-PadRN3)")
  (net 11 "Net-(J2-PadTN4)")
  (net 12 "Net-(J2-PadR22)")
  (net 13 +3V3)
  (net 14 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(J1-PadR2)")
    (add_net "Net-(J1-PadR22)")
    (add_net "Net-(J1-PadRN23)")
    (add_net "Net-(J1-PadRN3)")
    (add_net "Net-(J1-PadTN24)")
    (add_net "Net-(J1-PadTN4)")
    (add_net "Net-(J2-PadR2)")
    (add_net "Net-(J2-PadR22)")
    (add_net "Net-(J2-PadRN23)")
    (add_net "Net-(J2-PadRN3)")
    (add_net "Net-(J2-PadTN24)")
    (add_net "Net-(J2-PadTN4)")
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5F8DD717)
    (at 109.474 91.694)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference " " (at 0 2.25) (layer F.SilkS))
    (fp_text value Pin_D1.0mm_L10.0mm (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 5.1 3.1) (drill oval 5 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5F8DCD5F)
    (at 109.4105 48.26)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference " " (at 0 2.25) (layer F.SilkS))
    (fp_text value Pin_D1.0mm_L10.0mm (at 0 -2.05) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 5.1 3.1) (drill oval 5 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B10B-XH-AM_1x10_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 124.9045 58.0485 270)
    (descr "JST XH series connector, B10B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry boss")
    (fp_text reference J3 (at 6.5945 1.7145 90) (layer F.SilkS))
    (fp_text value Conn_01x10_Female (at 11.25 4.6 90) (layer F.Fab))
    (fp_text user %R (at 11.25 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 14 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-PadR22)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-PadRN23)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-PadR2)"))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-PadRN3)"))
    (pad 6 thru_hole oval (at 12.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-PadRN3)"))
    (pad 7 thru_hole oval (at 15 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-PadR2)"))
    (pad 8 thru_hole oval (at 17.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-PadRN23)"))
    (pad 9 thru_hole oval (at 20 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-PadR22)"))
    (pad 10 thru_hole oval (at 22.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 +3V3))
    (pad "" np_thru_hole circle (at -1.6 2 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B10B-XH-AM_1x10_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_DoubleStack (layer F.Cu) (tedit 5F863BC1)
    (at 110.744 59.055)
    (fp_text reference J1 (at -3.81 2.794) (layer F.SilkS))
    (fp_text value AudioJack3_Dual_Stacked (at 0 -22.852) (layer F.Fab))
    (pad MB thru_hole oval (at 7.5 -6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
    (pad MB thru_hole oval (at -3.8 -6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
    (pad RN23 thru_hole oval (at 4.99 1.25 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-PadRN23)") (die_length 3))
    (pad TN24 thru_hole oval (at 4.99 -1.25 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-PadTN24)") (die_length 3))
    (pad T25 thru_hole oval (at 4.99 -3.75 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 13 +3V3) (die_length 3))
    (pad R22 thru_hole oval (at 4.99 3.75 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-PadR22)") (die_length 3))
    (pad R2 thru_hole oval (at 0 5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-PadR2)") (die_length 3))
    (pad RN3 thru_hole oval (at 0 2.5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-PadRN3)") (die_length 3))
    (pad S1 thru_hole oval (at 0 0 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 14 GND) (die_length 3))
    (pad T5 thru_hole oval (at 0 -5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 13 +3V3) (die_length 3))
    (pad TN4 thru_hole oval (at 0 -2.5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-PadTN4)") (die_length 3))
    (pad MB thru_hole oval (at 7.5 6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
    (pad MB thru_hole oval (at -3.8 6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
    (pad PH thru_hole circle (at -3.8 0 270) (size 2.1 2.1) (drill 2) (layers *.Cu))
  )
  (module Connector_Audio:Jack_3.5mm_DoubleStack (layer F.Cu) (tedit 5F863BC1)
    (at 110.744 78.8035)
    (fp_text reference J2 (at -3.81 2.794) (layer F.SilkS))
    (fp_text value AudioJack3_Dual_Stacked (at 0 -22.852) (layer F.Fab))
    (pad PH thru_hole circle (at -3.8 0 270) (size 2.1 2.1) (drill 2) (layers *.Cu))
    (pad MB thru_hole oval (at -3.8 6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
    (pad MB thru_hole oval (at 7.5 6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
    (pad TN4 thru_hole oval (at 0 -2.5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-PadTN4)") (die_length 3))
    (pad T5 thru_hole oval (at 0 -5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 13 +3V3) (die_length 3))
    (pad S1 thru_hole oval (at 0 0 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 14 GND) (die_length 3))
    (pad RN3 thru_hole oval (at 0 2.5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-PadRN3)") (die_length 3))
    (pad R2 thru_hole oval (at 0 5 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-PadR2)") (die_length 3))
    (pad R22 thru_hole oval (at 4.99 3.75 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-PadR22)") (die_length 3))
    (pad T25 thru_hole oval (at 4.99 -3.75 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 13 +3V3) (die_length 3))
    (pad TN24 thru_hole oval (at 4.99 -1.25 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-PadTN24)") (die_length 3))
    (pad RN23 thru_hole oval (at 4.99 1.25 270) (size 1.25 2.5) (drill oval 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-PadRN23)") (die_length 3))
    (pad MB thru_hole oval (at -3.8 -6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
    (pad MB thru_hole oval (at 7.5 -6.04 270) (size 2.4 2.4) (drill oval 2.3) (layers *.Cu))
  )
  (dimension 25.908 (width 0.12) (layer F.CrtYd)
    (gr_text "25.908 mm" (at 115.8875 32.766) (layer F.CrtYd))
    (feature1 (pts (xy 128.8415 47.117) (xy 128.8415 33.449579)))
    (feature2 (pts (xy 102.9335 47.117) (xy 102.9335 33.449579)))
    (crossbar (pts (xy 102.9335 34.036) (xy 128.8415 34.036)))
    (arrow1a (pts (xy 128.8415 34.036) (xy 127.714996 34.622421)))
    (arrow1b (pts (xy 128.8415 34.036) (xy 127.714996 33.449579)))
    (arrow2a (pts (xy 102.9335 34.036) (xy 104.060004 34.622421)))
    (arrow2b (pts (xy 102.9335 34.036) (xy 104.060004 33.449579)))
  )
  (dimension 7.0485 (width 0.12) (layer F.Fab)
    (gr_text "7.048 mm" (at 105.94975 42.2275) (layer F.Fab))
    (feature1 (pts (xy 109.474 53.015) (xy 109.474 42.911079)))
    (feature2 (pts (xy 102.4255 53.015) (xy 102.4255 42.911079)))
    (crossbar (pts (xy 102.4255 43.4975) (xy 109.474 43.4975)))
    (arrow1a (pts (xy 109.474 43.4975) (xy 108.347496 44.083921)))
    (arrow1b (pts (xy 109.474 43.4975) (xy 108.347496 42.911079)))
    (arrow2a (pts (xy 102.4255 43.4975) (xy 103.552004 44.083921)))
    (arrow2b (pts (xy 102.4255 43.4975) (xy 103.552004 42.911079)))
  )
  (dimension 57.277 (width 0.12) (layer F.SilkS)
    (gr_text "57.277 mm" (at 139.0015 70.104 270) (layer F.SilkS))
    (feature1 (pts (xy 132.6515 98.7425) (xy 138.317921 98.7425)))
    (feature2 (pts (xy 132.6515 41.4655) (xy 138.317921 41.4655)))
    (crossbar (pts (xy 137.7315 41.4655) (xy 137.7315 98.7425)))
    (arrow1a (pts (xy 137.7315 98.7425) (xy 137.145079 97.615996)))
    (arrow1b (pts (xy 137.7315 98.7425) (xy 138.317921 97.615996)))
    (arrow2a (pts (xy 137.7315 41.4655) (xy 137.145079 42.592004)))
    (arrow2b (pts (xy 137.7315 41.4655) (xy 138.317921 42.592004)))
  )
  (dimension 7.0485 (width 0.12) (layer F.Fab)
    (gr_text "7.048 mm" (at 105.96825 100.076) (layer F.Fab))
    (feature1 (pts (xy 109.4925 85.3515) (xy 109.4925 99.392421)))
    (feature2 (pts (xy 102.444 85.3515) (xy 102.444 99.392421)))
    (crossbar (pts (xy 102.444 98.806) (xy 109.4925 98.806)))
    (arrow1a (pts (xy 109.4925 98.806) (xy 108.365996 99.392421)))
    (arrow1b (pts (xy 109.4925 98.806) (xy 108.365996 98.219579)))
    (arrow2a (pts (xy 102.444 98.806) (xy 103.570504 99.392421)))
    (arrow2b (pts (xy 102.444 98.806) (xy 103.570504 98.219579)))
  )
  (dimension 43.4975 (width 0.12) (layer F.Fab)
    (gr_text "43.498 mm" (at 95.123 69.94525 270) (layer F.Fab))
    (feature1 (pts (xy 109.982 91.694) (xy 95.806579 91.694)))
    (feature2 (pts (xy 109.982 48.1965) (xy 95.806579 48.1965)))
    (crossbar (pts (xy 96.393 48.1965) (xy 96.393 91.694)))
    (arrow1a (pts (xy 96.393 91.694) (xy 95.806579 90.567496)))
    (arrow1b (pts (xy 96.393 91.694) (xy 96.979421 90.567496)))
    (arrow2a (pts (xy 96.393 48.1965) (xy 95.806579 49.323004)))
    (arrow2b (pts (xy 96.393 48.1965) (xy 96.979421 49.323004)))
  )
  (gr_line (start 102.8065 93.7895) (end 102.8065 46.0375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.4415 94.4245) (end 102.8065 93.7895) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.2065 94.4245) (end 103.4415 94.4245) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.8415 93.7895) (end 128.2065 94.4245) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.8415 46.0375) (end 128.8415 93.7895) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.2065 45.4025) (end 128.8415 46.0375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.4415 45.4025) (end 128.2065 45.4025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.4415 45.4025) (end 102.8065 46.0375) (layer Edge.Cuts) (width 0.05))
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.143 93.98) (xy 103.3145 93.98) (xy 103.3145 46.101) (xy 128.143 46.101)
      )
    )
  )
  (zone (net 13) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.143 93.98) (xy 103.3145 93.98) (xy 103.3145 46.101) (xy 128.143 46.101)
      )
    )
  )
)
