<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="21.59" y1="9.525" x2="21.59" y2="1.734409375" width="0.1524" layer="20"/>
<wire x1="21.59" y1="1.734409375" x2="23.324409375" y2="0" width="0.1524" layer="20" curve="90"/>
<wire x1="23.324409375" y1="0" x2="50.292" y2="0" width="0.1524" layer="20"/>
<wire x1="50.292" y1="0" x2="51.562" y2="1.27" width="0.1524" layer="20" curve="90"/>
<wire x1="51.562" y1="1.27" x2="51.562" y2="34.692609375" width="0.1524" layer="20"/>
<wire x1="51.562" y1="34.692609375" x2="50.694609375" y2="35.55983125" width="0.1524" layer="20" curve="90.011149"/>
<wire x1="50.694609375" y1="35.55983125" x2="0.850178125" y2="35.550165625" width="0.1524" layer="20"/>
<wire x1="0.850178125" y1="35.550165625" x2="0" y2="34.699821875" width="0.1524" layer="20" curve="89.742744"/>
<wire x1="0" y1="34.699821875" x2="0" y2="10.599921875" width="0.1524" layer="20"/>
<wire x1="0" y1="10.599921875" x2="1.074921875" y2="9.525" width="0.1524" layer="20" curve="90"/>
<wire x1="1.074921875" y1="9.525" x2="21.59" y2="9.525" width="0.1524" layer="20"/>
<text>Cut Tabs Off</text>
<text>Cut Tabs Off</text>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
<text>Wiper</text>
<text>Wiper</text>
<text>GND</text>
<text>+5V</text>
<text>GND</text>
<text>+5V</text>
<text>Trigger</text>
<text>Remote Input</text>
<text>Remote PWM Adj</text>
<text>RV-Project.Com</text>
<text>Analog Interface</text>
<text>PAIB-1A</text>
<text>Rev C</text>
<text>4/8/2018</text>
<text>Remote</text>
<text>Input Trigger</text>
<text>Inverting</text>
<text>  Non-
Inverting</text>
<text>Level Adjust</text>
<text>NOTE: If external voltage 
source for the input is used,
an external pull-up resistor 
to Vcc is required.</text>
<text>Trigger</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="D041-3.5MIL">
</package>
<package name="WAFER3PINVERTICAL">
</package>
<package name="WAFERHOUSING2P">
</package>
<package name="WAFERHOUSING3P">
</package>
<package name="KF7.62CONNECTOR2">
</package>
<package name="GENERIC_0200_DEVICE_200_SPACING">
</package>
<package name="BIGFOOT_MEDIUM">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="BOURNS3362_P">
<description>Standard Bourns Cermet Trimmer
&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/54/3362-55248.pdf"&gt;Data Sheet&lt;/a&gt;</description>
</package>
<package name="1/4W_AXIAL">
<description>Standard Axial 1/4Watt Resistor&lt;p&gt;0.45" footprint</description>
</package>
<package name="GENERIC_0100_DEVICE_150_SPACING">
<description>&lt;h3&gt;Ceramic Capacitor&lt;/h3&gt;
Commonly used for small ceramic capacitors 0150 spacing.</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="1X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D2" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="J1" library="a-lib" package="WAFER3PINVERTICAL" value="WAFER3PVERTICAL"/>
<element name="J2" library="a-lib" package="WAFERHOUSING2P" value="WAFER2PHOUSING">
<attribute name="MATING" value="26-60-4020"/>
<attribute name="PN" value="09-48-4028"/>
</element>
<element name="J3" library="a-lib" package="WAFERHOUSING3P" value="WAFER3PHOUSING">
<attribute name="MATING" value="26-60-4020"/>
<attribute name="PARTNUM" value="0009484038"/>
</element>
<element name="J5" library="a-lib" package="KF7.62CONNECTOR2" value="KF762-2CONNECTOR"/>
<element name="C1" library="a-lib" package="GENERIC_0200_DEVICE_200_SPACING" value="0.1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="a-lib" package="WAFER3PINVERTICAL" value="WAFER3PVERTICAL"/>
<element name="F1" library="a-lib" package="GENERIC_0200_DEVICE_200_SPACING" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="a-lib" package="BIGFOOT_MEDIUM" value=""/>
<element name="U1" library="a-lib" package="DIL08" value="LM393OPAMP">
<attribute name="NAME"/>
</element>
<element name="R1" library="a-lib" package="BOURNS3362_P" value="10k">
<attribute name="MARKING" value="103"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a-lib" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="a-lib" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1/4W_AXIAL" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="a-lib" package="1X03" value="M3HEADER"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="P$1"/>
<contactref element="J5" pad="2A"/>
<contactref element="D2" pad="A"/>
<contactref element="C1" pad="2"/>
<contactref element="J4" pad="P$1"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="J3" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="P$2"/>
<contactref element="J5" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="J4" pad="P$3"/>
<contactref element="U1" pad="8"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="P$3"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="C"/>
<contactref element="J4" pad="P$2"/>
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J3" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="K"/>
<contactref element="J6" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="7"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="1"/>
<contactref element="J6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
