<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="13.97" x2="40.62" y2="13.97" width="0" layer="20"/>
<wire x1="40.62" y1="13.97" x2="40.62" y2="44.12" width="0" layer="20"/>
<wire x1="40.62" y1="44.12" x2="0" y2="44.12" width="0" layer="20"/>
<wire x1="0" y1="44.12" x2="0" y2="13.97" width="0" layer="20"/>
<text>DCC DRIVER 9
GB 2015</text>
<text>GND</text>
<text>+5V</text>
<text>D8</text>
<text>D11</text>
<text>D12</text>
<text>D13</text>
<text>D14</text>
<text>D15</text>
<text>D16</text>
<text>D17</text>
<text>D10</text>
<text>D9</text>
<text>12V</text>
<text>5V</text>
</plain>
<libraries>
<library name="HBridge">
<packages>
<package name="DIP16">
</package>
</packages>
</library>
<library name="cap-master">
<description>&lt;b&gt;CAP MASTER! v4.02 - Electrolytic, Film and Tantalum&lt;/b&gt;&lt;br&gt;
&lt;p&gt;This library is a collection of SMD and through hole capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CNP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;small&gt;DISCLAIMER: The author does not warrant that this library is free from error or that it will meet your specific requirements.&lt;/small&gt;&lt;/p&gt;
&lt;author&gt;by Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 05/28/2005 - Rev 4.02&lt;/author&gt;&lt;br&gt;&lt;br&gt;</description>
<packages>
<package name="7343-TE-D">
<description>&lt;b&gt;SMD TANTALUM&lt;/b&gt; - Panasonic Size D&lt;p&gt; 
EIA Code 7343, Size D, 7.3 mm x 4.3 mm, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="1X12">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP08SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GB2015" library="HBridge" package="DIP16" value="SN754410"/>
<element name="C1" library="cap-master" package="7343-TE-D" value="22"/>
<element name="C2" library="cap-master" package="7343-TE-D" value="22"/>
<element name="MOT" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="DCC" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="+PWR-" library="SparkFun-Connectors" package="1X02" value=""/>
<element name=".." library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP7" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP8" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP9" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP10" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP11" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP12" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="..." library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X12" value=".."/>
<element name="JP2" library="SparkFun-Connectors" package="1X12" value="."/>
<element name="7805__" library="linear" package="TO220V" value="."/>
<element name="TP1" library="testpad" package="TP08SQ" value="TPTP08SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="TP08SQ" value="TPTP08SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="TP08SQ" value="TPTP08SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="GB2015" pad="4"/>
<contactref element="GB2015" pad="13"/>
<contactref element="GB2015" pad="12"/>
<contactref element="GB2015" pad="5"/>
<contactref element="+PWR-" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element=".." pad="1"/>
<contactref element="JP12" pad="1"/>
<contactref element="JP11" pad="1"/>
<contactref element="JP10" pad="1"/>
<contactref element="..." pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP2" pad="11"/>
<contactref element="7805__" pad="2"/>
</signal>
<signal name="VCC">
<contactref element=".." pad="2"/>
<contactref element="GB2015" pad="16"/>
<contactref element="C2" pad="+"/>
<contactref element="JP9" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP11" pad="2"/>
<contactref element="JP12" pad="2"/>
<contactref element="JP10" pad="2"/>
<contactref element="..." pad="2"/>
<contactref element="JP2" pad="9"/>
<contactref element="7805__" pad="3"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="N$1">
<contactref element="GB2015" pad="7"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="GB2015" pad="2"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="GB2015" pad="1"/>
<contactref element="GB2015" pad="9"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="GB2015" pad="15"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="GB2015" pad="10"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="GB2015" pad="6"/>
<contactref element="MOT" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="GB2015" pad="3"/>
<contactref element="MOT" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="GB2015" pad="14"/>
<contactref element="DCC" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="GB2015" pad="11"/>
<contactref element="DCC" pad="2"/>
</signal>
<signal name="N$7">
<contactref element=".." pad="3"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="JP7" pad="3"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="JP8" pad="3"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="JP9" pad="3"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="JP10" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="JP11" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="JP12" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="..." pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="+PWR-" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="JP2" pad="12"/>
<contactref element="7805__" pad="1"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$18">
<contactref element="GB2015" pad="8"/>
<contactref element="TP1" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
