(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (grid_origin 116.0124 80.3094)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "/HALL0_VCC")
  (net 4 "/HALL0_VOUT")
  (net 5 "/HALL0_GND")
  (net 6 "/~{SLEEP0}")
  (net 7 "/HALL1_VCC")
  (net 8 "/HALL1_VOUT")
  (net 9 "/HALL1_GND")
  (net 10 "/~{SLEEP1}")
  (net 11 "/HALL2_VCC")
  (net 12 "/HALL2_VOUT")
  (net 13 "/HALL2_GND")
  (net 14 "/~{SLEEP2}")
  (net 15 "/HALL3_VCC")
  (net 16 "/HALL3_VOUT")
  (net 17 "/HALL3_GND")
  (net 18 "/~{SLEEP3}")
  (net 19 "/HALL4_VCC")
  (net 20 "/HALL4_VOUT")
  (net 21 "/HALL4_GND")
  (net 22 "/~{SLEEP4}")
  (net 23 "/HALL5_VCC")
  (net 24 "/HALL5_VOUT")
  (net 25 "/HALL5_GND")
  (net 26 "/~{SLEEP5}")
  (net 27 "/HALL6_VCC")
  (net 28 "/HALL6_VOUT")
  (net 29 "/HALL6_GND")
  (net 30 "/~{SLEEP6}")
  (net 31 "/HALL7_VCC")
  (net 32 "/HALL7_VOUT")
  (net 33 "/HALL7_GND")
  (net 34 "/~{SLEEP7}")
  (net 35 "/HALL8_VCC")
  (net 36 "/HALL8_VOUT")
  (net 37 "/HALL8_GND")
  (net 38 "/~{SLEEP8}")
  (net 39 "/HALL9_VCC")
  (net 40 "/HALL9_VOUT")
  (net 41 "/HALL9_GND")
  (net 42 "/~{SLEEP9}")
  (net 43 "/HALL10_VCC")
  (net 44 "/HALL10_VOUT")
  (net 45 "/HALL10_GND")
  (net 46 "/~{SLEEP10}")
  (net 47 "/HALL11_VCC")
  (net 48 "/HALL11_VOUT")
  (net 49 "/HALL11_GND")
  (net 50 "/~{SLEEP11}")
  (net 51 "/HALL12_VCC")
  (net 52 "/HALL12_VOUT")
  (net 53 "/HALL12_GND")
  (net 54 "/~{SLEEP12}")
  (net 55 "/HALL13_VCC")
  (net 56 "/HALL13_VOUT")
  (net 57 "/HALL13_GND")
  (net 58 "/~{SLEEP13}")
  (net 59 "/HALL14_VCC")
  (net 60 "/HALL14_VOUT")
  (net 61 "/HALL14_GND")
  (net 62 "/~{SLEEP14}")
  (net 63 "/HALL15_VCC")
  (net 64 "/HALL15_VOUT")
  (net 65 "/HALL15_GND")
  (net 66 "/~{SLEEP15}")
  (net 67 "/HALL16_VCC")
  (net 68 "/HALL16_VOUT")
  (net 69 "/HALL16_GND")
  (net 70 "/~{SLEEP16}")
  (net 71 "/HALL17_VCC")
  (net 72 "/HALL17_VOUT")
  (net 73 "/HALL17_GND")
  (net 74 "/~{SLEEP17}")
  (net 75 "/HALL18_VCC")
  (net 76 "/HALL18_VOUT")
  (net 77 "/HALL18_GND")
  (net 78 "/~{SLEEP18}")
  (net 79 "/HALL19_VCC")
  (net 80 "/HALL19_VOUT")
  (net 81 "/HALL19_GND")
  (net 82 "/~{SLEEP19}")
  (net 83 "Net-(BJT0-Pad1)")
  (net 84 "/GATE")
  (net 85 "/VRAW1")
  (net 86 "/DTR")
  (net 87 "/RESET")
  (net 88 "/CS_SHIFT_REG")
  (net 89 "/AVCC")
  (net 90 "/AGND")
  (net 91 "/VBAT")
  (net 92 "/HALL0_~{SLEEP}")
  (net 93 "/HALL0_OUTPUT")
  (net 94 "/HALL0_~{SLEEP_IN}")
  (net 95 "/HALL1_~{SLEEP}")
  (net 96 "/HALL1_OUTPUT")
  (net 97 "/HALL1_~{SLEEP_IN}")
  (net 98 "/HALL2_~{SLEEP}")
  (net 99 "/HALL2_OUTPUT")
  (net 100 "/HALL2_~{SLEEP_IN}")
  (net 101 "/HALL3_~{SLEEP}")
  (net 102 "/HALL3_OUTPUT")
  (net 103 "/HALL3_~{SLEEP_IN}")
  (net 104 "/HALL4_~{SLEEP}")
  (net 105 "/HALL4_OUTPUT")
  (net 106 "/HALL4_~{SLEEP_IN}")
  (net 107 "/HALL5_~{SLEEP}")
  (net 108 "/HALL5_OUTPUT")
  (net 109 "/HALL5_~{SLEEP_IN}")
  (net 110 "/HALL6_~{SLEEP}")
  (net 111 "/HALL6_OUTPUT")
  (net 112 "/HALL6_~{SLEEP_IN}")
  (net 113 "/HALL7_~{SLEEP}")
  (net 114 "/HALL7_OUTPUT")
  (net 115 "/HALL7_~{SLEEP_IN}")
  (net 116 "/HALL8_~{SLEEP}")
  (net 117 "/HALL8_OUTPUT")
  (net 118 "/HALL8_~{SLEEP_IN}")
  (net 119 "/HALL9_~{SLEEP}")
  (net 120 "/HALL9_OUTPUT")
  (net 121 "/HALL9_~{SLEEP_IN}")
  (net 122 "/HALL10_~{SLEEP}")
  (net 123 "/HALL10_OUTPUT")
  (net 124 "/HALL10_~{SLEEP_IN}")
  (net 125 "/HALL11_~{SLEEP}")
  (net 126 "/HALL11_OUTPUT")
  (net 127 "/HALL11_~{SLEEP_IN}")
  (net 128 "/HALL12_~{SLEEP}")
  (net 129 "/HALL12_OUTPUT")
  (net 130 "/HALL12_~{SLEEP_IN}")
  (net 131 "/HALL13_~{SLEEP}")
  (net 132 "/HALL13_OUTPUT")
  (net 133 "/HALL13_~{SLEEP_IN}")
  (net 134 "/HALL14_~{SLEEP}")
  (net 135 "/HALL14_OUTPUT")
  (net 136 "/HALL14_~{SLEEP_IN}")
  (net 137 "/HALL15_~{SLEEP}")
  (net 138 "/HALL15_OUTPUT")
  (net 139 "/HALL15_~{SLEEP_IN}")
  (net 140 "/HALL16_~{SLEEP_IN}")
  (net 141 "/HALL17_~{SLEEP_IN}")
  (net 142 "/HALL18_~{SLEEP_IN}")
  (net 143 "/HALL19_~{SLEEP_IN}")
  (net 144 "/MISO")
  (net 145 "/SCK")
  (net 146 "/MOSI")
  (net 147 "/TO_FTDI_TX")
  (net 148 "unconnected-(U3-Pad3)")
  (net 149 "unconnected-(U3-Pad4)")
  (net 150 "/TO_FTDI_RX")
  (net 151 "Net-(LED1-PadA)")
  (net 152 "Net-(LED2-PadA)")
  (net 153 "/SCL")
  (net 154 "/SDA")
  (net 155 "Net-(P-FET0-Pad3)")
  (net 156 "/PB7")
  (net 157 "/LED_RED")
  (net 158 "/LED_GRN")
  (net 159 "Net-(R4-Pad1)")
  (net 160 "Net-(R5-Pad1)")
  (net 161 "/32KHZ")
  (net 162 "/SHIFT_CLEAR")
  (net 163 "/ANALOG_0")
  (net 164 "/MUX_~{EN}")
  (net 165 "/BATT_MONITOR")
  (net 166 "/BATT_MONITOR_EN")
  (net 167 "unconnected-(RESET0-PadP$1)")
  (net 168 "unconnected-(RESET0-PadP$3)")
  (net 169 "Net-(SHIFT_0-Pad9)")
  (net 170 "unconnected-(SHIFT_1-Pad9)")
  (net 171 "unconnected-(U$1-PadCARD_DETECT1)")
  (net 172 "unconnected-(U$1-PadCARD_DETECT2)")
  (net 173 "/CS_SD")
  (net 174 "/MUX_S0")
  (net 175 "/MUX_S1")
  (net 176 "/MUX_S3")
  (net 177 "/MUX_S2")
  (net 178 "/BUTTON1")
  (net 179 "/BUTTON2")
  (net 180 "/AREF")
  (net 181 "unconnected-(U2-Pad3)")
  (net 182 "unconnected-(U2-Pad4)")
  (net 183 "unconnected-(U2-Pad10)")
  (net 184 "unconnected-(UNK2,1MM_JACK0-PadP$3)")
  (net 185 "unconnected-(BUTTON2-PadP)")
  (net 186 "unconnected-(BUTTON2-PadS)")
  (net 187 "unconnected-(BUTTON1-PadP)")
  (net 188 "unconnected-(BUTTON1-PadS)")
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 172.4494 123.3594)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 195.4124 123.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 183.0705 96.3297 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C55" (at -1.5547 -0.9581 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.102 -0.9581 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/HALL5_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/HALL5_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 187.0329 106.8453 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R60" (at -1.6141 1.0545 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0109 1.0295 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "/HALL10_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/~{SLEEP10}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 92.7844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.9874 92.0344)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "SOT23-3" (layer "F.Cu")
    (tedit 0)
    (at 108.9 88.75 180)
    (descr "SOT23-3 package<br>\nPad size 0.8 x 0.9mm")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P-FET" (at 1.3626 0.0656) (layer "F.SilkS"))
    (fp_text value "MOSFET-PCHANNELBSH203" (at -1.016 0.1905 180) (layer "F.Fab") hide)
    (fp_text user "3" (at -0.1 -0.28 180) (layer "F.Fab"))
    (fp_text user "2" (at 1.02 0.54 180) (layer "F.Fab"))
    (fp_text user "1" (at -1.24 0.53 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1 180) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/GATE") (pinfunction "G") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.95 1 180) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/VRAW1") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at 0 -1.1 180) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(P-FET0-Pad3)") (pinfunction "D") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 192.024 79.1094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 114.973086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 110.2997 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL7_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 33 "/HALL7_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 31 "/HALL7_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 32 "/HALL7_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 115 "/HALL7_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 131.7844 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 125.1841 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL1" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/HALL1_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/HALL1_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/HALL1_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/~{SLEEP1}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/HALL1_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 179.8955 85.5347 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R67" (at -1.5997 1.1919 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.1524 1.0919 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "/HALL17_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/~{SLEEP17}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 79.0844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 99.6317 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL5_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 25 "/HALL5_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 23 "/HALL5_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 24 "/HALL5_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 109 "/HALL5_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "SOT95P237X112-3N" (layer "F.Cu")
    (tedit 0)
    (at 114.975 78.375 90)
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "MCP1700T-3302" (at -1.9812 -2.159 90) (layer "F.SilkS") hide)
    (fp_text value "MCP1700T-3302E/TT" (at -1.651 2.9718 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.9398 1.0414 90) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.9398 1.0414 90) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VOUT") (pintype "output") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at 0 -1.0414 90) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/VRAW1") (pinfunction "VIN") (pintype "input") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.6124 92.0594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 93.1547 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL9" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HALL9_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/HALL9_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HALL9_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/~{SLEEP9}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HALL9_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 121.975 95.475 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R9" (at -2.0864 0.8594) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "/32KHZ") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8358 76.8604)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 85.2474 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.724282 92.036886)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 197.7124 123.3094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 134.8105 117.3101)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R3" (at -1.5875 -1.1559) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.3019 -1.1507) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/CS_SHIFT_REG") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 187.0329 128.2321 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R64" (at -1.596 1.427 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -0.008 1.472 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "/HALL14_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/~{SLEEP14}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 130.3655 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$3" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 87 "/RESET") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "STAND-OFF" (layer "F.Cu")
    (tedit 0)
    (at 102.6795 106.1341)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447\nOuter keepout is 0.127\" radius (0.254\" diameter).")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFF4-40" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 180.1244 123.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "PUSHBUTTON_DPST_SMD" (layer "F.Cu")
    (tedit 0)
    (at 105.3846 115.2652)
    (descr "PUSHBUTTON Omron B3S-1000 SMD DPST")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "BUTTON2" (at -2.4892 -3.5814) (layer "F.SilkS"))
    (fp_text value "PUSHBUTTON_DPST_SMDSTANDARD" (at -3.81 5.08) (layer "F.Fab") hide)
    (pad "P" smd rect (at 3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "unconnected-(BUTTON2-PadP)") (pinfunction "P") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$1" smd rect (at -3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "/BUTTON2") (pinfunction "P1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "S" smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "unconnected-(BUTTON2-PadS)") (pinfunction "S") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "S$1" smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S1") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 103.8227 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL11" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/HALL11_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/HALL11_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/HALL11_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/~{SLEEP11}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/HALL11_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 194.1195 128.2321 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R65" (at -1.5023 1.0679 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0477 1.0429 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "/HALL15_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/~{SLEEP15}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 124.879086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 100.2921)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL6" (at 5.5969 1.317 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "/HALL6_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "/HALL6_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 103.8227 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL10" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/HALL10_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/HALL10_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/HALL10_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/~{SLEEP10}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/HALL10_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 183.9374 123.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.984082 104.2594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 113.449086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 194.1195 106.8453 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R61" (at -1.5141 1.0679 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.1109 1.0429 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "/HALL11_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/~{SLEEP11}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 175.8061 106.9723 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C56" (at -1.5621 -1.0187 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.1879 -1.0937 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/HALL6_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/HALL6_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7896 121.0818 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9986 110.3844 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 81.4578)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 93.1547 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL5" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/HALL5_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/HALL5_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/HALL5_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/~{SLEEP5}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/HALL5_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 132.6515 104.2291)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$10" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 163 "/ANALOG_0") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 187.7494 91.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 125.1841 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL4" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/HALL4_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/HALL4_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/HALL4_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/~{SLEEP4}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/HALL4_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 109.8171)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL9" (at -5.4951 1.0673 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "/HALL9_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "/HALL9_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 121.0564 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 197.8374 101.9844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "SO16" (layer "F.Cu")
    (tedit 0)
    (at 141.5415 123.6601)
    (descr "<b>Small Outline package</b> 150 mil")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SHIFT_1" (at -5.461 1.778 90) (layer "F.SilkS") hide)
    (fp_text value "74HC595D" (at -2.9291 0.0993) (layer "F.SilkS"))
    (pad "1" smd rect (at -4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "/HALL9_~{SLEEP}") (pinfunction "QB") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "/HALL10_~{SLEEP}") (pinfunction "QC") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "/HALL11_~{SLEEP}") (pinfunction "QD") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "/HALL12_~{SLEEP}") (pinfunction "QE") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at 0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "/HALL13_~{SLEEP}") (pinfunction "QF") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at 1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "/HALL14_~{SLEEP}") (pinfunction "QG") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at 3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "/HALL15_~{SLEEP}") (pinfunction "QH") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at 4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "9" smd rect (at 4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "unconnected-(SHIFT_1-Pad9)") (pinfunction "QH*") (pintype "tri_state+no_connect") (solder_mask_margin 0.0762))
    (pad "10" smd rect (at 3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "/SHIFT_CLEAR") (pinfunction "~{SRCLR}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "11" smd rect (at 1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "/SCK") (pinfunction "SRCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "12" smd rect (at 0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/CS_SHIFT_REG") (pinfunction "RCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "13" smd rect (at -0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "~{OE}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "14" smd rect (at -1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "Net-(SHIFT_0-Pad9)") (pinfunction "SER") (pintype "input") (solder_mask_margin 0.0762))
    (pad "15" smd rect (at -3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "/HALL8_~{SLEEP}") (pinfunction "QA") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "16" smd rect (at -4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "PANASONIC_B" (layer "F.Cu")
    (tedit 0)
    (at 112.1 81.425 90)
    (descr "<b>Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B</b>")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C1" (at 4.2156 -0.7126) (layer "F.SilkS"))
    (fp_text value "1µF" (at -2.15 3.275 90) (layer "F.Fab") hide)
    (pad "+" smd rect (at 2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/VRAW1") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "-" smd rect (at -2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.724282 93.560886)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 89.0594 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.984082 103.4844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 134.9375 120.4851 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C8" (at -1.5365 1.1557 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.2923 1.1303 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "I_0805" (layer "F.Cu")
    (tedit 0)
    (at 133.4643 110.0965)
    (descr "<b>0805 (2012) Inductor footprint<br></b>\nExample:\nTaiyo Yuden inductor # LBR2012T100K<br>\nDigikey PN 587-2045-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "INDUCTOR" (at 1.1981 -1.2121) (layer "F.SilkS"))
    (fp_text value "10µH" (at 2.9231 -0.6621) (layer "F.SilkS"))
    (pad "P$1" smd rect (at -0.85 0) (size 0.7 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/AVCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0.85 0) (size 0.7 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 130.81 102.4636 180)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R14" (at -0.8128 -1.143) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -3.1242 0.2286) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 180) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "/SHIFT_CLEAR") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 180) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 195.3744 91.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "PUSHBUTTON_SPST_PTS525_SERIES" (layer "F.Cu")
    (tedit 0)
    (at 130.1115 127.7241 90)
    (descr "C&K PTS525 series tactile switch<br>\nSmall surface mount switches")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "RESET" (at -2.6603 3.9009 90) (layer "F.SilkS"))
    (fp_text value "PUSHBUTTON_DPST_SMDSMALL" (at -3.81 3.81 90) (layer "F.Fab") hide)
    (fp_text user "1" (at -2.73 -1.785 90) (layer "F.Fab"))
    (fp_text user "2" (at 2.72 -1.845 90) (layer "F.Fab"))
    (fp_text user "3" (at -2.78 2.005 90) (layer "F.Fab"))
    (fp_text user "4" (at 2.58 2.04 90) (layer "F.Fab"))
    (pad "P$1" smd rect (at -3.2 -1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "unconnected-(RESET0-PadP$1)") (pinfunction "P") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 3.2 -1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "P1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" smd rect (at -3.2 1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "unconnected-(RESET0-PadP$3)") (pinfunction "S") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$4" smd rect (at 3.2 1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/RESET") (pinfunction "S1") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "SOT23" (layer "F.Cu")
    (tedit 0)
    (at 116.9 88.9 180)
    (descr "<b>SOT-23</b>")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "BJT" (at 1.9626 0.6906 90) (layer "F.SilkS"))
    (fp_text value "KSC1623_BJT_TRANSISTOR" (at -1.645 2.585) (layer "F.Fab") hide)
    (fp_text user "3" (at -0.1 -0.23) (layer "F.Fab"))
    (fp_text user "2" (at 1.04 0.52) (layer "F.Fab"))
    (fp_text user "1" (at -1.25 0.52) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1.1 180) (size 1 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(BJT0-Pad1)") (pinfunction "B") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.95 1.1 180) (size 1 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at 0 -1.1 180) (size 1 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/GATE") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 183.9244 91.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 116.8021)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL10" (at 5.5969 1.5573 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "/HALL10_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "/HALL10_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "CHIPLED_0805" (layer "F.Cu")
    (tedit 0)
    (at 111.1885 99.4031 90)
    (descr "Surface mount LED 0805 footprint with marker for positive (anode) terminal")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "LED2" (at -1.27 1.27 180) (layer "F.SilkS") hide)
    (fp_text value "GREEN_LED" (at 1.27 1.27 180) (layer "F.Fab") hide)
    (fp_text user "+" (at -0.1778 1.651 90) (layer "F.Fab"))
    (pad "A" smd rect (at 0 1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(LED2-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "C" smd rect (at 0 -1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "PUSHBUTTON_DPST_SMD" (layer "F.Cu")
    (tedit 0)
    (at 110.7948 107.0102)
    (descr "PUSHBUTTON Omron B3S-1000 SMD DPST")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "BUTTON1" (at -2.7324 -2.032) (layer "F.SilkS"))
    (fp_text value "PUSHBUTTON_DPST_SMDSTANDARD" (at -3.81 5.08) (layer "F.Fab") hide)
    (pad "P" smd rect (at 3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "unconnected-(BUTTON1-PadP)") (pinfunction "P") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$1" smd rect (at -3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "/BUTTON1") (pinfunction "P1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "S" smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "unconnected-(BUTTON1-PadS)") (pinfunction "S") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "S$1" smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S1") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X3" (layer "F.Cu")
    (tedit 0)
    (at 127.9779 117.5133 180)
    (descr "ISP programming header for Arduino<br>\nKeepout area gives approximate footprint of connector from AVR MKII ISP")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "J1" (at -3.81 -4.445 180) (layer "F.SilkS") hide)
    (fp_text value "AVR_SPI_PRG_6PTH" (at -3.81 3.175 180) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at -2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 144 "/MISO") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole roundrect (at -2.54 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole roundrect (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 145 "/SCK") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole roundrect (at 0 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 146 "/MOSI") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "5" thru_hole roundrect (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 87 "/RESET") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "6" thru_hole roundrect (at 2.54 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 120.9677 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL3_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 17 "/HALL3_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 15 "/HALL3_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 16 "/HALL3_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 103 "/HALL3_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 82.1844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9874 106.5594 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "STAND-OFF_M2" (layer "F.Cu")
    (tedit 0)
    (at 112.25 88.775)
    (descr "M2 stand-off hole<p>\nDrill diam = 2.2mm <br>\nOuter keepout diameter = 3.175mm (0.125\")")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF5_M2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFFM2" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 95.8724 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 198.3624 80.6844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 81.3844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 125.6594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 131.6611 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL1_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 9 "/HALL1_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 7 "/HALL1_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 8 "/HALL1_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 97 "/HALL1_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 114.947686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 130.7 88.55)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$17" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 180 "/AREF") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 116.8021)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL11" (at -5.4951 1.5573 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "/HALL11_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "/HALL11_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 179.8955 117.5387 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R53" (at -1.342 1.0419 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "/HALL3_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/~{SLEEP3}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.724282 92.798886)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 130.7721)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL15" (at -5.5451 1.5373 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 137 "/HALL15_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "/HALL15_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 113.423686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 120.9677 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL12_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 53 "/HALL12_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 51 "/HALL12_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 52 "/HALL12_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 130 "/HALL12_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 175.8315 85.6617 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C66" (at -1.4977 -1.0191 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.3302 -1.1191 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/HALL16_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/HALL16_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 182.8165 117.6657 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C53" (at -1.2437 -0.9541 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.1313 -0.9541 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/HALL3_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/HALL3_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 99.6696 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 114.185686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 117.2464 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 135.6868 103.9751 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R15" (at -1.8921 1.1176 90) (layer "F.SilkS"))
    (fp_text value "100k Ω" (at -0.1649 1.0006 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "/ANALOG_0") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 99.3775 108.9281)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$6" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 178 "/BUTTON1") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 99.3775 111.4681)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$7" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 122.1613 131.2547 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R4" (at -2.0445 1.3843 90) (layer "F.SilkS"))
    (fp_text value "100k Ω" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(R4-Pad1)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 113.4106 85.904)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R32" (at -0.2732 -1.1446) (layer "F.SilkS"))
    (fp_text value "10k" (at 0.0518 1.1804) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "/BATT_MONITOR_EN") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 194.1195 96.2027 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R59" (at -1.6067 1.0679 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0933 1.0429 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "/HALL9_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/~{SLEEP9}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 119.5705 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "PB7" (at -0.9352 -1.5228) (layer "F.SilkS"))
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 156 "/PB7") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 109.8546 85.904 180)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R33" (at -1.1328 1.1196) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.6922 -0.0554) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 180) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/GATE") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 180) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/VRAW1") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 176.1374 112.649)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 197.5874 112.649)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 89.1286 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 187.0329 96.2027 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R58" (at -1.6317 1.0545 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0683 1.0795 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "/HALL8_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/~{SLEEP8}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 197.2945 128.3591 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C65" (at -1.5003 -0.9321 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.229 -1.0821 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/HALL15_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/HALL15_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 99.6317 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL8_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 37 "/HALL8_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 35 "/HALL8_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 36 "/HALL8_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 118 "/HALL8_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 190.0809 117.6657 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C62" (at -1.3687 -1.0185 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.3813 -1.1185 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/HALL12_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/HALL12_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 121.0564 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8358 79.9084)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "CHIPLED_0805" (layer "F.Cu")
    (tedit 0)
    (at 111.1885 97.4981 90)
    (descr "Surface mount LED 0805 footprint with marker for positive (anode) terminal")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "LED1" (at 1.0887 0.7489) (layer "F.SilkS") hide)
    (fp_text value "RED_LED" (at 1.27 1.27 180) (layer "F.Fab") hide)
    (fp_text user "+" (at -0.1778 1.651 90) (layer "F.Fab"))
    (pad "A" smd rect (at 0 1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(LED1-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "C" smd rect (at 0 -1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 131.6611 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL4_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 21 "/HALL4_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 19 "/HALL4_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 20 "/HALL4_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 106 "/HALL4_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "STAND-OFF" (layer "F.Cu")
    (tedit 0)
    (at 138.6205 131.4071)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447\nOuter keepout is 0.127\" radius (0.254\" diameter).")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFF4-40" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 187.8874 101.9844)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8358 77.6224)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 198.5874 101.9844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 110.3884 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 172.7835 96.2027 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R50" (at -1.5817 1.0789 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.119 1.0789 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/HALL0_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/~{SLEEP0}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "PANASONIC_B" (layer "F.Cu")
    (tedit 0)
    (at 118.325 81.45 90)
    (descr "<b>Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B</b>")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C2" (at 4.3656 -0.6376) (layer "F.SilkS"))
    (fp_text value "1µF" (at -2.15 3.275 90) (layer "F.Fab") hide)
    (pad "+" smd rect (at 2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "-" smd rect (at -2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 174.0281 103.7973 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL6" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/HALL6_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/HALL6_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/HALL6_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/~{SLEEP6}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/HALL6_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 114.4907 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL2" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/HALL2_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/HALL2_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/HALL2_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/~{SLEEP2}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/HALL2_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 79.3371)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL0" (at 5.5469 1.1473 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "/HALL0_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "/HALL0_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 110.2997 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL11_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 49 "/HALL11_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 47 "/HALL11_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 48 "/HALL11_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 127 "/HALL11_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 133.4897 107.2263)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C23" (at -2.5023 -0.9669) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.2921 -1.0797) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/AVCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 117.1575 107.5311 180)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C3" (at 0.4445 1.2575) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -1.524 1.397 180) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 180) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 180) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 124.853686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 198.3624 112.649)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 121.0818 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 78.3094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 174.0281 110.2743 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL6_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 29 "/HALL6_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 27 "/HALL6_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 28 "/HALL6_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 112 "/HALL6_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 172.5994 101.9844)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 124.091686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 93.1547 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL8" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/HALL8_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/HALL8_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/HALL8_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/~{SLEEP8}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/HALL8_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.0744 101.9844)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 187.7624 123.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 88.9637 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL18_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 77 "/HALL18_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 75 "/HALL18_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 76 "/HALL18_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 142 "/HALL18_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 123.7871)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL12" (at 5.5469 1.5473 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "/HALL12_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "/HALL12_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 135.4455 113.2461 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R28" (at -1.4349 -1.2065 90) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at -1.9683 0.8763 180) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "/MUX_~{EN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 117.0305 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "GND" (at -1.2181 -1.5427) (layer "F.SilkS"))
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 99.6317 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL0_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 5 "/HALL0_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 3 "/HALL0_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 4 "/HALL0_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 94 "/HALL0_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 192.024 78.3344)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "CR1220_BATTERY_HOLDER_SMD" (layer "F.Cu")
    (tedit 0)
    (at 137.4775 83.1471)
    (descr "CR1220 Battery Holder, SMD\nKeystone Part # 3000")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "CR1220_BATTERY0" (at -2.54 8.89) (layer "F.SilkS") hide)
    (fp_text value "CR1220_BATTERY_HOLDERSMD" (at 0 0) (layer "F.Fab") hide)
    (pad "GND" smd rect (at 0 0) (size 4.064 4.064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "P$1" smd rect (at -7.62 0) (size 3.429 3.429) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/VBAT") (pinfunction "VBAT") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 7.62 0) (size 3.429 3.429) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/VBAT") (pinfunction "P$2") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 93.1547 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL0" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/HALL0_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/HALL0_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/HALL0_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/~{SLEEP0}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/HALL0_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 110.2997 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL10_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 45 "/HALL10_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 43 "/HALL10_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 44 "/HALL10_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 124 "/HALL10_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 176.8624 80.645)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 115.7 95.575 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R6" (at -2.0626 0.9374) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/RESET") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 125.1587 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL15" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/HALL15_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/HALL15_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/HALL15_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/~{SLEEP15}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/HALL15_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 79.121)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 99.3775 114.0081)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$8" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 179 "/BUTTON2") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 109.8171)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL8" (at 5.5719 1.0673 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "/HALL8_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "/HALL8_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 86.3221)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL2" (at 5.5969 1.3123 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "/HALL2_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 "/HALL2_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.4494 112.649)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 81.407 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 114.211086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 117.1956 101.346 -90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R1" (at 0.5334 -2.2606) (layer "F.SilkS"))
    (fp_text value "100 Ω" (at -1.524 1.397 -90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(LED1-PadA)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "/LED_RED") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 192.1374 80.6594)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 93.5594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 120.5992 91.567 -90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R29" (at -1.2321 1.4097 90) (layer "F.SilkS"))
    (fp_text value "10k" (at -1.3576 -1.3132 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/BATT_MONITOR") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 124.117086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 197.1675 96.3297 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C59" (at -1.5297 -1.0051 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.356 -1.0551 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HALL9_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HALL9_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 120.9677 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL2_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 13 "/HALL2_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 11 "/HALL2_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 12 "/HALL2_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 100 "/HALL2_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 88.9637 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL16_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 69 "/HALL16_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 67 "/HALL16_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 68 "/HALL16_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 140 "/HALL16_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 99.6844 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 189.9539 96.3297 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C58" (at -1.5047 -0.9915 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.229 -1.0915 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/HALL8_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/HALL8_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 85.1974 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7874 106.5344 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 99.6844 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 117.2464 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 76.7594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 176.4374 101.981)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 194.1195 85.5347 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R69" (at -1.5997 1.1679 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.1753 1.0429 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "/HALL19_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/~{SLEEP19}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 198.4874 91.3344)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 137.3505 112.3571 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C6" (at 1.9727 0.7369) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -1.8159 0.7239) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 124.6251 125.3111 -90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R5" (at 1.9733 1.1627 90) (layer "F.SilkS"))
    (fp_text value "100k Ω" (at -1.524 1.397 -90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "Net-(R5-Pad1)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 197.6874 91.3344)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 182.9435 128.3591 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C54" (at -1.3003 -0.9561 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/HALL4_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/HALL4_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 172.4744 91.3094)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "1X06-RIGHT_ANGLE" (layer "F.Cu")
    (tedit 0)
    (at 105.7275 102.0701 90)
    (descr "1x06 0.1\" spacing right angle header<p>\nExample: Sullins PPPC061LGBN-RC, Digikey PN S5481-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "JP1" (at -1.3462 -1.8288 90) (layer "F.SilkS") hide)
    (fp_text value "FTDI_HEADER" (at -1.27 2.54 90) (layer "F.Fab") hide)
    (fp_text user "4" (at 7.62 -8.89 90) (layer "F.Fab"))
    (fp_text user "1" (at 0 -8.89 90) (layer "F.Fab"))
    (fp_text user "3" (at 5.08 -8.89 90) (layer "F.Fab"))
    (fp_text user "6" (at 12.7 -8.89 90) (layer "F.Fab"))
    (fp_text user "2" (at 2.54 -8.89 90) (layer "F.Fab"))
    (fp_text user "5" (at 10.16 -8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole roundrect (at 2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole roundrect (at 5.08 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 2 "VCC") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole roundrect (at 7.62 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 147 "/TO_FTDI_TX") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "5" thru_hole roundrect (at 10.16 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 150 "/TO_FTDI_RX") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "6" thru_hole roundrect (at 12.7 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 86 "/DTR") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 125.1587 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL14" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/HALL14_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/HALL14_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/HALL14_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/~{SLEEP14}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/HALL14_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 127.9398 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7374 106.5474 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 114.4907 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL12" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/HALL12_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/HALL12_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/HALL12_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/~{SLEEP12}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/HALL12_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 197.1675 85.6617 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C69" (at -1.4727 -1.0801 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.3023 -1.1051 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/HALL19_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/HALL19_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7874 110.3594 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 125.641086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 117.975 95.5 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R7" (at -2.0868 0.7446) (layer "F.SilkS"))
    (fp_text value "4.7k" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "/SCL") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 82.4867 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL18" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/HALL18_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/HALL18_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/HALL18_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/~{SLEEP18}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/HALL18_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 76.835)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 99.3775 116.5481)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$9" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.5624 91.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7896 117.2718 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "SO16" (layer "F.Cu")
    (tedit 0)
    (at 141.7955 99.2761)
    (descr "<b>Small Outline package</b> 150 mil")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SHIFT_0" (at -5.461 1.778 90) (layer "F.SilkS") hide)
    (fp_text value "74HC595D" (at -2.8081 0.1583) (layer "F.SilkS"))
    (pad "1" smd rect (at -4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/HALL1_~{SLEEP}") (pinfunction "QB") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "/HALL2_~{SLEEP}") (pinfunction "QC") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "/HALL3_~{SLEEP}") (pinfunction "QD") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "/HALL4_~{SLEEP}") (pinfunction "QE") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at 0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "/HALL5_~{SLEEP}") (pinfunction "QF") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at 1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "/HALL6_~{SLEEP}") (pinfunction "QG") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at 3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/HALL7_~{SLEEP}") (pinfunction "QH") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at 4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "9" smd rect (at 4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "Net-(SHIFT_0-Pad9)") (pinfunction "QH*") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "10" smd rect (at 3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "/SHIFT_CLEAR") (pinfunction "~{SRCLR}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "11" smd rect (at 1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "/SCK") (pinfunction "SRCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "12" smd rect (at 0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/CS_SHIFT_REG") (pinfunction "RCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "13" smd rect (at -0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "~{OE}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "14" smd rect (at -1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "/MOSI") (pinfunction "SER") (pintype "input") (solder_mask_margin 0.0762))
    (pad "15" smd rect (at -3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/HALL0_~{SLEEP}") (pinfunction "QA") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "16" smd rect (at -4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 124.879086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 77.597)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 103.8227 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL7" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/HALL7_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/HALL7_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/HALL7_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/~{SLEEP7}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/HALL7_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 77.5344)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 78.359)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 175.8315 117.6657 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C52" (at -1.2792 -0.9441 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.0813 -1.0691 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/HALL2_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/HALL2_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 114.4907 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL13" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/HALL13_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/HALL13_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/HALL13_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/~{SLEEP13}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/HALL13_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8358 79.1464)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 93.5844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 114.211086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 188.3029 131.6357 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL14_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 61 "/HALL14_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 59 "/HALL14_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 60 "/HALL14_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 136 "/HALL14_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 125.2855 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$4" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 195.5374 101.98354)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 119.975 95.475 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R8" (at -2.0356 0.8782) (layer "F.SilkS"))
    (fp_text value "4.7k" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "/SDA") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "STAND-OFF_M2" (layer "F.Cu")
    (tedit 0)
    (at 112.275 112.55)
    (descr "M2 stand-off hole<p>\nDrill diam = 2.2mm <br>\nOuter keepout diameter = 3.175mm (0.125\")")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF4_M2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFFM2" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 179.8955 106.8453 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R57" (at -1.5891 1.0669 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0359 1.0419 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "/HALL7_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/~{SLEEP7}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 127.9144 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 103.517686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 114.4907 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL3" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/HALL3_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/HALL3_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/HALL3_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/~{SLEEP3}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/HALL3_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 131.7498 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 175.8315 96.3297 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C50" (at -1.3797 -0.9441 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.3703 -1.1191 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/HALL0_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/HALL0_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 135.8138 100.4316 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C9" (at 1.397 -0.4826 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 4.6228 0.381 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 102.755686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 190.0809 128.3591 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C64" (at -1.4503 -0.9185 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.102 -0.721 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/HALL14_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/HALL14_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 125.615686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 131.7244 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "22-23-2021" (layer "F.Cu")
    (tedit 0)
    (at 124.175 79.025 90)
    (descr ".100\" (2.54mm) Center Headers - 2 Pin")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "MOLEX_KK0" (at -2.54 -3.81 90) (layer "F.SilkS") hide)
    (fp_text value "22-23-2021" (at -2.54 5.08 90) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at -1.27 0 180) (size 3 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 3 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 85 "/VRAW1") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 179.8955 128.2321 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R54" (at -1.4773 1.0669 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -1.524 1.397 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "/HALL4_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/~{SLEEP4}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 82.4867 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL17" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/HALL17_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/HALL17_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/HALL17_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/~{SLEEP17}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/HALL17_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 100.2921)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL7" (at -5.4951 1.2673 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "/HALL7_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "/HALL7_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 181.1655 88.9637 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL17_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 73 "/HALL17_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 71 "/HALL17_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 72 "/HALL17_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 141 "/HALL17_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8358 78.3844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 123.7871)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL13" (at -5.5201 1.4973 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "/HALL13_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "/HALL13_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 113.449086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 180.6874 80.6344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 125.641086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "MICROSD_SOCKET_MOLEX_REVERSEMOUNT" (layer "F.Cu")
    (tedit 0)
    (at 113.3475 132.2707 90)
    (descr "<b>Molex micro SD card slot, push-push spring-loaded style \"reverse mount\"</b><br>\nMolex PN 5027740891<br>\nDigikey PN WM24066CT-ND<br>\nThis version has the surface mount pins easily accessible at the rear of the housing rather than underneath it like most other sockets.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$1" (at 3.81 -8.89 90) (layer "F.SilkS") hide)
    (fp_text value "MICROSD_MOLEX_REVERSECURRENT" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text user "MOSI" (at 6.985 1.524 180) (layer "F.Fab"))
    (fp_text user "MISO" (at 2.54 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at 12.446 1.524 180) (layer "F.Fab"))
    (fp_text user "CD1" (at -0.762 -7.874 90) (layer "F.Fab"))
    (fp_text user "VDD" (at 5.715 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at -0.254 -13.462 180) (layer "F.Fab"))
    (fp_text user "SCK" (at 4.699 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at 12.954 -13.462 180) (layer "F.Fab"))
    (fp_text user "GND" (at -0.254 1.524 180) (layer "F.Fab"))
    (fp_text user "CS" (at 8.001 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at 3.556 1.524 180) (layer "F.Fab"))
    (fp_text user "RSV1" (at 9.144 1.524 180) (layer "F.Fab"))
    (fp_text user "CD2" (at -0.762 -0.508 90) (layer "F.Fab"))
    (fp_text user "RSV8" (at 1.524 1.524 180) (layer "F.Fab"))
    (pad "CARD_DETECT1" smd rect (at -0.645 -8.12 90) (size 1.29 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "unconnected-(U$1-PadCARD_DETECT1)") (pinfunction "CARD_DETECT") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "CARD_DETECT2" smd rect (at -0.645 -0.65 90) (size 1.29 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "unconnected-(U$1-PadCARD_DETECT2)") (pinfunction "CARD_DETECT1") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "CS2" smd rect (at 7.8 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "/CS_SD") (pinfunction "CS") (pintype "input") (solder_mask_margin 0.0762))
    (pad "GND6" smd rect (at 3.4 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MISO7" smd rect (at 2.3 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "/MISO") (pinfunction "DATA_OUT_MISO") (pintype "output") (solder_mask_margin 0.0762))
    (pad "MNT1" smd rect (at -0.2 0.93 270) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND1") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MNT2" smd rect (at 12.45 0.93 90) (size 1.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND2") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MNT3" smd rect (at -0.54 -13.92 90) (size 1.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND3") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MNT4" smd rect (at 12.75 -13.92 90) (size 1.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND4") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MOSI3" smd rect (at 6.7 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "/MOSI") (pinfunction "DATA_IN_MOSI") (pintype "input") (solder_mask_margin 0.0762))
    (pad "NC1" smd rect (at 8.9 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "Net-(R5-Pad1)") (pinfunction "DAT1_NC") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "RES8" smd rect (at 1.2 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(R4-Pad1)") (pinfunction "DAT2_RES") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "SCK5" smd rect (at 4.5 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "/SCK") (pinfunction "SCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "VDD4" smd rect (at 5.6 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "STAND-OFF" (layer "F.Cu")
    (tedit 0)
    (at 143.4465 91.7831)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447\nOuter keepout is 0.127\" radius (0.254\" diameter).")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFF4-40" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 121.7295 127.5971 -90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C4" (at 0.6221 1.2573 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -1.524 1.397 -90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 270) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 270) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 93.3071)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL4" (at 5.5719 1.2523 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "/HALL4_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "/HALL4_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 79.3371)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL1" (at -5.5201 1.1473 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "/HALL1_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "/HALL1_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 99.7204 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 183.0705 106.9723 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C57" (at -1.5371 -0.9831 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.2379 -1.0831 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/HALL7_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/HALL7_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 197.1675 106.9723 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C61" (at -1.4371 -0.9551 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.2379 -1.0801 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/HALL11_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/HALL11_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 183.8124 112.649)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 179.8955 96.2027 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R55" (at -1.5817 1.0419 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0683 1.0669 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "/HALL5_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/~{SLEEP5}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 92.8094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 95.9104 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 89.0094 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 197.2945 117.6657 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C63" (at -1.2187 -0.9571 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.3813 -1.0821 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/HALL13_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/HALL13_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 85.217 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 187.6374 112.649)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 194.1195 117.5387 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R63" (at -1.4707 1.0179 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.1293 1.0179 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "/HALL13_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/~{SLEEP13}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 124.8844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 106.5784 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 93.611686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 195.9624 80.6594)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "1X01_SMALL" (layer "F.Cu")
    (tedit 0)
    (at 145.2245 131.9151)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$11" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 90 "/AGND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 192.024 77.5594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 198.4874 123.3094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 117.2718 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 152.5905 130.7721)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL14" (at 5.5719 1.5373 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "/HALL14_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "/HALL14_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 82.9594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 114.225 91.5 -90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R30" (at -0.9744 1.2966 90) (layer "F.SilkS"))
    (fp_text value "15k" (at -0.8474 -1.3196 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/BATT_MONITOR") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(P-FET0-Pad3)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 92.849686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 95.8596 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 172.3136 112.649)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 187.0329 85.5347 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R68" (at -1.5997 1.1545 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.1753 1.0295 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "/HALL18_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/~{SLEEP18}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7896 127.9398 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "POWER_JACK_DC_2,1MM" (layer "F.Cu")
    (tedit 0)
    (at 106.8705 80.6071 180)
    (descr "2.1 mm DC power jack. Digikey PN CP-202AH-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "UNK2,1MM_JACK0" (at 8.89 -5.08 180) (layer "F.SilkS") hide)
    (fp_text value "POWER_JACK_2,1MM" (at 8.89 6.35 180) (layer "F.Fab") hide)
    (fp_text user "+" (at -1.4795 2.1321 180) (layer "F.SilkS"))
    (fp_text user "GND" (at 7.7205 2.5571 180) (layer "F.SilkS"))
    (pad "P$1" thru_hole circle (at 0 0 270) (size 4.572 4.572) (drill 3.175) (layers *.Cu *.Mask)
      (net 85 "/VRAW1") (pinfunction "PWR") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole rect (at 6.096 0 180) (size 4.191 4.191) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole rect (at 3.048 -4.826 180) (size 3.816 3.816) (drill 2.8) (layers *.Cu *.Mask)
      (net 184 "unconnected-(UNK2,1MM_JACK0-PadP$3)") (pinfunction "GNDBREAK") (pintype "bidirectional+no_connect") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 192.024 76.7844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 179.9624 112.649)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 112.2553 94.9073)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C5" (at -2.1209 -1.1305) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -1.524 1.397) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/DTR") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/RESET") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.7124 101.98354)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 117.0305 127.5971 -90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C10" (at 0.0887 -1.2319 90) (layer "F.SilkS"))
    (fp_text value "10µF" (at -2.7877 -1.1819 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 270) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 270) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 104.2344)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.8874 81.3594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 131.6357 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL15_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 65 "/HALL15_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 63 "/HALL15_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 64 "/HALL15_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 139 "/HALL15_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 174.0535 82.4867 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL16" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/HALL16_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/HALL16_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/HALL16_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/~{SLEEP16}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/HALL16_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 122.3824 99.3144 180)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C7" (at 0.72 -1.11) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.19 -1.1) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0 180) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 180) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 114.554 101.3714 -90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R2" (at 0.5842 2.2352) (layer "F.SilkS"))
    (fp_text value "100 Ω" (at -1.524 1.397 -90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(LED2-PadA)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 270) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "/LED_GRN") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "A139*_HALL_EFFECT" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 82.4867 90)
    (descr "Allegro A193* series hall effect sensors<br>\n6-pin MLP/DFN package<br>\n\nExample Digikey PN 620-1031-1-ND")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "A139_HALL19" (at -1.35 -2.25 90) (layer "F.SilkS") hide)
    (fp_text value "HALL_EFFECT_ALLEGRO_A139MLP/DFN-6" (at 0 0 90) (layer "F.Fab") hide)
    (pad "P$1" smd rect (at -0.5 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/HALL19_VCC") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0 1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/HALL19_VOUT") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3_4" smd rect (at 0.5 0 90) (size 0.15 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/HALL19_GND") (pinfunction "P$3") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$5" smd rect (at 0 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/~{SLEEP19}") (pinfunction "P$5") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$6" smd rect (at -0.5 -1.475 90) (size 0.3 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/HALL19_VCC") (pinfunction "P$6") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 99.6317 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL9_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 41 "/HALL9_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 39 "/HALL9_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 40 "/HALL9_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 121 "/HALL9_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 79.8594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 129.6924 96.1644)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "DS3231MZ" (at 0 3.4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "/32KHZ") (pinfunction "32KHZ") (pintype "open_collector"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "unconnected-(U3-Pad3)") (pinfunction "~{INT}/SQW") (pintype "open_collector+no_connect"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "unconnected-(U3-Pad4)") (pinfunction "~{RST}") (pintype "bidirectional+no_connect"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/VBAT") (pinfunction "VBAT") (pintype "power_in"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "/SCL") (pinfunction "SCL") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 124.117086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.5874 123.3344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "SSOP24" (layer "F.Cu")
    (tedit 0)
    (at 142.5575 111.9761 180)
    (descr "TSSOP-24 or SSOP-24<p>\n0.65mm between pad centers, 0.348mm pad width x 1.397mm pad length<br>\n7.312mm between pad centers across body <br>(appropriate for body width of 5.03mm/0.209\")")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$2" (at -3.81 -1.27 180) (layer "F.SilkS") hide)
    (fp_text value "74HC4067SM96" (at -3.4798 0.4064) (layer "F.SilkS"))
    (pad "1" smd rect (at -3.575 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "/ANALOG_0") (pinfunction "COM") (pintype "output") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -2.925 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/HALL7_OUTPUT") (pinfunction "X7") (pintype "input") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -2.275 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/HALL6_OUTPUT") (pinfunction "X6") (pintype "input") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -1.625 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "/HALL5_OUTPUT") (pinfunction "X5") (pintype "input") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at -0.975 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "/HALL4_OUTPUT") (pinfunction "X4") (pintype "input") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at -0.325 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "/HALL3_OUTPUT") (pinfunction "X3") (pintype "input") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at 0.325 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/HALL2_OUTPUT") (pinfunction "X2") (pintype "input") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at 0.975 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "/HALL1_OUTPUT") (pinfunction "X1") (pintype "input") (solder_mask_margin 0.0762))
    (pad "9" smd rect (at 1.625 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "/HALL0_OUTPUT") (pinfunction "X0") (pintype "input") (solder_mask_margin 0.0762))
    (pad "10" smd rect (at 2.275 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "/MUX_S0") (pinfunction "S0") (pintype "input") (solder_mask_margin 0.0762))
    (pad "11" smd rect (at 2.925 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "/MUX_S1") (pinfunction "S1") (pintype "input") (solder_mask_margin 0.0762))
    (pad "12" smd rect (at 3.575 3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "13" smd rect (at 3.575 -3.656) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "/MUX_S3") (pinfunction "S3") (pintype "input") (solder_mask_margin 0.0762))
    (pad "14" smd rect (at 2.925 -3.656) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "/MUX_S2") (pinfunction "S2") (pintype "input") (solder_mask_margin 0.0762))
    (pad "15" smd rect (at 2.275 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "/MUX_~{EN}") (pinfunction "~{E}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "16" smd rect (at 1.625 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "/HALL15_OUTPUT") (pinfunction "X15") (pintype "input") (solder_mask_margin 0.0762))
    (pad "17" smd rect (at 0.975 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "/HALL14_OUTPUT") (pinfunction "X14") (pintype "input") (solder_mask_margin 0.0762))
    (pad "18" smd rect (at 0.325 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "/HALL13_OUTPUT") (pinfunction "X13") (pintype "input") (solder_mask_margin 0.0762))
    (pad "19" smd rect (at -0.325 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "/HALL12_OUTPUT") (pinfunction "X12") (pintype "input") (solder_mask_margin 0.0762))
    (pad "20" smd rect (at -0.975 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "/HALL11_OUTPUT") (pinfunction "X11") (pintype "input") (solder_mask_margin 0.0762))
    (pad "21" smd rect (at -1.625 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "/HALL10_OUTPUT") (pinfunction "X10") (pintype "input") (solder_mask_margin 0.0762))
    (pad "22" smd rect (at -2.275 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/HALL9_OUTPUT") (pinfunction "X9") (pintype "input") (solder_mask_margin 0.0762))
    (pad "23" smd rect (at -2.925 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "/HALL8_OUTPUT") (pinfunction "X8") (pintype "input") (solder_mask_margin 0.0762))
    (pad "24" smd rect (at -3.575 -3.656 180) (size 0.348 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 180.1124 91.3094)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 176.2744 123.3424)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 102.6844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 86.3221)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL3" (at -5.4951 1.317 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "/HALL3_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "/HALL3_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 110.3594 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 189.9539 106.9723 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C60" (at -1.4871 -0.9665 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.1129 -1.0665 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/HALL10_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/HALL10_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 114.973086)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 82.1344)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 170.775082 103.4594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 192.024 79.8844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 82.2198)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 114.947686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 85.3186 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 172.7835 85.5347 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R66" (at -1.5997 1.1539 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.2753 1.0789 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "/HALL16_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/~{SLEEP16}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 102.7094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 175.8315 128.3591 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C51" (at -1.457 -0.9441 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.229 -0.848 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/HALL1_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/HALL1_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 124.1094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 103.4844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "SOIC127P1032X265-16N" (layer "F.Cu")
    (tedit 63852657)
    (at 129.525 95.7 90)
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0.4754 -4.4808 90) (layer "F.SilkS"))
    (fp_text value "DS3231M+TRL" (at 6.85 6.062 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -4.655 -4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 161 "/32KHZ") (pinfunction "32KHZ") (pintype "output"))
    (pad "2" smd roundrect locked (at -4.655 -3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "3" smd roundrect locked (at -4.655 -1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 181 "unconnected-(U2-Pad3)") (pinfunction "~{NT/SQW}") (pintype "output+no_connect"))
    (pad "4" smd roundrect locked (at -4.655 -0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 182 "unconnected-(U2-Pad4)") (pinfunction "~{RST}") (pintype "bidirectional+no_connect"))
    (pad "5" smd roundrect locked (at -4.655 0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "6" smd roundrect locked (at -4.655 1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "7" smd roundrect locked (at -4.655 3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "8" smd roundrect locked (at -4.655 4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "9" smd roundrect locked (at 4.655 4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "10" smd roundrect locked (at 4.655 3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "11" smd roundrect locked (at 4.655 1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "12" smd roundrect locked (at 4.655 0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 183 "unconnected-(U2-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect locked (at 4.655 -0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect locked (at 4.655 -1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 91 "/VBAT") (pinfunction "VBAT") (pintype "power_in"))
    (pad "15" smd roundrect locked (at 4.655 -3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 154 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at 4.655 -4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 153 "/SCL") (pinfunction "SCL") (pintype "input"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 82.9094)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "1X04_LOCK" (layer "F.Cu")
    (tedit 0)
    (at 124.12 87.623)
    (descr "0.035\" drills, 0.056\" pad width<br>\nStaggered holes to help hold header in position while soldering.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "OLED" (at -2.3826 -1.7886) (layer "F.SilkS"))
    (fp_text value "PINHD-1X4LOCK" (at -5.08 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at -3.81 -0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole roundrect (at -1.27 0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole roundrect (at 1.27 -0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 153 "/SCL") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole roundrect (at 3.81 0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 154 "/SDA") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.8612 95.8594 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 88.9637 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL19_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 81 "/HALL19_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 79 "/HALL19_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 80 "/HALL19_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 143 "/HALL19_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 177.7492 127.9594 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7388 89.027 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 192.0624 102.6844)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "JST-PH-4-THM" (layer "F.Cu")
    (tedit 0)
    (at 164.7825 93.3071)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL5" (at -5.4701 1.2273 90) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "/HALL5_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "/HALL5_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "TQFP32-08" (layer "F.Cu")
    (tedit 0)
    (at 125.4125 107.9121)
    (descr "<B>Thin Plasic Quad Flat Package</B> Grid 0.8 mm")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U1" (at -3.175 -5.08) (layer "F.SilkS") hide)
    (fp_text value "ATMEGA328P" (at 2.2499 -5.5527) (layer "F.SilkS"))
    (pad "1" smd rect (at -4.2926 -2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "/BUTTON2") (pinfunction "PD3(INT1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -4.2926 -2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "/LED_RED") (pinfunction "PD4(XCK/T0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -4.2926 -1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND@1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -4.2926 -0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC@1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at -4.2926 0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND@2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at -4.2926 1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC@2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at -4.2926 2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "/32KHZ") (pinfunction "PB6(XTAL1/TOSC1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at -4.2926 2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "/PB7") (pinfunction "PB7(XTAL2/TOSC2)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "9" smd rect (at -2.8 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "/MUX_S1") (pinfunction "PD5(T1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "10" smd rect (at -2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "/MUX_S2") (pinfunction "PD6(AIN0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "11" smd rect (at -1.2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "/MUX_S3") (pinfunction "PD7(AIN1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "12" smd rect (at -0.4 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "/MUX_~{EN}") (pinfunction "PB0(ICP)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "13" smd rect (at 0.4 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "/MUX_S0") (pinfunction "PB1(OC1A)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "14" smd rect (at 1.2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "/CS_SD") (pinfunction "PB2(SS/OC1B)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "15" smd rect (at 2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "/MOSI") (pinfunction "PB3(MOSI/OC2)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "16" smd rect (at 2.8 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "/MISO") (pinfunction "PB4(MISO)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "17" smd rect (at 4.2926 2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "/SCK") (pinfunction "PB5(SCK)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "18" smd rect (at 4.2926 2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/AVCC") (pinfunction "AVCC") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "19" smd rect (at 4.2926 1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/BATT_MONITOR") (pinfunction "ADC6") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "20" smd rect (at 4.2926 0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "/AREF") (pinfunction "AREF") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "21" smd rect (at 4.2926 -0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/AGND") (pinfunction "AGND") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "22" smd rect (at 4.2926 -1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "/ANALOG_0") (pinfunction "ADC7") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "23" smd rect (at 4.2926 -2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "/BATT_MONITOR_EN") (pinfunction "PC0(ADC0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "24" smd rect (at 4.2926 -2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "/SHIFT_CLEAR") (pinfunction "PC1(ADC1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "25" smd rect (at 2.8 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/CS_SHIFT_REG") (pinfunction "PC2(ADC2)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "26" smd rect (at 2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "/LED_GRN") (pinfunction "PC3(ADC3)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "27" smd rect (at 1.2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "/SDA") (pinfunction "PC4(ADC4/SDA)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "28" smd rect (at 0.4 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "/SCL") (pinfunction "PC5(ADC5/SCL)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "29" smd rect (at -0.4 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/RESET") (pinfunction "PC6(/RESET)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "30" smd rect (at -1.2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "/TO_FTDI_TX") (pinfunction "PD0(RXD)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "31" smd rect (at -2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "/TO_FTDI_RX") (pinfunction "PD1(TXD)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "32" smd rect (at -2.8 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "/BUTTON1") (pinfunction "PD2(INT0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 195.2874 112.649)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 188.3244 80.6344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 189.9539 85.6594 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C68" (at -1.5 -1.0165 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.325 -1.0665 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/HALL18_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/HALL18_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.734682 113.423686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 176.2874 91.313)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 180.2624 101.9844)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "2X2_1.5MM" (layer "F.Cu")
    (tedit 0)
    (at 195.3895 120.9677 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL13_HEADER0" (at -1.5 -1.495 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -1.715 2.2 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 57 "/HALL13_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 0.75 -0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 55 "/HALL13_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 56 "/HALL13_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 0.75 0.75 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 133 "/HALL13_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 172.7581 106.8453 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R56" (at -1.6641 1.0293 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0859 1.0793 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "/HALL6_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/~{SLEEP6}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 172.7835 128.2321 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R51" (at -1.596 1.427 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -0.008 1.472 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "/HALL1_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/~{SLEEP1}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.9732 82.9818)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 116.8396 85.904)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R31" (at -1.2772 -1.1196) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.5978 -0.4196) (layer "F.SilkS"))
    (pad "1" smd rect (at -0.85 0) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "/BATT_MONITOR_EN") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(BJT0-Pad1)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "0603" (layer "F.Cu")
    (tedit 0)
    (at 183.0705 85.6617 90)
    (descr "0603 surface mount part")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C67" (at -1.4727 -1.0581 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.3023 -1.0581 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/HALL17_VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/HALL17_GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 104.279686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 184.846682 114.185686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 184.5124 80.6344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 173.0374 80.6344)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.762 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 187.0329 117.5387 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R62" (at -1.4707 1.1045 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0293 1.1045 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/HALL12_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/~{SLEEP12}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Mousebite_0.02in_x_0.03in_spacing" (layer "F.Cu")
    (tedit 0)
    (at 170.7896 131.7498 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -1.725 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Mousebite_0.02in_x_0.03in_spacing" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at -0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.5) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.762 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.525 0 90) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.7374 104.2594)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 191.958682 92.087686)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.508) (layers F&B.Cu *.Mask))
  )
  (footprint "R0603" (layer "F.Cu")
    (tedit 0)
    (at 172.7835 117.5387 90)
    (descr "<b>RESISTOR</b><p>\nchip 0603 size")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R52" (at -1.4182 1.0539 90) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at -0.0457 1.0539 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "/HALL2_~{SLEEP_IN}") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.85 0 90) (size 1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/~{SLEEP2}") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "SJ_2S-TRACE" (layer "B.Cu")
    (tedit 0)
    (at 133.5151 109.6393)
    (descr "Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.")
    (property "Sheetfile" "File: MusselGapeTracker_RevF.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "GROUND_CON0" (at -0.9525 1.27 180) (layer "B.SilkS") hide)
    (fp_text value "SOLDER_JUMPER_TRACESTANDARD" (at -0.9525 -1.651 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -0.508 0) (size 0.635 1.27) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.508 0) (size 0.635 1.27) (layers "B.Cu" "B.Mask")
      (net 90 "/AGND") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (gr_line (start 97.9805 133.9471) (end 199.0217 133.9471) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 97.9805 76.1621) (end 97.9805 133.9471) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 199.0217 133.9471) (end 199.0217 76.1621) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 199.0217 76.1621) (end 97.9805 76.1621) (layer "Edge.Cuts") (width 0.05))
  (gr_text "VCC" (at 167.7035 81.3691 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 189.9031 133.0327 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 88.4811 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.4475 125.6921 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.6395 81.3691 -90) (layer "B.SilkS"))
  (gr_text "SCK" (at 129.0955 115.4051) (layer "B.SilkS"))
  (gr_text "SLP" (at 186.6519 108.7757 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 172.4025 119.4437 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 179.4637 110.3251 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 169.1005 100.1651 -90) (layer "B.SilkS"))
  (gr_text "BUTTON1" (at 104.2035 109.1821) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.4155 102.0701 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 81.2421 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 128.7401 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 102.1971 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 118.7071 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 189.9793 88.6589 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 186.7281 132.0421 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 181.0131 82.4613) (layer "B.SilkS"))
  (gr_text "MOSI" (at 128.9685 121.8821) (layer "B.SilkS"))
  (gr_text "RX" (at 99.3775 90.8941 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 99.3775 100.4191 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 189.9031 111.4427 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 193.6877 120.9931 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 173.9265 82.4613) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 128.6131 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 197.1167 111.4427 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.8615 111.7221 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 179.4891 89.1161 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 193.7385 98.1077 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 172.4025 98.1077 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 173.9265 125.1841) (layer "B.SilkS"))
  (gr_text "GND" (at 189.9031 122.1107 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 189.9539 120.7391 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 189.9539 110.0711 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 88.4811 -90) (layer "B.SilkS"))
  (gr_text "HALL13" (at 167.5765 122.2885) (layer "B.SilkS"))
  (gr_text "-" (at 122.6024 79.2444 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 81.3691 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 95.2121 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 174.0535 114.4907) (layer "B.SilkS"))
  (gr_text "SLP" (at 172.3771 108.6233 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 118.5801 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 186.6519 130.2387 -90) (layer "B.SilkS"))
  (gr_text "HALL14" (at 155.1305 132.6771) (layer "B.SilkS"))
  (gr_text "SLP" (at 172.4025 87.3127 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 175.7045 90.2337 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 189.9539 99.4031 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 102.1971 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 179.5145 119.4437 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 197.0659 88.5827 -90) (layer "B.SilkS"))
  (gr_text "HALL8" (at 154.7495 108.6741) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 181.1655 114.4907) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 111.8491 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 111.9761 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 186.6519 98.1077 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 182.7657 132.9311 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 128.6131 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.6075 81.3691 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 175.7045 120.8661 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 99.3775 97.7521 -90) (layer "B.SilkS"))
  (gr_text "POWER" (at 120.1124 77.2594 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 111.8491 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 172.3517 131.9405 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 175.6537 122.2377 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 121.2596 89.7594) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 188.3029 93.1547) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 88.2271 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 125.6921 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 111.9761 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 88.3541 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.6385 118.7071 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 182.8165 90.2337 -90) (layer "B.SilkS"))
  (gr_text "MISO" (at 132.1435 115.4051) (layer "B.SilkS"))
  (gr_text "VOUT" (at 197.0405 131.5341 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 128.6131 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 102.5525 116.9291) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 95.0851 -90) (layer "B.SilkS"))
  (gr_text "BUTTON2" (at 104.3305 114.2621) (layer "B.SilkS"))
  (gr_text "VOUT" (at 182.8165 99.5301 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 175.7045 99.4031 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 188.1759 82.4359) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 118.7071 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 128.7401 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 193.6877 110.4521 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 111.9761 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 118.7071 -90) (layer "B.SilkS"))
  (gr_text "HALL6" (at 154.3685 98.8951) (layer "B.SilkS"))
  (gr_text "VOUT" (at 182.8165 131.5595 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 193.7385 119.4437 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 102.1971 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 193.7385 108.7757 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 102.0701 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 195.5165 125.1587) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 95.2121 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 175.6283 111.2903 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 81.3691 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 182.7657 122.2377 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 102.1971 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 81.2421 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 182.8419 88.6843 -90) (layer "B.SilkS"))
  (gr_text "HALL10" (at 154.1145 115.0241) (layer "B.SilkS"))
  (gr_text "SLP" (at 193.7385 130.1117 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 193.7639 89.1415 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 175.7045 131.4325 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 111.9761 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 197.0405 120.7391 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 179.5399 87.4397 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 193.6877 131.7881 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 188.4299 103.8227) (layer "B.SilkS"))
  (gr_text "RST" (at 123.1011 118.1991 -90) (layer "B.SilkS"))
  (gr_text "millerlp@gmail.com" (at 102.6033 95.6185 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 111.9761 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.6715 125.6921 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 179.5145 108.7757 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 175.6537 100.9017 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 195.2625 103.8227) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 195.3387 82.4613) (layer "B.SilkS"))
  (gr_text "VCC" (at 186.6011 121.1201 -90) (layer "B.SilkS"))
  (gr_text "HALL15" (at 167.4495 132.6771) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 128.7401 -90) (layer "B.SilkS"))
  (gr_text "+" (at 122.7874 78.6094) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 88.4811 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 179.5145 130.1371 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 182.7657 100.9017 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 195.6435 114.4907) (layer "B.SilkS"))
  (gr_text "VOUT" (at 189.9539 131.6611 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 125.6921 -90) (layer "B.SilkS"))
  (gr_text "HALL11" (at 167.5765 115.2781) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 118.7071 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.6385 102.0701 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 195.2625 93.1547) (layer "B.SilkS"))
  (gr_text "HALL5" (at 167.1955 91.9101) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 95.2121 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 186.6773 87.4143 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 186.7027 89.1415 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 188.3029 125.2857) (layer "B.SilkS"))
  (gr_text "VCC" (at 123.7742 89.7094) (layer "B.SilkS"))
  (gr_text "HALL2" (at 154.8765 84.9251) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 125.5651 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 88.3541 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 197.0405 110.0711 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 182.8927 111.4427 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 173.9011 103.7973) (layer "B.SilkS"))
  (gr_text "HALL9" (at 166.8145 108.6741) (layer "B.SilkS"))
  (gr_text "GND" (at 99.3775 103.2131 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 179.4637 99.7841 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 193.7639 87.4397 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 123.8885 121.8567 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 125.5651 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 132.0165 121.3741 -90) (layer "B.SilkS"))
  (gr_text "TX" (at 108.0135 93.6881 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 196.9897 100.7747 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 128.7401 -90) (layer "B.SilkS"))
  (gr_text "TX" (at 99.3775 93.4341 -90) (layer "B.SilkS"))
  (gr_text "SCL" (at 126.3124 89.6344) (layer "B.SilkS"))
  (gr_text "VCC" (at 186.7281 110.4521 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 182.8165 120.8661 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 102.5525 111.7221) (layer "B.SilkS"))
  (gr_text "HALL7" (at 167.1955 98.8951) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.8305 88.3541 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 172.4533 110.4267 -90) (layer "B.SilkS"))
  (gr_text "RX" (at 108.2675 91.0211 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 118.5801 -90) (layer "B.SilkS"))
  (gr_text "Mussel\nGape\nTracker\nRev F" (at 104.7115 122.1361) (layer "B.SilkS"))
  (gr_text "GND" (at 128.4605 133.5661) (layer "B.SilkS"))
  (gr_text "VCC" (at 179.4637 131.9405 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 95.2121 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 186.7281 99.7841 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 172.4787 121.2471 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 193.6877 99.6571 -90) (layer "B.SilkS"))
  (gr_text "HALL12" (at 154.2161 122.2377) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 181.1655 125.1841) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 95.2121 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 125.5651 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 95.0851 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 182.8165 109.9441 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 196.9897 132.9057 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.6395 118.7071 -90) (layer "B.SilkS"))
  (gr_text "DTR" (at 99.3775 88.1001 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 95.2121 -90) (layer "B.SilkS"))
  (gr_text "VOUT" (at 175.6791 109.9187 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 181.4195 103.8227) (layer "B.SilkS"))
  (gr_text "VCC" (at 172.4025 89.1923 -90) (layer "B.SilkS"))
  (gr_text "HALL0" (at 154.8765 77.8131) (layer "B.SilkS"))
  (gr_text "GND" (at 197.0405 90.1829 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 188.3029 114.4907) (layer "B.SilkS"))
  (gr_text "GND" (at 196.9897 122.1107 -90) (layer "B.SilkS"))
  (gr_text "SDA" (at 128.8124 89.6594) (layer "B.SilkS"))
  (gr_text "RESET" (at 135.0645 133.5661) (layer "B.SilkS"))
  (gr_text "L P MILLER\n2023" (at 104.7115 127.9781) (layer "B.SilkS"))
  (gr_text "HALL3" (at 167.3225 84.9251) (layer "B.SilkS"))
  (gr_text "SLP" (at 172.4025 130.1371 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 179.5145 98.1077 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 172.3517 99.9111 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 189.9793 90.2337 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 175.6537 132.8041 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 128.7401 -90) (layer "B.SilkS"))
  (gr_text "HALL4" (at 153.8605 91.6561) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 81.3691 -90) (layer "B.SilkS"))
  (gr_text "HALL1" (at 166.9415 77.9401) (layer "B.SilkS"))
  (gr_text "VOUT" (at 175.7299 88.6081 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 88.3541 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 186.6519 119.4437 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 179.4637 121.1201 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 180.9115 93.1547) (layer "B.SilkS"))
  (gr_text "VOUT" (at 197.0405 99.4031 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 125.5651 -90) (layer "B.SilkS"))
  (gr_text "HALL\nEFFECT\nA139x" (at 173.9265 93.1547) (layer "B.SilkS"))
  (gr_text "GND" (at 189.9031 100.7747 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 121.7676 89.7594) (layer "F.SilkS"))
  (gr_text "VCC" (at 172.4533 101.0033 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 172.4279 133.0073 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 186.6519 88.5065 90) (layer "F.SilkS"))
  (gr_text "GND" (at 197.5485 111.4427 90) (layer "F.SilkS"))
  (gr_text "GND" (at 183.3245 111.4427 90) (layer "F.SilkS"))
  (gr_text "SDA" (at 128.9124 89.0094) (layer "F.SilkS"))
  (gr_text "VCC" (at 186.7027 111.5443 90) (layer "F.SilkS"))
  (gr_text "GRN" (at 114.1124 99.2761) (layer "F.SilkS"))
  (gr_text "GND" (at 197.4469 90.1575 90) (layer "F.SilkS"))
  (gr_text "+" (at 113.2205 100.1651) (layer "F.SilkS"))
  (gr_text "HALL10" (at 147.3835 118.6594 90) (layer "F.SilkS"))
  (gr_text "GND" (at 107.3023 100.8001 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 179.5653 88.5319 90) (layer "F.SilkS"))
  (gr_text "10k " (at 181.1124 117.1844 90) (layer "F.SilkS"))
  (gr_text "VREG" (at 115.189 80.4926) (layer "F.SilkS"))
  (gr_text "VOUT" (at 176.1363 88.6335 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 186.6773 110.0457 90) (layer "F.SilkS"))
  (gr_text "GND" (at 100.0374 115.9131) (layer "F.SilkS"))
  (gr_text "HALL7" (at 162.9624 103.6094) (layer "F.SilkS"))
  (gr_text "VCC" (at 186.7027 100.8763 90) (layer "F.SilkS"))
  (gr_text "RST" (at 123.8631 118.1991 90) (layer "F.SilkS"))
  (gr_text "POWER" (at 130.5374 80.9844 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 197.4215 120.7137 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 179.5145 122.2377 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 172.4279 99.3777 90) (layer "F.SilkS"))
  (gr_text "°" (at 125.7624 94.3344) (layer "F.SilkS"))
  (gr_text "SLP" (at 193.7385 99.3777 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 172.4279 111.5189 90) (layer "F.SilkS"))
  (gr_text "New Molex \nmicroSD\n502774-0891" (at 108.2675 125.5651 90) (layer "F.SilkS"))
  (gr_text "CR1220" (at 134.6835 77.5591) (layer "F.SilkS"))
  (gr_text "VCC" (at 193.7385 122.1107 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 193.7385 109.9187 90) (layer "F.SilkS"))
  (gr_text "100k Ω" (at 123.7361 125.6413 90) (layer "F.SilkS"))
  (gr_text "GND" (at 108.1405 98.3871 90) (layer "F.SilkS"))
  (gr_text "RED" (at 114.0124 97.4981) (layer "F.SilkS"))
  (gr_text "GND" (at 176.1109 100.9271 90) (layer "F.SilkS"))
  (gr_text "AGND" (at 144.0815 132.6771 90) (layer "F.SilkS"))
  (gr_text "GND" (at 197.4215 100.7747 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 172.4279 90.2845 90) (layer "F.SilkS"))
  (gr_text "HALL4" (at 147.3835 93.8151 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 186.6773 90.2337 90) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 119.0625 106.3881) (layer "F.SilkS"))
  (gr_text "10k" (at 121.3824 98.5344) (layer "F.SilkS"))
  (gr_text "AREF" (at 130.9624 87.0094) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 120.4624 126.1844 90) (layer "F.SilkS"))
  (gr_text "GND" (at 176.0347 132.8041 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 197.4723 88.5827 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 186.7027 122.2123 90) (layer "F.SilkS"))
  (gr_text "GND" (at 121.285 89.0844) (layer "F.SilkS"))
  (gr_text "GND" (at 190.3603 111.4681 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 190.3349 110.0711 90) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 182.0545 128.1051 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 179.5145 99.3777 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 179.5145 100.9017 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 197.5485 110.0457 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 176.0601 109.9187 90) (layer "F.SilkS"))
  (gr_text "GND" (at 183.1975 100.9017 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 183.1975 99.5047 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 179.5399 90.2083 90) (layer "F.SilkS"))
  (gr_text "GND" (at 126.4285 133.5661) (layer "F.SilkS"))
  (gr_text "SLP" (at 172.4279 131.4579 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 193.7893 90.2337 90) (layer "F.SilkS"))
  (gr_text "MISO" (at 129.6035 115.4051) (layer "F.SilkS"))
  (gr_text "100Ω" (at 115.4874 103.0344) (layer "F.SilkS"))
  (gr_text "VCC" (at 179.5145 133.0581 90) (layer "F.SilkS"))
  (gr_text "GND" (at 190.3603 100.8001 90) (layer "F.SilkS"))
  (gr_text "10k" (at 115.1374 98.6844) (layer "F.SilkS"))
  (gr_text "HALL0" (at 147.2565 80.9881 90) (layer "F.SilkS"))
  (gr_text "HALL14" (at 147.3374 132.2344 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 179.5145 131.4071 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 179.5145 111.4427 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 183.3245 109.9187 90) (layer "F.SilkS"))
  (gr_text "°" (at 124.206 100.8634) (layer "F.SilkS"))
  (gr_text "GND" (at 190.3124 133.0344 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 172.4533 122.3393 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 126.4624 89.0094) (layer "F.SilkS"))
  (gr_text "GND" (at 183.2229 90.2337 90) (layer "F.SilkS"))
  (gr_text "4.7k" (at 117.2972 98.7044) (layer "F.SilkS"))
  (gr_text "VOUT" (at 197.4215 99.3777 90) (layer "F.SilkS"))
  (gr_text "GND" (at 197.4215 132.9057 90) (layer "F.SilkS"))
  (gr_text "Mussel\nGape\nTracker\nRev F" (at 118.8374 120.4844) (layer "F.SilkS"))
  (gr_text "B1" (at 100.3874 109.7094) (layer "F.SilkS"))
  (gr_text "FTDI 3.3V ONLY!" (at 109.1057 101.7399 90) (layer "F.SilkS"))
  (gr_text "+" (at 127.0624 78.4094) (layer "F.SilkS"))
  (gr_text "GND" (at 190.3857 90.2591 90) (layer "F.SilkS"))
  (gr_text "ICSP\nHEADER" (at 124.1124 114.5344) (layer "F.SilkS"))
  (gr_text "SLP" (at 179.5145 109.7917 90) (layer "F.SilkS"))
  (gr_text "GND" (at 176.1109 90.2337 90) (layer "F.SilkS"))
  (gr_text "GND" (at 183.1975 122.2377 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 186.6773 131.6357 90) (layer "F.SilkS"))
  (gr_text "-" (at 128.8288 81.534 90) (layer "F.SilkS"))
  (gr_text "DTR" (at 107.9374 91.5344 90) (layer "F.SilkS"))
  (gr_text "RX" (at 107.9874 93.0594 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 193.7385 111.5697 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 190.3349 99.4031 90) (layer "F.SilkS"))
  (gr_text "LP MILLER\n2023" (at 117.2874 114.8344) (layer "F.SilkS"))
  (gr_text "SLP" (at 193.7385 131.5087 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 172.4025 88.4557 90) (layer "F.SilkS"))
  (gr_text "ADC7" (at 130.6374 105.8094) (layer "F.SilkS"))
  (gr_text "HALL15" (at 162.1155 133.6931) (layer "F.SilkS"))
  (gr_text "VCC" (at 193.7385 132.9057 90) (layer "F.SilkS"))
  (gr_text "1" (at 107.4928 107.7468 90) (layer "F.SilkS"))
  (gr_text "100Ω" (at 118.1608 103.0986) (layer "F.SilkS"))
  (gr_text "VCC" (at 193.7385 100.7747 90) (layer "F.SilkS"))
  (gr_text "HALL14" (at 150.0505 133.6931) (layer "F.SilkS"))
  (gr_text "RTC" (at 128.7018 95.758) (layer "F.SilkS"))
  (gr_text "SLP" (at 193.7385 120.7137 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 183.1975 120.8407 90) (layer "F.SilkS"))
  (gr_text "2" (at 110.6874 116.1344 90) (layer "F.SilkS"))
  (gr_text "HALL6" (at 150.4874 103.4094) (layer "F.SilkS"))
  (gr_text "VOUT" (at 190.4111 88.6335 90) (layer "F.SilkS"))
  (gr_text "GND" (at 190.3603 122.1361 90) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 112.141 93.98) (layer "F.SilkS"))
  (gr_text "TX" (at 108.1405 95.0851 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 132.7785 121.3741 90) (layer "F.SilkS"))
  (gr_text "B2" (at 100.3124 114.6344) (layer "F.SilkS"))
  (gr_text "+" (at 113.2205 98.2601) (layer "F.SilkS"))
  (gr_text "100k Ω" (at 123.6345 131.4594 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 183.1975 131.5341 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 197.4215 131.5087 90) (layer "F.SilkS"))
  (gr_text "I2C HEADER" (at 124.9426 86.0806) (layer "F.SilkS"))
  (gr_text "VCC" (at 186.7027 133.1343 90) (layer "F.SilkS"))
  (gr_text "GND" (at 100.2665 111.0094) (layer "F.SilkS"))
  (gr_text "RESET" (at 131.6355 133.5661) (layer "F.SilkS"))
  (gr_text "HALL9" (at 162.8874 106.2844) (layer "F.SilkS"))
  (gr_text "VCC" (at 108.1405 95.7201 90) (layer "F.SilkS"))
  (gr_text "4.7k" (at 119.2724 98.7044) (layer "F.SilkS"))
  (gr_text "10k " (at 181.2925 127.8511 90) (layer "F.SilkS"))
  (gr_text "SCK" (at 126.9365 115.4051) (layer "F.SilkS"))
  (gr_text "VOUT" (at 176.0855 120.8661 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 176.0601 131.4579 90) (layer "F.SilkS"))
  (gr_text "HALL2" (at 147.2565 89.1094 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 183.2483 88.6335 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 179.5145 120.7137 90) (layer "F.SilkS"))
  (gr_text "HALL8" (at 150.4624 106.6344) (layer "F.SilkS"))
  (gr_text "GND" (at 123.9393 121.8821 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 172.4279 120.7137 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 172.4025 109.8933 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 190.3349 120.7391 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 193.7639 88.5573 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 190.3349 131.6611 90) (layer "F.SilkS"))
  (gr_text "GND" (at 183.1975 132.9311 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 186.6773 120.7137 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 186.6773 99.3777 90) (layer "F.SilkS"))
  (gr_text "GND" (at 176.0855 111.3157 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 176.0855 99.5301 90) (layer "F.SilkS"))
  (gr_text "GND" (at 197.4215 122.1107 90) (layer "F.SilkS"))
  (gr_text "GND" (at 176.1109 122.2631 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.0889) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2278) (thermal_bridge_width 0.2278))
    (polygon
      (pts
        (xy 142.5194 106.096)
        (xy 133.6294 106.096)
        (xy 133.6294 116.0782)
        (xy 142.5194 116.0782)
        (xy 142.5194 132.5882)
        (xy 143.7894 132.5882)
        (xy 143.7894 134.036)
        (xy 97.8916 134.036)
        (xy 97.8916 76.0732)
        (xy 142.5194 76.0732)
      )
    )
  )
  (zone (net 90) (net_name "/AGND") (layer "B.Cu") (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.0889) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2278) (thermal_bridge_width 0.2278))
    (polygon
      (pts
        (xy 170.4594 134.036)
        (xy 144.8816 134.036)
        (xy 144.8816 113.716)
        (xy 134.7216 113.716)
        (xy 134.7216 107.1882)
        (xy 143.6116 107.1882)
        (xy 143.6116 76.0732)
        (xy 170.4594 76.0732)
      )
    )
  )
)
