(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 29)
    (no_connects 0)
    (area 62.711667 90.01 131.176429 146.965333)
    (thickness 1.6)
    (drawings 88)
    (tracks 57)
    (zones 0)
    (modules 17)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2.5)
    (trace_clearance 0.4)
    (zone_clearance 1)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.52)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 147.955 86.36)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x010ff_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/v2/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad3)")
  (net 2 "Net-(F1-Pad1)")
  (net 3 GND)
  (net 4 VCC)
  (net 5 /PHASE1_OUT)
  (net 6 /PHASE)
  (net 7 /ZERO)
  (net 8 /EN1)
  (net 9 "Net-(R2-Pad2)")
  (net 10 "Net-(C1-Pad1)")
  (net 11 "Net-(R5-Pad2)")
  (net 12 "Net-(R6-Pad2)")
  (net 13 /ZC)
  (net 14 "Net-(J5-Pad5)")
  (net_class Default "Это класс цепей по умолчанию."
    (clearance 0.4)
    (trace_width 2.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /EN1)
    (add_net /PHASE)
    (add_net /PHASE1_OUT)
    (add_net /ZC)
    (add_net /ZERO)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net VCC)
  )
  (module .pretty:bornier2_2 (layer F.Cu) (tedit 59647C21)
    (at 75.6285 101.5365)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference J1 (at 2.54 -5.08) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_1x02 (at 2.54 5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 2 2) (drill 1.52) (layers *.Cu *.Mask)
      (net 7 /ZERO))
    (model Connectors.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:HLK-PM12 (layer F.Cu) (tedit 596493FB)
    (at 89.535 106.045 270)
    (fp_text reference U1 (at 18 -2 270) (layer F.SilkS) hide)
    (fp_text value HI-LINKPM12 (at 18 -4 270) (layer F.Fab))
    (fp_text user +Vo (at 29 18 270) (layer F.SilkS))
    (fp_text user -Vo (at 29 3 270) (layer F.SilkS))
    (fp_text user AC (at 2.159 14.732 270) (layer F.SilkS))
    (fp_text user AC (at 2.159 5.08 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.3 7.5 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /PHASE))
    (pad 2 thru_hole circle (at 2.3 12.5 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /ZERO))
    (pad 3 thru_hole circle (at 31.7 2.3 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 31.7 17.7 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:C_Rect_L13.5mm_W5.0mm_P10.00mm_FKS3_FKP3_MKS4 (layer F.Cu) (tedit 596487EC)
    (at 93.091 115.316 70)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13.5*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13.5mm width 5mm Capacitor")
    (fp_text reference C1 (at 5 -3.56 70) (layer F.SilkS) hide)
    (fp_text value 0.1u (at 5 3.56 70) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 70) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 70) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /PHASE1_OUT))
    (model Capacitors_THT.3dshapes/C_Rect_L13.5mm_W5.0mm_P10.00mm_FKS3_FKP3_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:TO-220_Horizontal_2 (layer B.Cu) (tedit 59635FD8)
    (at 98.171 120.904 270)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (fp_text reference D1 (at 2.54 20.58 270) (layer B.SilkS) hide)
    (fp_text value BT137-600 (at 2.54 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 2.54 20.58 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 /PHASE1_OUT))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad3)"))
    (pad 2 smd circle (at 2.55 16.65 270) (size 3.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /PHASE))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59635FDD)
    (at 80.899 135.636 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value 360 (at 0 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 /EN1))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J5-Pad5)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59635F83)
    (at 88.519 130.048)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 360 (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 1.85) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /PHASE))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 59635FE1)
    (at 93.091 137.668 90)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.39 90) (layer F.SilkS) hide)
    (fp_text value MOC3063M (at 3.81 7.47 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /EN1))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:bornier2_2 (layer F.Cu) (tedit 59647C28)
    (at 85.725 101.5365)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference J2 (at 2.54 -5.08) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_1x02 (at 2.54 5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.52) (layers *.Cu *.Mask)
      (net 7 /ZERO))
    (pad 2 thru_hole circle (at 5.08 0) (size 2 2) (drill 1.52) (layers *.Cu *.Mask)
      (net 5 /PHASE1_OUT))
    (model Connectors.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59647EC2)
    (at 92.456 123.2154 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value 360 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /PHASE1_OUT))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 596487F4)
    (at 68.7705 118.999 225)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 1.85 225) (layer B.SilkS) hide)
    (fp_text value 68k (at 0 -1.9 225) (layer B.Fab))
    (fp_text user %R (at 0 1.85 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 225) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 7 /ZERO))
    (pad 2 smd rect (at 2 0 225) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 596487F1)
    (at 74.803 122.2375 225)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 1.850001 225) (layer B.SilkS) hide)
    (fp_text value 68k (at 0 -1.9 225) (layer B.Fab))
    (fp_text user %R (at 0 1.850001 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 225) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /PHASE))
    (pad 2 smd rect (at 2 0 225) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm_SMD (layer B.Cu) (tedit 59649407)
    (at 69.469 130.048 270)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil SMD")
    (attr smd)
    (fp_text reference U3 (at 0 3.66 270) (layer B.SilkS) hide)
    (fp_text value LTV-814 (at 0 -3.66 270) (layer B.Fab))
    (pad 1 smd rect (at -3.81 1.27 270) (size 2 1.78) (layers B.Cu B.Mask)
      (net 11 "Net-(R5-Pad2)"))
    (pad 3 smd rect (at 3.81 -1.27 270) (size 2 1.78) (layers B.Cu B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -3.81 -1.27 270) (size 2 1.78) (layers B.Cu B.Mask)
      (net 12 "Net-(R6-Pad2)"))
    (pad 4 smd rect (at 3.81 1.27 270) (size 2 1.78) (layers B.Cu B.Mask)
      (net 13 /ZC))
    (model Housings_DIP.3dshapes/DIP-4_W7.62mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm_2 (layer B.Cu) (tedit 59649401)
    (at 68.58 110.49)
    (descr "Fuseholder, 5x20, Semi closed, horizontal, Casing 10x25mm,")
    (tags "Fuseholder 5x20 Semi closed horizontal Casing 10x25mm Sicherungshalter halbgeschlossen ")
    (fp_text reference F1 (at 11 7.62) (layer B.SilkS) hide)
    (fp_text value Fuse (at 12.27 -7.62) (layer B.Fab))
    (pad 2 thru_hole oval (at 22 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 /PHASE))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59647EC8)
    (at 88.4555 116.9035 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value 39 (at 0 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /PHASE))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 75.311 141.732 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J5 (at 0 -2.39 90) (layer F.SilkS))
    (fp_text value CONN_01X07 (at 0 17.63 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:LOGO_SILK (layer F.Cu) (tedit 595F8ADD)
    (at 79.883 123.444 90)
    (fp_text reference G*** (at 0.4 -8.1 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.2 -10.8 90) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 596490E6)
    (at 67.945 136.906)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 0 -2.39) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.39) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ZC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 68.961 114.046) (end 74.295 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.041 108.458) (end 68.707 113.792) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.707 113.792) (end 68.961 114.046) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.295 108.712) (end 74.041 108.458) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.851 100.584) (end 77.851 102.616) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.851 100.584) (end 76.835 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.835 99.568) (end 77.343 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.343 99.568) (end 77.851 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.851 100.076) (end 78.359 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.359 100.076) (end 78.867 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.867 99.568) (end 79.375 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.375 99.568) (end 78.359 100.584) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.359 102.616) (end 78.359 100.584) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.851 103.124) (end 78.359 102.616) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.851 102.616) (end 76.835 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.835 103.632) (end 77.343 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.343 103.632) (end 77.851 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.03492 97.47854) (end 93.47878 97.47854) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.04254 97.47854) (end 72.59868 97.47854) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 83.04 120.19) (end 100.71767 102.51233) (angle -20.30710659) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 83.04 120.19) (end 72.59614 97.476) (angle -20.30710659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.297 119.634) (end 90.551 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.297 120.904) (end 90.297 119.634) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.043 120.904) (end 90.297 120.904) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.043 119.38) (end 90.043 120.904) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.551 118.872) (end 90.043 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.805 118.872) (end 90.551 118.872) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.631 118.872) (end 90.805 118.872) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.631 119.126) (end 95.631 118.872) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.805 119.126) (end 95.631 119.126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.551 119.38) (end 90.805 119.126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.469 122.682) (end 69.723 122.936) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.057 117.094) (end 69.469 122.682) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.311 117.348) (end 75.057 117.094) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.695 123.698) (end 99.695 123.444) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.139 123.444) (end 99.695 123.444) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.139 123.698) (end 96.139 123.444) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.723 122.936) (end 70.231 122.428) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.231 122.428) (end 75.311 117.348) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.043 132.588) (end 87.503 132.588) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.551 133.096) (end 90.043 132.588) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.503 133.096) (end 90.551 133.096) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.551 114.808) (end 90.043 114.808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.107 111.252) (end 90.551 114.808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.107 110.744) (end 94.107 111.252) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.043 114.808) (end 94.107 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.091 106.172) (end 93.091 105.664) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.139 109.22) (end 93.091 106.172) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.139 108.712) (end 96.139 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.091 105.664) (end 96.139 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.391 105.664) (end 79.375 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.899 105.664) (end 80.391 105.664) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.883 106.68) (end 80.899 105.664) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.883 109.22) (end 79.883 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.359 110.744) (end 79.883 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.851 110.744) (end 78.359 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.375 109.22) (end 77.851 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.375 106.68) (end 79.375 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.139 123.698) (end 99.695 123.698) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.503 133.096) (end 83.947 133.096) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.947 132.588) (end 87.503 132.588) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.423 131.572) (end 82.423 131.064) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.947 133.096) (end 82.423 131.572) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.423 131.064) (end 83.947 132.588) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.011 102.616) (end 88.011 100.584) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.995 103.632) (end 88.011 102.616) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.503 103.632) (end 86.995 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.011 103.124) (end 87.503 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.519 103.124) (end 88.011 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.027 103.632) (end 88.519 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.535 103.632) (end 89.027 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.519 102.616) (end 89.535 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.519 100.584) (end 88.519 102.616) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.535 99.568) (end 88.519 100.584) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.027 99.568) (end 89.535 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.519 100.076) (end 89.027 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.011 100.076) (end 88.519 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.503 99.568) (end 88.011 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.995 99.568) (end 87.503 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.011 100.584) (end 86.995 99.568) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text HOT (at 94.615 101.092 90) (layer F.SilkS))
  (gr_text HOT (at 71.755 101.092 90) (layer F.SilkS))
  (dimension 50 (width 0.3) (layer Margin)
    (gr_text "50,000 мм" (at 125.105 119.96 270) (layer Margin))
    (feature1 (pts (xy 83.555 144.96) (xy 126.455 144.96)))
    (feature2 (pts (xy 83.555 94.96) (xy 126.455 94.96)))
    (crossbar (pts (xy 123.755 94.96) (xy 123.755 144.96)))
    (arrow1a (pts (xy 123.755 144.96) (xy 123.168579 143.833496)))
    (arrow1b (pts (xy 123.755 144.96) (xy 124.341421 143.833496)))
    (arrow2a (pts (xy 123.755 94.96) (xy 123.168579 96.086504)))
    (arrow2b (pts (xy 123.755 94.96) (xy 124.341421 96.086504)))
  )
  (dimension 17.78 (width 0.3) (layer Margin)
    (gr_text "17,780 мм" (at 92.075 91.36) (layer Margin))
    (feature1 (pts (xy 100.965 110.49) (xy 100.965 90.01)))
    (feature2 (pts (xy 83.185 110.49) (xy 83.185 90.01)))
    (crossbar (pts (xy 83.185 92.71) (xy 100.965 92.71)))
    (arrow1a (pts (xy 100.965 92.71) (xy 99.838496 93.296421)))
    (arrow1b (pts (xy 100.965 92.71) (xy 99.838496 92.123579)))
    (arrow2a (pts (xy 83.185 92.71) (xy 84.311504 93.296421)))
    (arrow2b (pts (xy 83.185 92.71) (xy 84.311504 92.123579)))
  )
  (dimension 17.78 (width 0.3) (layer Margin)
    (gr_text "17,780 мм" (at 74.295 91.36) (layer Margin))
    (feature1 (pts (xy 65.405 110.49) (xy 65.405 90.01)))
    (feature2 (pts (xy 83.185 110.49) (xy 83.185 90.01)))
    (crossbar (pts (xy 83.185 92.71) (xy 65.405 92.71)))
    (arrow1a (pts (xy 65.405 92.71) (xy 66.531504 92.123579)))
    (arrow1b (pts (xy 65.405 92.71) (xy 66.531504 93.296421)))
    (arrow2a (pts (xy 83.185 92.71) (xy 82.058496 92.123579)))
    (arrow2b (pts (xy 83.185 92.71) (xy 82.058496 93.296421)))
  )
  (gr_line (start 65.36233 137.86767) (end 65.36233 102.51233) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.71767 102.51233) (end 100.71767 137.86767) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 83.04 120.19) (end 65.36233 137.86767) (angle -90) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 72.771 131.064) (xy 73.787 132.08) (xy 81.915 132.08) (xy 83.439 133.604) (xy 100.711 133.604)
        (xy 100.711 145.288) (xy 65.151 145.288) (xy 65.151 131.064) (xy 69.723 131.064)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 69.977 136.144) (xy 69.977 144.78) (xy 82.169 144.78) (xy 82.169 139.446) (xy 76.835 139.446)
        (xy 76.835 136.144) (xy 76.327 136.144)
      )
    )
  )
  (zone (net 6) (net_name /PHASE) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 1))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.09 119.761) (xy 85.09 120.523) (xy 88.519 120.523) (xy 88.519 126.238) (xy 84.963 126.238)
        (xy 84.963 126.873) (xy 83.439 128.397) (xy 78.613 128.397) (xy 78.613 118.364) (xy 83.693 118.364)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Paste) (hatch edge 0.508)
    (connect_pads yes (clearance 3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.09 119.761) (xy 85.09 120.523) (xy 88.519 120.523) (xy 88.519 126.238) (xy 84.963 126.238)
        (xy 84.963 126.873) (xy 83.439 128.397) (xy 78.613 128.397) (xy 78.613 118.364) (xy 83.693 118.364)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.613 118.364) (xy 83.693 118.364) (xy 84.963 119.634) (xy 84.963 120.523) (xy 88.519 120.523)
        (xy 88.519 126.238) (xy 84.963 126.238) (xy 84.963 126.873) (xy 83.439 128.397) (xy 78.613 128.397)
      )
    )
  )
)
