<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<board>
<plain>
<wire x1="19.68" y1="26.82" x2="1.679996875" y2="21.819996875" width="0.001" layer="20" curve="211.048236"/>
<wire x1="1.68" y1="21.82" x2="19.68" y2="-3.18" width="0.001" layer="20"/>
<wire x1="37.68" y1="21.82" x2="19.68" y2="-3.18" width="0.001" layer="20"/>
<wire x1="37.68" y1="21.82" x2="19.68" y2="26.82" width="0.001" layer="20" curve="211.048186"/>
<text>"Love Heart" 
By Eric Navarrete</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LED3535">
</package>
<package name="1X2-3.5MM">
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="adafruit" package="R0805" value="470"/>
<element name="LED17" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="LED18" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="LED19" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="LED20" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="LED21" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="LED22" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="LED23" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="LED24" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="DIP08" value="TINY85-20-DIP">
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="J1" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM"/>
<element name="C1" library="adafruit" package="C0805" value="0.1uf"/>
<element name="C2" library="adafruit" package="C0805" value="0.1uf"/>
<element name="C3" library="adafruit" package="C0805" value="0.1uf"/>
<element name="C4" library="adafruit" package="C0805" value="0.1uf"/>
<element name="LED2" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0805" value="0.1uf"/>
</elements>
<signals>
<signal name="GND">
<contactref element="LED19" pad="4"/>
<contactref element="LED20" pad="4"/>
<contactref element="LED21" pad="4"/>
<contactref element="LED22" pad="4"/>
<contactref element="LED23" pad="4"/>
<contactref element="LED24" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="LED18" pad="4"/>
<contactref element="LED17" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="LED2" pad="4"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="LED18" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED18" pad="3"/>
<contactref element="LED17" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED17" pad="3"/>
<contactref element="LED19" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="LED19" pad="3"/>
<contactref element="LED20" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="LED20" pad="3"/>
<contactref element="LED21" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LED21" pad="3"/>
<contactref element="LED22" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="LED22" pad="3"/>
<contactref element="LED23" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="LED23" pad="3"/>
<contactref element="LED24" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="LED18" pad="2"/>
<contactref element="LED17" pad="2"/>
<contactref element="LED19" pad="2"/>
<contactref element="LED20" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="LED21" pad="2"/>
<contactref element="LED22" pad="2"/>
<contactref element="LED23" pad="2"/>
<contactref element="LED24" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="LED2" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="LED24" pad="3"/>
<contactref element="LED2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
