(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "IN1")
  (net 2 "IN2")
  (net 3 "IN3")
  (net 4 "GND")
  (net 5 "IN4")
  (net 6 "OUTA")
  (net 7 "OUTB")
  (net 8 "OUTC")
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126.492 84.455)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at -3.302 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 145.415 93.98)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -1.397 -2.032 45) (layer "F.SilkS"))
    (fp_text value "Conn_02x04_Odd_Even" (at 1.27 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "OUTB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "OUTC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 126.365 93.98)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -1.397 -2.032 45) (layer "F.SilkS"))
    (fp_text value "Conn_02x04_Odd_Even" (at 1.27 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "IN4") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "IN4") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "OUTB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "IN4") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "OUTC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "IN4") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.828 84.455)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "footprints:KPJX-4S" (layer "F.Cu")
    (tedit 5BFBD38F)
    (at 137.16 83.82)
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -5.842 -5.969) (layer "F.SilkS"))
    (fp_text value "Conn_01x09" (at 0 -8.89) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.5 -3.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.5 -3.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 2.9 3.65) (size 4 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_1") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval (at -2.9 3.65) (size 4 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.5 0) (size 4 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_3") (pintype "passive") (zone_connect 2))
    (pad "4" thru_hole oval (at -2.5 0) (size 4 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 5 "IN4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.5) (size 3.4 2) (drill oval 2.2 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -7.8 5) (size 2 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 7.8 5) (size 2 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -7.8 -3.5) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 7.8 -3.5) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (model "D:/Notas prace/kicad_libs_prusa/User Library-KPJX-4S-S.step"
      (offset (xyz 0 -6.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 130.81 105.918 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.778 -1.524 45) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTA") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "OUTB") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "OUTC") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 139.065 93.98)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -1.397 -2.032 45) (layer "F.SilkS"))
    (fp_text value "Conn_02x04_Odd_Even" (at 1.27 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "OUTB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "OUTC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.828 105.791)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126.492 105.791)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at -3.556 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 132.715 93.98)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "kpjx-4s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -1.397 -2.032 45) (layer "F.SilkS"))
    (fp_text value "Conn_02x04_Odd_Even" (at 1.27 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "OUTB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "OUTC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 150.114 105.797433) (mid 149.44633 107.40933) (end 147.834433 108.077) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 147.831217 76.962) (end 126.488784 76.962) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 124.209217 79.241567) (end 124.206 105.797433) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 126.485567 108.077) (mid 124.87367 107.40933) (end 124.206 105.797433) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 126.485567 108.077) (end 147.834433 108.077) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 124.209217 79.241567) (mid 124.876896 77.629679) (end 126.488784 76.962) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 147.831217 76.962) (mid 149.443126 77.629668) (end 150.110784 79.241567) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150.114 105.797433) (end 150.110784 79.241567) (layer "Edge.Cuts") (width 0.1))
  (gr_text "github.com/xunker/kycon_breakout" (at 137.16 103.886) (layer "B.SilkS"))
  (gr_text "4" (at 132.461 83.82) (layer "B.SilkS"))
  (gr_text "KYCON© KPJX-4S BREAKOUT" (at 137.16 91.8972) (layer "B.SilkS"))
  (gr_text "3" (at 141.859 83.82) (layer "B.SilkS"))
  (gr_text "1" (at 142.24 87.376) (layer "B.SilkS"))
  (gr_text "2" (at 132.08 87.63) (layer "B.SilkS"))
  (gr_text "C" (at 137.668 99.06) (layer "F.SilkS"))
  (gr_text "C" (at 143.891 99.06) (layer "F.SilkS"))
  (gr_text "B" (at 143.891 96.52) (layer "F.SilkS"))
  (gr_text "GND" (at 143.51 104.14) (layer "F.SilkS"))
  (gr_text "A" (at 143.891 93.98) (layer "F.SilkS"))
  (gr_text "A" (at 130.81 103.886) (layer "F.SilkS"))
  (gr_text "PIN 2" (at 134.874 91.694) (layer "F.SilkS"))
  (gr_text "PIN 3" (at 147.574 91.694) (layer "F.SilkS"))
  (gr_text "B" (at 137.668 96.52) (layer "F.SilkS"))
  (gr_text "C" (at 131.318 99.06) (layer "F.SilkS"))
  (gr_text "GND" (at 138.46 104.14) (layer "F.SilkS"))
  (gr_text "A" (at 131.191 93.98) (layer "F.SilkS"))
  (gr_text "C" (at 140.97 103.886) (layer "F.SilkS"))
  (gr_text "B" (at 135.89 103.886) (layer "F.SilkS"))
  (gr_text "GND" (at 130.81 101.6 90) (layer "F.SilkS"))
  (gr_text "BOARD\n©2024" (at 143.51 84.709 90) (layer "F.SilkS"))
  (gr_text "GND" (at 133.35 104.14) (layer "F.SilkS"))
  (gr_text "PIN 4" (at 128.524 91.694) (layer "F.SilkS"))
  (gr_text "A" (at 137.668 93.98) (layer "F.SilkS"))
  (gr_text "GND" (at 143.51 101.6 90) (layer "F.SilkS"))
  (gr_text "B" (at 131.318 96.52) (layer "F.SilkS"))
  (gr_text "GND" (at 137.16 101.6 90) (layer "F.SilkS"))
  (gr_text "PIN 1" (at 141.224 91.694) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 126.492 105.791) (xy 147.828 105.791))
    (height 7.239)
    (gr_text "21.3360 mm" (at 137.16 111.88) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 126.492 84.455) (xy 126.492 105.7974))
    (height 5.334)
    (gr_text "21.3424 mm" (at 120.008 95.1262 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 150.114 76.962) (xy 150.114 108.077))
    (height -1.905)
    (gr_text "31.1150 mm" (at 150.869 92.5195 90) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 124.206 109.22) (xy 150.114 109.22))
    (height 2.54)
    (gr_text "25.9080 mm" (at 137.16 110.61) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 4) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.94 114.3)
        (xy 116.84 114.3)
        (xy 116.84 71.12)
        (xy 154.94 71.12)
      )
    )
  )
)
