(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 89)
    (no_connects 0)
    (area 140.354429 77.0395 183.876572 105.375)
    (thickness 1.6)
    (drawings 21)
    (tracks 444)
    (zones 0)
    (modules 32)
    (nets 39)
  )
  (page A4)
  (title_block
    (title sharpbreak)
    (date 2016-10-02)
    (rev 0.01)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (trace_clearance 0.1)
    (zone_clearance 0.7)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 R0)
  (net 2 R1)
  (net 3 R2)
  (net 4 R3)
  (net 5 R4)
  (net 6 R5)
  (net 7 R6)
  (net 8 R7)
  (net 9 G0)
  (net 10 G1)
  (net 11 G2)
  (net 12 G3)
  (net 13 G4)
  (net 14 G5)
  (net 15 G6)
  (net 16 G7)
  (net 17 B0)
  (net 18 B1)
  (net 19 B2)
  (net 20 B3)
  (net 21 B4)
  (net 22 B5)
  (net 23 B6)
  (net 24 B7)
  (net 25 GND)
  (net 26 VCC_2V5)
  (net 27 VSYNC)
  (net 28 HSYNC)
  (net 29 CLOCK)
  (net 30 BACKL_EN)
  (net 31 V_LED_CATHODE)
  (net 32 V_LED_ANODE)
  (net 33 "Net-(C5-Pad2)")
  (net 34 "Net-(R10-Pad1)")
  (net 35 VCC_5V)
  (net 36 "Net-(L1-Pad2)")
  (net 37 DISP_ENABLE)
  (net 38 /LED_VIN)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R10-Pad1)")
  )
  (net_class PWR ""
    (clearance 0.1)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LED_VIN)
    (add_net GND)
    (add_net VCC_2V5)
    (add_net VCC_5V)
    (add_net V_LED_ANODE)
    (add_net V_LED_CATHODE)
  )
  (net_class SIG ""
    (clearance 0.1)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net B0)
    (add_net B1)
    (add_net B2)
    (add_net B3)
    (add_net B4)
    (add_net B5)
    (add_net B6)
    (add_net B7)
    (add_net BACKL_EN)
    (add_net CLOCK)
    (add_net DISP_ENABLE)
    (add_net G0)
    (add_net G1)
    (add_net G2)
    (add_net G3)
    (add_net G4)
    (add_net G5)
    (add_net G6)
    (add_net G7)
    (add_net HSYNC)
    (add_net R0)
    (add_net R1)
    (add_net R2)
    (add_net R3)
    (add_net R4)
    (add_net R5)
    (add_net R6)
    (add_net R7)
    (add_net VSYNC)
  )
  (module mylib:sc70-6_mod0 (layer F.Cu) (tedit 57F1CB41)
    (at 179.1995 92.66 270)
    (descr SC70-6)
    (fp_text reference U1 (at -0.077 -2.0295 270) (layer F.SilkS))
    (fp_text value TPS61220-22 (at 0 0.3556 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.66 1.016 270) (size 0.35 0.66) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5) (clearance 0.2))
    (pad 3 smd rect (at 0.66 1.016 270) (size 0.35 0.66) (layers F.Cu F.Paste F.Mask)
      (net 25 GND) (clearance 0.2))
    (pad 2 smd rect (at 0 1.016 270) (size 0.35 0.66) (layers F.Cu F.Paste F.Mask)
      (net 35 VCC_5V) (clearance 0.2))
    (pad 4 smd rect (at 0.66 -1.016 270) (size 0.35 0.66) (layers F.Cu F.Paste F.Mask)
      (net 35 VCC_5V) (clearance 0.2))
    (pad 6 smd rect (at -0.66 -1.016 270) (size 0.35 0.66) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5) (clearance 0.2))
    (pad 5 smd rect (at 0 -1.016 270) (size 0.35 0.66) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(L1-Pad2)") (clearance 0.2))
    (model walter/smd_trans/sc70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 57F1D021)
    (at 150.5585 93.091 270)
    (descr SOT23-6)
    (fp_text reference U2 (at 1.9685 1.0795 360) (layer F.SilkS))
    (fp_text value LT1932 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 38 /LED_VIN))
    (pad 3 smd rect (at 0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 31 V_LED_CATHODE))
    (pad 2 smd rect (at 0 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 4 smd rect (at 0.9525 -1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R10-Pad1)"))
    (pad 6 smd rect (at -0.9525 -1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 5 smd rect (at 0 -1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 BACKL_EN))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_diode:sod323 (layer F.Cu) (tedit 57F1C801)
    (at 147.0025 92.0115 180)
    (descr SOD323)
    (fp_text reference D1 (at -0.0635 1.2065 180) (layer F.SilkS))
    (fp_text value DIODESCH (at 0 1.19888 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.09982 0 180) (size 1.00076 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 32 V_LED_ANODE))
    (pad 1 smd rect (at -1.09982 0 180) (size 1.00076 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 38 /LED_VIN))
    (model walter/smd_diode/sod323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C89)
    (at 145.2245 81.0895)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at -0.3175 0.889) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 R1))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 R0))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C87)
    (at 146.558 82.042)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at 0 0.9525) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 R2))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 R1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C84)
    (at 147.7645 81.0895)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at 0.9525 0.889) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 R3))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 R2))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C7E)
    (at 155.067 81.0895)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at 0.4445 0.889) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 G1))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 G0))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C7C)
    (at 157.734 81.0895)
    (descr "SMT resistor, 0402")
    (fp_text reference R5 (at 0.6985 0.889) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 G2))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 G1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C10)
    (at 165.735 81.026)
    (descr "SMT resistor, 0402")
    (fp_text reference R6 (at -0.0635 0.8255) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 B1))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 B0))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C0D)
    (at 166.9415 81.9785)
    (descr "SMT resistor, 0402")
    (fp_text reference R7 (at 0 0.889) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 B2))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 B1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C0B)
    (at 168.2115 81.026)
    (descr "SMT resistor, 0402")
    (fp_text reference R8 (at 0.762 0.8255) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 B3))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 B2))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F1C39C)
    (at 145.8595 97.5995 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R9 (at 0.0254 -0.8509 270) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F1C38F)
    (at 151.13 95.0595)
    (descr "SMT resistor, 0402")
    (fp_text reference R10 (at -0.0254 0.889) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F1CCE1)
    (at 153.289 93.091 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R11 (at -0.3175 -0.8255 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 BACKL_EN))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 57F1F515)
    (at 179.197 84.074 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 1.651 -0.127 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 57F1C7FE)
    (at 146.939 93.6625 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C3 (at 2.032 0 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0.9906 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 32 V_LED_ANODE))
    (pad 2 smd rect (at -0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 57F1C397)
    (at 145.8595 95.4405 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C5 (at 0.0508 -0.8255 90) (layer F.SilkS))
    (fp_text value 47n (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 32 V_LED_ANODE))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 57F1D034)
    (at 153.9875 90.7415 270)
    (descr "SMT capacitor, 0805")
    (fp_text reference C7 (at -0.1905 -1.3335 270) (layer F.SilkS))
    (fp_text value 4u7 (at 0 0.9906 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 270) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 2 smd rect (at -0.9525 0 270) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_8x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C83)
    (at 149.098 79.8195)
    (fp_text reference P1 (at 1.27 1.2065) (layer F.SilkS) hide)
    (fp_text value CONN_8 (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -4.445 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 1 R0))
    (pad 2 thru_hole circle (at -3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 2 R1))
    (pad 3 thru_hole circle (at -1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 3 R2))
    (pad 4 thru_hole circle (at -0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 4 R3))
    (pad 5 thru_hole circle (at 0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 5 R4))
    (pad 6 thru_hole circle (at 1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 6 R5))
    (pad 7 thru_hole circle (at 3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 7 R6))
    (pad 8 thru_hole circle (at 4.445 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 8 R7))
  )
  (module mylib:pin_header_8x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C79)
    (at 159.258 79.8195)
    (fp_text reference P2 (at -0.127 1.2065) (layer F.SilkS) hide)
    (fp_text value CONN_8 (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -4.445 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 9 G0))
    (pad 2 thru_hole circle (at -3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 10 G1))
    (pad 3 thru_hole circle (at -1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 11 G2))
    (pad 4 thru_hole circle (at -0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 12 G3))
    (pad 5 thru_hole circle (at 0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 13 G4))
    (pad 6 thru_hole circle (at 1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 14 G5))
    (pad 7 thru_hole circle (at 3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 15 G6))
    (pad 8 thru_hole circle (at 4.445 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 16 G7))
  )
  (module mylib:pin_header_8x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C09)
    (at 169.418 79.8195)
    (fp_text reference P3 (at 0.635 1.2065) (layer F.SilkS) hide)
    (fp_text value CONN_8 (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -4.445 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 17 B0))
    (pad 2 thru_hole circle (at -3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 18 B1))
    (pad 3 thru_hole circle (at -1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 19 B2))
    (pad 4 thru_hole circle (at -0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 20 B3))
    (pad 5 thru_hole circle (at 0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 21 B4))
    (pad 6 thru_hole circle (at 1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 22 B5))
    (pad 7 thru_hole circle (at 3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 23 B6))
    (pad 8 thru_hole circle (at 4.445 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 24 B7))
  )
  (module mylib:pin_header_2x1_1.27mm_pitch (layer F.Cu) (tedit 57F09BF7)
    (at 180.848 79.8195 180)
    (fp_text reference P4 (at -0.152 -1.4665 180) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 1.905 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 25 GND))
    (pad 2 thru_hole circle (at 0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 26 VCC_2V5))
  )
  (module mylib:pin_header_4x1_1.27mm_pitch (layer F.Cu) (tedit 57F18BF1)
    (at 177.038 79.8195 180)
    (fp_text reference P5 (at 0 -1.2065 180) (layer F.SilkS) hide)
    (fp_text value CONN_4 (at 0 1.905 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 27 VSYNC))
    (pad 2 thru_hole circle (at -0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 28 HSYNC))
    (pad 3 thru_hole circle (at 0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 37 DISP_ENABLE))
    (pad 4 thru_hole circle (at 1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 29 CLOCK))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C8C)
    (at 143.383 79.8195)
    (fp_text reference P6 (at 0 1.2065) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 30 BACKL_EN))
  )
  (module mylib:WM1386CT-ND (layer F.Cu) (tedit 57F1C80B)
    (at 151.35 98.45)
    (fp_text reference P7 (at 0.034 -1.1045) (layer F.SilkS))
    (fp_text value CONN_4 (at 1.05 5.95) (layer F.Fab) hide)
    (pad "" connect rect (at 1.65 2.8) (size 0.5 1) (layers F.Cu F.Mask))
    (pad 3 smd rect (at 0.25 0) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.75 0) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 32 V_LED_ANODE))
    (pad 2 smd rect (at -0.25 0) (size 0.3 1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -0.75 0) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 31 V_LED_CATHODE))
    (pad "" connect rect (at -1.65 2.8) (size 0.5 1) (layers F.Cu F.Mask))
  )
  (module w_smd_cap:c_0603 (layer F.Cu) (tedit 57F13BA1)
    (at 176.911 92.6465 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C4 (at 0.0135 -1.0185 90) (layer F.SilkS))
    (fp_text value 10u (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.Cu) (tedit 57F09CB8)
    (at 179.197 94.615)
    (descr "SMT capacitor, 0603")
    (fp_text reference C6 (at 1.8505 0.0675) (layer F.SilkS))
    (fp_text value 10u (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 35 VCC_5V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:l_1210 (layer F.Cu) (tedit 57F191AD)
    (at 150.5585 89.9795 180)
    (descr "SMT resistor, 1210")
    (fp_text reference L2 (at -0.0635 1.8415 180) (layer F.SilkS))
    (fp_text value 6u8 (at 0 1.7018 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 38 /LED_VIN))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:inductor_smd_1008_mod (layer F.Cu) (tedit 57F1F5A3)
    (at 178.943 89.5985)
    (descr "Inductor SMD, 1008")
    (fp_text reference L1 (at -2.667 -0.1905 90) (layer F.SilkS))
    (fp_text value 4u7 (at 1.3505 -2.2255) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.3 0) (size 1.7 3.3) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 2 smd rect (at 1.3 -0.05) (size 1.7 3.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(L1-Pad2)"))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:62684-401100ALF (layer F.Cu) (tedit 57F2C489)
    (at 168.65 98.3)
    (fp_text reference P8 (at -13.0115 1.3315 90) (layer F.SilkS))
    (fp_text value LQ043T3DX02 (at 0.9 2.7) (layer F.Fab) hide)
    (fp_text user 40 (at 10.5 -0.7) (layer F.SilkS))
    (fp_text user 1 (at -10.3 -0.7) (layer F.SilkS))
    (pad "" connect rect (at 11.6 2.7 180) (size 1.6 2.4) (layers F.Cu F.Mask))
    (pad "" connect rect (at 12.8 3.1 180) (size 0.8 1.6) (layers F.Cu F.Mask))
    (pad "" connect rect (at -12.8 3.1) (size 0.8 1.6) (layers F.Cu F.Mask))
    (pad 1 smd rect (at -9.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 8 smd rect (at -6.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 R3))
    (pad 9 smd rect (at -5.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 R4))
    (pad 7 smd rect (at -6.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 R2))
    (pad 6 smd rect (at -7.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 R1))
    (pad 2 smd rect (at -9.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 3 smd rect (at -8.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 5 smd rect (at -7.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 R0))
    (pad 4 smd rect (at -8.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 36 smd rect (at 7.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 VCC_5V))
    (pad 37 smd rect (at 8.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 7.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 VCC_5V))
    (pad 34 smd rect (at 6.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 8.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 9.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 40 smd rect (at 9.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 32 smd rect (at 5.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 HSYNC))
    (pad 33 smd rect (at 6.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 VSYNC))
    (pad 31 smd rect (at 5.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 DISP_ENABLE))
    (pad 30 smd rect (at 4.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 CLOCK))
    (pad 26 smd rect (at 2.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 B5))
    (pad 27 smd rect (at 3.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 B6))
    (pad 29 smd rect (at 4.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 28 smd rect (at 3.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 B7))
    (pad 12 smd rect (at -4.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 R7))
    (pad 13 smd rect (at -3.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 G0))
    (pad 11 smd rect (at -4.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 R6))
    (pad 10 smd rect (at -5.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 R5))
    (pad 14 smd rect (at -3.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 G1))
    (pad 15 smd rect (at -2.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 G2))
    (pad 17 smd rect (at -1.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 G4))
    (pad 16 smd rect (at -2.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 G3))
    (pad 24 smd rect (at 1.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 B3))
    (pad 25 smd rect (at 2.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 B4))
    (pad 23 smd rect (at 1.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 B2))
    (pad 22 smd rect (at 0.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 B1))
    (pad 18 smd rect (at -1.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 G5))
    (pad 19 smd rect (at -0.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 G6))
    (pad 21 smd rect (at 0.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 B0))
    (pad 20 smd rect (at -0.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 G7))
    (pad "" connect rect (at -11.6 2.7) (size 1.6 2.4) (layers F.Cu F.Mask))
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 57F1F504)
    (at 179.197 85.598 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C1 (at 2.159 0 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0.9906 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 26 VCC_2V5))
    (pad 2 smd rect (at -0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:sot23_mod0 (layer F.Cu) (tedit 57F622A2)
    (at 147.955 96.5835)
    (descr SOT23)
    (fp_text reference Q1 (at -0.889 -1.2065 180) (layer F.SilkS))
    (fp_text value NPN (at 0 0.3302) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 3 smd rect (at 0 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 32 V_LED_ANODE))
    (pad 1 smd rect (at 0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 31 V_LED_CATHODE))
    (model walter/smd_trans/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 182.3085 78.994) (end 142.5575 78.994) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.3085 102.6795) (end 182.3085 78.994) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.5575 102.6795) (end 182.3085 102.6795) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.5575 78.994) (end 142.5575 102.6795) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 0 (at 144.5895 82.2325) (layer F.SilkS))
  (gr_text 0 (at 154.813 82.2325) (layer F.SilkS))
  (gr_text 0 (at 165.1 82.2325) (layer F.SilkS))
  (gr_text BACKLIGHT_EN (at 143.383 80.5815 90) (layer F.SilkS))
  (gr_text BLUE (at 172.847 82.2325) (layer F.SilkS))
  (gr_text GREEN (at 162.433 82.2325) (layer F.SilkS))
  (gr_text RED (at 152.8445 82.2325) (layer F.SilkS))
  (gr_text "CLOCK\n" (at 175.133 80.518 90) (layer F.SilkS))
  (gr_text DISP_EN (at 176.403 80.518 90) (layer F.SilkS))
  (gr_text HSYNC (at 177.673 80.5815 90) (layer F.SilkS))
  (gr_text VSYNC (at 178.943 80.5815 90) (layer F.SilkS))
  (gr_text "sharpbreak\nrev0.01\nrel/2016" (at 174.371 86.9315) (layer F.SilkS))
  (gr_text GND (at 181.483 80.518 90) (layer F.SilkS))
  (gr_text VCC3V3 (at 180.213 80.5815 90) (layer F.SilkS))
  (zone (net 25) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.3085 102.6795) (xy 142.5575 102.6795) (xy 142.5575 78.994) (xy 182.3085 78.994)
      )
    )
  )
  (zone (net 25) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.3085 102.6795) (xy 142.5575 102.6795) (xy 142.5575 78.994) (xy 182.3085 78.994)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.3365 97.2185) (xy 151.13 97.2185) (xy 150.0505 96.139) (xy 150.0505 95.504) (xy 152.3365 95.504)
      )
    )
  )
)
